**3GPP TSG-RAN WG2 Meeting #119e R2-2208849**

**E-Meeting, May 9-20, 2022**

**Title: [Draft]**LS on missing RRC parameter in IUC Scheme 2

**Response to:**

**Release:** Rel-17

**Work Item:** NR\_SL\_enh-Core

**Source:** Apple [To be RAN2]

**To:** RAN1

**Cc:**

**Contact Person:**

#### Name: Zhibin Wu

E-mail Address: <zhibin\_wu@apple.com>

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** none

**1. Overall Description:**

According to TS 38.213, for one of the options used to determine the conflict resource in IUC Scheme 2, there is a “delta RSRP threshold” parameter which is needed to be (pre-)configured by RRC layer. However, this parameter was not included in the original RRC parameter list from RAN1, thereby missing in current TS 38.331.

RAN2 has agreed to add “*deltaRSRP-Threshold*” parameter in the RRC specification to ensure IUC Scheme 2 can be correctly implemented in Rel-17.

Also, RAN2 assumes the same value range as normal sidelink RSRP threshold, i.e., (0..66) may be used for this new parameter. RAN2 would like to ask RAN1 to check whether this is appropriate or not.

**2. Actions:**

**To RAN1**: RAN2 respec tfully requests RAN1 to provide confirmation of the above RAN2 agreement and assumption on the value range for this new parameter, or feedback if any concern.

**3. Dates of Next TSG-RAN WG2 Meetings:**

TSG RAN WG2 Meeting #119bis October 10 – October 19 2022 E-meeting

TSG RAN WG2 Meeting #120 November 14 – November 18 2022 Europe (TBD)