**3GPP TSG-RAN WG2 Meeting #119e R2-2208849**

**E-Meeting, November 17-29, 2022**

**Title: [Draft]**LS on missing RRC parameter in IUC Scheme 2

**Response to:**

**Release:** Rel-17

**Work Item:** NR\_SL\_enh-Core

**Source:** Apple [To be RAN2]

**To:** RAN1

**Cc:**

**Contact Person:**

#### Name: Zhibin Wu

E-mail Address: <zhibin\_wu@apple.com>

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** none

**1. Overall Description:**

According to TS 38.213, for one of the options used to determine the conflict resource in IUC Scheme 2, there is a “delta RSRP threshold” parameter which is needed to be (pre-)configured by RRC layer. However, this parameter was not included in the original RRC parameter list from RAN1, thereby missing in current TS 38.331.

RAN2 has agreed to add “*deltaRSRP-Threshold*” parameter in the RRC specification to ensure IUC Scheme 2 can be correctly implemented in Rel-17.

Also, RAN2 assumes the same value range as normal sidelink RSRP threshold, i.e., (0..66) used for another IUC parameter *sl-ThresholdRSRP-Condition1-B-1-r17*, may be used for this new parameter. RAN2 would like to ask RAN1 to check whether this is appropriate or not.

**2. Actions:**

**To RAN1**: RAN2 respec tfully requests RAN1 to provide confirmation of the above RAN2 agreement and assumption on the value range for this new parameter, or feedback if any concern.

**3. Dates of Next TSG-RAN WG2 Meetings:**

TSG RAN WG2 Meeting #119bis October 10 – October 19 2022 E-meeting

TSG RAN WG2 Meeting #120 November 14 – November 18 2022 Europe (TBD)