**3GPP TSG- Meeting #**

**, , 26 Feb. – 1 Mar. 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | 1275 | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on MBS RAN sharing |
|  |  |
| ***Source to WG:*** | Samsung, Huawei, CBN, CATT, Nokia, Nokia Shanghai Bell, CMCC, Qualcomm, Ericsson, ZTE, Levono |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_MBS\_enh-Core |  | ***Date:*** | 2024-02-19 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In multiple cell broadcasting scenario, when the gNB-DU initiated F1-U setup by using BROADCAST TRANSPORT RESOURCE REQUEST message, it is beneficial that the gNB-DU can include *MRB ID* IEand *BC Bearer Context F1-U TNL Info at DU* IE in the message. Then the gNB-CU-CP sends BROADCAST BEARER MODIFICATION REQUEST message to the gNB-CU-UP, including *MRB ID* IE and *BC Bearer Context F1-U TNL Info at DU* IE. Currently the *F1-U tunnel Not Established* IE is introduced per MBS Session, in such case, in some scenarios, the gNB-CU and gNB-DU has to establish F1-U tunnels multiple times for some area sessions. In order to fulfil the agreement and avoid unnecessary cost, it is needed to introduce the *F1-U tunnel Not Established* IE also in per Area Session granularity. |
|  |  |
| ***Summary of change:*** | Include *MRB ID* IEand *BC Bearer Context F1-U TNL Info at DU* IE in BROADCAST TRANSPORT RESOURCE REQUEST message.Remove the *F1-U tunnel Not Established* IE in the BROADCAST CONTEXT SETUP RESPONSE message.Introduce *F1-U tunnel Not Established* IE in the *BC Bearer Context F1-U TNL Info* IE, in the location independent branch for the MBS session, and also in the location dependent branch in per Area Session granularity.Impact analysis:Impact assessment towards the previous version of the specification (same release):**The CR is non-backward compatible.**  |
|  |  |
| ***Consequences if not approved:*** | Unnecessary signalling and cost foreseen. |
|  |  |
| ***Clauses affected:*** | 9.2.13.2, 9.2.13.9, 9.3.2.7, 9.4.4, 9.4.5,  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<<<<<<<<<<<<<<<<<<<< First Change >>>>>>>>>>>>>>>>>>>>

#### 9.2.13.2 BROADCAST CONTEXT SETUP RESPONSE

This message is sent by the gNB-DU to confirm the setup of a broadcast context.

Direction: gNB-DU → gNB-CU.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU MBS F1AP ID | M |  | 9.3.1.219 |  | YES | reject |
| gNB-DU MBS F1AP ID | M |  | 9.3.1.220 |  | YES | reject |
| **Broadcast MRB Setup List** |  | *1* |  |  | YES | reject |
| **>Broadcast MRB Setup Item IEs** |  | *1 .. <maxnoofMRBs>* |  |  | EACH | reject |
| >>MRB ID | M |  | MRB ID9.3.1.224 |  | - |  |
| >>BC Bearer Context F1-U TNL Info at DU | M |  | BC Bearer Context F1-U TNL Info9.3.2.7 | gNB-DU endpoint(s) of the F1-U transport bearer(s). For delivery of DL PDUs. | - |  |
| **Broadcast MRB Failed To Be Setup List** |  | *0..1* |  |  | YES | ignore |
| **>Broadcast MRB Failed To Be Setup Item IEs** |  | *1 .. <maxnoofMRBs>* |  |  | EACH | ignore |
| >>MRB ID | M |  | MRB ID9.3.1.224 |  | - |  |
| >>Cause | O |  | 9.3.1.2 |  | - |  |
| Broadcast Area Scope | O |  | 9.3.1.287 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |
|  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| *maxnoofMRBs* | Maximum no. of MRB allowed to be setup for one MBS Session, the maximum value is 32. |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

#### 9.2.13.9 BROADCAST TRANSPORT RESOURCE REQUEST

This message is sent by the gNB-DU to request the gNB-CU to establish the F1-U resources for the broadcast Session.

Direction: gNB-DU → gNB-CU

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU MBS F1AP ID | M |  | 9.3.1.219 |  | YES | reject |
| gNB-DU MBS F1AP ID | M |  | 9.3.1.220 |  | YES | reject |
| **Broadcast MRB Transport Request List** |  | *0..1* |  |  | YES | reject |
| **>Broadcast MRB Transport Request Item IEs** |  | *1 .. <maxnoofMRBs>* |  |  | EACH | reject |
| >>MRB ID | M |  | MRB ID9.3.1.224 |  | - |  |
| >>BC Bearer Context F1-U TNL Info at DU | M |  | BC Bearer Context F1-U TNL Info9.3.2.7 | gNB-DU endpoint(s) of the F1-U transport bearer(s). For delivery of DL PDUs. | - |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| *maxnoofMRBs* | Maximum no. of MRB allowed to be setup for one MBS Session, the maximum value is 32. |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

#### 9.3.2.7 BC Bearer Context F1-U TNL Info

This IE contains F1-U TNL information for an MBS Session. In case of location dependent MBS sessions, it also contains per Area Session ID F1-U TNL information.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| CHOICE *MBS Session Type* | M |  |  |  | - | - |
| *>location independent* |  |  |  |  |  |  |
| >>MBS F1-U Information | M |  | UP Transport Layer Information9.3.2.1 |  | - | - |
| >>F1-U Tunnel Not Established | O |  | ENUMERATED (true, ...) | Indicates F1-U tunnel not established for this MBS Session. | YES | ignore |
| *>location dependent* |  |  |  |  |  |  |
| **>>Location dependent MBS F1-U Information Item** |  | *1..<maxnoofMBSAreaSessionIDs>* |  |  | - | - |
| >>>MBS Area Session ID | M |  | 9.3.1.221 |  | - | - |
| >>>MBS F1-U Information | M |  | UP Transport Layer Information9.3.2.1 |  | - | - |
| >>>F1-U Tunnel Not Established | O |  | ENUMERATED (true, ...) | Indicates F1-U tunnel not established for this MBS Session. | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofMBSAreaSessionIDs | Maximum no. of MBS Area Session IDs. Value is 256. |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for F1AP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 AssociatedSessionID,

 BroadcastMRBs-FailedToBeModified-Item,

 BroadcastMRBs-FailedToBeSetup-Item,

 BroadcastMRBs-FailedToBeSetupMod-Item,

 BroadcastMRBs-Modified-Item,

 BroadcastMRBs-Setup-Item,

 BroadcastMRBs-SetupMod-Item,

 BroadcastMRBs-ToBeModified-Item,

 BroadcastMRBs-ToBeReleased-Item,

 BroadcastMRBs-ToBeSetup-Item,

 BroadcastMRBs-ToBeSetupMod-Item,

 Candidate-SpCell-Item,

 Cause,

 Cells-Allowed-to-be-Deactivated-List-Item,

 Cells-Failed-to-be-Activated-List-Item,

 Cells-Status-Item,

 Cells-to-be-Activated-List-Item,

 Cells-to-be-Deactivated-List-Item,

 CellULConfigured,

 CriticalityDiagnostics,

 C-RNTI,

 CUtoDURRCInformation,

 DRB-Activity-Item,

 DRBID,

 DRBs-FailedToBeModified-Item,

 DRBs-FailedToBeSetup-Item,

 DRBs-FailedToBeSetupMod-Item,

 DRB-Notify-Item,

 DRBs-ModifiedConf-Item,

 DRBs-Modified-Item,

 DRBs-Required-ToBeModified-Item,

 DRBs-Required-ToBeReleased-Item,

 DRBs-Setup-Item,

 DRBs-SetupMod-Item,

 DRBs-ToBeModified-Item,

 DRBs-ToBeReleased-Item,

 DRBs-ToBeSetup-Item,

 DRBs-ToBeSetupMod-Item,

 DRXCycle,

 DRXConfigurationIndicator,

 DUtoCURRCInformation,

 EUTRANQoS,

 ExecuteDuplication,

 FullConfiguration,

 GNB-CU-MBS-F1AP-ID,

 GNB-CU-UE-F1AP-ID,

 GNB-DU-MBS-F1AP-ID,

 GNB-DU-UE-F1AP-ID,

 GNB-DU-ID,

 GNB-DU-Served-Cells-Item,

 GNB-DU-System-Information,

 GNB-CU-Name,

 GNB-DU-Name,

 InactivityMonitoringRequest,

 InactivityMonitoringResponse,

 LowerLayerPresenceStatusChange,

 MBS-Area-Session-ID,

 MBS-CUtoDURRCInformation,

 MBSMulticastF1UContextDescriptor,

 MBS-Session-ID,

 MBS-ServiceArea,

 MulticastF1UContextReferenceCU,

 MulticastF1UContext-ToBeSetup-Item,

 MulticastF1UContext-Setup-Item,

 MulticastF1UContext-FailedToBeSetup-Item,

 MulticastMBSSessionList,

 MulticastMRBs-ToBeSetup-Item,

 MulticastMRBs-Setup-Item,

 MulticastMRBs-FailedToBeSetup-Item,

 MulticastMRBs-ToBeSetupMod-Item,

 MulticastMRBs-ToBeModified-Item,

 MulticastMRBs-ToBeReleased-Item,

 MulticastMRBs-SetupMod-Item,

 MulticastMRBs-FailedToBeSetupMod-Item,

 MulticastMRBs-Modified-Item,

 MulticastMRBs-FailedToBeModified-Item,

 BroadcastAreaScope,

 NetworkControlledRepeaterAuthorized,

 NotificationControl,

 NRCGI,

 NRPCI,

 UEContextNotRetrievable,

 Potential-SpCell-Item,

 RAT-FrequencyPriorityInformation,

 RequestedSRSTransmissionCharacteristics,

 ResourceCoordinationTransferContainer,

 RRCContainer,

 RRCContainer-RRCSetupComplete,

 RRCReconfigurationCompleteIndicator,

 SCellIndex,

 SCell-ToBeRemoved-Item,

 SCell-ToBeSetup-Item,

 SCell-ToBeSetupMod-Item,

 SCell-FailedtoSetup-Item,

 SCell-FailedtoSetupMod-Item,

 SDT-Volume-Threshold,

 ServCellIndex,

 Served-Cell-Information,

 Served-Cells-To-Add-Item,

 Served-Cells-To-Delete-Item,

 Served-Cells-To-Modify-Item,

 ServingCellMO,

 SNSSAI,

 SRBID,

 SRBs-FailedToBeSetup-Item,

 SRBs-FailedToBeSetupMod-Item,

 SRBs-Required-ToBeReleased-Item,

 SRBs-ToBeReleased-Item,

 SRBs-ToBeSetup-Item,

 SRBs-ToBeSetupMod-Item,

 SRBs-Modified-Item,

 SRBs-Setup-Item,

 SRBs-SetupMod-Item,

 SupportedUETypeList,

 TimeToWait,

 TransactionID,

 TransmissionActionIndicator,

 UE-associatedLogicalF1-ConnectionItem,

 UEIdentity-List-For-Paging-Item,

 DUtoCURRCContainer,

 PagingCell-Item,

 SItype-List,

 UEIdentityIndexValue,

 GNB-CU-TNL-Association-Setup-Item,

 GNB-CU-TNL-Association-Failed-To-Setup-Item,

 GNB-CU-TNL-Association-To-Add-Item,

 GNB-CU-TNL-Association-To-Remove-Item,

 GNB-CU-TNL-Association-To-Update-Item,

 MaskedIMEISV,

 PagingDRX,

 PagingPriority,

 PagingIdentity,

 Cells-to-be-Barred-Item,

 PWSSystemInformation,

 Broadcast-To-Be-Cancelled-Item,

 Cells-Broadcast-Cancelled-Item,

 NR-CGI-List-For-Restart-Item,

 PWS-Failed-NR-CGI-Item,

 RepetitionPeriod,

 NumberofBroadcastRequest,

 Cells-To-Be-Broadcast-Item,

 Cells-Broadcast-Completed-Item,

 Cancel-all-Warning-Messages-Indicator,

 EUTRA-NR-CellResourceCoordinationReq-Container,

 EUTRA-NR-CellResourceCoordinationReqAck-Container,

 RequestType,

 PLMN-Identity,

 RLCFailureIndication,

 UplinkTxDirectCurrentListInformation,

 SULAccessIndication,

 Protected-EUTRA-Resources-Item,

 GNB-DUConfigurationQuery,

 BitRate,

 RRC-Version,

 GNBDUOverloadInformation,

 RRCDeliveryStatusRequest,

 NeedforGap,

 RRCDeliveryStatus,

 ResourceCoordinationTransferInformation,

 Dedicated-SIDelivery-NeededUE-Item,

 Associated-SCell-Item,

 IgnoreResourceCoordinationContainer,

 PagingOrigin,

 UAC-Assistance-Info,

 RANUEID,

 GNB-DU-TNL-Association-To-Remove-Item,

 NotificationInformation,

 TraceActivation,

 TraceID,

 Neighbour-Cell-Information-Item,

 SymbolAllocInSlot,

 NumDLULSymbols,

 AdditionalRRMPriorityIndex,

 DUCURadioInformationType,

 CUDURadioInformationType,

 Transport-Layer-Address-Info,

 BHChannels-ToBeSetup-Item,

 BHChannels-Setup-Item,

 BHChannels-FailedToBeSetup-Item,

 BHChannels-ToBeModified-Item,

 BHChannels-ToBeReleased-Item,

 BHChannels-ToBeSetupMod-Item,

 BHChannels-FailedToBeModified-Item,

 BHChannels-FailedToBeSetupMod-Item,

 BHChannels-Modified-Item,

 BHChannels-SetupMod-Item,

 BHChannels-Required-ToBeReleased-Item,

 BAPAddress,

 BAPPathID,

 BAPRoutingID,

 BH-Routing-Information-Added-List-Item,

 BH-Routing-Information-Removed-List-Item,

 Child-Nodes-List,

 Child-Nodes-List-Item,

 Child-Node-Cells-List,

 Child-Node-Cells-List-Item,

 Activated-Cells-to-be-Updated-List,

 Activated-Cells-to-be-Updated-List-Item,

 UL-BH-Non-UP-Traffic-Mapping,

 IABTNLAddressesRequested,

 IABIPv6RequestType,

 IAB-TNL-Addresses-To-Remove-Item,

 IABTNLAddress,

 IAB-Allocated-TNL-Address-Item,

 IABv4AddressesRequested,

 TrafficMappingInfo,

 UL-UP-TNL-Information-to-Update-List-Item,

 UL-UP-TNL-Address-to-Update-List-Item,

 DL-UP-TNL-Address-to-Update-List-Item,

 NRV2XServicesAuthorized,

 LTEV2XServicesAuthorized,

 NRUESidelinkAggregateMaximumBitrate,

 LTEUESidelinkAggregateMaximumBitrate,

 SLDRBs-SetupMod-Item,

 SLDRBs-ModifiedConf-Item,

 SLDRBID,

 SLDRBs-FailedToBeModified-Item,

 SLDRBs-FailedToBeSetup-Item,

 SLDRBs-FailedToBeSetupMod-Item,

 SLDRBs-Modified-Item,

 SLDRBs-Required-ToBeModified-Item,

 SLDRBs-Required-ToBeReleased-Item,

 SLDRBs-Setup-Item,

 SLDRBs-ToBeModified-Item,

 SLDRBs-ToBeReleased-Item,

 SLDRBs-ToBeSetup-Item,

 SLDRBs-ToBeSetupMod-Item,

 GNBCUMeasurementID,

 GNBDUMeasurementID,

 RegistrationRequest,

 ReportCharacteristics,

 CellToReportList,

 HardwareLoadIndicator,

 CellMeasurementResultList,

 ReportingPeriodicity,

 TNLCapacityIndicator,

 RAReportList,

 RLFReportInformationList,

 ReportingRequestType,

 TimeReferenceInformation,

 ConditionalInterDUMobilityInformation,

 ConditionalIntraDUMobilityInformation,

 TargetCellList,

 MDTPLMNList,

 PrivacyIndicator,

 TransportLayerAddress,

 URI-address,

 NID,

 PosAssistance-Information,

 PosBroadcast,

 PositioningBroadcastCells,

 RoutingID,

 PosAssistanceInformationFailureList,

 PosMeasurementQuantities,

 PosMeasurementResultList,

 PosReportCharacteristics,

 TRPInformationTypeItem,

 TRPInformationItem,

 LMF-MeasurementID,

 RAN-MeasurementID,

 SDT-Termination-Request,

 SRSResourceSetID,

 SpatialRelationInfo,

 SRSResourceTrigger,

 SRSConfiguration,

 TRPList,

 E-CID-MeasurementQuantities,

 MeasurementPeriodicity,

 E-CID-MeasurementResult,

 Cell-Portion-ID,

 LMF-UE-MeasurementID,

 RAN-UE-MeasurementID,

 RelativeTime1900,

 SystemFrameNumber,

 SlotNumber,

 AbortTransmission,

 TRP-MeasurementRequestList,

 MeasurementBeamInfoRequest,

 E-CID-ReportCharacteristics,

 Extended-GNB-CU-Name,

 Extended-GNB-DU-Name,

 F1CTransferPath,

 SCGIndicator,

 SpatialRelationPerSRSResource,

 MeasurementPeriodicityExtended,

 SuccessfulHOReportInformationList,

 Coverage-Modification-Notification,

 CCO-Assistance-Information,

 CellsForSON-List,

 IABCongestionIndication,

 IABConditionalRRCMessageDeliveryIndication,

 F1CTransferPathNRDC,

 BufferSizeThresh,

 IAB-TNL-Addresses-Exception,

 BAP-Header-Rewriting-Added-List-Item,

 Re-routingEnableIndicator,

 NonF1terminatingTopologyIndicator,

 EgressNonF1terminatingTopologyIndicator,

 IngressNonF1terminatingTopologyIndicator,

 Neighbour-Node-Cells-List,

 Neighbour-Node-Cells-List-Item,

 NA-Resource-Configuration-List,

 NA-Resource-Configuration-Item,

 Serving-Cells-List,

 Serving-Cells-List-Item,

 RBSetConfiguration,

 PDCMeasurementPeriodicity,

 PDCMeasurementQuantities,

 PDCMeasurementResult,

 PDCReportType,

 RAN-UE-PDC-MeasID,

 SCGActivationRequest,

 SCGActivationStatus,

 TRP-MeasurementUpdateList,

 PRSTRPList,

 PRSTransmissionTRPList,

 ResponseTime,

 TRP-PRS-Info-List,

 PRS-Measurement-Info-List,

 PRSConfigRequestType,

 MeasurementCharacteristicsRequestIndicator,

 MeasurementTimeOccasion,

 UEReportingInformation,

 PosConextRevIndication,

 NRRedCapUEIndication,

 NRPagingeDRXInformation,

 NRPagingeDRXInformationforRRCINACTIVE,

 QoEInformation,

 CG-SDTQueryIndication,

 CG-SDTKeptIndicator,

 CG-SDTSessionInfo,

 SDTInformation,

 FiveG-ProSeAuthorized,

 UuRLCChannelToBeSetupList,

 UuRLCChannelToBeModifiedList,

 UuRLCChannelToBeReleasedList,

 UuRLCChannelSetupList,

 UuRLCChannelFailedToBeSetupList,

 UuRLCChannelModifiedList,

 UuRLCChannelFailedToBeModifiedList,

 UuRLCChannelRequiredToBeModifiedList,

 UuRLCChannelRequiredToBeReleasedList,

 PC5RLCChannelToBeSetupList,

 PC5RLCChannelToBeModifiedList,

 PC5RLCChannelToBeReleasedList,

 PC5RLCChannelSetupList,

 PC5RLCChannelFailedToBeSetupList,

 PC5RLCChannelFailedToBeModifiedList,

 PC5RLCChannelRequiredToBeModifiedList,

 PC5RLCChannelRequiredToBeReleasedList,

 PC5RLCChannelModifiedList,

 RemoteUELocalID,

 PathSwitchConfiguration,

 SidelinkRelayConfiguration,

 PagingCause,

 PEIPSAssistanceInfo,

 UEPagingCapability,

 GNBDUUESliceMaximumBitRateList,

 MDTPollutedMeasurementIndicator,

 UE-MulticastMRBs-ConfirmedToBeModified-Item,

 UE-MulticastMRBs-RequiredToBeModified-Item,

 UE-MulticastMRBs-RequiredToBeReleased-Item,

 UE-MulticastMRBs-Setup-Item,

 UE-MulticastMRBs-Setupnew-Item,

 UE-MulticastMRBs-ToBeReleased-Item,

 UE-MulticastMRBs-ToBeSetup-Item,

 UE-MulticastMRBs-ToBeSetup-atModify-Item,

 PosMeasurementAmount,

 BAP-Header-Rewriting-Removed-List-Item,

 SLDRXCycleList,

 MDTPLMNModificationList,

 ActivationRequestType,

 PosMeasGapPreConfigList,

 PosMeasurementPeriodicityNR-AoA,

 SRSPosRRCInactiveConfig,

 SDTBearerConfigurationQueryIndication,

 SDTBearerConfigurationInfo,

 ServingCellMO-List-Item,

 ServingCellMO-encoded-in-CGC-List,

 PosSItypeList,

 DAPS-HO-Status,

 UuRLCChannelID,

 UplinkTxDirectCurrentTwoCarrierListInfo,

 SRSPosRRCInactiveQueryIndication,

 MC-PagingCell-Item,

 UlTxDirectCurrentMoreCarrierInformation,

 CPACMCGInformation,

 ExtendedUEIdentityIndexValue,

 HashedUEIdentityIndexValue,

 DedicatedSIDeliveryIndication,

 Configured-BWP-List,

 MT-SDT-Information,

 LTMInformation-Setup,

 LTMConfigurationIDMappingList, LTMInformation-Modify,

 LTMCells-ToBeReleased-List, LTMConfiguration,

 EarlySyncInformation-Request,

 EarlySyncInformation,

 EarlySyncInformation-List,

 LTMCellSwitchInformation,

 TAInformation-List,

 DeactivationIndication,

 RAReportIndicationList,

 SuccessfulPSCellChangeReportInformationList,

 PathAdditionInformation,

 RANTSSRequestType,

 RANTimingSynchronisationStatusInfo,

 GlobalGNB-ID,

 Activated-Cells-Mapping-List-Item,

 RRC-Terminating-IAB-Donor-Related-Info,

 NCGI-to-be-Updated-List-Item,

 Mobile-IAB-MTUserLocationInformation,

 TAI,

 IndicationMCInactiveReception,

 MulticastCU2DURRCInfo,

 MulticastDU2CURRCInfo,

 MBSMulticastSessionReceptionState,

 MulticastCU2DUCommonRRCInfo,

 NRA2XServicesAuthorized,

 LTEA2XServicesAuthorized,

 NReRedCapUEIndication,

 NRPaginglongeDRXInformationforRRCINACTIVE,

 Cells-With-SSBs-Activated-List,

 Recommended-SSBs-for-Paging-List

FROM F1AP-IEs

 PrivateIE-Container{},

 ProtocolExtensionContainer{},

 ProtocolIE-Container{},

 ProtocolIE-ContainerPair{},

 ProtocolIE-SingleContainer{},

 F1AP-PRIVATE-IES,

 F1AP-PROTOCOL-EXTENSION,

 F1AP-PROTOCOL-IES,

 F1AP-PROTOCOL-IES-PAIR

FROM F1AP-Containers

 id-AssociatedSessionID,

 id-BroadcastMRBs-FailedToBeModified-List,

 id-BroadcastMRBs-FailedToBeModified-Item,

 id-BroadcastMRBs-FailedToBeSetup-List,

 id-BroadcastMRBs-FailedToBeSetup-Item,

 id-BroadcastMRBs-FailedToBeSetupMod-List,

 id-BroadcastMRBs-FailedToBeSetupMod-Item,

 id-BroadcastMRBs-Modified-List,

 id-BroadcastMRBs-Modified-Item,

 id-BroadcastMRBs-Setup-List,

 id-BroadcastMRBs-Setup-Item,

 id-BroadcastMRBs-SetupMod-List,

 id-BroadcastMRBs-SetupMod-Item,

 id-BroadcastMRBs-ToBeModified-List,

 id-BroadcastMRBs-ToBeModified-Item,

 id-BroadcastMRBs-ToBeReleased-List,

 id-BroadcastMRBs-ToBeReleased-Item,

 id-BroadcastMRBs-ToBeSetup-List,

 id-BroadcastMRBs-ToBeSetup-Item,

 id-BroadcastMRBs-ToBeSetupMod-List,

 id-BroadcastMRBs-ToBeSetupMod-Item,

 id-Candidate-SpCell-Item,

 id-Candidate-SpCell-List,

 id-Cause,

 id-Cancel-all-Warning-Messages-Indicator,

 id-Cells-Failed-to-be-Activated-List,

 id-Cells-Failed-to-be-Activated-List-Item,

 id-Cells-Status-Item,

 id-Cells-Status-List,

 id-Cells-to-be-Activated-List,

 id-Cells-to-be-Activated-List-Item,

 id-Cells-to-be-Deactivated-List,

 id-Cells-to-be-Deactivated-List-Item,

 id-Cells-Allowed-to-be-Deactivated-List,

 id-Cells-Allowed-to-be-Deactivated-List-Item,

 id-Cells-With-SSBs-Activated-List,

 id-Recommended-SSBs-for-Paging-List,

 id-ConfirmedUEID,

 id-CriticalityDiagnostics,

 id-C-RNTI,

 id-CUtoDURRCInformation,

 id-DRB-Activity-Item,

 id-DRB-Activity-List,

 id-DRBs-FailedToBeModified-Item,

 id-DRBs-FailedToBeModified-List,

 id-DRBs-FailedToBeSetup-Item,

 id-DRBs-FailedToBeSetup-List,

 id-DRBs-FailedToBeSetupMod-Item,

 id-DRBs-FailedToBeSetupMod-List,

 id-DRBs-ModifiedConf-Item,

 id-DRBs-ModifiedConf-List,

 id-DRBs-Modified-Item,

 id-DRBs-Modified-List,

 id-DRB-Notify-Item,

 id-DRB-Notify-List,

 id-DRBs-Required-ToBeModified-Item,

 id-DRBs-Required-ToBeModified-List,

 id-DRBs-Required-ToBeReleased-Item,

 id-DRBs-Required-ToBeReleased-List,

 id-DRBs-Setup-Item,

 id-DRBs-Setup-List,

 id-DRBs-SetupMod-Item,

 id-DRBs-SetupMod-List,

 id-DRBs-ToBeModified-Item,

 id-DRBs-ToBeModified-List,

 id-DRBs-ToBeReleased-Item,

 id-DRBs-ToBeReleased-List,

 id-DRBs-ToBeSetup-Item,

 id-DRBs-ToBeSetup-List,

 id-DRBs-ToBeSetupMod-Item,

 id-DRBs-ToBeSetupMod-List,

 id-DRXCycle,

 id-DUtoCURRCInformation,

 id-ExecuteDuplication,

 id-FullConfiguration,

 id-gNB-CU-MBS-F1AP-ID,

 id-gNB-CU-UE-F1AP-ID,

 id-gNB-DU-MBS-F1AP-ID,

 id-gNB-DU-UE-F1AP-ID,

 id-gNB-DU-ID,

 id-GNB-DU-Served-Cells-Item,

 id-gNB-DU-Served-Cells-List,

 id-gNB-CU-Name,

 id-gNB-DU-Name,

 id-Extended-GNB-CU-Name,

 id-Extended-GNB-DU-Name,

 id-InactivityMonitoringRequest,

 id-InactivityMonitoringResponse,

 id-MBS-Area-Session-ID,

 id-MBS-CUtoDURRCInformation,

 id-MBS-Session-ID,

 id-MBS-ServiceArea,

 id-MBSMulticastF1UContextDescriptor,

 id-MC-PagingCell-Item,

 id-MC-PagingCell-List,

 id-MulticastF1UContextReferenceCU,

 id-MulticastMBSSessionSetupList,

 id-MulticastMBSSessionRemoveList,

 id-MulticastMRBs-FailedToBeModified-List,

 id-MulticastMRBs-FailedToBeModified-Item,

 id-MulticastMRBs-FailedToBeSetup-List,

 id-MulticastMRBs-FailedToBeSetup-Item,

 id-MulticastMRBs-FailedToBeSetupMod-List,

 id-MulticastMRBs-FailedToBeSetupMod-Item,

 id-MulticastMRBs-Modified-List,

 id-MulticastMRBs-Modified-Item,

 id-MulticastMRBs-Setup-List,

 id-MulticastMRBs-Setup-Item,

 id-MulticastMRBs-SetupMod-List,

 id-MulticastMRBs-SetupMod-Item,

 id-MulticastMRBs-ToBeModified-List,

 id-MulticastMRBs-ToBeModified-Item,

 id-MulticastMRBs-ToBeReleased-List,

 id-MulticastMRBs-ToBeReleased-Item,

 id-MulticastMRBs-ToBeSetup-List,

 id-MulticastMRBs-ToBeSetup-Item,

 id-MulticastMRBs-ToBeSetupMod-List,

 id-MulticastMRBs-ToBeSetupMod-Item,

 id-MulticastF1UContext-ToBeSetup-List,

 id-MulticastF1UContext-ToBeSetup-Item,

 id-MulticastF1UContext-Setup-List,

 id-MulticastF1UContext-Setup-Item,

 id-MulticastF1UContext-FailedToBeSetup-List,

 id-MulticastF1UContext-FailedToBeSetup-Item,

 id-BroadcastAreaScope,

 id-new-gNB-CU-UE-F1AP-ID,

 id-new-gNB-DU-UE-F1AP-ID,

 id-oldgNB-DU-UE-F1AP-ID,

 id-PLMNAssistanceInfoForNetShar,

 id-Potential-SpCell-Item,

 id-Potential-SpCell-List,

 id-RAT-FrequencyPriorityInformation,

 id-RedirectedRRCmessage,

 id-ResetType,

 id-RequestedSRSTransmissionCharacteristics,

 id-ResourceCoordinationTransferContainer,

 id-RRCContainer,

 id-RRCContainer-RRCSetupComplete,

 id-RRCReconfigurationCompleteIndicator,

 id-SCell-FailedtoSetup-List,

 id-SCell-FailedtoSetup-Item,

 id-SCell-FailedtoSetupMod-List,

 id-SCell-FailedtoSetupMod-Item,

 id-SCell-ToBeRemoved-Item,

 id-SCell-ToBeRemoved-List,

 id-SCell-ToBeSetup-Item,

 id-SCell-ToBeSetup-List,

 id-SCell-ToBeSetupMod-Item,

 id-SCell-ToBeSetupMod-List,

 id-SDT-Termination-Request,

 id-SDT-Volume-Threshold,

 id-SelectedPLMNID,

 id-Served-Cells-To-Add-Item,

 id-Served-Cells-To-Add-List,

 id-Served-Cells-To-Delete-Item,

 id-Served-Cells-To-Delete-List,

 id-Served-Cells-To-Modify-Item,

 id-Served-Cells-To-Modify-List,

 id-ServCellIndex,

 id-ServingCellMO,

 id-SNSSAI,

 id-SpCell-ID,

 id-SpCellULConfigured,

 id-SRBID,

 id-SRBs-FailedToBeSetup-Item,

 id-SRBs-FailedToBeSetup-List,

 id-SRBs-FailedToBeSetupMod-Item,

 id-SRBs-FailedToBeSetupMod-List,

 id-SRBs-Required-ToBeReleased-Item,

 id-SRBs-Required-ToBeReleased-List,

 id-SRBs-ToBeReleased-Item,

 id-SRBs-ToBeReleased-List,

 id-SRBs-ToBeSetup-Item,

 id-SRBs-ToBeSetup-List,

 id-SRBs-ToBeSetupMod-Item,

 id-SRBs-ToBeSetupMod-List,

 id-SRBs-Modified-Item,

 id-SRBs-Modified-List,

 id-SRBs-Setup-Item,

 id-SRBs-Setup-List,

 id-SRBs-SetupMod-Item,

 id-SRBs-SetupMod-List,

 id-SupportedUETypeList,

 id-TimeToWait,

 id-TransactionID,

 id-TransmissionActionIndicator,

 id-UEContextNotRetrievable,

 id-UE-associatedLogicalF1-ConnectionItem,

 id-UE-associatedLogicalF1-ConnectionListResAck,

 id-UEIdentity-List-For-Paging-List,

 id-UEIdentity-List-For-Paging-Item,

 id-UE-MulticastMRBs-ConfirmedToBeModified-List,

 id-UE-MulticastMRBs-ConfirmedToBeModified-Item,

 id-UE-MulticastMRBs-RequiredToBeModified-List,

 id-UE-MulticastMRBs-RequiredToBeModified-Item,

 id-UE-MulticastMRBs-RequiredToBeReleased-List,

 id-UE-MulticastMRBs-RequiredToBeReleased-Item,

 id-UE-MulticastMRBs-Setup-List,

 id-UE-MulticastMRBs-Setup-Item,

 id-UE-MulticastMRBs-Setupnew-List,

 id-UE-MulticastMRBs-Setupnew-Item,

 id-UE-MulticastMRBs-ToBeReleased-List,

 id-UE-MulticastMRBs-ToBeReleased-Item,

 id-UE-MulticastMRBs-ToBeSetup-atModify-List,

 id-UE-MulticastMRBs-ToBeSetup-atModify-Item,

 id-UE-MulticastMRBs-ToBeSetup-List,

 id-UE-MulticastMRBs-ToBeSetup-Item,

 id-DUtoCURRCContainer,

 id-NRCGI,

 id-PagingCell-Item,

 id-PagingCell-List,

 id-PagingDRX,

 id-PagingPriority,

 id-SItype-List,

 id-UEIdentityIndexValue,

 id-GNB-CU-TNL-Association-Setup-List,

 id-GNB-CU-TNL-Association-Setup-Item,

 id-GNB-CU-TNL-Association-Failed-To-Setup-List,

 id-GNB-CU-TNL-Association-Failed-To-Setup-Item,

 id-GNB-CU-TNL-Association-To-Add-Item,

 id-GNB-CU-TNL-Association-To-Add-List,

 id-GNB-CU-TNL-Association-To-Remove-Item,

 id-GNB-CU-TNL-Association-To-Remove-List,

 id-GNB-CU-TNL-Association-To-Update-Item,

 id-GNB-CU-TNL-Association-To-Update-List,

 id-MaskedIMEISV,

 id-PagingIdentity,

 id-Cells-to-be-Barred-List,

 id-Cells-to-be-Barred-Item,

 id-PWSSystemInformation,

 id-RepetitionPeriod,

 id-NumberofBroadcastRequest,

 id-Cells-To-Be-Broadcast-List,

 id-Cells-To-Be-Broadcast-Item,

 id-Cells-Broadcast-Completed-List,

 id-Cells-Broadcast-Completed-Item,

 id-Broadcast-To-Be-Cancelled-List,

 id-Broadcast-To-Be-Cancelled-Item,

 id-Cells-Broadcast-Cancelled-List,

 id-Cells-Broadcast-Cancelled-Item,

 id-NR-CGI-List-For-Restart-List,

 id-NR-CGI-List-For-Restart-Item,

 id-PWS-Failed-NR-CGI-List,

 id-PWS-Failed-NR-CGI-Item,

 id-EUTRA-NR-CellResourceCoordinationReq-Container,

 id-EUTRA-NR-CellResourceCoordinationReqAck-Container,

 id-Protected-EUTRA-Resources-List,

 id-RequestType,

 id-ServingPLMN,

 id-DRXConfigurationIndicator,

 id-RLCFailureIndication,

 id-UplinkTxDirectCurrentListInformation,

 id-SULAccessIndication,

 id-Protected-EUTRA-Resources-Item,

 id-GNB-DUConfigurationQuery,

 id-GNB-DU-UE-AMBR-UL,

 id-GNB-CU-RRC-Version,

 id-GNB-DU-RRC-Version,

 id-GNBDUOverloadInformation,

 id-NeedforGap,

 id-RRCDeliveryStatusRequest,

 id-RRCDeliveryStatus,

 id-Dedicated-SIDelivery-NeededUE-List,

 id-Dedicated-SIDelivery-NeededUE-Item,

 id-ResourceCoordinationTransferInformation,

 id-Associated-SCell-List,

 id-Associated-SCell-Item,

 id-IgnoreResourceCoordinationContainer,

 id-UAC-Assistance-Info,

 id-RANUEID,

 id-PagingOrigin,

 id-GNB-DU-TNL-Association-To-Remove-Item,

 id-GNB-DU-TNL-Association-To-Remove-List,

 id-NotificationInformation,

 id-TraceActivation,

 id-TraceID,

 id-Neighbour-Cell-Information-List,

 id-Neighbour-Cell-Information-Item,

 id-SymbolAllocInSlot,

 id-NumDLULSymbols,

 id-AdditionalRRMPriorityIndex,

 id-DUCURadioInformationType,

 id-CUDURadioInformationType,

 id-LowerLayerPresenceStatusChange,

 id-Transport-Layer-Address-Info,

 id-BHChannels-ToBeSetup-List,

 id-BHChannels-ToBeSetup-Item,

 id-BHChannels-Setup-List,

 id-BHChannels-Setup-Item,

 id-BHChannels-ToBeModified-Item,

 id-BHChannels-ToBeModified-List,

 id-BHChannels-ToBeReleased-Item,

 id-BHChannels-ToBeReleased-List,

 id-BHChannels-ToBeSetupMod-Item,

 id-BHChannels-ToBeSetupMod-List,

 id-BHChannels-FailedToBeSetup-Item,

 id-BHChannels-FailedToBeSetup-List,

 id-BHChannels-FailedToBeModified-Item,

 id-BHChannels-FailedToBeModified-List,

 id-BHChannels-FailedToBeSetupMod-Item,

 id-BHChannels-FailedToBeSetupMod-List,

 id-BHChannels-Modified-Item,

 id-BHChannels-Modified-List,

 id-BHChannels-SetupMod-Item,

 id-BHChannels-SetupMod-List,

 id-BHChannels-Required-ToBeReleased-Item,

 id-BHChannels-Required-ToBeReleased-List,

 id-BAPAddress,

 id-ConfiguredBAPAddress,

 id-BH-Routing-Information-Added-List,

 id-BH-Routing-Information-Added-List-Item,

 id-BH-Routing-Information-Removed-List,

 id-BH-Routing-Information-Removed-List-Item,

 id-UL-BH-Non-UP-Traffic-Mapping,

 id-Child-Nodes-List,

 id-Activated-Cells-to-be-Updated-List,

 id-IABIPv6RequestType,

 id-IAB-TNL-Addresses-To-Remove-List,

 id-IAB-TNL-Addresses-To-Remove-Item,

 id-IAB-Allocated-TNL-Address-List,

 id-IAB-Allocated-TNL-Address-Item,

 id-IABv4AddressesRequested,

 id-TrafficMappingInformation,

 id-UL-UP-TNL-Information-to-Update-List,

 id-UL-UP-TNL-Information-to-Update-List-Item,

 id-UL-UP-TNL-Address-to-Update-List,

 id-UL-UP-TNL-Address-to-Update-List-Item,

 id-DL-UP-TNL-Address-to-Update-List,

 id-DL-UP-TNL-Address-to-Update-List-Item,

 id-NRV2XServicesAuthorized,

 id-LTEV2XServicesAuthorized,

 id-NRUESidelinkAggregateMaximumBitrate,

 id-LTEUESidelinkAggregateMaximumBitrate,

 id-PC5LinkAMBR,

 id-SLDRBs-FailedToBeModified-Item,

 id-SLDRBs-FailedToBeModified-List,

 id-SLDRBs-FailedToBeSetup-Item,

 id-SLDRBs-FailedToBeSetup-List,

 id-SLDRBs-Modified-Item,

 id-SLDRBs-Modified-List,

 id-SLDRBs-Required-ToBeModified-Item,

 id-SLDRBs-Required-ToBeModified-List,

 id-SLDRBs-Required-ToBeReleased-Item,

 id-SLDRBs-Required-ToBeReleased-List,

 id-SLDRBs-Setup-Item,

 id-SLDRBs-Setup-List,

 id-SLDRBs-ToBeModified-Item,

 id-SLDRBs-ToBeModified-List,

 id-SLDRBs-ToBeReleased-Item,

 id-SLDRBs-ToBeReleased-List,

 id-SLDRBs-ToBeSetup-Item,

 id-SLDRBs-ToBeSetup-List,

 id-SLDRBs-ToBeSetupMod-Item,

 id-SLDRBs-ToBeSetupMod-List,

 id-SLDRBs-SetupMod-List,

 id-SLDRBs-FailedToBeSetupMod-List,

 id-SLDRBs-SetupMod-Item,

 id-SLDRBs-FailedToBeSetupMod-Item,

 id-SLDRBs-ModifiedConf-List,

 id-SLDRBs-ModifiedConf-Item,

 id-gNBCUMeasurementID,

 id-gNBDUMeasurementID,

 id-RegistrationRequest,

 id-ReportCharacteristics,

 id-CellToReportList,

 id-CellMeasurementResultList,

 id-HardwareLoadIndicator,

 id-ReportingPeriodicity,

 id-TNLCapacityIndicator,

 id-RAReportList,

 id-RLFReportInformationList,

 id-ReportingRequestType,

 id-TimeReferenceInformation,

 id-ConditionalInterDUMobilityInformation,

 id-ConditionalIntraDUMobilityInformation,

 id-targetCellsToCancel,

 id-requestedTargetCellGlobalID,

 id-TraceCollectionEntityIPAddress,

 id-ManagementBasedMDTPLMNList,

 id-PrivacyIndicator,

 id-TraceCollectionEntityURI,

 id-ServingNID,

 id-PosAssistance-Information,

 id-PosBroadcast,

 id-PositioningBroadcastCells,

 id-RoutingID,

 id-PosAssistanceInformationFailureList,

 id-PosMeasurementQuantities,

 id-PosMeasurementResultList,

 id-PosMeasurementPeriodicity,

 id-PosReportCharacteristics,

 id-TRPInformationTypeListTRPReq,

 id-TRPInformationTypeItem,

 id-TRPInformationListTRPResp,

 id-TRPInformationItem,

 id-LMF-MeasurementID,

 id-RAN-MeasurementID,

 id-SRSType,

 id-ActivationTime,

 id-AbortTransmission,

 id-SRSConfiguration,

 id-TRPList,

 id-E-CID-MeasurementQuantities,

 id-E-CID-MeasurementPeriodicity,

 id-E-CID-MeasurementResult,

 id-Cell-Portion-ID,

 id-LMF-UE-MeasurementID,

 id-RAN-UE-MeasurementID,

 id-SFNInitialisationTime,

 id-SystemFrameNumber,

 id-SlotNumber,

 id-TRP-MeasurementRequestList,

 id-MeasurementBeamInfoRequest,

 id-E-CID-ReportCharacteristics,

 id-F1CTransferPath,

 id-SCGIndicator,

 id-SRSSpatialRelationPerSRSResource,

 id-PosMeasurementPeriodicityExtended,

 id-SuccessfulHOReportInformationList,

 id-Coverage-Modification-Notification,

 id-CCO-Assistance-Information,

 id-CellsForSON-List,

 id-IABCongestionIndication,

 id-IABConditionalRRCMessageDeliveryIndication,

 id-F1CTransferPathNRDC,

 id-BufferSizeThresh,

 id-IAB-TNL-Addresses-Exception,

 id-BAP-Header-Rewriting-Added-List,

 id-BAP-Header-Rewriting-Added-List-Item,

 id-Re-routingEnableIndicator,

 id-NonF1terminatingTopologyIndicator,

 id-EgressNonF1terminatingTopologyIndicator,

 id-IngressNonF1terminatingTopologyIndicator,

 id-Neighbour-Node-Cells-List,

 id-Serving-Cells-List,

 id-MDTPollutedMeasurementIndicator,

 id-PDCMeasurementPeriodicity,

 id-PDCMeasurementQuantities,

 id-PDCMeasurementResult,

 id-PDCReportType,

 id-RAN-UE-PDC-MeasID,

 id-SCGActivationRequest,

 id-SCGActivationStatus,

 id-TRP-MeasurementUpdateList,

 id-PRSTRPList,

 id-PRSTransmissionTRPList,

 id-ResponseTime,

 id-TRP-PRS-Info-List,

 id-PRS-Measurement-Info-List,

 id-PRSConfigRequestType,

 id-MeasurementCharacteristicsRequestIndicator,

 id-MeasurementTimeOccasion,

 id-UEReportingInformation,

 id-PosConextRevIndication,

 id-NRRedCapUEIndication,

 id-RANUEPagingDRX,

 id-CNUEPagingDRX,

 id-NRPagingeDRXInformation,

 id-NRPagingeDRXInformationforRRCINACTIVE,

 id-QoEInformation,

 id-CG-SDTQueryIndication,

 id-CG-SDTKeptIndicator,

 id-CG-SDTSessionInfoOld,

 id-SDTInformation,

 id-FiveG-ProSeAuthorized,

 id-FiveG-ProSePC5LinkAMBR,

 id-FiveG-ProSeUEPC5AggregateMaximumBitrate,

 id-UuRLCChannelToBeSetupList,

 id-UuRLCChannelToBeModifiedList,

 id-UuRLCChannelToBeReleasedList,

 id-UuRLCChannelSetupList,

 id-UuRLCChannelFailedToBeSetupList,

 id-UuRLCChannelModifiedList,

 id-UuRLCChannelFailedToBeModifiedList,

 id-UuRLCChannelRequiredToBeModifiedList,

 id-UuRLCChannelRequiredToBeReleasedList,

 id-PC5RLCChannelToBeSetupList,

 id-PC5RLCChannelToBeModifiedList,

 id-PC5RLCChannelToBeReleasedList,

 id-PC5RLCChannelSetupList,

 id-PC5RLCChannelFailedToBeSetupList,

 id-PC5RLCChannelModifiedList,

 id-PC5RLCChannelFailedToBeModifiedList,

 id-PC5RLCChannelRequiredToBeModifiedList,

 id-PC5RLCChannelRequiredToBeReleasedList,

 id-SidelinkRelayConfiguration,

 id-UpdatedRemoteUELocalID,

 id-PathSwitchConfiguration,

 id-PagingCause,

 id-PEIPSAssistanceInfo,

 id-UEPagingCapability,

 id-GNBDUUESliceMaximumBitRateList,

 id-PosMeasurementAmount,

 id-BAP-Header-Rewriting-Removed-List,

 id-BAP-Header-Rewriting-Removed-List-Item,

 id-SLDRXCycleList,

 id-ManagementBasedMDTPLMNModificationList,

 id-ActivationRequestType,

 id-PosMeasGapPreConfigList,

 id-PosMeasurementPeriodicityNR-AoA,

 id-SRSPosRRCInactiveConfig,

 id-SDTBearerConfigurationQueryIndication,

 id-SDTBearerConfigurationInfo,

 id-ServingCellMO-List,

 id-ServingCellMO-List-Item,

 id-ServingCellMO-encoded-in-CGC-List,

 id-PosSItypeList,

 id-DAPS-HO-Status,

 id-SRBMappingInfo,

 id-UplinkTxDirectCurrentTwoCarrierListInfo,

 id-SRSPosRRCInactiveQueryIndication,

 id-UlTxDirectCurrentMoreCarrierInformation,

 id-CPACMCGInformation,

 id-ExtendedUEIdentityIndexValue,

 id-HashedUEIdentityIndexValue,

 id-DedicatedSIDeliveryIndication,

 id-Configured-BWP-List,

 id-NetworkControlledRepeaterAuthorized,

 id-MT-SDT-Information,

 id-LTMInformation-Setup, id-LTMConfigurationIDMappingList,

 id-LTMInformation-Modify,

 id-LTMCells-ToBeReleased-List,

 id-LTMConfiguration,

 id-EarlySyncInformation-Request,

 id-EarlySyncInformation,

 id-EarlySyncInformation-List,

 id-LTMCellSwitchInformation,

 id-TAInformation-List,

 id-Source-gNB-DU-ID,

 id-DeactivationIndication,

 id-RAReportIndicationList,

 id-SuccessfulPSCellChangeReportInformationList,

 id-PathAdditionInformation,

 id-RANTSSRequestType,

 id-RANTimingSynchronisationStatusInfo,

 id-Target-gNB-ID,

 id-Target-gNB-IP-address,

 id-Target-SeGW-IP-address,

 id-Activated-Cells-Mapping-List,

 id-Activated-Cells-Mapping-List-Item,

 id-F1SetupOutcome,

 id-RRC-Terminating-IAB-Donor-Related-Info,

 id-RRC-Terminating-IAB-Donor-gNB-ID,

 id-NCGI-to-be-Updated-List,

 id-NCGI-to-be-Updated-List-Item,

 id-Mobile-IAB-MTUserLocationInformation,

 id-IndicationMCInactiveReception,

 id-MulticastCU2DURRCInfo,

 id-MulticastDU2CURRCInfo,

 id-MBSMulticastSessionReceptionState,

 id-MulticastCU2DUCommonRRCInfo,

 id-NRA2XServicesAuthorized,

 id-LTEA2XServicesAuthorized,

 id-NRUESidelinkAggregateMaximumBitrateForA2X,

 id-LTEUESidelinkAggregateMaximumBitrateForA2X,

 id-NReRedCapUEIndication,

 id-NRPaginglongeDRXInformationforRRCINACTIVE,

 id-Broadcast-MRBs-Transport-Request-List,

 id-Broadcast-MRBs-Transport-Request-Item,

 maxCellingNBDU,

 maxnoofCandidateSpCells,

 maxnoofDRBs,

 maxnoofErrors,

 maxnoofIndividualF1ConnectionsToReset,

 maxnoofPotentialSpCells,

 maxnoofSCells,

 maxnoofSRBs,

 maxnoofPagingCells,

 maxnoofTNLAssociations,

 maxCellineNB,

 maxnoofUEIDs,

 maxnoofBHRLCChannels,

 maxnoofRoutingEntries,

 maxnoofChildIABNodes,

 maxnoofServedCellsIAB,

 maxnoofTLAsIAB,

 maxnoofULUPTNLInformationforIAB,

 maxnoofUPTNLAddresses,

 maxnoofSLDRBs,

 maxnoofTRPInfoTypes,

 maxnoofTRPs,

 maxnoofMRBs,

 maxnoofUEIDforPaging,

 maxnoofNeighbourNodeCellsIAB,

 maxnoofMRBsforUE,

 maxnoofServingCellMOs,

 maxnoofLTMCells

<<<<<<<<<<<<<<<<<<<< unchanged part omit >>>>>>>>>>>>>>>>>>>>

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BROADCAST CONTEXT SETUP RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BroadcastContextSetupResponse ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { { BroadcastContextSetupResponseIEs} },

 ...

}

BroadcastContextSetupResponseIEs F1AP-PROTOCOL-IES ::= {

 { ID id-gNB-CU-MBS-F1AP-ID CRITICALITY reject TYPE GNB-CU-MBS-F1AP-ID PRESENCE mandatory }|

 { ID id-gNB-DU-MBS-F1AP-ID CRITICALITY reject TYPE GNB-DU-MBS-F1AP-ID PRESENCE mandatory }|

 { ID id-BroadcastMRBs-Setup-List CRITICALITY reject TYPE BroadcastMRBs-Setup-List PRESENCE mandatory }|

 { ID id-BroadcastMRBs-FailedToBeSetup-List CRITICALITY ignore TYPE BroadcastMRBs-FailedToBeSetup-List PRESENCE optional }|

 { ID id-BroadcastAreaScope CRITICALITY ignore TYPE BroadcastAreaScope PRESENCE optional }|

 { ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }, ...

}

BroadcastMRBs-Setup-List ::= SEQUENCE (SIZE(1..maxnoofMRBs)) OF ProtocolIE-SingleContainer { { BroadcastMRBs-Setup-ItemIEs} }

BroadcastMRBs-FailedToBeSetup-List ::= SEQUENCE (SIZE(1..maxnoofMRBs)) OF ProtocolIE-SingleContainer { { BroadcastMRBs-FailedToBeSetup-ItemIEs} }

BroadcastMRBs-Setup-ItemIEs F1AP-PROTOCOL-IES ::= {

 { ID id-BroadcastMRBs-Setup-Item CRITICALITY reject TYPE BroadcastMRBs-Setup-Item PRESENCE mandatory},

 ...

}

<<<<<<<<<<<<<<<<<<<< unchanged part omit >>>>>>>>>>>>>>>>>>>>

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BROADCAST TRANSPORT RESOURCE REQUEST ELEMENTARY PROCEDURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BROADCAST TRANSPORT RESOURCE REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BroadcastTransportResourceRequest ::= SEQUENCE {

 protocolIEs ProtocolIE-Container {{ BroadcastTransportResourceRequestIEs}},

 ...

}

BroadcastTransportResourceRequestIEs F1AP-PROTOCOL-IES ::= {

 { ID id-gNB-CU-MBS-F1AP-ID CRITICALITY reject TYPE GNB-CU-MBS-F1AP-ID PRESENCE mandatory }|

 { ID id-gNB-DU-MBS-F1AP-ID CRITICALITY reject TYPE GNB-DU-MBS-F1AP-ID PRESENCE mandatory }|

 { ID id-Broadcast-MRBs-Transport-Request-List CRITICALITY reject TYPE Broadcast-MRBs-Transport-Request-List PRESENCE optional },

 ...

}

Broadcast-MRBs-Transport-Request-List ::= SEQUENCE (SIZE(1..maxnoofMRBs)) OF ProtocolIE-SingleContainer { { Broadcast-MRBs-Transport-Request-ItemIEs} }

Broadcast-MRBs-Transport-Request-ItemIEs F1AP-PROTOCOL-IES ::= {

 { ID id-Broadcast-MRBs-Transport-Request-Item CRITICALITY reject TYPE Broadcast-MRBs-Transport-Request-Item PRESENCE mandatory},

 ...

}

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

<<<<<<<<<<<<<<<<<<<< unchanged part omit >>>>>>>>>>>>>>>>>>>>

 id-N6JitterInformation,

 id-ECNMarkingorCongestionInformationReportingRequest,

 id-ECNMarkingorCongestionInformationReportingStatus,

 id-ERedcap-Bcast-Information,

 id-NeedForInterruptionInfoNR,

 id-LTMCells-ToBeReleased-Item,

 id-F1UTunnelNotEstablished,

 maxNRARFCN,

 maxnoofErrors,

 maxnoofBPLMNs,

 maxnoofBPLMNsNR,

 maxnoofDLUPTNLInformation,

 maxnoofNrCellBands,

 maxnoofULUPTNLInformation,

<<<<<<<<<<<<<<<<<<<< unchanged part omit >>>>>>>>>>>>>>>>>>>>

Broadcast-MRBs-Transport-Request-Item ::= SEQUENCE {

 mRB-ID MRB-ID,

 bcBearerCtxtF1U-TNLInfoatDU BCBearerContextF1U-TNLInfo,

 iE-Extensions ProtocolExtensionContainer { {Broadcast-MRBs-Transport-Request-Item-ExtIEs} } OPTIONAL,

 ...

}

Broadcast-MRBs-Transport-Request-Item-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

<<<<<<<<<<<<<<<<<<<< unchanged part omit >>>>>>>>>>>>>>>>>>>>

LMF-MeasurementID ::= INTEGER (1.. 65536, ...)

LMF-UE-MeasurementID ::= INTEGER (1.. 256, ...)

LocationDependentMBSF1UInformation ::= SEQUENCE (SIZE(1..maxnoofMBSAreaSessionIDs)) OF LocationDependentMBSF1UInformation-Item

LocationDependentMBSF1UInformation-Item ::= SEQUENCE {

 mbsAreaSession-ID MBS-Area-Session-ID,

 mbs-f1u-info-at-CU UPTransportLayerInformation,

 iE-Extensions ProtocolExtensionContainer { { LocationDependentMBSF1UInformation-Item-ExtIEs } } OPTIONAL,

 ...

}

LocationDependentMBSF1UInformation-Item-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 { ID id-F1UTunnelNotEstablished CRITICALITY ignore EXTENSION F1UTunnelNotEstablished PRESENCE optional },

 ...

}

LocationMeasurementInformation ::= OCTET STRING

LocationUncertainty ::= SEQUENCE {

 horizontalUncertainty INTEGER (0..255),

 horizontalConfidence INTEGER (0..100),

 verticalUncertainty INTEGER (0..255),

 verticalConfidence INTEGER (0..100),

 iE-Extensions ProtocolExtensionContainer { { LocationUncertainty-ExtIEs} } OPTIONAL

}

LocationUncertainty-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

<<<<<<<<<<<<<<<<<<<< unchanged part omit >>>>>>>>>>>>>>>>>>>>

MBS-Flows-Mapped-To-MRB-Item ::= SEQUENCE {

 mBS-QoSFlowIdentifier QoSFlowIdentifier,

 mbs-QoSFlowLevelQoSParameters QoSFlowLevelQoSParameters,

 iE-Extensions ProtocolExtensionContainer { { MBS-Flows-Mapped-To-MRB-Item-ExtIEs} } OPTIONAL

}

MBS-Flows-Mapped-To-MRB-Item-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

MBSF1UInformation ::= SEQUENCE {

 mbs-f1u-info UPTransportLayerInformation,

 iE-Extensions ProtocolExtensionContainer { { MBSF1UInformation-ExtIEs } } OPTIONAL,

 ...

}

MBSF1UInformation-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 { ID id-F1UTunnelNotEstablished CRITICALITY ignore EXTENSION F1UTunnelNotEstablished PRESENCE optional },

 ...

}

MBSInterestIndication ::= OCTET STRING

MBS-Session-ID ::= SEQUENCE {

 tMGI TMGI,

 nID NID OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { MBS-Session-ID-ExtIEs} } OPTIONAL,

 ...

}

MBS-Session-ID-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM F1AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Reset ProcedureCode ::= 0

id-F1Setup ProcedureCode ::= 1

id-ErrorIndication ProcedureCode ::= 2

id-gNBDUConfigurationUpdate ProcedureCode ::= 3

id-gNBCUConfigurationUpdate ProcedureCode ::= 4

id-UEContextSetup ProcedureCode ::= 5

id-UEContextRelease ProcedureCode ::= 6

id-UEContextModification ProcedureCode ::= 7

id-UEContextModificationRequired ProcedureCode ::= 8

id-UEMobilityCommand ProcedureCode ::= 9

id-UEContextReleaseRequest ProcedureCode ::= 10

id-InitialULRRCMessageTransfer ProcedureCode ::= 11

id-DLRRCMessageTransfer ProcedureCode ::= 12

id-ULRRCMessageTransfer ProcedureCode ::= 13

id-privateMessage ProcedureCode ::= 14

id-UEInactivityNotification ProcedureCode ::= 15

id-GNBDUResourceCoordination ProcedureCode ::= 16

id-SystemInformationDeliveryCommand ProcedureCode ::= 17

id-Paging ProcedureCode ::= 18

id-Notify ProcedureCode ::= 19

id-WriteReplaceWarning ProcedureCode ::= 20

id-PWSCancel ProcedureCode ::= 21

id-PWSRestartIndication ProcedureCode ::= 22

id-PWSFailureIndication ProcedureCode ::= 23

id-GNBDUStatusIndication ProcedureCode ::= 24

id-RRCDeliveryReport ProcedureCode ::= 25

id-F1Removal ProcedureCode ::= 26

id-NetworkAccessRateReduction ProcedureCode ::= 27

id-TraceStart ProcedureCode ::= 28

id-DeactivateTrace ProcedureCode ::= 29

id-DUCURadioInformationTransfer ProcedureCode ::= 30

id-CUDURadioInformationTransfer ProcedureCode ::= 31

id-BAPMappingConfiguration ProcedureCode ::= 32

id-GNBDUResourceConfiguration ProcedureCode ::= 33

id-IABTNLAddressAllocation ProcedureCode ::= 34

id-IABUPConfigurationUpdate ProcedureCode ::= 35

id-resourceStatusReportingInitiation ProcedureCode ::= 36

id-resourceStatusReporting ProcedureCode ::= 37

id-accessAndMobilityIndication ProcedureCode ::= 38

id-accessSuccess ProcedureCode ::= 39

id-cellTrafficTrace ProcedureCode ::= 40

id-PositioningMeasurementExchange ProcedureCode ::= 41

id-PositioningAssistanceInformationControl ProcedureCode ::= 42

id-PositioningAssistanceInformationFeedback ProcedureCode ::= 43

id-PositioningMeasurementReport ProcedureCode ::= 44

id-PositioningMeasurementAbort ProcedureCode ::= 45

id-PositioningMeasurementFailureIndication ProcedureCode ::= 46

id-PositioningMeasurementUpdate ProcedureCode ::= 47

id-TRPInformationExchange ProcedureCode ::= 48

id-PositioningInformationExchange ProcedureCode ::= 49

id-PositioningActivation ProcedureCode ::= 50

id-PositioningDeactivation ProcedureCode ::= 51

id-E-CIDMeasurementInitiation ProcedureCode ::= 52

id-E-CIDMeasurementFailureIndication ProcedureCode ::= 53

id-E-CIDMeasurementReport ProcedureCode ::= 54

id-E-CIDMeasurementTermination ProcedureCode ::= 55

id-PositioningInformationUpdate ProcedureCode ::= 56

id-ReferenceTimeInformationReport ProcedureCode ::= 57

id-ReferenceTimeInformationReportingControl ProcedureCode ::= 58

id-BroadcastContextSetup ProcedureCode ::= 59

id-BroadcastContextRelease ProcedureCode ::= 60

id-BroadcastContextReleaseRequest ProcedureCode ::= 61

id-BroadcastContextModification ProcedureCode ::= 62

id-MulticastGroupPaging ProcedureCode ::= 63

id-MulticastContextSetup ProcedureCode ::= 64

id-MulticastContextRelease ProcedureCode ::= 65

id-MulticastContextReleaseRequest ProcedureCode ::= 66

id-MulticastContextModification ProcedureCode ::= 67

id-MulticastDistributionSetup ProcedureCode ::= 68

id-MulticastDistributionRelease ProcedureCode ::= 69

id-PDCMeasurementInitiation ProcedureCode ::= 70

id-PDCMeasurementReport ProcedureCode ::= 71

id-PDCMeasurementInitiationRequest ProcedureCode ::= 72

id-PDCMeasurementInitiationResponse ProcedureCode ::= 73

id-PDCMeasurementInitiationFailure ProcedureCode ::= 74

id-pRSConfigurationExchange ProcedureCode ::= 75

id-measurementPreconfiguration ProcedureCode ::= 76

id-measurementActivation ProcedureCode ::= 77

id-QoEInformationTransfer ProcedureCode ::= 78

id-PDCMeasurementTerminationCommand ProcedureCode ::= 79

id-PDCMeasurementFailureIndication ProcedureCode ::= 80

id-PosSystemInformationDeliveryCommand ProcedureCode ::= 81

id-DUCUCellSwitchNotification ProcedureCode ::= 82

id-CUDUCellSwitchNotification ProcedureCode ::= 83

id-DUCUTAInformationTransfer ProcedureCode ::= 84

id-CUDUTAInformationTransfer ProcedureCode ::= 85

id-QoEInformationTransferControl ProcedureCode ::= 86

id-RachIndication ProcedureCode ::= 87

id-TimingSynchronisationStatus ProcedureCode ::= 88

id-TimingSynchronisationStatusReport ProcedureCode ::= 89

id-MIABF1SetupTriggering ProcedureCode ::= 90

id-MIABF1SetupOutcomeNotification ProcedureCode ::= 91

id-MulticastContextNotification ProcedureCode ::= 92

id-MulticastCommonConfiguration ProcedureCode ::= 93

id-BroadcastTransportResourceRequest ProcedureCode ::= 94

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Extension constants

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxPrivateIEs INTEGER ::= 65535

maxProtocolExtensions INTEGER ::= 65535

maxProtocolIEs INTEGER ::= 65535

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxNRARFCN INTEGER ::= 3279165

maxnoofErrors INTEGER ::= 256

maxnoofIndividualF1ConnectionsToReset INTEGER ::= 65536

maxCellingNBDU INTEGER ::= 512

maxnoofSCells INTEGER ::= 32

maxnoofSRBs INTEGER ::= 8

maxnoofDRBs INTEGER ::= 64

maxnoofULUPTNLInformation INTEGER ::= 2

maxnoofDLUPTNLInformation INTEGER ::= 2

maxnoofBPLMNs INTEGER ::= 6

maxnoofCandidateSpCells INTEGER ::= 64

maxnoofPotentialSpCells INTEGER ::= 64

maxnoofNrCellBands INTEGER ::= 32

maxnoofSIBTypes INTEGER ::= 32

maxnoofSITypes INTEGER ::= 32

maxnoofPagingCells INTEGER ::= 512

maxnoofTNLAssociations INTEGER ::= 32

maxnoofQoSFlows INTEGER ::= 64

maxnoofSliceItems INTEGER ::= 1024

maxCellineNB INTEGER ::= 256

maxnoofExtendedBPLMNs INTEGER ::= 6

maxnoofUEIDs INTEGER ::= 65536

maxnoofBPLMNsNR INTEGER ::= 12

maxnoofUACPLMNs INTEGER ::= 12

maxnoofUACperPLMN INTEGER ::= 64

maxnoofAdditionalSIBs INTEGER ::= 63

maxnoofslots INTEGER ::= 5120

maxnoofTLAs INTEGER ::= 16

maxnoofGTPTLAs INTEGER ::= 16

maxnoofBHRLCChannels INTEGER ::= 65536

maxnoofRoutingEntries INTEGER ::= 1024

maxnoofIABSTCInfo INTEGER ::= 45

maxnoofSymbols INTEGER ::= 14

maxnoofServingCells INTEGER ::= 32

maxnoofDUFSlots INTEGER ::= 320

maxnoofHSNASlots INTEGER ::= 5120

maxnoofServedCellsIAB INTEGER ::= 512

maxnoofSSBarea INTEGER ::=64

maxnoofChildIABNodes INTEGER ::= 1024

maxnoofNonUPTrafficMappings INTEGER ::= 32

maxnoofTLAsIAB INTEGER ::= 1024

maxnoofMappingEntries INTEGER ::= 67108864

maxnoofDSInfo INTEGER ::= 64

maxnoofEgressLinks INTEGER ::= 2

maxnoofULUPTNLInformationforIAB INTEGER ::= 32678

maxnoofUPTNLAddresses INTEGER ::= 8

maxnoofSLDRBs INTEGER ::= 512

maxnoofQoSParaSets INTEGER ::= 8

maxnoofPC5QoSFlows INTEGER ::= 2048

maxnoofSSBAreas INTEGER ::= 64

maxnoofPhysicalResourceBlocks INTEGER ::= 275

maxnoofPhysicalResourceBlocks-1 INTEGER ::= 274

maxnoofPRACHconfigs INTEGER ::= 16

maxnoofRAReports INTEGER ::= 64

maxnoofRLFReports INTEGER ::= 64

maxnoofAdditionalPDCPDuplicationTNL INTEGER ::= 2

maxnoofRLCDuplicationState INTEGER ::= 3

maxnoofCHOcells INTEGER ::= 8

maxnoofMDTPLMNs INTEGER ::= 16

maxnoofCAGsupported INTEGER ::= 12

maxnoofNIDsupported INTEGER ::= 12

maxnoofNRSCSs INTEGER ::= 5

maxnoofExtSliceItems INTEGER ::= 65535

maxnoofPosMeas INTEGER ::= 16384

maxnoofTRPInfoTypes INTEGER ::= 64

maxnoofTRPs INTEGER ::= 65535

maxnoofSRSTriggerStates INTEGER ::= 3

maxnoofSpatialRelations INTEGER ::= 64

maxnoBcastCell INTEGER ::= 16384

maxnoofAngleInfo INTEGER ::= 65535

maxnooflcs-gcs-translation INTEGER ::= 3

maxnoofPath INTEGER ::= 2

maxnoofMeasE-CID INTEGER ::= 64

maxnoofSSBs INTEGER ::= 255

maxnoSRS-ResourceSets INTEGER ::= 16

maxnoSRS-ResourcePerSet INTEGER ::= 16

maxnoSRS-Carriers INTEGER ::= 32

maxnoSCSs INTEGER ::= 5

maxnoSRS-Resources INTEGER ::= 64

maxnoSRS-PosResources INTEGER ::= 64

maxnoSRS-PosResourceSets INTEGER ::= 16

maxnoSRS-PosResourcePerSet INTEGER ::= 16

maxnoofPRS-ResourceSets INTEGER ::= 2

maxnoofPRS-ResourcesPerSet INTEGER ::= 64

maxNoOfMeasTRPs INTEGER ::= 64

maxnoofPRSresourceSets INTEGER ::= 8

maxnoofPRSresources INTEGER ::= 64

maxnoofSuccessfulHOReports INTEGER ::= 64

maxnoofNR-UChannelIDs INTEGER ::= 16

maxServedCellforSON INTEGER ::= 256

maxNeighbourCellforSON INTEGER ::= 32

maxAffectedCells INTEGER ::= 32

maxnoofMRBs INTEGER ::= 32

maxnoofMBSQoSFlows INTEGER ::= 64

maxnoofMBSFSAs INTEGER ::= 256

maxnoofUEIDforPaging INTEGER ::= 4096

maxnoofCellsforMBS INTEGER ::= 512

maxnoofTAIforMBS INTEGER ::= 512

maxnoofMBSAreaSessionIDs INTEGER ::= 256

maxnoofMBSServiceAreaInformation INTEGER ::= 256

maxnoofIABCongInd INTEGER ::= 1024

maxnoofNeighbourNodeCellsIAB INTEGER ::= 1024

maxnoofRBsetsPerCell INTEGER ::= 8

maxnoofRBsetsPerCell-1 INTEGER ::= 7

maxnoofMeasPDC INTEGER ::= 16

maxnoARPs INTEGER ::= 16

maxnoofULAoAs INTEGER ::= 8

maxNoPathExtended INTEGER ::= 8

maxnoTRPTEGs INTEGER ::= 8

maxFreqLayers INTEGER ::= 4

maxNumResourcesPerAngle INTEGER ::= 24

maxnoAzimuthAngles INTEGER ::= 3600

maxnoElevationAngles INTEGER ::= 1801

maxnoofPRSTRPs INTEGER ::= 256

maxnoofQoEInformation INTEGER ::= 16

maxnoofUuRLCChannels INTEGER ::= 32

maxnoofPC5RLCChannels INTEGER ::= 512

maxnoofSMBRValues INTEGER ::= 8

maxnoofMRBsforUE INTEGER ::= 64

maxnoofMBSSessionsofUE INTEGER ::= 256

maxnoofSLdestinations INTEGER ::= 32

maxnoofNSAGs INTEGER ::= 256

maxnoofSDTBearers INTEGER ::= 72

maxnoofServingCellMOs INTEGER ::= 16

maxNrofBWPs INTEGER ::= 8

maxnoofPosSITypes INTEGER ::= 32

maxnoofUETypes INTEGER ::= 8

maxnoofLTMCells INTEGER ::= 8

maxnoofJointorDLTCIStates INTEGER ::= 128

maxnoofULTCIStates INTEGER ::= 64

maxnoofTAList INTEGER ::= 8

maxnoofUEsInQMCTransferControlMessage INTEGER ::= 512

maxnoofUEsforRAReportIndications INTEGER ::= 64

maxnoofSuccessfulPSCellChangeReports INTEGER ::= 64

maxnoofPeriodicities INTEGER ::= 8

maxnoofThresholdMBS INTEGER ::= 64

maxMBSSessionsinSessionInfoList INTEGER ::= 1024

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Cause ProtocolIE-ID ::= 0

id-Cells-Failed-to-be-Activated-List ProtocolIE-ID ::= 1

id-Cells-Failed-to-be-Activated-List-Item ProtocolIE-ID ::= 2

id-Cells-to-be-Activated-List ProtocolIE-ID ::= 3

id-Cells-to-be-Activated-List-Item ProtocolIE-ID ::= 4

id-Cells-to-be-Deactivated-List ProtocolIE-ID ::= 5

id-Cells-to-be-Deactivated-List-Item ProtocolIE-ID ::= 6

id-CriticalityDiagnostics ProtocolIE-ID ::= 7

id-CUtoDURRCInformation ProtocolIE-ID ::= 9

id-DRBs-FailedToBeModified-Item ProtocolIE-ID ::= 12

id-DRBs-FailedToBeModified-List ProtocolIE-ID ::= 13

id-DRBs-FailedToBeSetup-Item ProtocolIE-ID ::= 14

id-DRBs-FailedToBeSetup-List ProtocolIE-ID ::= 15

id-DRBs-FailedToBeSetupMod-Item ProtocolIE-ID ::= 16

id-DRBs-FailedToBeSetupMod-List ProtocolIE-ID ::= 17

id-DRBs-ModifiedConf-Item ProtocolIE-ID ::= 18

id-DRBs-ModifiedConf-List ProtocolIE-ID ::= 19

id-DRBs-Modified-Item ProtocolIE-ID ::= 20

id-DRBs-Modified-List ProtocolIE-ID ::= 21

id-DRBs-Required-ToBeModified-Item ProtocolIE-ID ::= 22

id-DRBs-Required-ToBeModified-List ProtocolIE-ID ::= 23

id-DRBs-Required-ToBeReleased-Item ProtocolIE-ID ::= 24

id-DRBs-Required-ToBeReleased-List ProtocolIE-ID ::= 25

id-DRBs-Setup-Item ProtocolIE-ID ::= 26

id-DRBs-Setup-List ProtocolIE-ID ::= 27

id-DRBs-SetupMod-Item ProtocolIE-ID ::= 28

id-DRBs-SetupMod-List ProtocolIE-ID ::= 29

id-DRBs-ToBeModified-Item ProtocolIE-ID ::= 30

id-DRBs-ToBeModified-List ProtocolIE-ID ::= 31

id-DRBs-ToBeReleased-Item ProtocolIE-ID ::= 32

id-DRBs-ToBeReleased-List ProtocolIE-ID ::= 33

id-DRBs-ToBeSetup-Item ProtocolIE-ID ::= 34

id-DRBs-ToBeSetup-List ProtocolIE-ID ::= 35

id-DRBs-ToBeSetupMod-Item ProtocolIE-ID ::= 36

id-DRBs-ToBeSetupMod-List ProtocolIE-ID ::= 37

id-DRXCycle ProtocolIE-ID ::= 38

id-DUtoCURRCInformation ProtocolIE-ID ::= 39

id-gNB-CU-UE-F1AP-ID ProtocolIE-ID ::= 40

id-gNB-DU-UE-F1AP-ID ProtocolIE-ID ::= 41

id-gNB-DU-ID ProtocolIE-ID ::= 42

id-GNB-DU-Served-Cells-Item ProtocolIE-ID ::= 43

id-gNB-DU-Served-Cells-List ProtocolIE-ID ::= 44

id-gNB-DU-Name ProtocolIE-ID ::= 45

id-NRCellID ProtocolIE-ID ::= 46

id-oldgNB-DU-UE-F1AP-ID ProtocolIE-ID ::= 47

id-ResetType ProtocolIE-ID ::= 48

id-ResourceCoordinationTransferContainer ProtocolIE-ID ::= 49

id-RRCContainer ProtocolIE-ID ::= 50

id-SCell-ToBeRemoved-Item ProtocolIE-ID ::= 51

id-SCell-ToBeRemoved-List ProtocolIE-ID ::= 52

id-SCell-ToBeSetup-Item ProtocolIE-ID ::= 53

id-SCell-ToBeSetup-List ProtocolIE-ID ::= 54

id-SCell-ToBeSetupMod-Item ProtocolIE-ID ::= 55

id-SCell-ToBeSetupMod-List ProtocolIE-ID ::= 56

id-Served-Cells-To-Add-Item ProtocolIE-ID ::= 57

id-Served-Cells-To-Add-List ProtocolIE-ID ::= 58

id-Served-Cells-To-Delete-Item ProtocolIE-ID ::= 59

id-Served-Cells-To-Delete-List ProtocolIE-ID ::= 60

id-Served-Cells-To-Modify-Item ProtocolIE-ID ::= 61

id-Served-Cells-To-Modify-List ProtocolIE-ID ::= 62

id-SpCell-ID ProtocolIE-ID ::= 63

id-SRBID ProtocolIE-ID ::= 64

id-SRBs-FailedToBeSetup-Item ProtocolIE-ID ::= 65

id-SRBs-FailedToBeSetup-List ProtocolIE-ID ::= 66

id-SRBs-FailedToBeSetupMod-Item ProtocolIE-ID ::= 67

id-SRBs-FailedToBeSetupMod-List ProtocolIE-ID ::= 68

id-SRBs-Required-ToBeReleased-Item ProtocolIE-ID ::= 69

id-SRBs-Required-ToBeReleased-List ProtocolIE-ID ::= 70

id-SRBs-ToBeReleased-Item ProtocolIE-ID ::= 71

id-SRBs-ToBeReleased-List ProtocolIE-ID ::= 72

id-SRBs-ToBeSetup-Item ProtocolIE-ID ::= 73

id-SRBs-ToBeSetup-List ProtocolIE-ID ::= 74

id-SRBs-ToBeSetupMod-Item ProtocolIE-ID ::= 75

id-SRBs-ToBeSetupMod-List ProtocolIE-ID ::= 76

id-TimeToWait ProtocolIE-ID ::= 77

id-TransactionID ProtocolIE-ID ::= 78

id-TransmissionActionIndicator ProtocolIE-ID ::= 79

id-UE-associatedLogicalF1-ConnectionItem ProtocolIE-ID ::= 80

id-UE-associatedLogicalF1-ConnectionListResAck ProtocolIE-ID ::= 81

id-gNB-CU-Name ProtocolIE-ID ::= 82

id-SCell-FailedtoSetup-List ProtocolIE-ID ::= 83

id-SCell-FailedtoSetup-Item ProtocolIE-ID ::= 84

id-SCell-FailedtoSetupMod-List ProtocolIE-ID ::= 85

id-SCell-FailedtoSetupMod-Item ProtocolIE-ID ::= 86

id-RRCReconfigurationCompleteIndicator ProtocolIE-ID ::= 87

id-Cells-Status-Item ProtocolIE-ID ::= 88

id-Cells-Status-List ProtocolIE-ID ::= 89

id-Candidate-SpCell-List ProtocolIE-ID ::= 90

id-Candidate-SpCell-Item ProtocolIE-ID ::= 91

id-Potential-SpCell-List ProtocolIE-ID ::= 92

id-Potential-SpCell-Item ProtocolIE-ID ::= 93

id-FullConfiguration ProtocolIE-ID ::= 94

id-C-RNTI ProtocolIE-ID ::= 95

id-SpCellULConfigured ProtocolIE-ID ::= 96

id-InactivityMonitoringRequest ProtocolIE-ID ::= 97

id-InactivityMonitoringResponse ProtocolIE-ID ::= 98

id-DRB-Activity-Item ProtocolIE-ID ::= 99

id-DRB-Activity-List ProtocolIE-ID ::= 100

id-EUTRA-NR-CellResourceCoordinationReq-Container ProtocolIE-ID ::= 101

id-EUTRA-NR-CellResourceCoordinationReqAck-Container ProtocolIE-ID ::= 102

id-Protected-EUTRA-Resources-List ProtocolIE-ID ::= 105

id-RequestType ProtocolIE-ID ::= 106

id-ServCellIndex ProtocolIE-ID ::= 107

id-RAT-FrequencyPriorityInformation ProtocolIE-ID ::= 108

id-ExecuteDuplication ProtocolIE-ID ::= 109

id-NRCGI ProtocolIE-ID ::= 111

id-PagingCell-Item ProtocolIE-ID ::= 112

id-PagingCell-List ProtocolIE-ID ::= 113

id-PagingDRX ProtocolIE-ID ::= 114

id-PagingPriority ProtocolIE-ID ::= 115

id-SItype-List ProtocolIE-ID ::= 116

id-UEIdentityIndexValue ProtocolIE-ID ::= 117

id-gNB-CUSystemInformation ProtocolIE-ID ::= 118

id-HandoverPreparationInformation ProtocolIE-ID ::= 119

id-GNB-CU-TNL-Association-To-Add-Item ProtocolIE-ID ::= 120

id-GNB-CU-TNL-Association-To-Add-List ProtocolIE-ID ::= 121

id-GNB-CU-TNL-Association-To-Remove-Item ProtocolIE-ID ::= 122

id-GNB-CU-TNL-Association-To-Remove-List ProtocolIE-ID ::= 123

id-GNB-CU-TNL-Association-To-Update-Item ProtocolIE-ID ::= 124

id-GNB-CU-TNL-Association-To-Update-List ProtocolIE-ID ::= 125

id-MaskedIMEISV ProtocolIE-ID ::= 126

id-PagingIdentity ProtocolIE-ID ::= 127

id-DUtoCURRCContainer ProtocolIE-ID ::= 128

id-Cells-to-be-Barred-List ProtocolIE-ID ::= 129

id-Cells-to-be-Barred-Item ProtocolIE-ID ::= 130

id-TAISliceSupportList ProtocolIE-ID ::= 131

id-GNB-CU-TNL-Association-Setup-List ProtocolIE-ID ::= 132

id-GNB-CU-TNL-Association-Setup-Item ProtocolIE-ID ::= 133

id-GNB-CU-TNL-Association-Failed-To-Setup-List ProtocolIE-ID ::= 134

id-GNB-CU-TNL-Association-Failed-To-Setup-Item ProtocolIE-ID ::= 135

id-DRB-Notify-Item ProtocolIE-ID ::= 136

id-DRB-Notify-List ProtocolIE-ID ::= 137

id-NotficationControl ProtocolIE-ID ::= 138

id-RANAC ProtocolIE-ID ::= 139

id-PWSSystemInformation ProtocolIE-ID ::= 140

id-RepetitionPeriod ProtocolIE-ID ::= 141

id-NumberofBroadcastRequest ProtocolIE-ID ::= 142

id-Cells-To-Be-Broadcast-List ProtocolIE-ID ::= 144

id-Cells-To-Be-Broadcast-Item ProtocolIE-ID ::= 145

id-Cells-Broadcast-Completed-List ProtocolIE-ID ::= 146

id-Cells-Broadcast-Completed-Item ProtocolIE-ID ::= 147

id-Broadcast-To-Be-Cancelled-List ProtocolIE-ID ::= 148

id-Broadcast-To-Be-Cancelled-Item ProtocolIE-ID ::= 149

id-Cells-Broadcast-Cancelled-List ProtocolIE-ID ::= 150

id-Cells-Broadcast-Cancelled-Item ProtocolIE-ID ::= 151

id-NR-CGI-List-For-Restart-List ProtocolIE-ID ::= 152

id-NR-CGI-List-For-Restart-Item ProtocolIE-ID ::= 153

id-PWS-Failed-NR-CGI-List ProtocolIE-ID ::= 154

id-PWS-Failed-NR-CGI-Item ProtocolIE-ID ::= 155

id-ConfirmedUEID ProtocolIE-ID ::= 156

id-Cancel-all-Warning-Messages-Indicator ProtocolIE-ID ::= 157

id-GNB-DU-UE-AMBR-UL ProtocolIE-ID ::= 158

id-DRXConfigurationIndicator ProtocolIE-ID ::= 159

id-RLC-Status ProtocolIE-ID ::= 160

id-DLPDCPSNLength ProtocolIE-ID ::= 161

id-GNB-DUConfigurationQuery ProtocolIE-ID ::= 162

id-MeasurementTimingConfiguration ProtocolIE-ID ::= 163

id-DRB-Information ProtocolIE-ID ::= 164

id-ServingPLMN ProtocolIE-ID ::= 165

id-Protected-EUTRA-Resources-Item ProtocolIE-ID ::= 168

id-GNB-CU-RRC-Version ProtocolIE-ID ::= 170

id-GNB-DU-RRC-Version ProtocolIE-ID ::= 171

id-GNBDUOverloadInformation ProtocolIE-ID ::= 172

id-CellGroupConfig ProtocolIE-ID ::= 173

id-RLCFailureIndication ProtocolIE-ID ::= 174

id-UplinkTxDirectCurrentListInformation ProtocolIE-ID ::= 175

id-DC-Based-Duplication-Configured ProtocolIE-ID ::= 176

id-DC-Based-Duplication-Activation ProtocolIE-ID ::= 177

id-SULAccessIndication ProtocolIE-ID ::= 178

id-AvailablePLMNList ProtocolIE-ID ::= 179

id-PDUSessionID ProtocolIE-ID ::= 180

id-ULPDUSessionAggregateMaximumBitRate ProtocolIE-ID ::= 181

id-ServingCellMO ProtocolIE-ID ::= 182

id-QoSFlowMappingIndication ProtocolIE-ID ::= 183

id-RRCDeliveryStatusRequest ProtocolIE-ID ::= 184

id-RRCDeliveryStatus ProtocolIE-ID ::= 185

id-BearerTypeChange ProtocolIE-ID ::= 186

id-RLCMode ProtocolIE-ID ::= 187

id-Duplication-Activation ProtocolIE-ID ::= 188

id-Dedicated-SIDelivery-NeededUE-List ProtocolIE-ID ::= 189

id-Dedicated-SIDelivery-NeededUE-Item ProtocolIE-ID ::= 190

id-DRX-LongCycleStartOffset ProtocolIE-ID ::= 191

id-ULPDCPSNLength ProtocolIE-ID ::= 192

id-SelectedBandCombinationIndex ProtocolIE-ID ::= 193

id-SelectedFeatureSetEntryIndex ProtocolIE-ID ::= 194

id-ResourceCoordinationTransferInformation ProtocolIE-ID ::= 195

id-ExtendedServedPLMNs-List ProtocolIE-ID ::= 196

id-ExtendedAvailablePLMN-List ProtocolIE-ID ::= 197

id-Associated-SCell-List ProtocolIE-ID ::= 198

id-latest-RRC-Version-Enhanced ProtocolIE-ID ::= 199

id-Associated-SCell-Item ProtocolIE-ID ::= 200

id-Cell-Direction ProtocolIE-ID ::= 201

id-SRBs-Setup-List ProtocolIE-ID ::= 202

id-SRBs-Setup-Item ProtocolIE-ID ::= 203

id-SRBs-SetupMod-List ProtocolIE-ID ::= 204

id-SRBs-SetupMod-Item ProtocolIE-ID ::= 205

id-SRBs-Modified-List ProtocolIE-ID ::= 206

id-SRBs-Modified-Item ProtocolIE-ID ::= 207

id-Ph-InfoSCG ProtocolIE-ID ::= 208

id-RequestedBandCombinationIndex ProtocolIE-ID ::= 209

id-RequestedFeatureSetEntryIndex ProtocolIE-ID ::= 210

id-RequestedP-MaxFR2 ProtocolIE-ID ::= 211

id-DRX-Config ProtocolIE-ID ::= 212

id-IgnoreResourceCoordinationContainer ProtocolIE-ID ::= 213

id-UEAssistanceInformation ProtocolIE-ID ::= 214

id-NeedforGap ProtocolIE-ID ::= 215

id-PagingOrigin ProtocolIE-ID ::= 216

id-new-gNB-CU-UE-F1AP-ID ProtocolIE-ID ::= 217

id-RedirectedRRCmessage ProtocolIE-ID ::= 218

id-new-gNB-DU-UE-F1AP-ID ProtocolIE-ID ::= 219

id-NotificationInformation ProtocolIE-ID ::= 220

id-PLMNAssistanceInfoForNetShar ProtocolIE-ID ::= 221

id-UEContextNotRetrievable ProtocolIE-ID ::= 222

id-BPLMN-ID-Info-List ProtocolIE-ID ::= 223

id-SelectedPLMNID ProtocolIE-ID ::= 224

id-UAC-Assistance-Info ProtocolIE-ID ::= 225

id-RANUEID ProtocolIE-ID ::= 226

id-GNB-DU-TNL-Association-To-Remove-Item ProtocolIE-ID ::= 227

id-GNB-DU-TNL-Association-To-Remove-List ProtocolIE-ID ::= 228

id-TNLAssociationTransportLayerAddressgNBDU ProtocolIE-ID ::= 229

id-portNumber ProtocolIE-ID ::= 230

id-AdditionalSIBMessageList ProtocolIE-ID ::= 231

id-Cell-Type ProtocolIE-ID ::= 232

id-IgnorePRACHConfiguration ProtocolIE-ID ::= 233

id-CG-Config ProtocolIE-ID ::= 234

id-PDCCH-BlindDetectionSCG ProtocolIE-ID ::= 235

id-Requested-PDCCH-BlindDetectionSCG ProtocolIE-ID ::= 236

id-Ph-InfoMCG ProtocolIE-ID ::= 237

id-MeasGapSharingConfig ProtocolIE-ID ::= 238

id-systemInformationAreaID ProtocolIE-ID ::= 239

id-areaScope ProtocolIE-ID ::= 240

id-RRCContainer-RRCSetupComplete ProtocolIE-ID ::= 241

id-TraceActivation ProtocolIE-ID ::= 242

id-TraceID ProtocolIE-ID ::= 243

id-Neighbour-Cell-Information-List ProtocolIE-ID ::= 244

id-SymbolAllocInSlot ProtocolIE-ID ::= 246

id-NumDLULSymbols ProtocolIE-ID ::= 247

id-AdditionalRRMPriorityIndex ProtocolIE-ID ::= 248

id-DUCURadioInformationType ProtocolIE-ID ::= 249

id-CUDURadioInformationType ProtocolIE-ID ::= 250

id-AggressorgNBSetID ProtocolIE-ID ::= 251

id-VictimgNBSetID ProtocolIE-ID ::= 252

id-LowerLayerPresenceStatusChange ProtocolIE-ID ::= 253

id-Transport-Layer-Address-Info ProtocolIE-ID ::= 254

id-Neighbour-Cell-Information-Item ProtocolIE-ID ::= 255

id-IntendedTDD-DL-ULConfig ProtocolIE-ID ::= 256

id-QosMonitoringRequest ProtocolIE-ID ::= 257

id-BHChannels-ToBeSetup-List ProtocolIE-ID ::= 258

id-BHChannels-ToBeSetup-Item ProtocolIE-ID ::= 259

id-BHChannels-Setup-List ProtocolIE-ID ::= 260

id-BHChannels-Setup-Item ProtocolIE-ID ::= 261

id-BHChannels-ToBeModified-Item ProtocolIE-ID ::= 262

id-BHChannels-ToBeModified-List ProtocolIE-ID ::= 263

id-BHChannels-ToBeReleased-Item ProtocolIE-ID ::= 264

id-BHChannels-ToBeReleased-List ProtocolIE-ID ::= 265

id-BHChannels-ToBeSetupMod-Item ProtocolIE-ID ::= 266

id-BHChannels-ToBeSetupMod-List ProtocolIE-ID ::= 267

id-BHChannels-FailedToBeModified-Item ProtocolIE-ID ::= 268

id-BHChannels-FailedToBeModified-List ProtocolIE-ID ::= 269

id-BHChannels-FailedToBeSetupMod-Item ProtocolIE-ID ::= 270

id-BHChannels-FailedToBeSetupMod-List ProtocolIE-ID ::= 271

id-BHChannels-Modified-Item ProtocolIE-ID ::= 272

id-BHChannels-Modified-List ProtocolIE-ID ::= 273

id-BHChannels-SetupMod-Item ProtocolIE-ID ::= 274

id-BHChannels-SetupMod-List ProtocolIE-ID ::= 275

id-BHChannels-Required-ToBeReleased-Item ProtocolIE-ID ::= 276

id-BHChannels-Required-ToBeReleased-List ProtocolIE-ID ::= 277

id-BHChannels-FailedToBeSetup-Item ProtocolIE-ID ::= 278

id-BHChannels-FailedToBeSetup-List ProtocolIE-ID ::= 279

id-BHInfo ProtocolIE-ID ::= 280

id-BAPAddress ProtocolIE-ID ::= 281

id-ConfiguredBAPAddress ProtocolIE-ID ::= 282

id-BH-Routing-Information-Added-List ProtocolIE-ID ::= 283

id-BH-Routing-Information-Added-List-Item ProtocolIE-ID ::= 284

id-BH-Routing-Information-Removed-List ProtocolIE-ID ::= 285

id-BH-Routing-Information-Removed-List-Item ProtocolIE-ID ::= 286

id-UL-BH-Non-UP-Traffic-Mapping ProtocolIE-ID ::= 287

id-Activated-Cells-to-be-Updated-List ProtocolIE-ID ::= 288

id-Child-Nodes-List ProtocolIE-ID ::= 289

id-IAB-Info-IAB-DU ProtocolIE-ID ::= 290

id-IAB-Info-IAB-donor-CU ProtocolIE-ID ::= 291

id-IAB-TNL-Addresses-To-Remove-List ProtocolIE-ID ::= 292

id-IAB-TNL-Addresses-To-Remove-Item ProtocolIE-ID ::= 293

id-IAB-Allocated-TNL-Address-List ProtocolIE-ID ::= 294

id-IAB-Allocated-TNL-Address-Item ProtocolIE-ID ::= 295

id-IABIPv6RequestType ProtocolIE-ID ::= 296

id-IABv4AddressesRequested ProtocolIE-ID ::= 297

id-IAB-Barred ProtocolIE-ID ::= 298

id-TrafficMappingInformation ProtocolIE-ID ::= 299

id-UL-UP-TNL-Information-to-Update-List ProtocolIE-ID ::= 300

id-UL-UP-TNL-Information-to-Update-List-Item ProtocolIE-ID ::= 301

id-UL-UP-TNL-Address-to-Update-List ProtocolIE-ID ::= 302

id-UL-UP-TNL-Address-to-Update-List-Item ProtocolIE-ID ::= 303

id-DL-UP-TNL-Address-to-Update-List ProtocolIE-ID ::= 304

id-DL-UP-TNL-Address-to-Update-List-Item ProtocolIE-ID ::= 305

id-NRV2XServicesAuthorized ProtocolIE-ID ::= 306

id-LTEV2XServicesAuthorized ProtocolIE-ID ::= 307

id-NRUESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 308

id-LTEUESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 309

id-SIB12-message ProtocolIE-ID ::= 310

id-SIB13-message ProtocolIE-ID ::= 311

id-SIB14-message ProtocolIE-ID ::= 312

id-SLDRBs-FailedToBeModified-Item ProtocolIE-ID ::= 313

id-SLDRBs-FailedToBeModified-List ProtocolIE-ID ::= 314

id-SLDRBs-FailedToBeSetup-Item ProtocolIE-ID ::= 315

id-SLDRBs-FailedToBeSetup-List ProtocolIE-ID ::= 316

id-SLDRBs-Modified-Item ProtocolIE-ID ::= 317

id-SLDRBs-Modified-List ProtocolIE-ID ::= 318

id-SLDRBs-Required-ToBeModified-Item ProtocolIE-ID ::= 319

id-SLDRBs-Required-ToBeModified-List ProtocolIE-ID ::= 320

id-SLDRBs-Required-ToBeReleased-Item ProtocolIE-ID ::= 321

id-SLDRBs-Required-ToBeReleased-List ProtocolIE-ID ::= 322

id-SLDRBs-Setup-Item ProtocolIE-ID ::= 323

id-SLDRBs-Setup-List ProtocolIE-ID ::= 324

id-SLDRBs-ToBeModified-Item ProtocolIE-ID ::= 325

id-SLDRBs-ToBeModified-List ProtocolIE-ID ::= 326

id-SLDRBs-ToBeReleased-Item ProtocolIE-ID ::= 327

id-SLDRBs-ToBeReleased-List ProtocolIE-ID ::= 328

id-SLDRBs-ToBeSetup-Item ProtocolIE-ID ::= 329

id-SLDRBs-ToBeSetup-List ProtocolIE-ID ::= 330

id-SLDRBs-ToBeSetupMod-Item ProtocolIE-ID ::= 331

id-SLDRBs-ToBeSetupMod-List ProtocolIE-ID ::= 332

id-SLDRBs-SetupMod-List ProtocolIE-ID ::= 333

id-SLDRBs-FailedToBeSetupMod-List ProtocolIE-ID ::= 334

id-SLDRBs-SetupMod-Item ProtocolIE-ID ::= 335

id-SLDRBs-FailedToBeSetupMod-Item ProtocolIE-ID ::= 336

id-SLDRBs-ModifiedConf-List ProtocolIE-ID ::= 337

id-SLDRBs-ModifiedConf-Item ProtocolIE-ID ::= 338

id-UEAssistanceInformationEUTRA ProtocolIE-ID ::= 339

id-PC5LinkAMBR ProtocolIE-ID ::= 340

id-SL-PHY-MAC-RLC-Config ProtocolIE-ID ::= 341

id-SL-ConfigDedicatedEUTRA-Info ProtocolIE-ID ::= 342

id-AlternativeQoSParaSetList ProtocolIE-ID ::= 343

id-CurrentQoSParaSetIndex ProtocolIE-ID ::= 344

id-gNBCUMeasurementID ProtocolIE-ID ::= 345

id-gNBDUMeasurementID ProtocolIE-ID ::= 346

id-RegistrationRequest ProtocolIE-ID ::= 347

id-ReportCharacteristics ProtocolIE-ID ::= 348

id-CellToReportList ProtocolIE-ID ::= 349

id-CellMeasurementResultList ProtocolIE-ID ::= 350

id-HardwareLoadIndicator ProtocolIE-ID ::= 351

id-ReportingPeriodicity ProtocolIE-ID ::= 352

id-TNLCapacityIndicator ProtocolIE-ID ::= 353

id-CarrierList ProtocolIE-ID ::= 354

id-ULCarrierList ProtocolIE-ID ::= 355

id-FrequencyShift7p5khz ProtocolIE-ID ::= 356

id-SSB-PositionsInBurst ProtocolIE-ID ::= 357

id-NRPRACHConfig ProtocolIE-ID ::= 358

id-RAReportList ProtocolIE-ID ::= 359

id-RLFReportInformationList ProtocolIE-ID ::= 360

id-TDD-UL-DLConfigCommonNR ProtocolIE-ID ::= 361

id-CNPacketDelayBudgetDownlink ProtocolIE-ID ::= 362

id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 363

id-TSCTrafficCharacteristics ProtocolIE-ID ::= 364

id-ReportingRequestType ProtocolIE-ID ::= 365

id-TimeReferenceInformation ProtocolIE-ID ::= 366

id-CNPacketDelayBudgetUplink ProtocolIE-ID ::= 369

id-AdditionalPDCPDuplicationTNL-List ProtocolIE-ID ::= 370

id-RLCDuplicationInformation ProtocolIE-ID ::= 371

id-AdditionalDuplicationIndication ProtocolIE-ID ::= 372

id-ConditionalInterDUMobilityInformation ProtocolIE-ID ::= 373

id-ConditionalIntraDUMobilityInformation ProtocolIE-ID ::= 374

id-targetCellsToCancel ProtocolIE-ID ::= 375

id-requestedTargetCellGlobalID ProtocolIE-ID ::= 376

id-ManagementBasedMDTPLMNList ProtocolIE-ID ::= 377

id-TraceCollectionEntityIPAddress ProtocolIE-ID ::= 378

id-PrivacyIndicator ProtocolIE-ID ::= 379

id-TraceCollectionEntityURI ProtocolIE-ID ::= 380

id-mdtConfiguration ProtocolIE-ID ::= 381

id-ServingNID ProtocolIE-ID ::= 382

id-NPNBroadcastInformation ProtocolIE-ID ::= 383

id-NPNSupportInfo ProtocolIE-ID ::= 384

id-NID ProtocolIE-ID ::= 385

id-AvailableSNPN-ID-List ProtocolIE-ID ::= 386

id-SIB10-message ProtocolIE-ID ::= 387

id-DLCarrierList ProtocolIE-ID ::= 389

 id-ExtendedTAISliceSupportList ProtocolIE-ID ::= 390

id-RequestedSRSTransmissionCharacteristics ProtocolIE-ID ::= 391

id-PosAssistance-Information ProtocolIE-ID ::= 392

id-PosBroadcast ProtocolIE-ID ::= 393

id-RoutingID ProtocolIE-ID ::= 394

id-PosAssistanceInformationFailureList ProtocolIE-ID ::= 395

id-PosMeasurementQuantities ProtocolIE-ID ::= 396

id-PosMeasurementResultList ProtocolIE-ID ::= 397

id-TRPInformationTypeListTRPReq ProtocolIE-ID ::= 398

id-TRPInformationTypeItem ProtocolIE-ID ::= 399

id-TRPInformationListTRPResp ProtocolIE-ID ::= 400

id-TRPInformationItem ProtocolIE-ID ::= 401

id-LMF-MeasurementID ProtocolIE-ID ::= 402

id-SRSType ProtocolIE-ID ::= 403

id-ActivationTime ProtocolIE-ID ::= 404

id-AbortTransmission ProtocolIE-ID ::= 405

id-PositioningBroadcastCells ProtocolIE-ID ::= 406

id-SRSConfiguration ProtocolIE-ID ::= 407

id-PosReportCharacteristics ProtocolIE-ID ::= 408

id-PosMeasurementPeriodicity ProtocolIE-ID ::= 409

id-TRPList ProtocolIE-ID ::= 410

id-RAN-MeasurementID ProtocolIE-ID ::= 411

id-LMF-UE-MeasurementID ProtocolIE-ID ::= 412

id-RAN-UE-MeasurementID ProtocolIE-ID ::= 413

id-E-CID-MeasurementQuantities ProtocolIE-ID ::= 414

id-E-CID-MeasurementQuantities-Item ProtocolIE-ID ::= 415

id-E-CID-MeasurementPeriodicity ProtocolIE-ID ::= 416

id-E-CID-MeasurementResult ProtocolIE-ID ::= 417

id-Cell-Portion-ID ProtocolIE-ID ::= 418

id-SFNInitialisationTime ProtocolIE-ID ::= 419

id-SystemFrameNumber ProtocolIE-ID ::= 420

id-SlotNumber ProtocolIE-ID ::= 421

id-TRP-MeasurementRequestList ProtocolIE-ID ::= 422

id-MeasurementBeamInfoRequest ProtocolIE-ID ::= 423

id-E-CID-ReportCharacteristics ProtocolIE-ID ::= 424

id-ConfiguredTACIndication ProtocolIE-ID ::= 425

id-Extended-GNB-CU-Name ProtocolIE-ID ::= 426

id-Extended-GNB-DU-Name ProtocolIE-ID ::= 427

id-F1CTransferPath ProtocolIE-ID ::= 428

id-SFN-Offset ProtocolIE-ID ::= 429

id-TransmissionStopIndicator ProtocolIE-ID ::= 430

id-SrsFrequency ProtocolIE-ID ::= 431

id-SCGIndicator ProtocolIE-ID ::= 432

id-EstimatedArrivalProbability ProtocolIE-ID ::= 433

id-TRPType ProtocolIE-ID ::= 434

id-SRSSpatialRelationPerSRSResource ProtocolIE-ID ::= 435

id-PDCPTerminatingNodeDLTNLAddrInfo ProtocolIE-ID ::= 436

id-ENBDLTNLAddress ProtocolIE-ID ::= 437

id-PosMeasurementPeriodicityExtended ProtocolIE-ID ::= 438

id-PRS-Resource-ID ProtocolIE-ID ::= 439

id-LocationMeasurementInformation ProtocolIE-ID ::= 440

id-SliceRadioResourceStatus ProtocolIE-ID ::= 441

id-CompositeAvailableCapacity-SUL ProtocolIE-ID ::= 442

id-SuccessfulHOReportInformationList ProtocolIE-ID ::= 443

id-NR-U-Channel-List ProtocolIE-ID ::= 444

id-NR-U ProtocolIE-ID ::= 445

id-Coverage-Modification-Notification ProtocolIE-ID ::= 446

id-CCO-Assistance-Information ProtocolIE-ID ::= 447

id-Neighbor-node-CCO-Assistance-Information-List ProtocolIE-ID ::= 448

id-CellsForSON-List ProtocolIE-ID ::= 449

id-MIMOPRBusageInformation ProtocolIE-ID ::= 450

id-gNB-CU-MBS-F1AP-ID ProtocolIE-ID ::= 451

id-gNB-DU-MBS-F1AP-ID ProtocolIE-ID ::= 452

id-MBS-Area-Session-ID ProtocolIE-ID ::= 453

id-MBS-CUtoDURRCInformation ProtocolIE-ID ::= 454

id-MBS-Session-ID ProtocolIE-ID ::= 455

id-SNSSAI ProtocolIE-ID ::= 456

id-MBS-Broadcast-NeighbourCellList ProtocolIE-ID ::= 457

id-BroadcastMRBs-FailedToBeModified-List ProtocolIE-ID ::= 458

id-BroadcastMRBs-FailedToBeModified-Item ProtocolIE-ID ::= 459

id-BroadcastMRBs-FailedToBeSetup-List ProtocolIE-ID ::= 460

id-BroadcastMRBs-FailedToBeSetup-Item ProtocolIE-ID ::= 461

id-BroadcastMRBs-FailedToBeSetupMod-List ProtocolIE-ID ::= 462

id-BroadcastMRBs-FailedToBeSetupMod-Item ProtocolIE-ID ::= 463

id-BroadcastMRBs-Modified-List ProtocolIE-ID ::= 464

id-BroadcastMRBs-Modified-Item ProtocolIE-ID ::= 465

id-BroadcastMRBs-Setup-List ProtocolIE-ID ::= 466

id-BroadcastMRBs-Setup-Item ProtocolIE-ID ::= 467

id-BroadcastMRBs-SetupMod-List ProtocolIE-ID ::= 468

id-BroadcastMRBs-SetupMod-Item ProtocolIE-ID ::= 469

id-BroadcastMRBs-ToBeModified-List ProtocolIE-ID ::= 470

id-BroadcastMRBs-ToBeModified-Item ProtocolIE-ID ::= 471

id-BroadcastMRBs-ToBeReleased-List ProtocolIE-ID ::= 472

id-BroadcastMRBs-ToBeReleased-Item ProtocolIE-ID ::= 473

id-BroadcastMRBs-ToBeSetup-List ProtocolIE-ID ::= 474

id-BroadcastMRBs-ToBeSetup-Item ProtocolIE-ID ::= 475

id-BroadcastMRBs-ToBeSetupMod-List ProtocolIE-ID ::= 476

id-BroadcastMRBs-ToBeSetupMod-Item ProtocolIE-ID ::= 477

id-Supported-MBS-FSA-ID-List ProtocolIE-ID ::= 478

id-UEIdentity-List-For-Paging-List ProtocolIE-ID ::= 479

id-UEIdentity-List-For-Paging-Item ProtocolIE-ID ::= 480

id-MBS-ServiceArea ProtocolIE-ID ::= 481

id-MulticastMRBs-FailedToBeModified-List ProtocolIE-ID ::= 482

id-MulticastMRBs-FailedToBeModified-Item ProtocolIE-ID ::= 483

id-MulticastMRBs-FailedToBeSetup-List ProtocolIE-ID ::= 484

id-MulticastMRBs-FailedToBeSetup-Item ProtocolIE-ID ::= 485

id-MulticastMRBs-FailedToBeSetupMod-List ProtocolIE-ID ::= 486

id-MulticastMRBs-FailedToBeSetupMod-Item ProtocolIE-ID ::= 487

id-MulticastMRBs-Modified-List ProtocolIE-ID ::= 488

id-MulticastMRBs-Modified-Item ProtocolIE-ID ::= 489

id-MulticastMRBs-Setup-List ProtocolIE-ID ::= 490

id-MulticastMRBs-Setup-Item ProtocolIE-ID ::= 491

id-MulticastMRBs-SetupMod-List ProtocolIE-ID ::= 492

id-MulticastMRBs-SetupMod-Item ProtocolIE-ID ::= 493

id-MulticastMRBs-ToBeModified-List ProtocolIE-ID ::= 494

id-MulticastMRBs-ToBeModified-Item ProtocolIE-ID ::= 495

id-MulticastMRBs-ToBeReleased-List ProtocolIE-ID ::= 496

id-MulticastMRBs-ToBeReleased-Item ProtocolIE-ID ::= 497

id-MulticastMRBs-ToBeSetup-List ProtocolIE-ID ::= 498

id-MulticastMRBs-ToBeSetup-Item ProtocolIE-ID ::= 499

id-MulticastMRBs-ToBeSetupMod-List ProtocolIE-ID ::= 500

id-MulticastMRBs-ToBeSetupMod-Item ProtocolIE-ID ::= 501

id-MBSMulticastF1UContextDescriptor ProtocolIE-ID ::= 502

id-MulticastF1UContext-ToBeSetup-List ProtocolIE-ID ::= 503

id-MulticastF1UContext-ToBeSetup-Item ProtocolIE-ID ::= 504

id-MulticastF1UContext-Setup-List ProtocolIE-ID ::= 505

id-MulticastF1UContext-Setup-Item ProtocolIE-ID ::= 506

id-MulticastF1UContext-FailedToBeSetup-List ProtocolIE-ID ::= 507

id-MulticastF1UContext-FailedToBeSetup-Item ProtocolIE-ID ::= 508

id-IABCongestionIndication ProtocolIE-ID ::= 509

id-IABConditionalRRCMessageDeliveryIndication ProtocolIE-ID ::= 510

id-F1CTransferPathNRDC ProtocolIE-ID ::= 511

id-BufferSizeThresh ProtocolIE-ID ::= 512

id-IAB-TNL-Addresses-Exception ProtocolIE-ID ::= 513

id-BAP-Header-Rewriting-Added-List ProtocolIE-ID ::= 514

id-BAP-Header-Rewriting-Added-List-Item ProtocolIE-ID ::= 515

id-Re-routingEnableIndicator ProtocolIE-ID ::= 516

id-NonF1terminatingTopologyIndicator ProtocolIE-ID ::= 517

id-EgressNonF1terminatingTopologyIndicator ProtocolIE-ID ::= 518

id-IngressNonF1terminatingTopologyIndicator ProtocolIE-ID ::= 519

id-rBSetConfiguration ProtocolIE-ID ::= 520

id-frequency-Domain-HSNA-Configuration-List ProtocolIE-ID ::= 521

id-child-IAB-Nodes-NA-Resource-List ProtocolIE-ID ::= 522

id-Parent-IAB-Nodes-NA-Resource-Configuration-List ProtocolIE-ID ::= 523

id-uL-FreqInfo ProtocolIE-ID ::= 524

id-uL-Transmission-Bandwidth ProtocolIE-ID ::= 525

id-dL-FreqInfo ProtocolIE-ID ::= 526

id-dL-Transmission-Bandwidth ProtocolIE-ID ::= 527

id-uL-NR-Carrier-List ProtocolIE-ID ::= 528

id-dL-NR-Carrier-List ProtocolIE-ID ::= 529

id-nRFreqInfo ProtocolIE-ID ::= 530

id-transmission-Bandwidth ProtocolIE-ID ::= 531

id-nR-Carrier-List ProtocolIE-ID ::= 532

id-Neighbour-Node-Cells-List ProtocolIE-ID ::= 533

id-Serving-Cells-List ProtocolIE-ID ::= 534

id-permutation ProtocolIE-ID ::= 535

id-MDTPollutedMeasurementIndicator ProtocolIE-ID ::= 536

id-M5ReportAmount ProtocolIE-ID ::= 537

id-M6ReportAmount ProtocolIE-ID ::= 538

id-M7ReportAmount ProtocolIE-ID ::= 539

id-SurvivalTime ProtocolIE-ID ::= 540

id-PDCMeasurementPeriodicity ProtocolIE-ID ::= 541

id-PDCMeasurementQuantities ProtocolIE-ID ::= 542

id-PDCMeasurementQuantities-Item ProtocolIE-ID ::= 543

id-PDCMeasurementResult ProtocolIE-ID ::= 544

id-PDCReportType ProtocolIE-ID ::= 545

id-RAN-UE-PDC-MeasID ProtocolIE-ID ::= 546

id-SCGActivationRequest ProtocolIE-ID ::= 547

id-SCGActivationStatus ProtocolIE-ID ::= 548

id-PRSTRPList ProtocolIE-ID ::= 549

id-PRSTransmissionTRPList ProtocolIE-ID ::= 550

id-OnDemandPRS ProtocolIE-ID ::= 551

id-AoA-SearchWindow ProtocolIE-ID ::= 552

id-TRP-MeasurementUpdateList ProtocolIE-ID ::= 553

id-ZoAInformation ProtocolIE-ID ::= 554

id-ResponseTime ProtocolIE-ID ::= 555

id-ARPLocationInfo ProtocolIE-ID ::= 556

id-ARP-ID ProtocolIE-ID ::= 557

id-MultipleULAoA ProtocolIE-ID ::= 558

id-UL-SRS-RSRPP ProtocolIE-ID ::= 559

id-SRSResourcetype ProtocolIE-ID ::= 560

id-ExtendedAdditionalPathList ProtocolIE-ID ::= 561

id-LoS-NLoSInformation ProtocolIE-ID ::= 562

id-NumberOfTRPRxTEG ProtocolIE-ID ::= 564

id-NumberOfTRPRxTxTEG ProtocolIE-ID ::= 565

id-TRPTxTEGAssociation ProtocolIE-ID ::= 566

id-TRPTEGInformation ProtocolIE-ID ::= 567

id-TRPRx-TEGInformation ProtocolIE-ID ::= 568

id-TRP-PRS-Info-List ProtocolIE-ID ::= 569

id-PRS-Measurement-Info-List ProtocolIE-ID ::= 570

id-PRSConfigRequestType ProtocolIE-ID ::= 571

id-MeasurementTimeOccasion ProtocolIE-ID ::= 573

id-MeasurementCharacteristicsRequestIndicator ProtocolIE-ID ::= 574

id-UEReportingInformation ProtocolIE-ID ::= 575

id-PosConextRevIndication ProtocolIE-ID ::= 576

id-TRPBeamAntennaInformation ProtocolIE-ID ::= 577

id-NRRedCapUEIndication ProtocolIE-ID ::= 578

id-Redcap-Bcast-Information ProtocolIE-ID ::= 579

id-RANUEPagingDRX ProtocolIE-ID ::= 580

id-CNUEPagingDRX ProtocolIE-ID ::= 581

id-NRPagingeDRXInformation ProtocolIE-ID ::= 582

id-NRPagingeDRXInformationforRRCINACTIVE ProtocolIE-ID ::= 583

id-NR-TADV ProtocolIE-ID ::= 584

id-QoEInformation ProtocolIE-ID ::= 585

id-CG-SDTQueryIndication ProtocolIE-ID ::= 586

id-SDT-MAC-PHY-CG-Config ProtocolIE-ID ::= 587

id-CG-SDTKeptIndicator ProtocolIE-ID ::= 588

id-CG-SDTindicatorSetup ProtocolIE-ID ::= 589

id-CG-SDTindicatorMod ProtocolIE-ID ::= 590

id-CG-SDTSessionInfoOld ProtocolIE-ID ::= 591

id-SDTInformation ProtocolIE-ID ::= 592

id-SDTRLCBearerConfiguration ProtocolIE-ID ::= 593

id-FiveG-ProSeAuthorized ProtocolIE-ID ::= 594

id-FiveG-ProSeUEPC5AggregateMaximumBitrate ProtocolIE-ID ::= 595

id-FiveG-ProSePC5LinkAMBR ProtocolIE-ID ::= 596

id-SRBMappingInfo ProtocolIE-ID ::= 597

id-DRBMappingInfo ProtocolIE-ID ::= 598

id-UuRLCChannelToBeSetupList ProtocolIE-ID ::= 599

id-UuRLCChannelToBeModifiedList ProtocolIE-ID ::= 600

id-UuRLCChannelToBeReleasedList ProtocolIE-ID ::= 601

id-UuRLCChannelSetupList ProtocolIE-ID ::= 602

id-UuRLCChannelFailedToBeSetupList ProtocolIE-ID ::= 603

id-UuRLCChannelModifiedList ProtocolIE-ID ::= 604

id-UuRLCChannelFailedToBeModifiedList ProtocolIE-ID ::= 605

id-UuRLCChannelRequiredToBeModifiedList ProtocolIE-ID ::= 606

id-UuRLCChannelRequiredToBeReleasedList ProtocolIE-ID ::= 607

id-PC5RLCChannelToBeSetupList ProtocolIE-ID ::= 608

id-PC5RLCChannelToBeModifiedList ProtocolIE-ID ::= 609

id-PC5RLCChannelToBeReleasedList ProtocolIE-ID ::= 610

id-PC5RLCChannelSetupList ProtocolIE-ID ::= 611

id-PC5RLCChannelFailedToBeSetupList ProtocolIE-ID ::= 612

id-PC5RLCChannelFailedToBeModifiedList ProtocolIE-ID ::= 613

id-PC5RLCChannelRequiredToBeModifiedList ProtocolIE-ID ::= 614

id-PC5RLCChannelRequiredToBeReleasedList ProtocolIE-ID ::= 615

id-PC5RLCChannelModifiedList ProtocolIE-ID ::= 616

id-SidelinkRelayConfiguration ProtocolIE-ID ::= 617

id-UpdatedRemoteUELocalID ProtocolIE-ID ::= 618

id-PathSwitchConfiguration ProtocolIE-ID ::= 619

id-PagingCause ProtocolIE-ID ::= 620

id-MUSIM-GapConfig ProtocolIE-ID ::= 621

id-PEIPSAssistanceInfo ProtocolIE-ID ::= 622

id-UEPagingCapability ProtocolIE-ID ::= 623

id-LastUsedCellIndication ProtocolIE-ID ::= 624

id-SIB17-message ProtocolIE-ID ::= 625

id-GNBDUUESliceMaximumBitRateList ProtocolIE-ID ::= 626

id-SIB20-message ProtocolIE-ID ::= 627

id-UE-MulticastMRBs-ToBeReleased-List ProtocolIE-ID ::= 628

id-UE-MulticastMRBs-ToBeReleased-Item ProtocolIE-ID ::= 629

id-UE-MulticastMRBs-ToBeSetup-List ProtocolIE-ID ::= 630

id-UE-MulticastMRBs-ToBeSetup-Item ProtocolIE-ID ::= 631

id-MulticastMBSSessionSetupList ProtocolIE-ID ::= 632

id-MulticastMBSSessionRemoveList ProtocolIE-ID ::= 633

id-PosMeasurementAmount ProtocolIE-ID ::= 634

id-SDT-Termination-Request ProtocolIE-ID ::= 635

id-pathPower ProtocolIE-ID ::= 636

id-DU-RX-MT-RX-Extend ProtocolIE-ID ::= 637

id-DU-TX-MT-TX-Extend ProtocolIE-ID ::= 638

id-DU-RX-MT-TX-Extend ProtocolIE-ID ::= 639

id-DU-TX-MT-RX-Extend ProtocolIE-ID ::= 640

id-BAP-Header-Rewriting-Removed-List ProtocolIE-ID ::= 641

id-BAP-Header-Rewriting-Removed-List-Item ProtocolIE-ID ::= 642

id-SLDRXCycleList ProtocolIE-ID ::= 643

id-TAINSAGSupportList ProtocolIE-ID ::= 644

id-SL-RLC-ChannelToAddModList ProtocolIE-ID ::= 645

id-BroadcastAreaScope ProtocolIE-ID ::= 646

id-ManagementBasedMDTPLMNModificationList ProtocolIE-ID ::= 647

id-SIB15-message ProtocolIE-ID ::= 648

id-ActivationRequestType ProtocolIE-ID ::= 649

id-PosMeasGapPreConfigList ProtocolIE-ID ::= 650

id-InterFrequencyConfig-NoGap ProtocolIE-ID ::= 651

id-MBSInterestIndication ProtocolIE-ID ::= 652

id-UE-MulticastMRBs-ConfirmedToBeModified-List ProtocolIE-ID ::= 653

id-UE-MulticastMRBs-ConfirmedToBeModified-Item ProtocolIE-ID ::= 654

id-UE-MulticastMRBs-RequiredToBeModified-List ProtocolIE-ID ::= 655

id-UE-MulticastMRBs-RequiredToBeModified-Item ProtocolIE-ID ::= 656

id-UE-MulticastMRBs-RequiredToBeReleased-List ProtocolIE-ID ::= 657

id-UE-MulticastMRBs-RequiredToBeReleased-Item ProtocolIE-ID ::= 658

id-L571Info ProtocolIE-ID ::= 659

id-L1151Info ProtocolIE-ID ::= 660

id-SCS-480 ProtocolIE-ID ::= 661

id-SCS-960 ProtocolIE-ID ::= 662

id-SRSPortIndex ProtocolIE-ID ::= 663

id-PEISubgroupingSupportIndication ProtocolIE-ID ::= 664

id-NeedForGapsInfoNR ProtocolIE-ID ::= 665

id-NeedForGapNCSGInfoNR ProtocolIE-ID ::= 666

id-NeedForGapNCSGInfoEUTRA ProtocolIE-ID ::= 667

id-procedure-code-668-not-to-be-used ProtocolIE-ID ::= 668

id-procedure-code-669-not-to-be-used ProtocolIE-ID ::= 669

id-procedure-code-670-not-to-be-used ProtocolIE-ID ::= 670

id-Source-MRB-ID ProtocolIE-ID ::= 671

id-PosMeasurementPeriodicityNR-AoA ProtocolIE-ID ::= 672

id-RedCapIndication ProtocolIE-ID ::= 673

id-SRSPosRRCInactiveConfig ProtocolIE-ID ::= 674

id-SDTBearerConfigurationQueryIndication ProtocolIE-ID ::= 675

id-SDTBearerConfigurationInfo ProtocolIE-ID ::= 676

id-UL-GapFR2-Config ProtocolIE-ID ::= 677

id-ConfigRestrictInfoDAPS ProtocolIE-ID ::= 678

id-UE-MulticastMRBs-Setup-List ProtocolIE-ID ::= 679

id-UE-MulticastMRBs-Setup-Item ProtocolIE-ID ::= 680

id-MulticastF1UContextReferenceCU ProtocolIE-ID ::= 681

id-PosSItypeList ProtocolIE-ID ::= 682

id-DAPS-HO-Status ProtocolIE-ID ::= 683

id-UplinkTxDirectCurrentTwoCarrierListInfo ProtocolIE-ID ::= 684

id-UE-MulticastMRBs-ToBeSetup-atModify-List ProtocolIE-ID ::= 685

id-UE-MulticastMRBs-ToBeSetup-atModify-Item ProtocolIE-ID ::= 686

id-MC-PagingCell-List ProtocolIE-ID ::= 687

id-MC-PagingCell-Item ProtocolIE-ID ::= 688

id-SRSPosRRCInactiveQueryIndication ProtocolIE-ID ::= 689

id-UlTxDirectCurrentMoreCarrierInformation ProtocolIE-ID ::= 690

id-CPACMCGInformation ProtocolIE-ID ::= 691

id-TwoPHRModeMCG ProtocolIE-ID ::= 692

id-TwoPHRModeSCG ProtocolIE-ID ::= 693

id-ExtendedUEIdentityIndexValue ProtocolIE-ID ::= 694

id-ServingCellMO-List ProtocolIE-ID ::= 695

id-ServingCellMO-List-Item ProtocolIE-ID ::= 696

id-ServingCellMO-encoded-in-CGC-List ProtocolIE-ID ::= 697

id-HashedUEIdentityIndexValue ProtocolIE-ID ::= 698

id-UE-MulticastMRBs-Setupnew-List ProtocolIE-ID ::= 699

id-UE-MulticastMRBs-Setupnew-Item ProtocolIE-ID ::= 700

id-ncd-SSB-RedCapInitialBWP-SDT ProtocolIE-ID ::= 701

id-nrofSymbolsExtended ProtocolIE-ID ::= 702

id-repetitionFactorExtended ProtocolIE-ID ::= 703

id-startRBHopping ProtocolIE-ID ::= 704

id-startRBIndex ProtocolIE-ID ::= 705

id-transmissionCombn8 ProtocolIE-ID ::= 706

id-ServCellInfoList ProtocolIE-ID ::= 707

id-DedicatedSIDeliveryIndication ProtocolIE-ID ::= 708

id-Configured-BWP-List ProtocolIE-ID ::= 709

id-Preconfigured-measurement-GAP-Request ProtocolIE-ID ::= 710

id-BWP-Id ProtocolIE-ID ::= 711

id-NetworkControlledRepeaterAuthorized ProtocolIE-ID ::= 712

id-MT-SDT-Information ProtocolIE-ID ::= 713

id-ExtendedResourceSymbolOffset ProtocolIE-ID ::= 714

id-NeedForInterruptionInfoNR ProtocolIE-ID ::= 715

id-SDT-Volume-Threshold ProtocolIE-ID ::= 716

id-SupportedUETypeList ProtocolIE-ID ::= 717

id-MusimCapabilityRestrictionIndication ProtocolIE-ID ::= 718

id-duplicationIndication ProtocolIE-ID ::= 719

id-LTMInformation-Setup ProtocolIE-ID ::= 720

id-LTMConfigurationIDMappingList ProtocolIE-ID ::= 721

id-LTMInformation-Modify ProtocolIE-ID ::= 722

id-LTMCells-ToBeReleased-List ProtocolIE-ID ::= 723

id-LTMCells-ToBeReleased-Item ProtocolIE-ID ::= 724

id-LTMConfiguration ProtocolIE-ID ::= 725

id-EarlySyncInformation-Request ProtocolIE-ID ::= 726

id-EarlySyncInformation ProtocolIE-ID ::= 727

id-EarlySyncInformation-List ProtocolIE-ID ::= 728

id-LTMCellSwitchInformation ProtocolIE-ID ::= 729

id-TAInformation-List ProtocolIE-ID ::= 730

id-Source-gNB-DU-ID ProtocolIE-ID ::= 731

id-dRB-List ProtocolIE-ID ::= 732

id-DeactivationIndication ProtocolIE-ID ::= 733

id-RAReportIndicationList ProtocolIE-ID ::= 734

id-ChannelOccupancyTimePercentageUL ProtocolIE-ID ::= 735

id-SuccessfulPSCellChangeReportInformationList ProtocolIE-ID ::= 736

id-RadioResourceStatusNR-U ProtocolIE-ID ::= 737

id-FiveG-ProSeLayer2Multipath ProtocolIE-ID ::= 738

id-FiveG-ProSeLayer2UEtoUERelay ProtocolIE-ID ::= 739

id-FiveG-ProSeLayer2UEtoUERemote ProtocolIE-ID ::= 740

id-PathAdditionInformation ProtocolIE-ID ::= 741

id-Recommended-SSBs-List ProtocolIE-ID ::= 742

id-Recommended-SSBs-for-Paging-List ProtocolIE-ID ::= 743

id-SSBs-withinTheCell-tobe-Activated-List ProtocolIE-ID ::= 744

id-Cells-With-SSBs-Activated-List ProtocolIE-ID ::= 745

id-Cells-Allowed-to-be-Deactivated-List ProtocolIE-ID ::= 746

id-Cells-Allowed-to-be-Deactivated-List-Item ProtocolIE-ID ::= 747

id-Coverage-Modification-Cause ProtocolIE-ID ::= 748

id-RANTSSRequestType ProtocolIE-ID ::= 749

id-RANTimingSynchronisationStatusInfo ProtocolIE-ID ::= 750

id-TSCTrafficCharacteristicsFeedback ProtocolIE-ID ::= 751

id-RANfeedbacktype ProtocolIE-ID ::= 752

id-Mobile-TRP-LocationInformation ProtocolIE-ID ::= 753

id-Mobile-IAB-MT-UE-ID ProtocolIE-ID ::= 754

id-Target-gNB-ID ProtocolIE-ID ::= 755

id-Target-gNB-IP-address ProtocolIE-ID ::= 756

id-Target-SeGW-IP-address ProtocolIE-ID ::= 757

id-Activated-Cells-Mapping-List ProtocolIE-ID ::= 758

id-Activated-Cells-Mapping-List-Item ProtocolIE-ID ::= 759

id-F1SetupOutcome ProtocolIE-ID ::= 760

id-RRC-Terminating-IAB-Donor-Related-Info ProtocolIE-ID ::= 761

id-RRC-Terminating-IAB-Donor-gNB-ID ProtocolIE-ID ::= 762

id-NCGI-to-be-Updated-List ProtocolIE-ID ::= 763

id-NCGI-to-be-Updated-List-Item ProtocolIE-ID ::= 764

id-Mobile-IAB-MTUserLocationInformation ProtocolIE-ID ::= 765

id-MobileAccessPointLocation ProtocolIE-ID ::= 766

id-AssociatedSessionID ProtocolIE-ID ::= 767

id-IndicationMCInactiveReception ProtocolIE-ID ::= 768

id-MulticastCU2DURRCInfo ProtocolIE-ID ::= 769

id-MBSMulticastSessionReceptionState ProtocolIE-ID ::= 770

id-F1UTunnelNotEstablished ProtocolIE-ID ::= 771

id-MulticastDU2CURRCInfo ProtocolIE-ID ::= 772

id-SIBX-message ProtocolIE-ID ::= 773

id-MulticastCU2DUCommonRRCInfo ProtocolIE-ID ::= 774

id-PDUSetQoSParameters ProtocolIE-ID ::= 775

id-N6JitterInformation ProtocolIE-ID ::= 776

id-ECNMarkingorCongestionInformationReportingRequest ProtocolIE-ID ::= 777

id-ECNMarkingorCongestionInformationReportingStatus ProtocolIE-ID ::= 778

id-NRA2XServicesAuthorized ProtocolIE-ID ::= 779

id-LTEA2XServicesAuthorized ProtocolIE-ID ::= 780

id-NRUESidelinkAggregateMaximumBitrateForA2X ProtocolIE-ID ::= 781

id-LTEUESidelinkAggregateMaximumBitrateForA2X ProtocolIE-ID ::= 782

id-NReRedCapUEIndication ProtocolIE-ID ::= 783

id-ERedcap-Bcast-Information ProtocolIE-ID ::= 784

id-NRPaginglongeDRXInformationforRRCINACTIVE ProtocolIE-ID ::= 785

id-Broadcast-MRBs-Transport-Request-List ProtocolIE-ID ::= aa1

id-Broadcast-MRBs-Transport-Request-Item ProtocolIE-ID ::= aa2

END

-- ASN1STOP

<<<<<<<<<<<<<<<<<<<< End of Change >>>>>>>>>>>>>>>>>>>>