**3GPP TSG-RAN WG3 Meeting #123 *R3-240940***

**Athens, Greece, 26 February – 1 March, 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.473** | **CR** | **1300** | **rev** | **1** | **Current version:** | **18.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Corrections on QoE enhancements |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_ENDC\_SON\_MDT\_enh-Core |  | ***Date:*** | 2024-02-26 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)... Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Incomplete procedural text for QMC Information Transfer Control procedure, CHOICE alternatives are partly described by semantics description and partly described in procedural text.  |
|  |  |
| ***Summary of change:*** | Added procedural text description of gNB-CU behaviour upon reception of Deactivate ALL choice alternative. Removed corresponding semantics description from the tabular.Editorial correction. |
|  |  |
| ***Consequences if not approved:*** | Inconsistent description of QoE information transfer deactivation. |
|  |  |
| ***Clauses affected:*** | 8.16.2.2, 9.2.16.1, 9.2.16.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | r1: merging from R3-24…r0: submitted to RAN3#123 |

### 8.16.2 QoE Information Transfer Control

#### 8.16.2.1 General

The purpose of the QoE Information Transfer Control procedure is to control the RAN visible QoE information transfer from the gNB-CU to the gNB-DU. The procedure uses non-UE associated signalling.

#### 8.16.2.2 Successful operation



Figure 8.16.2.2-1: QoE Information Transfer Control procedure.

The gNB-DU initiates the procedure by sending the QOE INFORMATION TRANSFER CONTROL message to the gNB-CU.

If the *Deactivation Indication* IE is present in the message and set to ‘Per UE’, the gNB-CU shall, if supported, deactivate the QoE information transfer from gNB-CU to gNB-DU for the UEs indicated in the *Deactivation Indication List* IE.

If the *Deactivation Indication* IE is present in the message and set to ‘Deactivate ALL’, the gNB-CU shall, if supported, deactivate the QoE information transfer from gNB-CU to gNB-DU for all UEs served by the gNB-DU.

#### 8.16.2.3 Abnormal Conditions

Not applicable.

#### 9.2.16.1 QOE INFORMATION TRANSFER

This message is sent by a gNB-CU to a gNB-DU, to indicate information related to RAN visible QoE.

Direction: gNB-CU → gNB-DU.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | ignore |
| gNB-CU UE F1AP ID | M  |  | 9.3.1.4 |  | YES | reject |
| gNB-DU UE F1AP ID  | M |  | 9.3.1.5 |  | YES | reject |
| **QoE Information List** |  | *0..1* |  |  | YES | ignore |
| **>QoE Information Item** |  | *1..<maxnoofQoEInformation>* |  |  | EACH | ignore  |
| >>QoE Metrics | O |  | 9.3.1.260 |  | - | - |
| **>>DRB List** |  | *0..1* |  |  | YES | ignore |
| **>>>DRB List Item**  |  | *1 .. <maxnoofDRBs>* |  | The List of DRBs corresponding to the QoE Information.  |  |  |
| >>>>DRB ID | M |  | 9.3.1.8 |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofQoEInformation | Maximum no. of QoE information for one UE, the maximum value is 16. |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE, the maximum value is 64.  |

#### 9.2.16.2 QOE INFORMATION TRANSFER CONTROL

This message is sent by a gNB-DU to the gNB-CU, to control the QoE information transfer.

Direction: gNB-DU  gNB-CU

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type  | M |  | 9.3.1.1 |  | YES | ignore |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| CHOICE *Deactivation Indication* | O |  |  |  | YES | ignore |
| >*Per UE* |  |  |  |  |  |  |
| **>>Deactivation Indication List** |  | *1* |  |  | YES | ignore |
| **>>>Deactivation Indication Item** |  | *1..<maxnoofUEsInQMCTransferControlMessage>* |  |  | - |  |
| >>>> gNB-CU UE F1AP ID | M |  | 9.3.1.4 |  | - |  |
| >>>>gNB-DU UE F1AP ID | M |  | 9.3.1.5 |  | - |  |
| >*Deactivate ALL* |  |  | NULL |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofUEsInQMCTransferControlMessage | Maximum no. of UEs for which QoE transfer control information is received, the maximum value is 512. |