**3GPP TSG-RAN WG4 Meeting #103-e *revision of R4-2208854***

**Electronic Meeting, 9th May to 20th May, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **1** | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR to 38101-1-h50 for SUL combos supporting simultaneous RxTx correction |
|  |  |
| ***Source to WG:*** | MediaTek Inc.,  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | LTE\_NR\_Simult\_RxTx-Core |  | ***Date:*** | 2022-05-09 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | To correct note for SUL\_n41-n9**7** according to the discussion in R4-2208850 |
|  |  |
| ***Summary of change:*** | To add a note of mandatory simultaneous RxTx capability for SUL\_n41-n9**7 “**Note X: The implementation for mandatory simultaneous Rx/Tx is targeted for FWA form factor for this band combination**”** |
|  |  |
| ***Consequences if not approved:*** | SUL\_n41-n95 may not be feasible on smart phone for mandatory simultaneous RxTx capability |
|  |  |
| ***Clauses affected:*** | 5.2C |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-1  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<<< Start of changed sections >>>

## 5.2C Operating band combination for SUL

NR operation is designed to operate in the operating band combination defined in Table 5.2C-1, Table 5.2C-2, Table 5.2C-3 and Table 5.2C-4, where all operating bands are within FR1.

If the mandatory simultaneous Rx/Tx capability applies for a band combination, the mandatory simultaneous Rx/Tx capability also applies for the band combination when the applicable band combination is a subset of a higher order band combination.

Table 5.2C-1: Operating band combination for SUL in FR1

|  |  |
| --- | --- |
| NR Band combination for SUL | NR Band(Table 5.2-1) |
| SUL\_n24-n992 | n24, n99 |
| SUL\_n41-n80 | n41, n80 |
| SUL\_n41-n81 | n41, n81 |
| SUL\_n41-n832 | n41, n83 |
| SUL\_n41-n952 | n41, n95 |
| SUL\_n41-n972,X | n41, n97 |
| SUL\_n41-n982 | n41, n98 |
| SUL\_n41-n992 | n41, n99 |
| SUL\_n48-n992 | n48, n99 |
| SUL\_n77-n802 | n77, n80 |
| SUL\_n77-n842 | n77, n84 |
| SUL\_n77-n992 | n77, n99 |
| SUL\_n78-n802 | n78, n80 |
| SUL\_n78-n812 | n78, n81 |
| SUL\_n78-n822 | n78, n82 |
| SUL\_n78-n832 | n78, n83 |
| SUL\_n78-n842 | n78, n84 |
| SUL\_n78-n862 | n78, n86 |
| SUL\_n79-n802 | n79, n80 |
| SUL\_n79-n812 | n79, n81 |
| SUL\_n79-n832 | n79, n83 |
| SUL\_n79-n84 | n79, n84 |
| SUL\_n79-n952 | n79, n95 |
| SUL\_n79-n972 | n79, n97 |
| SUL\_n79-n982 | n79, n98 |
| NOTE 1: If a UE is configured with both NR UL and NR SUL carriers in a cell, the switching time between NR UL carrier and NR SUL carrier is 0 us.NOTE 2: For UE supporting SUL band combination simultaneous Rx/Tx capability is mandatory.Note X: The implementation for mandatory simultaneous Rx/Tx is targeted for FWA form factor for this band combination |

<<< End of changed sections >>>