**3GPP TSG-RAN4 Meeting #103-e *R4-2208901***

**Online, , May 9-20, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **2344** | **rev** | **1** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to TS 38.133: Introduction of band n100  |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_RAIL\_EU\_900MHz-Core |  | ***Date:*** | 2022-05-09 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** |  Add support for band n100 |
|  |  |
| ***Summary of change:*** |  Add n100 to the corresponding FR1 group |
|  |  |
| ***Consequences if not approved:*** | n100 won’t be correctly supported |
|  |  |
| ***Clauses affected:*** | 3.5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*<Start of the change>*

### 3.5.2 NR operating bands in FR1

NR frequency bands grouping for FR1 is specified in Table 3.5.2-1.

Table 3.5.2-1: NR frequency band groups for FR1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Group | NR FDD | NR TDD | NR SDL | NR CCA10 |
|  | Band group notation | Operating bands | Band group notation | Operating bands | Band group notation | Operating bands | Band group notation | Operating bands |
| A | NR\_FDD\_FR1\_A | n1, n18, n24, n70, n744, n91, n92, n93, n94, n100 | NR\_TDD\_FR1\_A | n34, n389, n39, n40, n50, n51, n53, n101 | NR\_SDL\_FR1\_A | n67, n75, n76 | NR\_CCA\_FR1\_A | - |
| B | NR\_FDD\_FR1\_B | n65, n66, n743 | NR\_TDD\_FR1\_B | n387 | NR\_SDL\_FR1\_B | - | NR\_CCA\_FR1\_B | - |
| C | NR\_FDD\_FR1\_C | n30 | NR\_TDD\_FR1\_C | n48, n771, n78, n79 | NR\_SDL\_FR1\_C | - | NR\_CCA\_FR1\_C | - |
| D | NR\_FDD\_FR1\_D | n28 | NR\_TDD\_FR1\_D | n772 | NR\_SDL\_FR1\_D | - | NR\_CCA\_FR1\_D | - |
| E | NR\_FDD\_FR1\_E | n2, n5, n7 | NR\_TDD\_FR1\_E | n41, n90 | NR\_SDL\_FR1\_E | - | NR\_CCA\_FR1\_E | - |
| F | NR\_FDD\_FR1\_F | n266 | NR\_TDD\_FR1\_F | - | NR\_SDL\_FR1\_F | - | NR\_CCA\_FR1\_F | - |
| G | NR\_FDD\_FR1\_G | n3, n8, n12, n13, n14, n20, n71, n85 | NR\_TDD\_FR1\_G | - | NR\_SDL\_FR1\_G | n29 | NR\_CCA\_FR1\_G | - |
| H | NR\_FDD\_FR1\_H | n25 | NR\_TDD\_FR1\_H | - | NR\_SDL\_FR1\_H | - | NR\_CCA\_FR1\_H | - |
| I | NR\_FDD\_FR1\_I | - | NR\_TDD\_FR1\_I |  | NR\_SDL\_FR1\_I | - | NR\_CCA\_FR1\_I | n46 |
| J | NR\_FDD\_FR1\_J | - | NR\_TDD\_FR1\_J | n478, n96 | NR\_SDL\_FR1\_J | - | NR\_CCA\_FR1\_J | n96 |
| NOTE 1: Except 3.8 GHz to 4.2 GHz.NOTE 2: Only 3.8 GHz to 4.2 GHz.NOTE 3: Except 1475.9 MHz to 1510.9 MHz.NOTE 4: Only when the band is confined in 1475.9 MHz to 1510.9 MHz.NOTE 5: These bands are used only in NR carrier aggregation with other NR bands according to NR CA band combinations specified in TS 38.101-1 [18] and TS 38.101-3 [20].NOTE 6: The minimum Io condition is reduced by 0.5 dB when the carrier frequency of the assigned NR channel bandwidth is within 865-894 MHz. NOTE 7: When this band is only used for V2X SL service, the band is exclusively used for NR V2X in particular regions.NOTE 8: This band is unlicensed band used for V2X service. There is no expected network deployment in this band.NOTE 9: When this band is only used for WAN service.NOTE 10: Operating bands where operation on carrier frequencies with CCA is supported. |

*<End of the change>*