**3GPP TSG-RAN WG4 Meeting # 108bis R4-23XXXX**

**Xiamen, China, October 09 - October 13, 2023**

**Agenda item:** 5.13.8

**Source:** Moderator (CMCC)

**Title:** Ad hoc minutes for [108bis][212] NR\_ATG

**Document for:** Approval

# Introduction

Summary of RRM core requirements maintenance and RRM performance requirements for Rel-18 NR ATG, including agenda 5.13.5 and 5.13.6 are in R4-2317204. The agreed way forward in previous meetings are R4-2314307, R4-2310159, R4-2306344, R4-2303226, R4-2220361, R4-2217256 and R4-2214737.

The adhoc session will focus on some maintenance issues first and then discuss issues of performance requirements.

# Maintainance

|  |
| --- |
| Last meeting agreements for phase antenna array impact:  **Issue 4-1-1: Phase antenna array impact for L3 measurements**   * Do not introduce scaling factor N and the existing measurement requirements can be reused for ATG UEs [with omnidirectional antennas] * Introduce scaling factor N for L3 measurements for ATG UEs with [antenna arrays]   + N = 3 for the case when network assistance on ATG cells reference locations is provided   + N = 4 otherwise   **Issue 4-1-2: Phase antenna array impact for L1measurements**   * Do not introduce scaling factor N. Existing measurement requirements can be reused, provided that beam steering based on the positioning is capable for the ATG UE. |

## Issue 5-1: Phase antenna array impact for L3 measurements

* Proposals
  + **For the applicability of scaling factor**
  + Option 1: The scaling factor should be also applied for L3 measurements with MG. (CMCC)
  + **For the specific value of scaling factor**
  + Option 1: (CMCC, HW, ZTE)
    - For intra-frequency L3 measurements without MG of ATG UE with antenna array
      * N = 3 for the case when network assistance on ATG cells reference BS locations is provided
      * N = 4 otherwise
    - For inter-frequency L3 measurements (also for RRC IDLE/INACTIVE mode) of ATG UE with antenna array
      * N = 2 for the case when network assistance on ATG cells reference BS locations is provided
      * Option 1-1: N = 3 otherwise (CMCC, ZTE)
      * Option 1-2: N =4 otherwise (HW)
* Recommended WF
  + To be discussed

## Issue 2-2: Tsearch in HO requirements for UE with antenna array

* Proposals
  + For HO requirements, when network assistance on ATG unknown target cell’s reference BS locations is provided,
    - Option 1-1: no need to scale the Tsearch (CMCC, ZTE)
  + For HO requirements, when network assistance on ATG unknown target cell’s reference BS locations is not provided,
    - Option 1-2: the Tsearch should be scaled with scaling factor N=3. (CMCC)
    - Option 1-3: the Tsearch should be scaled with scaling factor N=[3 or 4]. (ZTE)
* Recommended WF
  + Option 1-1 can be agreed.
  + Further discuss Option 1-2 and Option 1-3

## Issue 2-3: Tmeasure in CHO requirements for UE with antenna array

* Proposals
  + Option 1: For intra-frequency CHO requirements, when network assistance on ATG cells reference BS locations is provided to UE with antenna array, the scaling factor of Tidentify intra with index or Tidentify\_intra\_without\_index should be decreased to N=2, and N=3 otherwise. (CMCC)
* Recommended WF
  + To be discussed

## Issue 2-4: Requirement applicability for CHO requirement

* Proposals
  + Option 1: For CHO requirements, it should be applicable even if UE doesn’t have the valid and applicable parameters of BS location information and Koffset for target NR cell. (CMCC)
* Recommended WF
  + To be discussed

## Issue 2-5: Tidentify\_intra\_NR in RRC Re-establishment delay requirement for UE with antenna array

* Proposals
  + Option 1: For UE with antenna array, the scaling factor should be considered for unknown cells of intra-frequency and inter-frequency in RRC Re-establishment delay requirement requirements. The scaling factor of L3 measurements should be used. (CMCC)
    - For intra-frequency, N = 3 for the case when network assistance on ATG cells reference BS locations is provided, N = 4 otherwise.
    - For inter-frequency, N = 2 for the case when network assistance on ATG cells reference BS locations is provided, N = 3 otherwise.
  + Option 2: The consideration of phase array antenna should be extended to the requirement of Tidentify\_intra\_NR and Tidentify\_inter\_NR, i withinRRC re-establishment as: (ZTE)

Table 6.2X.1.2.1-1: Time to identify target NR cell for RRC connection re-establishment to NR intra-frequency cell

|  |  |  |  |
| --- | --- | --- | --- |
| Serving cell | FR of target NR | Tidentify\_intra\_NR [ms] | |
| SSB Ês/Iot (dB) | cell | Known NR cell | Unknown NR cell |
| ≥ -8 | FR1 | MAX (200 ms, 5 x N2 x TSMTC) | MAX (800 ms, 10 x N2 x TSMTC) |
| < -8 | FR1 | N/A | 800Note1 |
| Note 1: The UE is not required to successfullyidentify a cell on any NR frequency layer when TSMTC > 20 ms and serving cell SSB Ês/Iot < -8 dB.  Note 2: If [omnidirectional antennas] is assumed at UE, N = 1.  If [Phase antenna array] is assumed at UE,  - When [network assistance on ATG cells reference location] of the target cell is provided to UE, N = 3;  - Otherwise, N = [3 or 4]. | | | |

Table 6.2X.1.2.1-2: Time to identify target NR cell for RRC connection re-establishment to NR inter-frequency cell

|  |  |  |  |
| --- | --- | --- | --- |
| Serving cell SSB Ês/Iot (dB) | FR of target NR cell | Tidentify\_inter\_NR, i [ms] | |
|  |  | Known NR cell | Unknown NR cell |
| ≥ -8 | FR1 | MAX (200 ms, 6 x N2 x TSMTC, i) | MAX (800 ms, 13 x N2 x TSMTC, i) |
| < -8 | FR1 | N/A | 800Note1 |
| Note 1: The UE is not required to successfully identify a cell on any NR frequency layer when TSMTC,i > 20 ms and serving cell SSB Ês/Iot < -8 dB.  Note 2: If [omnidirectional antennas] is assumed at UE, N = 1.  If [Phase antenna array] is assumed at UE,  - When [network assistance on ATG cells reference location] of the target cell is provided to UE, N = 2;  - Otherwise, N = [3 or 4]. | | | |

* Recommended WF
  + Firstly, for the UE with antenna array, discuss whether the scaling factor is needed for known NR cell and unknown NR cell separately
  + Secondly, discuss the scaling number

## Issue 2-6: Tidentify\_NR in RRC connection release with redirection requirement for UE with antenna array

* Proposals
  + Option 1: For UE with antenna array, the scaling factor of L3 inter-frequency measurements are suggested to be used. N = 2 for the case when network assistance on ATG cells reference BS locations is provided, N = 3 otherwise. (CMCC)
  + Option 2: The consideration of phase array antenna should be extended to the requirement of Tidentify-NR within RRC connection release with redirection to NR as below: (ZTE)

Table 6.2X.3.2.1-1: Time to identify target NR cell for RRC connection release with redirection to NR

|  |  |
| --- | --- |
| FR of target NR cell | Tidentify-NR |
| FR1 | MAX (680 ms, 11 x N2 x Trs) |
| Note 1: If the UE has been provided with higher layer signaling of *smtc2*specified in TS 38.331 [2] prior to the redirection command, Trs follows *smtc1* or *smtc2* according to the physical cell ID of the target cell.  Note 2: If [omnidirectional antennas] is assumed at UE, N = 1.  If [Phase antenna array] is assumed at UE,  - When [network assistance on ATG cells reference location] of the target cell is provided to UE, N = 2;  - Otherwise, N = [3 or 4]. | |

* Recommended WF
  + Firstly, for the UE with antenna array, discuss whether the scaling factor is needed
  + Secondly, discuss the scaling number

## Issue 3-1: validity timer for ATG

* Proposals
  + Option 1: remove the brackets and keep the validity timer statement, since running validity timer for is a sign that the UE has received data in SIB regarding ATG gNB positions and is ready to transmit in UL. (Ericsson)

*The ATG UE shall meet the Te\_ATG requirement for an initial transmission provided that at least one SSB is available at the ATG UE during the last 160 ms. [and the ATG UE has a validity time running for NTA,UE-specific.] The reference point for the ATG UE initial transmit timing control requirement shall be the downlink timing of the reference cell minus .*

*The timing advance is initiated by ATG UE configured with only PCell [served by gNB upon initiating a validity timer for . ] The timing advance can be adjusted with MAC message that implies the adjustment of the timing advance, as defined in clause 5.2 of TS 38.321 [7].*

* Recommended WF
  + To be discussed

## Issue 5-2: If any additional UE capability is needed for ATG UEs with [antenna arrays]

* Proposals
  + Option 1: No capability is needed for ATG UE to support antenna arrays in FR1 4GHz. (Ericsson)
  + Option 2: Define a UE capability to differentiate UE with [omnidirectional antennas] and UE with [antenna arrays]. (HW)
  + Option 3: For the band n79 capable UE, it works with phase antenna array by default at band n79. (ZTE)
    - Regarding the antenna assumption, phase antenna array is tied with band n79, and omni-antenna is tied with other ATG bands.
* Recommended WF
  + To be discussed

# Performance requirements

## Issue 6-1-1: Measurement accuracy

* Proposals
  + Option 1: Reuse the Es/Iot side condition and measurement accuracy requirement of legacy TN network for ATG.(CMCC)
  + Option 2: The accuracy requirement of L1 measurement should be identified for ATG. Regarding L3 measurement accuracy, reuse the accuracy requirement of legacy FR1 TN for the non-phase array antenna assumption; it is better to identify the accuracy requirement for the phase array antenna assumption. (ZTE)
* Recommended WF
  + reuse the L3 and L1 accuracy requirement of legacy FR1 TN for the non-phase array antenna assumption
  + Further discuss whether to identify the incremental accuracy requirement for the phase array antenna assumption

## Issue 6-2-1: General test configuration

* Proposals
  + Option 1: (CMCC)
    - Configuration 1:15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode, only for UE with omnidirectional antennas
    - Configuration 2: 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode, for both UE with omnidirectional antennas and for UE with antenna array
  + Option 2: (ZTE)
    - Testing band:
      * Band n79 should be configured for the sake of phase array antenna relevant enhancements testing;
      * At least one band within {n1, n3, n34, n39, n41, n78} is considered to test other ATG enhancement besides the phase array antenna relevant enhancements testing;
    - Duplex:
      * Similar as in legacy, both FDD and TDD should be configured.
    - SCS:
      * Similar as in legacy, both 15kHz, 30kHz should be configured.
      * Not consider 60kHz since some RRM requirement is vacant for 60kHz.
    - TDD pattern:
      * TDD pattern ‘30D4S6U’, S=’14GP’ should be prioritized in the test.
  + Option 3: RAN4 to discuss additional test cases considering the new TDD pattern for ATG (if agreed). (Ericsson)
* Recommended WF
  + To be discussed based on Option 1, and further discuss whether and how to configure the testing band and TDD pattern

## Issue 6-2-2: Test scope

* Proposals
  + Option 1: Only define test case for non-DRX mode in connected mode (HW, Ericsson)
  + Option 2: Define test cases for both DRX mode and non-DRX mode. (CMCC)
  + Option 3: RAN4 not to define test cases for SCC. (Ericsson)
  + Option 4: A general principle is to only define the test cases for those requirements that are different from the TN deployment or not involved in the TN deployment. (ZTE)
* Recommended WF
  + RAN4 not to define test cases for SCC
  + For DRX configuration: To be discussed
  + Further discuss whether to define the test cases which has same core requirements as TN
  + Companies can show your support in the table below

|  |  |  |
| --- | --- | --- |
| **Test scope**  **RRC\_IDLE state mobility** | **Test number** | **Supporter** |
| Cell reselection to intra-frequency neighbour cell | ATG 1-1 | CMCC (Neighbour cell reference BS location is provided)  HW, Ericsson |
| Location based cell reselection to intra-frequency neighbour cell | ATG 1-2 | CMCC (Neighbour cell reference BS location is provided) |
| Cell reselection to inter-frequency neighbour cell | ATG 1-3 | CMCC (Neighbour cell reference BS location is not provided)  HW, Ericsson |
| Cell reselection to inter-frequency NR cell for UE configured with [enhanced requirements] | ATG 1-4 | CMCC (Neighbour cell reference BS location is provided)  HW, Ericsson, ZTE |
| Location based cell reselection to inter-frequency neighbour cell | ATG 1-5 | CMCC (Neighbour cell reference BS location is provided) |

|  |  |  |
| --- | --- | --- |
| **Test scope**  **RRC\_CONNECTED state mobility** | **Test number** | **Supporter** |
| Intra-frequency HO with known target cell | ATG 2-1 | CMCC, HW, Ericsson |
| Intra-frequency HO with unknown target cell | ATG 2-2 | CMCC (Neighbour cell reference BS location is provided)  HW, Ericsson |
| Inter-frequency HO with known target cell | ATG 2-3 | CMCC, [HW] |
| Inter-frequency HO with unknown target cell | ATG 2-4 | CMCC (Neighbour cell reference BS location is not provided)  HW, Ericsson |
| Intra-frequency location based CHO | ATG 2-5 | CMCC (Neighbour cell reference BS location is not provided)  HW, Ericsson |
| Inter-frequency location based CHO | ATG 2-6 | CMCC (Neighbour cell reference BS location is provided)  HW, Ericsson |
| Intra-frequency RRC Re-establishment with known target cell | ATG 2-7 | CMCC  HW, Ericsson |
| Intra-frequency RRC Re-establishment with unknown target cell | ATG 2-8 | CMCC (Neighbour cell reference BS location is not provided) |
| Inter-frequency RRC Re-establishment with known target cell | ATG 2-9 | CMCC |
| Inter-frequency RRC Re-establishment with unknown target cell | ATG 2-10 | CMCC (Neighbour cell reference BS location is provided)  HW, Ericsson |
| Inter-frequency RRC Re-establishment in FR1 without serving cell timing | ATG 2-11 | HW |
| 4-step RA type contention based random access test | ATG 2-12 | CMCC, HW, Ericsson |
| 4-step RA type Non-Contention based random access test | ATG 2-13 | CMCC, HW, Ericsson |
| 2-step RA type contention based random access test | ATG 2-14 | CMCC, Ericsson |
| 2-step RA type Non-Contention based random access test | ATG 2-15 | CMCC, Ericsson |
| RRC Connection Release with Redirection | ATG 2-16 | CMCC (Neighbour cell reference BS location is provided)  HW, Ericsson |

|  |  |  |
| --- | --- | --- |
| **Test scope**  **Timing** | **Test number** | **Supporter** |
| UE transmit timing test | ATG 3-1 | CMCC, Ericsson, ZTE |
| Timing advance adjustment delay and accuracy | ATG 3-2 | CMCC, Ericsson, ZTE |

|  |  |  |
| --- | --- | --- |
| **Test scope**  **Signalling characteristics** | **Test number** | **Supporter** |
| Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode | ATG 4-1 | CMCC, HW, Ericsson |
| Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode | ATG 4-2 | CMCC, HW, Ericsson |
| Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode | ATG 4-3 | CMCC |
| Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode | ATG 4-4 | CMCC |
| Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode | ATG 4-5 | CMCC, HW, Ericsson |
| Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode | ATG 4-6 | CMCC, HW, Ericsson |
| Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode | ATG 4-7 | CMCC |
| Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode | ATG 4-8 | CMCC |
| Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in non-DRX mode | ATG 4-9 | CMCC, HW, Ericsson |
| Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in DRX mode | ATG 4-10 | CMCC |
| Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in non-DRX mode | ATG 4-11 | CMCC, HW, Ericsson |
| Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in DRX mode | ATG 4-12 | CMCC |
| DCI-based and Timer-based Active BWP Switch | ATG 4-13 | CMCC, HW, Ericsson |
| RRC-based Active BWP Switch | ATG 4-14 | CMCC, HW, Ericsson |
| UE specific CBW change | ATG 4-15 | CMCC, HW, Ericsson |
| Pathloss reference signal switching delay | ATG 4-16 | CMCC |

|  |  |  |
| --- | --- | --- |
| **Test scope**  **Measurement procedure** | **Test number** | **Supporter** |
| Intra-frequency measurements event triggered reporting tests without gap under non-DRX | ATG 5-1 | CMCC (Neighbour cell reference BS location is provided)  HW, Ericsson, ZTE (under phase antenna array assumption) |
| Intra-frequency measurements event triggered reporting tests without gap under DRX | ATG 5-2 | CMCC (Neighbour cell reference BS location is not provided), ZTE (under phase antenna array assumption) |
| Intra-frequency measurements event triggered reporting tests with per-UE gaps under non-DRX | ATG 5-3 | CMCC (Neighbour cell reference BS location is not provided)  HW, Ericsson, ZTE (under phase antenna array assumption) |
| Intra-frequency measurements event triggered reporting tests with per-UE gaps under DRX | ATG 5-4 | CMCC (Neighbour cell reference BS location is provided), ZTE (under phase antenna array assumption) |
| Intra-frequency measurements event triggered reporting tests without gap under non-DRX with SSB index reading | ATG 5-5 | CMCC (Neighbour cell reference BS location is provided), ZTE (under phase antenna array assumption) |
| Intra-frequency measurements SA event triggered reporting tests with per-UE gaps under non-DRX with SSB index reading | ATG 5-6 | CMCC (Neighbour cell reference BS location is provided), ZTE (under phase antenna array assumption) |
| Inter-frequency measurements event triggered reporting tests for FR1 without SSB time index detection when DRX is not used | ATG 5-7 | CMCC (Neighbour cell reference BS location is not provided)  HW, Ericsson, ZTE (under phase antenna array assumption) |
| Inter-frequency measurements event triggered reporting tests for FR1 without SSB time index detection when DRX is used | ATG 5-8 | CMCC (Neighbour cell reference BS location is provided), ZTE (under phase antenna array assumption) |
| Inter-frequency measurements event triggered reporting tests for FR1 with SSB time index detection when DRX is not used | ATG 5-9 | CMCC (Neighbour cell reference BS location is provided)  HW, ZTE (under phase antenna array assumption) |
| Inter-frequency measurements event triggered reporting tests for FR1 with SSB time index detection when DRX is used | ATG 5-10 | CMCC (Neighbour cell reference BS location is not provided), ZTE (under phase antenna array assumption) |
| Inter-frequency measurements event triggered reporting tests for FR1 without gap when DRX is used | ATG 5-11 | CMCC (Neighbour cell reference BS location is provided), ZTE (under phase antenna array assumption) |
| Inter-frequency measurements event triggered reporting tests for FR1 without gap when DRX is not used | ATG 5-12 | CMCC (Neighbour cell reference BS location is provided)  HW, ZTE (under phase antenna array assumption) |
| SSB based L1-RSRP measurement when DRX is not used | ATG 5-13 | CMCC, HW, Ericsson, ZTE (under phase antenna array assumption) |
| SSB based L1-RSRP measurement when DRX is used | ATG 5-14 | CMCC, ZTE (under phase antenna array assumption) |
| CSI-RS based L1-RSRP measurement when DRX is not used | ATG 5-15 | CMCC, HW, Ericsson, ZTE (under phase antenna array assumption) |
| CSI-RS based L1-RSRP measurement when DRX is used | ATG 5-16 | CMCC, ZTE (under phase antenna array assumption) |
| L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured when DRX is used | ATG 5-17 | CMCC, ZTE (under phase antenna array assumption) |
| L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is not used | ATG 5-18 | CMCC, HW, ZTE (under phase antenna array assumption) |
| L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is not used | ATG 5-19 | CMCC, HW, ZTE (under phase antenna array assumption) |
| SA intra-frequency CGI identification of NR neighbor cell in FR1 | ATG 5-20 | CMCC |

|  |  |  |
| --- | --- | --- |
| **Test scope**  **Measurement Performance requirements** | **Test number** | **Supporter** |
| SS-RSRP intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-1 | CMCC, ZTE (under phase antenna array assumption) |
| SS-RSRP inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-2 | CMCC, ZTE (under phase antenna array assumption) |
| SS-RSRQ intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-3 | CMCC, ZTE (under phase antenna array assumption) |
| SS-RSRQ inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-4 | CMCC, ZTE (under phase antenna array assumption) |
| SS-SINR intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-5 | CMCC, ZTE (under phase antenna array assumption) |
| SS-SINR inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-6 | CMCC, ZTE (under phase antenna array assumption) |
| L1-RSRP measurement SSB based L1-RSRP measurement | ATG 6-7 | CMCC |
| L1-RSRP measurement CSI-RS based L1-RSRP measurement on resource set with repetition off | ATG 6-8 | CMCC |
| L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off | ATG 6-9 | CMCC |
| L1-SINR measurement with SSB based CMR and dedicated IMR | ATG 6-10 | CMCC |
| L1-SINR measurement with CSI-RS based CMR and dedicated IMR | ATG 6-11 | CMCC |
| CSI-RSRP intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-12 | CMCC |
| CSI-RSRP inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-13 | CMCC |
| CSI-RSRQ Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-14 | CMCC |
| CSI-RSRQ Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-15 | CMCC |
| CSI-SINR intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-16 | CMCC |
| CSI-SINR Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell | ATG 6-17 | CMCC |

## Issue 6-2-3: RMC

* Proposals
  + Option 1: The legacy NR RMCs defined in section A.3.1 of TS 38.133 are reused for ATG test cases. (Ericsson)
* Recommended WF
  + Option 1 can be the baseline

## Issue 6-2-4: OCNG

* Proposals
  + Option 1: Following legacy NR OCNGs are reused for ATG test cases: (Ericsson)
    - Generic OCNG pattern for all unused REs defined in A.3.2.1.1 in TS 38.133.
    - Generic OCNG pattern for unused REs in the same bandwidth as CORESET defined in A.3.2.1.3 of TS 38.133.
    - Generic OCNG pattern for all unused REs outside SSB slot(s) defined in A.3.2.1.4 in TS 38.133
* Recommended WF
  + Option 1 can be the baseline.

## Issue 6-2-5: Test method for UE with antenna array

* Proposals
  + Option 1: RAN4 to discuss whether and how to define test cases for an ATG UE with antenna array (HW)
  + Option 2: RAN4 to discuss how to model the L3 measurement test with beam sweeping in FR1 4GHz. (Ericsson)
* Recommended WF
  + To be discussed

## Issue 6-2-6: whether to define test cases for TCI switching delay requirements

* Proposals
  + Option 1: RAN4 to discuss the test cases for TCI switching delay requirements for MAC-, DCI and RRC-based TCI state switching delay requirements. (Ericsson)
* Recommended WF
  + To be discussed

## Issue 6-2-7: GNSS setup

* Proposals
  + Option 1: GNSS is viable via AT command for all test cases, and GNSS only changed during the test for location-based CHO. (HW)
* Recommended WF
  + To be discussed

## Issue 6-2-8: UE mobility assumption

* Proposals
  + Option 1: For the location-based cell re-selection tests, location-based CHO tests and UL transmit timing tests, the UE mobility should be assumed with 1200km/h. For the other tests, UE could be assumed with no mobility. (CMCC)
* Recommended WF
  + To be discussed

## Issue 6-2-9: Neighbour cell configuration

* Proposals
  + Option 1: For the FDD cell re-selection test and intra/inter-frequency measurement test for UE with omnidirectional antenna, configure 1 neighbour cell. For the TDD cell re-selection test and and intra/inter-frequency measurement test for UE with antenna array, choose some test cases to configure 2 neighbour cells. (CMCC)
* Recommended WF
  + To be discussed

## Issue 6-2-10: Channel model

* Proposals
  + Option 1: Use the AWGN with residual doppler channel model for RRM test cases. (CMCC)
* Recommended WF
  + To be discussed