**3GPP TSG-RAN5 Meeting #96-e *R5-22xxxx***

**Online, , 15th Aug 2022 - 26th Aug 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.521-1** | **CR** | **1868** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  | | | | | | | | |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)*** *on using this form: comprehensive instructions can be found at  <http://www.3gpp.org/Change-Requests>.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | General updates of clause 5 for R16 CADC configurations | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | China Unicom, Verizon, Ericsson, Qualcomm, Apple | | | | | | | | | |
| ***Source to TSG:*** | R5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_NR\_LTE\_DC\_R16-UEConTest | | | | |  | ***Date:*** | | | 2022-08-15 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Some R16 NR CADC combos which are already 100% completion in RAN4 and assigned to interested companies need to be added into operating bands and channel bandwidth of TS38.521-1 clause 5. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Added 7 CA combinations to Table 5.2A.2.1-1 and Table 5.5A.3.1-1.  CA\_n2A-n5A, CA\_n2A-n48A, CA\_n2A-n66A, CA\_n2A-n77A, CA\_n5A-n66A, CA\_n5A-n77A, CA\_n66A-n77A  Removed the original Table 5.5A.3.1-1, introduced a new Table to keep the format consistent with TS 38.101-1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The activated R16 CADC configurations in clause 5 will be still missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2A.2 5.5A.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## << Start of changes >>

### 5.2A.2 Inter-band CA

NR inter-band carrier aggregation is designed to operate in the operating bands defined in Table 5.2A.2.1-1, 5.2A.2.2-1 and Table 5.2A.2.3-1, where all operating bands are within FR1.

If the mandatory simultaneous Rx/Tx capability applies for a band combination, the mandatory simultaneous Rx/Tx capability also applies for the band combination when the applicable band combination is a subset of a higher order band combination.

Table 5.2A.2-1: Void

Table 5.2A.2-2: Void

Table 5.2A.2-3: Void

#### 5.2A.2.1 Inter-band CA (two bands)

Table 5.2A.2.1-1: Inter-band CA operating bands involving FR1 (two bands)

|  |  |  |
| --- | --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) | DL interruption allowed (Note 8) |
| CA\_n1-n3 | n1, n3 |  |
| CA\_n1-n8 | n1, n8 |  |
| CA\_n1-n77 | n1, n77 | No |
| CA\_n1-n78 | n1, n78 | No |
| CA\_n1-n79 | n1, n79 | No |
| CA\_n2-n5 | n2, n5 |  |
| CA\_n2-n48 | n2, n48 |  |
| CA\_n2-n66 | n2, n66 |  |
| CA\_n2-n77 | n2, n77 |  |
| CA\_n3-n5 | n3, n5 |  |
| CA\_n3-n411 | n3, n41 | No |
| CA\_n3-n771 | n3, n77 | No |
| CA\_n3-n781 | n3, n78 | No |
| CA\_n3-n791 | n3, n79 | No |
| CA\_n5-n7 | n5, n7 |  |
| CA\_n5-n66 | n5, n66 |  |
| CA\_n5-n77 | n5, n77 |  |
| CA\_n5--n781 | n5, n78 | No |
| CA\_n7-n781 | n7, n78 |  |
| CA\_n8-n751 | n8, n75 |  |
| CA n8-n781 | n8, n78 | No |
| CA\_n8-n791 | n8, n79 | No |
| CA\_n24-n41 | n24, n41 |  |
| CA\_n24-n48 | n24, n48 |  |
| CA\_n24-n77 | n24, n77 |  |
| CA\_n25-n466 | n25, n46 |  |
| CA\_n26-n66 | n26, n66 |  |
| CA\_n26-n70 | n26, n70 |  |
| CA\_n28-n41 | n28, n41 |  |
| CA\_n28-n752 | n28, n75 |  |
| CA\_n28\_n781 | n28, n78 | No |
| CA\_n28-n79 | n28, n79 |  |
| CA\_n29-n66 | n29, n66 |  |
| CA\_n29-n70 | n29, n70 |  |
| CA\_n29-n71 | n29, n71 |  |
| CA\_n41-n781 | n41, n78 |  |
| CA\_n41-n793 | n41, n79 | No |
| CA\_n46-n486 | n46, n48 |  |
| CA\_n46-n666 | n46, n66 |  |
| CA\_n48-n66 | n48, n66 |  |
| CA\_n48-n70 | n48, n70 |  |
| CA\_n48-n71 | n48, n71 |  |
| CA\_n66-n70 | n66, n70 |  |
| CA\_n66-n71 | n66, n71 |  |
| CA\_n66-n77 | n66, n77 |  |
| CA\_n70-n71 | n70, n71 |  |
| CA\_n75-n781 | n75, n78 |  |
| CA\_n76-n781 | n76, n78 |  |
| CA\_n77-n79 | n77, n79 |  |
| CA\_n78-n795 | n78, n79 |  |
| NOTE 1: Applicable for UE supporting inter-band carrier aggregation with mandatory simultaneous Rx/Tx capability.  NOTE 2: The frequency range in band n28 is restricted for this band combination to 703-733 MHz for the UL and 758-788 MHz for the DL.  NOTE 3: The frequency range below 2506MHz for Band n41 is not used in this combination.  NOTE 4: Applicable for frequency range above 4800 MHz for Band n79 in this combination.  NOTE 5: For UEs supporting band n77, the minimum requirements apply only when there is non-simultaneous Rx/Tx operation between n78-n79 NR carriers. This restriction applies also for these carriers when applicable NR CA configuration is part of a higher order configuration.  NOTE 6: The PCell is allocated in the licensed band in this combination.  NOTE 7: The minimum requirements apply only when there is non-simultaneous Rx/Tx operation between n77-n79 NR carriers. This restriction applies also for these carriers when applicable NR CA configuration is part of a higher order configuration.  NOTE 8: Applicable when dynamic Tx switching is conducted. The DL interruption requirement is specified in clause 8.2.2.2.10 of 38.133 [13]. | | |

## <<Unchaged sections skipped>>

### 5.5A.3 Configurations for inter-band CA

Table 5.5A.3-1: Void

Table 5.5A.3-2: Void

Table 5.5A.3-3: Void

#### 5.5A.3.1 Configurations for inter-band CA (two bands)

Table 5.5A.3.1-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier5 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n1A-n3A | CA\_n1A-n3A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n3A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1(2A)-n5A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
| CA\_n1A-n8A | CA\_n1A-n8A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1(2A)-n8A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n78A | CA\_n1A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n78(2A) | CA\_n1A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n78C | CA\_n1A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n78 | CA\_n78C\_BCS0 |  |
| CA\_n1(2A)-n78A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n79A | CA\_n1A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n2A-n5A | CA\_n2A-n5A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
| CA\_n2A-n48A | CA\_n2A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 501, 601, 801, 901, 1001 |  |
| CA\_n2A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n77A | n774  CA\_n2A-n77A4 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A | CA\_n3A-n5A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
| CA\_n3(2A)-n5A | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, |  |
| CA\_n3(2A)-n8A | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n3A-n41A | n414  CA\_n3A-n41A4 | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n77A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n78A | CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n78(2A) | CA\_n3A-n78A  CA\_n78(2A) | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3(2A)-n78A | - | n3 | CA\_n3(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n79A | CA\_n3A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n5A-n7A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n5A-n66A | CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n5A-n77A | n774  CA\_n5A-n77A4 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n78A | CA\_n5A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n78(2A) | CA\_n5A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n78A | CA\_n7A-n78A | n7 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n75A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
| CA\_n8A-n78A | CA\_n8A-n78A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n8 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n8A-n78(2A) | CA\_n8A-n78A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
| CA\_n8A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n79 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
| CA\_n24A-n41A | CA\_n24A-n41A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n24A-n41(2A) | CA\_n24A-n41A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
| CA\_n24A-n48A | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n24A-n48B | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
| CA\_n24A-n48(2A) | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n24A-n77A | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n77C | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n25A-n46A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
| CA\_n26A-n66A | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
| n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n66(2A) | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
| n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n26A-n70A | CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n28A-n41A | CA\_n28A-n41A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | 5, 10, 15, 20 | 1 |
|  |  | n41 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n75A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
| CA\_n28A-n78A | CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n78(2A) | CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n28A-n79A | CA\_n28A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n29A-n66A | - | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n29A-n66B | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n29A-n66(2A) | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n29A-n70A | - | n29 | 5, 10 | 0 |
|  |  | n70 | 5, 10, 15, 201,, 251 |  |
| CA\_n29A-n71A | - | n29 | 5, 10 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n41A-n78A | - | n41 | 10, 15, 20, 40, 50, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n41A-n79A | CA\_n41A-n79A | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60 | 1 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41C-n79A | CA\_n41A-n79A  CA\_n41C | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n46A-n48A | CA\_n46A-n48A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | 20 |  |
| CA\_n46B-n48A | CA\_n46A-n48A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 20 |  |
| CA\_n46C-n48A | CA\_n46A-n48A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 20 |  |
| CA\_n46D-n48A | CA\_n46A-n48A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 20 |  |
| CA\_n46A-n66A | - | n46 | 20, 40, 60, 80 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48A-n66A | CA\_n48A-n66A | n48 | 5, 10, 15, 20, 40, 501,601, 801,901,1001 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 501, 601, 801, 901, 1001 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 501, 601, 701 , 801, 901, 1001 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40, |  |
| CA\_n48A-n66(2A) | CA\_n48A-n66A | n48 | 5, 10, 15, 20, 30, 40, 501, 601, 701 , 801, 901, 1001 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n48B-n66A | CA\_n48A-n66A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n48 | CA\_n48B\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48(2A)-n66A | CA\_n48A-n66A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48A-n70A6 | CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 501, 601, 701 , 801, 901, 1001 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48(2A)-n70A | CA\_n48A-n70A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48B-n70A | CA\_n48A-n70A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n71A | CA\_n48A-n71A | n48 | 5, 10, 15, 20, 30, 40, 501, 601, 701, 801, 901, 1001 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n71(2A) | CA\_n48A-n71A | n48 | 5, 10, 15, 20, 30, 40, 501, 601, 701 , 801, 901, 1001 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48(2A)-n71A | CA\_n48A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n71A | CA\_n48A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A | - | n66 | 5, 10, 15, 20, 25 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66B-n70A | - | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66(2A)-n70A | - | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66A-n71A | CA\_n66A-n71A | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n71(2A) | - | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n66A-n71A | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n66(2A)-n71A | CA\_n66A-n71A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66(2A)-n71(2A) | CA\_n66A-n71A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n66B-n71A | CA\_n66A-n71A | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n77A | n774  CA\_n66A-n77A4 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n70A-n71A | CA\_n70A-n71A | n70 | 5, 10, 15, 201, 251 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n70A-n71(2A) | CA\_n70A-n71A | n70 | 5, 10, 15, 201 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n75A-n78A | - | n75 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n76A-n78A | - | n76 | 5 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n77A-n79A | - | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n78A-n79A | - | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| NOTE 1: This UE channel bandwidth is applicable only to downlink.  NOTE 2: The minimum requirements for intra-band contiguous or non-contiguous CA apply.  NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.  NOTE 4: Power Class 2 is allowed for this uplink combination or single uplink carrier in this downlink/uplink combination  NOTE 5: Only single uplink carriers with power class other than PC3 are listed.  NOTE 6: The same configuration applies to corresponding NR-DC configuration in Table 5.5B.1-1. If UE supporting NR-DC configuration do not support the corresponding CA configuration, NR-DC configuration is used in CA test cases | | | | |

### <<End of changes>>