**3GPP TSG-SA3 Meeting #107-e *S3-220798r2***

**e-meeting, 16 – 20 May 2022** Revision of S3-20xxxx

**Source: Huawei, HiSilicon**

**Title: conclusion for part 2 of KI#2**

**Document for: Approval**

**Agenda Item: 5.5 FS\_** **eNS2\_SEC**

# 1 Decision/action requested

***Approve the proposed conclusions to KI#1 for TR33.874***

# 2 References

[1] TR33.874

# 3 Rationale

This contribution proposes to conclude part 2 of the KI#2

# 4 Detailed proposal

pCR

\*\*\* BEGINNING OF CHANGES \*\*\*

## 7.2 Conclusions for KI#2

For the EAC issue under KI#2, it is concluded that no solution is required for the normative text. The following NOTE is recommended to be added for the EAC mode ~~implementation~~:

NOTE1: The operator sets the thre~~a~~sholds ~~setting~~ for the EAC mode activation/de-activation accordingly in order to mitigate ~~should consider~~ potential DoS due to a potential burst of registration requests requesting the same slice ~~in the slice requests~~.

NOTE2: Other working groups should be liaised to add the above NOTE in the relevant specifications.

\*\*\* END OF CHANGES \*\*\*