**3GPP TSG-S4 Meeting #117-eS4-220078**

**14th - 22nd February 2022, Online**

|  |
| --- |
| *CR-Form-v12.1* |
| **PSEUDO CHANGE REQUEST** |
|  |
|  | **26.531** | **CR** |  | **rev** |  | **Current version:** | 1.0.0 |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Conclusion for the BDT key issue |
|  |  |
| ***Source to WG:*** | Qualcomm Incorporated |
| ***Source to TSG:*** | S4 |
|  |  |
| ***Work item code:*** | 5GMS\_EXT |  | ***Date:*** | 8th February 2022 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Proposes a conclusion to the BDT key issue. |
|  |  |
| ***Summary of change:*** |  |
|  |  |
| ***Consequences if not approved:*** |  |
|  |  |
| ***Clauses affected:*** | 5.6.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First Change** |

### 5.6.7 Conclusion

Background Data Transfer is a feature that is offered by the 5G System to allow for data transfer during specific time windows with pre-arranged QoS and charging policies. Both PCF and NEF offer the required APIs to configure and use BDT. The discussion and the potential solution lay out the necessary extensions to integrate BDT as part of 5GMS procedures.

It is recommended that normative work is started to address the following objectives:

1. Define the necessary extensions to 5GMS stage 2 and stage 3 to define the procedures and APIs to enable the use of Background Data Transfer in 5GMS, including:

a) Provisioning of BDT for content hosting and distribution through M1

b) Configuration of BDT and subscribe/notification for transfer opportunities and time windows through M5.

c) Usage of BDT by the application through M6.

2. Liaise with other relevant 3GPP groups to align on the usage of the BDT feature.