**3GPP TSG-WG SA4 Meeting #117E e-meeting  *S4-220122***

**Elbonia, February 14 – 23, 2022 (revision of S4-220xxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **26.114** | **CR** | **0524** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Add support of per-slice QoE measurement | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | SA4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_QoE-Core | | | | |  | ***Date:*** | | | 2022-01-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In the LSes from RAN3 (R3-214477, R3-216225), the slice ID is agreed to be added into the QoE reports for per-slice QoE reporting and evalution.  So alignments are needed from the SA4 perspective. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add support of per-slice QoE measurements. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Unalignments between SA4 and RAN3. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 16.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* \* First change \* \* \* \*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 22.173: "IP Multimedia Core Network Subsystem (IMS) Multimedia Telephony Service and supplementary services; Stage 1".

[3] 3GPP TS 26.235: "Packet switched conversational multimedia applications; Default codecs".

[4] 3GPP TS 26.236: "Packet switched conversational multimedia applications; Transport protocols".

[5] 3GPP TR 26.914: "Multimedia telephony over IP Multimedia Subsystem (IMS); Optimization opportunities".

[6] 3GPP TR 22.973: "IMS Multimedia Telephony service; and supplementary services".

[7] 3GPP TS 24.229: "IP multimedia call control protocol based on Session Initiation Protocol (SIP) and Session Description Protocol (SDP); Stage 3".

[8] IETF RFC 4566 (2006): "SDP: Session Description Protocol", M. Handley, V. Jacobson and C. Perkins.

[9] IETF RFC 3550 (2003): "RTP: A Transport Protocol for Real-Time Applications", H. Schulzrinne, S. Casner, R. Frederick and V. Jacobson.

[10] IETF RFC 3551 (2003): "RTP Profile for Audio and Video Conferences with Minimal Control", H. Schulzrinne and S. Casner.

[11] 3GPP TS 26.071: "Mandatory Speech Codec speech processing functions; AMR Speech CODEC; General description".

[12] 3GPP TS 26.090: "Mandatory Speech Codec speech processing functions; Adaptive Multi-Rate (AMR) speech codec; Transcoding functions".

[13] 3GPP TS 26.073: "ANSI C code for the Adaptive Multi Rate (AMR) speech codec".

[14] 3GPP TS 26.104: "ANSI‑C code for the floating-point Adaptive Multi Rate (AMR) speech codec".

[15] 3GPP TS 26.093: "Mandatory speech codec speech processing functions; Adaptive Multi-Rate (AMR) speech codec; Source controlled rate operation".

[16] 3GPP TS 26.103: "Speech codec list for GSM and UMTS".

[17] 3GPP TS 26.171: "Speech codec speech processing functions; Adaptive Multi-Rate - Wideband (AMR-WB) speech codec; General description".

[18] 3GPP TS 26.190: "Speech codec speech processing functions; Adaptive Multi-Rate - Wideband (AMR-WB) speech codec; Transcoding functions".

[19] 3GPP TS 26.173: "ANCI-C code for the Adaptive Multi Rate - Wideband (AMR-WB) speech codec".

[20] 3GPP TS 26.204: "Speech codec speech processing functions; Adaptive Multi-Rate - Wideband (AMR-WB) speech codec; ANSI-C code".

[21] 3GPP TS 26.193: "Speech codec speech processing functions; Adaptive Multi-Rate - Wideband (AMR-WB) speech codec; Source controlled rate operation".

[22] Void.

[23] Void.

[24] Recommendation ITU-T H.264 (04/2017): "Advanced video coding for generic audiovisual services" | ISO/IEC 14496-10:2014: "Information technology – Coding of audio-visual objects – Part 10: Advanced Video Coding".

[25] IETF RFC 6184 (2011): "RTP Payload Format for H.264 Video", Y.-K. Wang, R. Even, T. Kristensen, R. Jesup.

[26] ITU-T Recommendation T.140 (02/1998): "Protocol for multimedia application text conversation".

[27] ITU-T Recommendation T.140 (02/2000): "Protocol for multimedia application text conversation - Addendum 1".

[28] IETF RFC 4867 (2007): "RTP Payload Format and File Storage Format for the Adaptive Multi-Rate (AMR) and Adaptive Multi-Rate Wideband (AMR-WB) Audio Codecs", J. Sjoberg, M. Westerlund, A. Lakaniemi and Q. Xie.

[29] Void

[30] Void.

[31] IETF RFC 4103 (2005): "RTP Payload for Text Conversation", G. Hellstrom and P. Jones.

[32] Void.

[33] 3GPP TR 25.993: "Typical examples of Radio Access Bearers (RABs) and Radio Bearers (RBs) supported by Universal Terrestrial Radio Access (UTRA)".

[34] 3GPP TS 22.105: "Services and service capabilities".

[35] 3GPP TS 26.131: "Terminal acoustic characteristics for telephony; Requirements".

[36] 3GPP TS 26.132: "Speech and video telephony terminal acoustic test specification".

[37] 3GPP TS 28.062: "Inband Tandem Free Operation (TFO) of speech codecs; Service description; Stage 3".

[38] 3GPP TS 23.153: "Out of band transcoder control; Stage 2".

[39] IETF RFC 0768 (1980): "User Datagram Protocol", J. Postel.

[40] IETF RFC 4585 (2006): "Extended RTP Profile for Real-time Transport Control Protocol (RTCP) - Based Feedback (RTP/AVPF)", J. Ott, S. Wenger, N. Sato, C. Burmeister and J. Rey.

[41] RTP Tools: <http://www.cs.columbia.edu/IRT/software/rtptools/>.

[42] IETF RFC 3556 (2003): "Session Description Protocol (SDP) Bandwidth Modifiers for RTP Control Protocol (RTCP) Bandwidth", S. Casner.

[43] IETF RFC 5104 (2008): "Codec Control Messages in the RTP Audio-Visual Profile with Feedback (AVPF)", S. Wenger, U. Chandra, M. Westerlund and B. Burman.

[44] Void.

[45] 3GPP TS 26.111: "Codec for circuit switched multimedia telephony service; Modifications to H.324".

[46] 3GPP TS 23.172: "Technical realization of Circuit Switched (CS) multimedia service; UDI/RDI fallback and service modification; Stage 2".

[47] 3GPP TS 23.002: "Network Architecture".

[48] IETF RFC 3388 (2002): "Grouping of Media Lines in the Session Description Protocol (SDP)", G. Camarillo, G. Eriksson, J. Holler and H. Schulzrinne.

[49] IETF RFC 4102 (2005): "Registration of the text/red MIME Sub-Type", P. Jones.

[50] ITU-T H.248 (06/2000): "Packages for text conversation, fax and call discrimination".

[51] ETSI EG 202 320, v1.2.1 (2005-10): "Human Factors (HF); Duplex Universal Speech and Text (DUST) communications".

[52] 3GPP TS 26.226: "Cellular text telephone modem; General description".

[53] IETF RFC 4504 (2006): "SIP Telephony Device Requirements and Configuration", H. Sinnreich, Ed., S. Lass and C. Stredicke.

[54] ITU-T Recommendation V.151 (05/2006): "Procedures for end-to-end connection of analogue PSTN text telephones over an IP network utilizing text relay".

[55] ITU-T Recommendation V.152 (09/2010): "Procedures for supporting Voice Band Data over IP networks".

[56] IETF RFC 3448 (2003): "TCP Friendly Rate Control (TFRC): Protocol Specification", M. Handley, S. Floyd, J. Padhye and J. Widmer.

[57] 3GPP TS 24.173: "IMS Multimedia Telephony Communication Service and Supplementary Services".

[58] IETF RFC 3264 (2002): "An Offer/Answer Model with the Session Description Protocol (SDP)", J. Rosenberg and H. Schulzrinne.

[59] 3GPP TS 26.141: "IP Multimedia System (IMS) Messaging and Presence; Media formats and codecs".

[60] 3GPP TS 26.234: "Transparent end-to-end Packet-switched Streaming Service; Protocols and codecs".

[61] IETF RFC 4733 (2006): "RTP Payload for DTMF Digits, Telephony Tones, and Telephony Signals", H. Schulzrinne and T.Taylor.

[62] 3GPP TS 23.014: "Support of Dual Tone Multi-Frequency (DTMF) signalling".

[63] ETSI ES 201 235-2, v1.2.1: "Specification of Dual Tone Multi-Frequency (DTMF); Transmitters and Receivers; Part 2: Transmitters".

[64] 3GPP TS 23.107: "Quality of Service (QoS) concept and architecture".

[65] 3GPP TS 29.163: "Interworking between the IP Multimedia (IM) Core Network (CN) subsystem and Circuit Switched (CS) networks".

[66] Void.

[67] OMA-ERELD-DM-V1\_2-20070209-A: "Enabler Release Definition for OMA Device Management, Approved Version 1.2".

[68] Void.

[69] IETF RFC 5939 (2010): "Session Description Protocol (SDP) Capability Negotiation", F. Andreasen.

[70] Void

[71] IETF RFC 1952 (May 1996): "GZIP file format specification version 4.3", P. Deutsch.

[72] IETF RFC 2326 (1998): "Real Time Streaming Protocol (RTSP)".

[73] IETF RFC 2616 (June 1999): "Hypertext Transfer Protocol -- HTTP/1.1".

[74] 3GPP TS 26.346 "Multimedia Broadcast/Multicast Service (MBMS); Protocols and codecs".

[75] Void

[76] IETF RFC 6236 (2011): "Negotiation of Generic Image Attributes in the Session Description Protocol (SDP)", I. Johansson and K. Jung.

[77] ITU-T G.711 (11/1988): "Pulse code modulation (PCM) of voice frequencies".

[78] ITU-T G.722 (09/2012): "7 kHz audio-coding within 64 kbit/s".

[79] IETF RFC 4821 (2007): "Packetization Layer Path MTU Discovery".

[80] 3GPP TS 23.003: "Numbering, addressing and identification".

[81] IETF RFC 4796 (2007): "The Session Description Protocol (SDP) Content Attribute", J. Hautakorpi and G. Camarillo.

[82] 3GPP TS 24.247: "Messaging service using the IP Multimedia (IM) Core Network (CN) subsystem".

[83] IETF RFC 3168 (2001): "The Addition of Explicit Congestion Notification (ECN) to IP", K. Ramakrishnan, S. Floyd and D. Black.

[84] IETF RFC 6679 (2012): "Explicit Congestion Notification (ECN) for RTP over UDP", M. Westerlund, et. al.

[85] 3GPP TS 36.300: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access Network (E-UTRAN); Overall description".

[86] Void

[87] IETF RFC 5506 (2009): "Support for Reduced-Size Real-Time Transport Control Protocol (RTCP): Opportunities and Consequences".

[88] IETF RFC 3611 (2003): "RTP Control Protocol Extended Reports (RTCP XR) ", T. Friedman, R. Caceres and A. Clark.

[89] 3GPP TS 25.401: "UTRAN overall description".

[90] 3GPP TS 23.203: "Policy and charging control architecture".

[91] ITU-T Recommendation T.4 (07/2003): "Standardization of Group 3 facsimile terminals for document transmission".

[92] ITU-T Recommendation T.30 (09/2005): "Procedures for document facsimile transmission in the general switched telephone network".

[93] ITU-T Recommendation T.38 (09/2010): "Procedures for real-time Group 3 facsimile communication over IP networks".

[94] IETF RFC 3362 (2002): "Real-time Facsimile (T.38) - image/t38 MIME Sub-type Registration".

[95] IETF RFC 5285 (2008): "A General Mechanism for RTP Header Extensions", D. Singer, H. Desineni.

[96] IETF RFC 5168 (2008): "XML Schema for Media Control", O. Levin, R. Even and P. Hagendorf.

[97] 3GPP2 C.S0055-A, version 1.0: "Packet Switched Video Telephony Service (PSVT/MCS)".

[98] ETSI TS 181 005, v3.3.1: "Telecommunications and Internet converged Services and Protocols for Advanced Networking (TISPAN); Service and Capability Requirements".

[99] 3GPP2 C.S0014-E, version 1.0: "Enhanced Variable Rate Codec (EVRC)".

[100] ITU-T Recommendation G.729 (06/2012): "Coding of speech at 8 kbit/s using conjugate-structure algebraic-code-excited linear prediction (CS-ACELP)".

[101] ITU-T Recommendation G.729.1 (05/2006): "G.729-based embedded variable bit-rate coder: An 8-32 kbit/s scalable wideband coder bitstream interoperable with G.729".

[102] 3GPP2 C.S0076, version 1.0: "Discontinuous Transmission (DTX) of Speech in cdma2000 Systems".

[103] IETF RFC 5188 (2008):"RTP Payload Format for the Enhanced Variable Rate Wideband Codec (EVRC-WB) and the Media Subtype Updates for EVRC-B Codec".

[104] IETF RFC 4749 (2006): "RTP Payload Format for the G.729.1 Audio Codec".

[105] IETF RFC 5459 (2009): "G.729.1 RTP Payload Format Update: Discontinuous Transmission (DTX) Support".

[106] IETF RFC 4788 (2007): "Enhancements to RTP Payload Formats for EVRC Family Codecs".

[107] IETF RFC 4855 (2007): "Media Type Registration of RTP Payload Formats".

[108] ITU-T Recommendation P.10 (07/2006): "Vocabulary and effects of transmission parameters on customer opinion of transmission quality".

[109] ETSI TS 103 737, v1.1.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for narrowband wireless terminals (handset and headset) from a QoS perspective as perceived by the user".

[110] ETSI TS 103 738, v1.1.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for narrowband wireless terminals (handsfree) from a QoS perspective as perceived by the user".

[111] ETSI TS 103 739, v1.1.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for wideband wireless terminals (handset and headset) from a QoS perspective as perceived by the user".

[112] ETSI TS 103 740, v1.1.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for wideband wireless terminals (handsfree) from a QoS perspective as perceived by the user".

[113] ETSI TS 202 737, v1.3.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for narrowband VoIP terminals (handset and headset) from a QoS perspective as perceived by the user".

[114] ETSI TS 202 738, v1.3.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for narrowband VoIP loudspeaking and handsfree terminals from a QoS perspective as perceived by the user".

[115] ETSI TS 202 739, v1.3.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for wideband VoIP terminals (handset and headset) from a QoS perspective as perceived by the user ".

[116] ETSI TS 202 740, v1.3.2: "Speech and multimedia Transmission Quality (STQ); Transmission requirements for wideband VoIP loudspeaking and handsfree terminals from a QoS perspective as perceived by the user ".

[117] ETSI EN 300 175-8, v2.5.1: "Digital Enhanced Cordless Telecommunications (DECT); Common Interface (CI); Part 8: Speech and audio coding and transmission".

[118] ETSI TS 300 176-2, v2.2.1: "Digital Enhanced Cordless Telecommunications (DECT); Test specification; Part 2: Audio and speech".

[119] Recommendation ITU-T H.265: "High efficiency video coding" | ISO/IEC 23008-2:2020: "High Efficiency Coding and Media Delivery in Heterogeneous Environments – Part 2: High Efficiency Video Coding". [120] IETF RFC 7798 (2016): "RTP Payload Format for High Efficiency Video Coding (HEVC)", Y.-K. Wang, Y. Sanchez, T. Schierl, S. Wenger, M. M. Hannuksela.

[121] 3GPP TS 26.441: "Codec for Enhanced Voice Services (EVS); General Overview".

[122] 3GPP TS 26.442: "Codec for Enhanced Voice Services (EVS); ANSI C code (fixed-point)".

[123] 3GPP TS 26.443: "Codec for Enhanced Voice Services (EVS); ANSI C code (floating-point)".

[124] 3GPP TS 26.444: "Codec for Enhanced Voice Services (EVS); Test Sequences".

[125] 3GPP TS 26.445: "Codec for Enhanced Voice Services (EVS); Detailed Algorithmic Description".

[126] 3GPP TS 26.446: "Codec for Enhanced Voice Services (EVS); AMR-WB Backward Compatible Functions".

[127] 3GPP TS 26.447: "Codec for Enhanced Voice Services (EVS); Error Concealment of Lost Packets".

[128] 3GPP TS 26.448: "Codec for Enhanced Voice Services (EVS); Jitter Buffer Management".

[129] 3GPP TS 26.449: "Codec for Enhanced Voice Services (EVS); Comfort Noise Generation (CNG) Aspects".

[130] 3GPP TS 26.450: "Codec for Enhanced Voice Services (EVS); Discontinuous Transmission (DTX)".

[131] 3GPP TS 26.451: "Codec for Enhanced Voice Services (EVS); Voice Activity Detection (VAD)".

[132] 3GPP TS 45.003: "Radio Access Network; Channel coding".

[133] 3GPP TS 23.216: "Single Radio Voice Call Continuity (SRVCC); Stage2".

[134] 3GPP TS 23.237: "IP Multimedia Subsystem (IMS) Service Continuity; Stage2".

[135] ITU-T Recommendation H.224 (01/05): "A real time control protocol for simplex applications using the H.221 LSD/HSD/MLP channels ".

[136] ITU-T Recommendation H.224 (2005): Corrigendum 1 (08/07).

[137] ITU-T Recommendation H.281 (11/94): Transmission of non-telephone signals "A far end camera control protocol for videoconferences using H.224".

[138] ITU-T Recommendation H.323 (12/2009): "Packet-based multimedia communications systems".

[139] IETF RFC 4573 (2006): "MIME Type Registration for RTP Payload Format for H.224".

[140] IETF RFC 4588 (2006): "RTP Retransmission Payload Format", J. Rey, D. Leon, A. Miyazaki, V. Varsa and R. Hakenberg.

[141] IETF RFC 8627 (2019): "RTP Payload Format for Flexible Forward Error Correction (FEC)".

[142] TR 26.922: "Video Telephony Robustness Improvements Extensions (VTRI\_EXT): Performance Evaluation".

[143] IETF RFC 5956 (2010): "Forward Error Correction Grouping Semantics in the Session Description Protocol", A. Cengiz.

[144] 3GPP TR 26.924: "Multimedia telephony over IP Multimedia Subsystem (IMS); Study on improved end-to-end Quality of Service (QoS) handling for Multimedia Telephony Service for IMS (MTSI)".

[145] Void

[146] Void.

[147] 3GPP TS 24.147: "Conferencing Using IP Multimedia Core Network; Stage 3".

[148] IETF RFC 4575 (2006): "A Session Initiation Protocol (SIP) Event Package for Conference State".

[149] IETF RFC 4582 (2006): "The Binary Floor Control Protocol (BFCP)".

[150] IETF RFC 4583 (2006): "Session Description Protocol (SDP) Format for Binary Floor Control (BFCP) Streams".

[151] Void.

[152] 3GPP TR 26.980: "Multimedia telephony over IP Multimedia Subsystem (IMS); Media handling aspects of multi-stream multiparty conferencing for Multimedia Telephony Service for IMS (MTSI)".

[153] IETF RFC 5234 (2008): "Augmented BNF for Syntax Specifications: ABNF", D. Crocker and P. Overell.

[154] IETF RFC 8853 (2021): "Using Simulcast in Session Description Protocol (SDP) and RTP Sessions"

[155] IETF RFC 8851 (2021): "RTP Payload Format Restrictions"

[156] IETF RFC 7728 (2016): "RTP Stream Pause and Resume".

[157] 3GPP TS 36.321: "Evolved Universal Terrestrial Radio Access (E-UTRA); Medium Access Control (MAC) protocol specification".

[158] 3GPP TS 25.331: "Radio Resource Control (RRC); Protocol specification".

[159] "Mobile Location Protocol (MLP)", Open Mobile Alliance, OMA-LIF-MLP-V3\_1, Approved Version 3.1 – 20 Sep 2011.

[160] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

[161] 3GPP TS 27.007: " Technical Specification Group Core Network and Terminals; AT command set for User Equipment (UE)".

[162] Void

[163] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol Specification".

[164] 3GPP TS 38.300: "NR; NR and NG-RAN Overall Description; Stage 2".

[165] 3GPP TS 26.452: "Codec for Enhanced Voice Services (EVS); ANSI C code; Alternative fixed-point using updated basic operators".

[166] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification".

[167] 3GPP TS 23.228: "IP Multimedia Subsystem (IMS); Stage 2".

[168] 3GPP TR 26.952: "Codec for Enhanced Voice Services (EVS); Performance characterization".

[169] 3GPP TR 26.959: "Study on enhanced Voice over LTE (VoLTE) performance".

[170] 3GPP TS 36.323: "Evolved Universal Terrestrial Radio Access (E-UTRA); Packet Data Convergence Protocol (PDCP) specification".

[171] 3GPP TS 37.324: "Evolved Universal Terrestrial Radio Access (E-UTRA) and NR; Service Data Adaptation Protocol (SDAP) specification".

[172] IETF RFC 8864 (2021): "Negotiation Data Channels Using the Session Description Protocol (SDP)"

[173] IETF RFC 4960 (2007): "Stream Control Transmission Protocol"

[174] IETF RFC 8261 (2017): "Datagram Transport Layer Security (DTLS) Encapsulation of SCTP Packets"

[175] IETF RFC 8831 (2021): "WebRTC Data Channels".

[176] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[177] IETF RFC 5688 (2010): "A Session Initiation Protocol (SIP) Media Feature Tag for MIME Application Subtypes".

[178] 3GPP TS 28.405; "Management of Quality of Experience (QoE) measurement collection; Control and configuration"

[179] ISO/IEC 23090-2:2019: " Information technology -- Coded representation of immersive media -- Part 2: Omnidirectional media format".

[180] 3GPP TS 26.118: "3GPP Virtual reality profiles for streaming applications".

[181] ITU-T Recommendation G.1028 (06/2019): "End-to-end quality of service for voice over 4G mobile networks".

[X] 3GPP TS 24.526: " User Equipment (UE) policies for 5G System (5GS); Stage 3".

\* \* \* \* Second change \* \* \* \*

## 16.4 Metrics Reporting

When a session is started, the MTSI client must determine whether QoE reporting is required for the session. If the parameter "Enabled" is set to false, no QoE reporting shall be done. If the "Enabled" parameter is set to true the optional "Rules" parameters are checked (sub-clause 16.3.3) to define if QoE reporting shall be done.

Once the need for QoE reporting has been established, the client shall continuously compute all specified metrics for each measurement interval period, according to the "Measure-Resolution" parameter (sub-clause 16.3.2). In order to bound the resources used by metrics reporting, the minimum values for the Measure-Resolution and Sending-Rate are specified to be 5 seconds and 30 seconds respectively. The computed metrics are represented in a vector format, adding an additional metric value to each metric vector after each new measurement interval period.

Note that the calculated metrics shall only cover one measurement interval. For instance, if the corruption duration extends longer than to the end of the current measurement interval, only the portion which fits into the current measurement interval shall be reported. The remaining portion of the corruption duration shall be reported as belonging to the next measurement interval.

The end of the session will normally not correspond to the end of a measurement interval period, so the metrics for the last measurement interval period will typically be calculated over a time shorter than the configured measurement interval. Note, however, that these last metrics shall still be added to the metrics vectors and reported to the server.

It is possible for the server to use the start and stop timestamps, together with the knowledge of the configured measurement interval, to derive the actual length of the last measurement interval period, but any specific action or interpretation of these last shorter measurements is out of scope of this specification.

The MTSI client shall send QoE report messages to the server in accordance with the specified reporting interval "Sending-Rate" (sub-clause 16.3.2). All stored metrics data shall then be sent to the server, and then deleted from the metrics storage.

Note that if the reporting interval is not an integer multiple of the measurement interval, only the measurement interval periods which have been fully passed shall be included in the report. The ongoing not-passed measurement interval period shall be included in the next report. The only exception is at the end of the session, where also the last ongoing measurement interval period shall be directly calculated and included in the report.

If QoE configuration has been done via the OMA MO, the client shall send QoE reports using the HTTP (RFC 2616 [73]) POST request carrying XML formatted metadata. If the optional "APN" parameter is defined in the OMA managed object, that APN shall be used for establishing the PDP context or EPS bearer on which the QoE metric reports will be transmitted. The MTSI client randomly selects one of the URIs from the MO "Server" parameter, with uniform distribution.

If QoE configuration has been done via the QMC functionality (see clause 16.5), the client shall also send the QoE reports as described in clause 16.5. Note that for QMC scheme, the S-NSSAI and DNN that correspond to the report data shall be included for support of per-slice QoE reporting and evaluation in OAM. This information may be retrieved via the AT Command +CGDCONT [161]) or the specific traffic mapping with URSP rule[X].

Each QoE report is formatted in XML according the following XML schema (sub-clause 16.4.1). An informative example of a single reception report XML object is also given (sub-clause 16.4.2). The reports should be compressed using GZIP only if the MO parameter "Format" specifies this.

Each QoE Metrics element has a set of attributes and any number of media level QoE Metrics elements. All attributes are defined in sub-clause 16.4.1 and correspond to the QoE metrics listed in sub-clause 16.2. Individual metrics can be selected as described in sub-clause 16.3.2.

Except for the media level QoE metrics, the following parameters shall be reported for each report:

- The *callId* attribute identifies the call identity of the SIP session.

- The *clientId* attribute is unique identifier for the receiver, e.g. an MSISDN of the UE as defined in [80].

- The *startTime* and *stopTime* attributes identifies the client NTP time when the measurements included in the report were started and stopped. The time is based on the local real-time clock in the client, and might not be consistent with the true NTP time. However, assuming that the reporting is done without any extra delay the server can use the *stopTime* attribute to correct the timestamps if necessary.

- The *mediaId* attribute shall be reported for each media level QoE report, and identifies the port number for the media.

If the attribute *qoeReferenceId* was defined in the QMC configuration (see clause 16.5.2), the value shall be copied into each QoE report, to facilitate network-side correlation (see [178]). If this attribute was defined, the attribute *recordingSessionId* shall also be returned for each QoE report. The *recordingSessionId* is a two-byte octet defined by the client. It shall remain the same for all QoE reports belonging to the same session, and it should be different for QoE reports belonging to different sessions.

### 16.4.1 XML schema for QoE report message

<?xml version="1.0" encoding="UTF-8"?>

<xs:schema xmlns:xs="http://www.w3.org/2001/XMLSchema"

targetNamespace="urn:3gpp:metadata:2008:MTSI:qoereport"

xmlns="urn:3gpp:metadata:2008:MTSI:qoereport"

elementFormDefault="qualified">

<xs:element name="QoeReport" type="QoeReportType"/>

<xs:complexType name="QoeReportType">

<xs:sequence>

<xs:element name="statisticalReport" type="starType" minOccurs="0"

maxOccurs="unbounded"/>

<xs:any namespace="##other" processContents="skip" minOccurs="0"

maxOccurs="unbounded"/>

</xs:sequence>

<xs:anyAttribute processContents="skip"/>

</xs:complexType>

<xs:complexType name="starType">

<xs:sequence>

<xs:element name="mediaLevelQoeMetrics" type="mediaLevelQoeMetricsType" minOccurs="1"

maxOccurs="unbounded"/>

</xs:sequence>

<xs:attribute name="startTime" type="xs:unsignedLong" use="required"/>

<xs:attribute name="stopTime" type="xs:unsignedLong" use="required"/>

<xs:attribute name="callId" type="xs:string" use="required"/>

<xs:attribute name="clientId" type="xs:string" use="required"/>

<xs:attribute name="qoeReferenceId" type="xs:hexBinary" use="optional"/>

<xs:attribute name="recordingSessionId" type="xs:hexBinary" use="optional"/>

<xs:attribute name="dnn" type="string" use="optional"/>

<xs:attribute name="snssai" type="unsignedLong" use=”optional"/>

<xs:anyAttribute processContents="skip"/>

</xs:complexType>

<xs:complexType name="mediaLevelQoeMetricsType">

<xs:sequence>

<xs:any namespace="##other" processContents="skip" minOccurs="0"

maxOccurs="unbounded"/>

</xs:sequence>

<xs:attribute name="mediaId" type="xs:integer" use="required"/>

<xs:attribute name="totalCorruptionDuration" type="unsignedLongVectorType"  
 use="optional"/>

<xs:attribute name="numberOfCorruptionEvents" type="unsignedLongVectorType"  
 use="optional"/>

<xs:attribute name="corruptionAlternative" type="xs:string" use="optional"/>

<xs:attribute name="totalNumberofSuccessivePacketLoss" type="unsignedLongVectorType"

use="optional"/>

<xs:attribute name="numberOfSuccessiveLossEvents" type="unsignedLongVectorType"   
 use="optional"/>

<xs:attribute name="numberOfReceivedPackets" type="unsignedLongVectorType"   
 use="optional"/>

<xs:attribute name="framerate" type="doubleVectorType" use="optional"/>

<xs:attribute name="totalJitterDuration" type="doubleVectorType" use="optional"/>

<xs:attribute name="numberOfJitterEvents" type="unsignedLongVectorType"

use="optional"/>

<xs:attribute name="totalSyncLossDuration" type="doubleVectorType" use="optional"/>

<xs:attribute name="numberOfSyncLossEvents" type="unsignedLongVectorType"

use="optional"/>

<xs:attribute name="networkRTT" type="unsignedLongVectorType" use="optional"/>

<xs:attribute name="internalRTT" type="unsignedLongVectorType" use="optional"/>

<xs:attribute name="codecInfo" type="stringVectorType" use="optional"/>

<xs:attribute name="codecProfileLevel" type="stringVectorType" use="optional"/>

<xs:attribute name="codecImageSize" type="stringVectorType" use="optional"/>

<xs:attribute name="averageCodecBitrate" type="doubleVectorType" use="optional"/>

<xs:attribute name="callSetupTime" type="xs:unsignedLong" use="optional"/>

<xs:anyAttribute processContents="skip"/>

</xs:complexType>

<xs:simpleType name="doubleVectorType">

<xs:list itemType="xs:double"/>

</xs:simpleType>

<xs:simpleType name="stringVectorType">

<xs:list itemType="xs:string"/>

</xs:simpleType>

<xs:simpleType name="unsignedLongVectorType">

<xs:list itemType="xs:unsignedLong"/>

</xs:simpleType>

</xs:schema>

### 16.4.2 Example XML for QoE report message

Below is one example of QoE report message, in this example the measurement interval is 20 seconds, the reporting interval is 5 minutes, but the call ends after 55 seconds.

<?xml version="1.0" encoding="UTF-8"?>

<QoeReport xmlns="urn:3gpp:metadata:2008:MTSI:qoereport"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xsi:schemaLocation="urn:3gpp:metadata:2008:MTSI:qoereport qoereport.xsd">

<statisticalReport

startTime="1219322514"

stopTime="1219322569"

clientId="clientID"

callId="callID">

qoeReferenceId="240F512A"

snssai="01000FFF"

dnn="internet.mnc015.mcc234.gprs"

recordingSessionId="0001"

<mediaLevelQoeMetrics

mediaId="1234"

totalCorruptionDuration="480 0 120"

numberOfCorruptionEvents="5 0 2"

corruptionAlternative="a"

totalNumberofSuccessivePacketLoss="24 0 6"

numberOfSuccessiveLossEvents="5 0 2"

numberOfReceivedPackets="535 645 300"

framerate="50.0 49.2 50.0"

numberOfJitterEvents="0 1 0"

totalJitterDuration="0 0.346 0"

networkRTT="120 132 125"

internalRTT="20 24 20"

codecInfo="AMR-WB/16000/1 = ="

averageCodecBitRate="12.4 12.65 12.7"/>

callSetupTime="345"

<mediaLevelQoeMetrics

mediaId="1236"

totalCorruptionDuration="83 0 0"

numberOfCorruptionEvents="1 0 0"

corruptionAlternative="b"

totalNumberofSuccessivePacketLoss="3 0 0"

numberOfSuccessiveLossEvents="2 0 0"

numberOfReceivedPackets="297 300 225"

framerate="14.7 15.0 14.9"

numberOfJitterEvents="0 0 0"

totalJitterDuration="0 0 0"

numberOfSyncLossEvents="0 1 0"

totalSyncLossDuration="0 0.789 0"

networkRTT="220 232 215"

internalRTT="27 20 25"

codecInfo="H263-2000/90000 = ="

codecProfileLevel="profile=0;level=45 = ="

codecImageSize="176x144 = ="

averageCodecBitRate="124.5 128.0 115.1"/>

callSetupTime="345"/>

</statisticalReport>

</QoeReport>

\* \* \* \* End of changes \* \* \* \*