|  |  |
| --- | --- |
| 3GPP TS 26.567 V0.1.0 (2024-04) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Services and System Aspects;  Split Rendering over IMS;  (Release 19) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  https://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 5

Introduction 6

1 Scope 7

2 References 7

3 Definitions of terms, symbols and abbreviations 7

3.1 Terms 7

3.2 Symbols 7

3.3 Abbreviations 8

4 System description 8

4.1 Overview 8

4.2 Reference Architecture 8

4.3 Network APIs 8

4.4 Split Rendering Client 8

4.5 Split Rendering Server 8

5 Media codecs, configuration, and data transport 8

5.1 General 8

5.2 Media codecs 8

5.3 Media configuration 9

5.4 Data transport 9

6 Split Rendering Metrics 9

7 Procedures 9

7.1 General procedures for session establishment 9

7.2 General procedures for session modification 9

7.3 Network support procedures 9

Annex <A> (normative): <Normative annex for a Technical Specification> 10

Annex <B> (informative): <Informative annex for a Technical Specification> 11

B.1 Heading levels in an annex 11

Annex <F> (informative): 12

Change history 12

For definitive guidance on drafting 3GPP TSs and TRs, see [3GPP TS 21.801](https://www.3gpp.org/DynaReport/21801.htm).

Ensure all blue guidance text is removed before submitting the TS/TR to the TSG for approval.

# Foreword

This clause is mandatory; do not alter the text in any way other than to choose between "Specification" and "Report".

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In drafting the TS/TR, pay particular attention to the use of modal auxiliary verbs! TRs shall not contain any normative provisions.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# Introduction

This clause is optional. If it exists, it shall be the second unnumbered clause.

# 1 Scope

The present document specifies functional entities, network APIs and protocols for IMS-based split rendering. It also provides codecs for delivery of split-render media and metadata of split rendered content for both uplink and downlink. The present document also contains procedures of split rendering session establishment, session management, adaption, as well as other procedures to support split rendering process based on network support functions.

Key use cases enabled by this specification include XR services incorporating real-time and non-real-time media in industrial (e.g., for monitoring, maintenance, collaboration and tele-operation), enterprise and educational environments; entertainment use-cases, including cloud-gaming, and shared and collaborative entertainment and productivity XR services.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.228: "IP Multimedia Subsystem (IMS); Stage 2".

[3] 3GPP TS 26.264: "IMS-based AR Real-Time Communication".

…

[x] <doctype> <#>[ ([up to and including]{yyyy[-mm]|V<a[.b[.c]]>}[onwards])]: "<Title>".

It is preferred that the reference to TR 21.905 be the first in the list.

# 3 Definitions of terms, symbols and abbreviations

This clause and its three (sub) clauses are mandatory. The contents shall be shown as "void" if the TS/TR does not define any terms, symbols, or abbreviations.

## 3.1 Terms

For the purposes of the present document, the terms given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

Definition format (Normal)

**<defined term>:** <definition>.

**example:** text used to clarify abstract rules by applying them literally.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

Symbol format (EW)

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

Abbreviation format (EW)

<ABBREVIATION> <Expansion>

# 4 System description

The main text of the document should start here, after the above clauses have been added.

The following styles and editing techniques are aimed to help in the formatting of the document using the 3GPP Template: 3GPP\_70.dot, available from the 3GPP FTP site (<https://www.3gpp.org/ftp/Information/All_Templates>).

## 4.1 Overview

*Editor’s note: document the background and existing TS/TR related with IMS-based split rendering, including potential requirements in terms of enhancement on functional entities/APIs to enable split rendering.*

The IMS stage-2 service description is specified in TS 23.228. The IMS architecture enhancements to support data channel services can be found in TS 23.228 Annex AC [2], which supports separation of signalling function and media function supporting data channel services.



Figure 4.1.1: Architecture of IMS supporting DC usage with MF

*Editor’s note: above content will be updated to align with TS 23.228 as well as SA2 R19 IMS related work and study items.*

Based on the architecture in Figure 4.1.1, TS 26.264 [3] provides the IMS-based conversational AR (Augmented reality) services, including the generalized end-to-end architecture to support AR communication over IMS DC, as shown in Figure 4.1.2.




Figure 4.1.2: Generalized IMS DC Architecture to support AR communication (TS 26.264)

Accordingly, AR Application Server (AR AS) is responsible for AR service control related to AR communication, including AR session media control and AR media capability negotiation with the UE.

The DCSF receives event reports from the IMS AS, and decides whether AR communication service is allowed to be provided during the IMS session. Additionally, the DCSF interacts with the AR AS for DC resource control.

MF/MRF supports AR conversational service by providing transcoding for terminals with limited capabilities. Additionally, the MF/MRF may collect spatial and media descriptions from UEs and create scene descriptions for symmetrical AR call experiences. MF/MRF also provide remote rendering for AR-MTSI clients in terminals with limited capabilities based on rendering negotiation. For remote rendering the AR-MTSI client provides AR metadata.

The IMS AS receives the media control instructions from the DCSF and accordingly interacts with the UE for connecting the UE's audio/video media termination to the MF/MRF and interacts with MF/MRF for data channel media resource management for AR media processing.

*Editor’s note: above content will be updated to align with TS 26.264 when it completes.*

According to the architectures above, the present document introduces a mapping to the IMS architecture for IMS-based split rendering.

## 4.2 Reference Architecture

*Editor’s note: identify function entities for IMS-based split rendering, introducing a mapping to the IMS architecture.*

The generalized IMS DC architecture to support split rendering is shown in Figure 4.2.1.

A screenshot of a computer

Description automatically generated

Figure 4.2.1: Generalized IMS DC Architecture to support split rendering

Split-Rendering Client (SRC): This function is responsible for acquiring the UE media capabilities and interacting with the SRS during the split-rendering process.

Split-Rendering Server (SRS): This function is responsible for interacting with SRC during split-rendering process, monitoring the server’s edge resource usage, and managing/running the split rendering process, etc.

DC Application Server (DC AS) is responsible for service control related to split-rendering, including session media control and media capability negotiation with the UE via MF, etc.

*Editor’s note: the detailed definition of SRC and SRS will be provided at section 4.4 and 4.5 of TS 26.567. Above text will be updated to align with those detailed functions*

## 4.3 Network APIs

*Editor’s note: Network APIs to enable split rendering.*

## 4.4 Split Rendering Client

*Editor’s note: detailed description of split-rending client.*

## 4.5 Split Rendering Server

*Editor’s note: detailed description of split-rending server.*

# 5 Media codecs, configuration, and data transport

## 5.1 General

*Editor’s note: this clause provides media formats, signalling protocols to support split rendering, etc.*

## 5.2 Media codecs

*Editor’s note: media format, where possible, references to TS 26.114, TS 26.264, TS 26.119, TS 26.522 and TS 26.565.*

## 5.3 Media configuration

## 5.4 Data transport

# 6 Split Rendering Metrics

*Editor’s note: this clause defines a set of metrics that are relevant to the operation of a split rendering session.*

# 7 Procedures

## 7.1 General procedures for session establishment

*Editor’s note: session establishment procedures*

## 7.2 General procedures for session modification

*Editor’s note: session modification/update procedures*

## 7.3 Network support procedures

*Editor’s note:* *procedures for adaption of split rendering client and server based on network support.*

Annex <A> (normative):  
<Normative annex for a Technical Specification>

Start each annex on a new page.

Annexes are labelled A, B, C, etc. and designated either "normative" or "informative" depending on their content.

Normative annexes only to appear in Technical Specifications. Use style "Heading 8".

Annex <B> (informative):  
<Informative annex for a Technical Specification>

Informative annexes may appear in both Technical Specifications and Technical Reports. Use style "Heading 8" for use in TSs.

Informative annexes shall not contain requirements for the implementation of the Technical Specification.

# B.1 Heading levels in an annex

Heading levels within an annex are used as in the main document, but for Heading level selection, the "A.", "B.", etc. are ignored. e.g. **B.1.2** is formatted using ***Heading 2*** style.

Annex <F> (informative):

Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Change history | | | | | | | |
| Date | Meeting | TDoc | CR | Rev | Cat | Subject/Comment | New version |
| 04-2024 | 127b-e | S4-240645 |  |  |  | [SR\_IMS]TS 26.567 Skeleton | 0.0.1 |
| 04-2024 | 127b-e | S4-240790 |  |  |  | [SR\_IMS] version agreed during SA4#127bis-e (including S4-240583 and S4-240651) | 0.1.0 |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |