**3GPP TSG-SA5 Meeting #133e *S5-205197***

**e-meeting 12th - 21st October 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **28.540** | **CR** |   | **rev** | **-** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  Add requirements of SLA management |
|  |  |
| ***Source to WG:*** |  China Mobile |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** |  EMA5SLA |  | ***Date:*** |  2020-10-02 |
|  |  |  |  |  |
| ***Category:*** |  B |  | ***Release:*** | Release 17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The SLA management has discussed to introduce GST into 3GPP management system. It is clear that the 3GPP management system will have the capability to decompose end-to-end SLA requirement to requirements for certain network slice subnet. So it is important to introduce this part into the requirements. |
|  |  |
| ***Summary of change:*** |  Add requirements of SLA management |
|  |  |
| ***Consequences if not approved:*** | The requirement is missing. |
|  |  |
| ***Clauses affected:*** | 5.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This is input to the Rel-17 28.540 DraftCR. |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **Start of Changes** |

5.6 Requirements for management of network slice and network slice subnet

The following requirements apply to network slice and network slice subnet:

**REQ-NS\_NRM-CON-001:** The NRM definitions shall support management of network slice.

**REQ-NS\_NRM-CON-002:** The NRM definitions shall support management of network slice subnet.

NOTE: Input data to network slice management can be information from an SLS associated with an SLA.

|  |
| --- |
| **End of Change** |