**3GPP TSG-SA5 Meeting #133-e *S5-205292***

**Online, , 12th Oct 2020 - 21st Oct 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.541** | **CR** |  | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **×** |

|  |
| --- |
|  |
| ***Title:***  | CR Rel-17 ServiceProfle to SliceProfile Translation |
|  |  |
| ***Source to WG:*** | Samsung Research America, Telefonica, China Mobile, Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | EMA5SLA |  | ***Date:*** | 2020-10-01 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | ServiceProfile to SliceProfile translation is required. All ServiceProfle attributes should be translated into either CN slice profile or RAN slice profile or both. |
|  |  |
| ***Summary of change:*** | * Two new <<dataType>> are introduced as CNSliceSubnetProfile<<dataType>> and RANSliceSubnetProfile <<datatype>> under SliceProfile
* CNSliceSubnetProfile<<dataType>> contains attributes related to CN, translated from corresponding attributes in ServiceProfile
* RANSliceSubnetProfile <<datatype>> contains attributes related to RAN, translated from corresponding attributes in ServiceProfile.

Attrbutes for CNSliceSubnetProfile and RANSliceSubnetProfile are defined in Attributes definition. |
|  |  |
| ***Consequences if not approved:*** | Incomplete GST solution. |
|  |  |
| ***Clauses affected:*** | 6.3.4.2, 6.3.x(new), 6.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **×** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **×** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **×** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This is input to the Rel-17 28.541 DraftCR for ServiceProfile to SliceProfile translation |
|  |  |
| ***This CR's revision history:*** |  |

# 6 Information model definitions for network slice NRM

## 6.1 Imported information entities and local labels

|  |  |
| --- | --- |
| Label reference | Local label |
| TS 28.622 [30], IOC, Top | Top |
| TS 28.622 [30], IOC, SubNetwork | SubNetwork |
| TS 28.622 [30], IOC, ManagedFunction | ManagedFunction |
| TS 28.658 [19], dataType, PLMNId | PLMNId |

## 6.2 Class diagram

### 6.2.1 Relationships



Figure 6.2.1-1: Network slice NRM fragment relationship

NOTE 1: The <<OpenModelClass>> NetworkService and <<OpenModelClass>> VNF are defined in [40].

NOTE 2: The target Network Service (NS) instance represents a group of VNFs and PNFs that are supporting the source network slice subnet instance.

NOTE 3: The instance tree of this NRM fragment would not contain the instances of NetworkService and VNF. However, the NetworkSliceSubNet instances would have an attribute holding the identifiers of NetworkService instances and the ManagedFunction instance would have an attribute holding identifiers of VNF instances.



Figure 6.2.1-2: Transport EP NRM fragment relationship

### 6.2.2 Inheritance





Figure 6.2.2-1: Network slice inheritance relationship

## 6.3 Class definitions

### 6.3.1 NetworkSlice

#### 6.3.1.1 Definition

This IOC represents the properties of a network slice instance in a 5G network. For more information about the network slice instance, see 3GPP TS 28.531 [26].

#### 6.3.1.2 Attributes

The NetworkSlice IOC includes attributes inherited from SubNetwork IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| operationalState | M | T | F | F | T |
| administrativeState | M | T | T | F | T |
| serviceProfileList | M | T | T | F | T |
| **Attribute related to role** |  |  |  |  |  |
| networkSliceSubnetRef | M | T | F | F | T |

#### 6.3.1.3 Attribute constraints

None.

#### 6.3.1.4 Notifications

The common notifications defined in subclause 6.5 are valid for this IOC, without exceptions or additions.

### 6.3.2 NetworkSliceSubnet

#### 6.3.2.1 Definition

This IOC represents the properties of a network slice subnet instance in a 5G network. For more information about the network slice subnet instance, see 3GPP TS 28.531 [26].

#### 6.3.2.2 Attributes

The NetworkSliceSubnet IOC includes attributes inherited from SubNetwork IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| operationalState | M | T | F | F | T |
| administrativeState | M | T | T | F | T |
| nsInfo | CM | T | F | F | T |
| sliceProfileList | M | T | T | F | T |
| **Attribute related to role** |  |  |  |  |  |
| managedFunctionRef | M | T | F | F | T |
| networkSliceSubnetRef | M | T | F | F | T |

#### 6.3.2.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| nsInfo Support Qualifier | Condition: It shall be supported if the NSS instance is realized in the virtualized environment. Otherwise this attribute shall be absent. |

#### 6.3.2.4 Notifications

The common notifications defined in subclause 6.5 are valid for this IOC, without exceptions or additions.

### 6.3.3 ServiceProfile <<dataType>>

#### 6.3.3.1 Definition

This data type represents the properties of network slice related requirement that should be supported by the network slice instance in 5G network. The network slice can be tailored based on the specific requirements adhered to SLA agreed between Network Slice Customer (NSC) and Network Slice Provider (NSP), see clause 2 of [50]. A network slicing provider may add additional requirements not directly derived from SLA’s, associated to the provider internal [business] goals. The GST defined by GSMA (see [50]) and the service performance requirements defined in 3GPP TS 22.261 [28] and TS 22.104 [51] are all considered as input for the network slice related requirements.

#### 6.3.3.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| serviceProfileId | M | T | F | T | T |
| sNSSAIList | M | T | T | F | T |
| pLMNIdList | M | T | T | F | T |
| maxNumberofUEs | O | T | T | F | T |
| coverageArea | O | T | T | F | T |
| latency | O | T | T | F | T |
| uEMobilityLevel | O | T | T | F | T |
| resourceSharingLevel | O | T | T | F | T |
| sST | M | T | T | F | T |
| availability | O | T | T | F | T |
| delayTolerance | O | T | T | F | T |
| deterministicComm | O | T | T | F | T |
| dLThptPerSlice | O | T | T | F | T |
| dLThptPerUE | O | T | T | F | T |
| uLThptPerSlic | O | T | T | F | T |
| uLThptPerUE | O | T | T | F | T |
| maxPktSize | O | T | T | F | T |
| maxNumberofConns | O | T | T | F | T |
| kPIMonitoring | O | T | T | F | T |
| supportedAccessTech | O | T | T | F | T |
| userMgmtOpen | O | T | T | F | T |
| v2XCommModels | O | T | T | F | T |
| termDensity | O | T | T | F | T |
| activityFactor | O | T | T | F | T |
| uESpeed | O | T | T | F | T |
| jitter | O | T | T | F | T |
| survivalTime | O | T | T | F | T |
| reliability | O | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

#### 6.3.3.3 Attribute constraints

None.

#### 6.3.3.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.4 SliceProfile <<dataType>>

#### 6.3.4.1 Definition

This data type represents the properties of network slice subnet related requirement that should be supported by the network slice subnet instance in a 5G network.

#### 6.3.4.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| sliceProfileId | M | T | F | T | T |
| sNSSAIList | M | T | T | F | T |
| pLMNIdList | M | T | T | F | T |
| perfReq | M | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| CNSliceSubnetProfile | CM | T | T | F | T |
| RANSliceSubnetProfile | CM | T | T | F | T |
| TopSliceSubnetProfile | CM | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

#### 6.3.4.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| CNSliceSubnetProfile Support Qualifier | Condition: It shall be present when the slice profile for CN domain is needed. |
| RANSliceSubnetProfile Support Qualifier | Condition: It shall be present when the slice profile for RAN domain is needed. |
| tOPSliceSubnetProfileSupport Qualifier | Condition: It shall be present when the slice profile is for top/root network slice subnet |

Editors Note 1: Need for specific slice profile for TN domain is FFS.

Editor's NOTE 2: Analysis on clashes/inconsistencies between perfReq attribute from SliceProfile (cf. Section 6.3.4.2) and attributes from domain-specific SliceProfiles is FFS.

Editor's NOTE 3: The common attributes of the three types of SliceProfile may be extracted out and put into the common part of the SliceProfile

Editor's NOTE 4: Whether SliceProfile is dataType or IOC is FFS.

Editor's NOTE 5: Whether RANSliceSubnetProfile is inherited from or contained by SliceProfile is FFS.

Editor's NOTE 6: Whether CNSliceSubnetProfile is inherited from or contained by SliceProfile is FFS.

Editor's NOTE 7: Whether tOPSliceSubnetProfile is inherited from or contained by SliceProfile is FFS.

Editor's NOTE 8: All the attributes of SliceProfile, CNSliceSubnetProfile, RANSliceSubnetProfile and topSliceSubnetProfile will be revisited later

#### 6.3.4.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.5 NsInfo <<dataType>>

#### 6.3.5.1 Definition

This data type represents the properties of network service information (See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]) corresponding to the network slice subnet instance.

#### 6.3.5.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| nSInstanceId | M | T | F | F | T |
| nsName | O | T | F | F | T |
| description | O | T | F | F | T |

#### 6.3.5.3 Attribute constraints

None.

#### 6.3.5.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.6 ServAttrCom <<dataType>>

#### 6.3.x.1 Definition

This data type represents the common properties of service requirement related attributes (see GSMA NG.116 [50] corresponding to Attribute categories, tagging and exposure).

#### 6.3.6.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| category | M | T | F | F | T |
| tagging | CM | T | F | F | T |
| exposure | M | T | F | F | T |

#### 6.3.6.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| tagging Support Qualifier | Condition: It shall be supported if the category is character. Otherwise this attribute shall be absent. |

#### 6.3.6.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.7 DelayTolerance<<dataType>>

#### 6.3.7.1 Definition

This data type represents the delay tolerance (See Clause 3.4.3 of GSMA NG.116 [50]).

#### 6.3.7.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| support | M | T | F | F | T |

#### 6.3.7.3 Attribute constraints

None.

#### 6.3.7.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.7 DeterminComm <<dataType>>

#### 6.3.7.1 Definition

This data type represents the properties of the deterministic communication for periodic user traffic. Periodic traffic refers to the type of traffic with periodic transmissions.

#### 6.3.7.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| availability | M | T | F | F | T |
| periodicityList | M | T | T | F | T |

#### 6.3.7.3 Attribute constraints

None.

#### 6.3.7.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.8 DLThpt<<dataType>>

#### 6.3.8.1 Definition

This data type represents the downlink throughput per slice or per UE (See Clause 3.4.5 and 3.4.6 of GSMA NG.116 [50]).

#### 6.3.8.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| guaThpt | M | T | F | F | T |
| maxThpt | C | T | F | F | T |

#### 6.3.8.3 Attribute constraints

None.

#### 6.3.8.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.9 ULThpt<<dataType>>

#### 6.3.9.1 Definition

This data type represents the uplink throughput per slice or per UE (See Clause 3.4.31 and 3.4.32 of GSMA NG.116 [50]).

#### 6.3.9.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| guaThpt | O | T | F | F | T |
| maxThpt | O | T | F | F | T |

#### 6.3.9.3 Attribute constraints

None.

#### 6.3.9.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.10 MaxPktSize <<dataType>>

#### 6.3.10.1 Definition

This data type represents the maximum packet size (See Clause 3.4.11 of GSMA NG.116 [50]).

#### 6.3.10.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| maxSize | M | T | F | F | T |

#### 6.3.10.3 Attribute constraints

None.

#### 6.3.10.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.11 MaxNumberofConns <<dataType>>

#### 6.3.11.1 Definition

This data type represents maximun number of connections (See Clause 3.4.15 of GSMA NG.116 [50]).

#### 6.3.11.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| nOofConn | M | T | F | F | T |

#### 6.3.11.3 Attribute constraints

None.

#### 6.3.11.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.12 SupportedAccessTech<<dataType>>

#### 6.3.12.1 Definition

This data type represents supported access technologies (See Clause 3.4.27 of GSMA NG.116 [50]).

#### 6.3.12.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| accTechList | M | T | F | F | T |

#### 6.3.12.3 Attribute constraints

None.

#### 6.3.12.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.13 KPIMonitoring <<dataType>>

#### 6.3.13.1 Definition

This data type represents performance monitoring (See Clause 3.4.17 of GSMA NG.116 [50]).

#### 6.3.13.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| kPIList | M | T | F | F | T |

#### 6.3.13.3 Attribute constraints

None.

#### 6.3.13.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.14 UserMgmtOpen<<dataType>>

#### 6.3.14.1 Definition

This data type represents User management openness (See Clause 3.4.33 of GSMA NG.116 [50]).

#### 6.3.14.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| support | M | T | F | F | T |

#### 6.3.14.3 Attribute constraints

None.

#### 6.3.14.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.15 V2XCommMode<<dataType>>

#### 6.3.15.1 Definition

This data type represents V2X communication mode (See Clause 3.4.35 of GSMA NG.116 [50]).

#### 6.3.15.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| v2XMode | M | T | F | F | T |

#### 6.3.15.3 Attribute constraints

None.

#### 6.3.15.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.16 TermDensity<<dataType>>

#### 6.3.16.1 Definition

This data type represents Terminal density (See Clause 3.4.30 of GSMA NG.116 [50]).

#### 6.3.16.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| density | M | T | F | F | T |

#### 6.3.16.3 Attribute constraints

None.

#### 6.3.16.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.17 EP\_Transport

#### 6.3.17.1 Definition

This IOC represents the logical transport interface or endpoint which including transport level information, e.g. transport address, reachability information and QoS profiles, etc.

The IOC is inherited from Top IOC.

#### 6.3.17.2 Attributes

The EP\_Transport IOC includes attributes inherited from Top IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| ipAddress | M | T | F | F | T |
| logicInterfaceId | M | T | T | F | T |
| nextHopInfo | O | T | F | F | T |
| qosProfile | O | T | T | F | T |

#### 6.3.17.3 Attribute constraints

None.

#### 6.3.17.4 Notifications

The common notifications defined in subclause 6.5 are valid for this IOC, without exceptions or additions.

### 6.3.x CNSliceSubnetProfile<<dataType>>

#### 6.3.x.1 Definition

This data type represents the requirements for CN slice profile.

Editor's NOTE: Whether CNSliceSubnetProfile is an IOC or dataType is FFS.

#### 6.3.x.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| maxNumberofUEs | O | T | T | F | T |
| latency | O | T | T | F | T |
| dLThptPerSlice | O | T | T | F | T |
| dLThptPerUE | O | T | T | F | T |
| uLThptPerSlice | O | T | T | F | T |
| uLThptPerUE | O | T | T | F | T |
| maxNumberOfPDUSessions | O | T | T | F | T |

#### 6.3.x.3 Attribute constraints

None.

#### 6.3.x.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.y RANSliceSubnetProfile<<dataType>>

#### 6.3.y.1 Definition

This data type represents the requirements for RAN slice profile.

Editor's NOTE 1: Whether the attributes of RANSliceSubnetProfile need to be modelled by one IOC or more than one IOC is FFS.

Editor's NOTE 2: Whether RANSliceSubnetProfile is an IOC or dataType is FFS.

#### 6.3.y.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| coverageAreaGeoPolygon | O | T | T | F | T |
| coverageAreaTAList | O | T | T | F | T |
| uEMobilityLevel | O | T | T | F | T |
| resourceSharingLevel | O | T | T | F | T |
| maxNumberofUEs | O | T | T | F | T |
| activityFactor | O | T | T | F | T |
| dLThptPerUE | O | T | T | F | T |
| uLThptPerUE | O | T | T | F | T |
| uESpeed | O | T | T | F | T |
| reliability | O | T | T | F | T |
| serviceType | O | T | T | F | T |

#### 6.3.y.3 Attribute constraints

None.

#### 6.3.y.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 6.3.z TopSliceSubnetProfile<<dataType>>

#### 6.3.z.1 Definition

This data type represents the requirements for the top slice associated with the network slice.

Editor's NOTE: Whether TopSliceSubnetProfile is an IOC or dataType is FFS.

#### 6.3.y.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| coverageArea | O | T | T | F | T |
| latency | O | T | T | F | T |
| maxNumberofUEs | O | T | T | F | T |
| dLThptPerSlice | O | T | T | F | T |
| dLThptPerUE | O | T | T | F | T |
| uLThptPerSlice | O | T | T | F | T |
| uLThptPerUE | O | T | T | F | T |
| maxPktSize | O | T | T | F | T |
| maxNumberofConns | O | T | T | F | T |

#### 6.3.y.3 Attribute constraints

None.

#### 6.3.y.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

## 6.4 Attribute definition

### 6.4.1 Attribute properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| availability | This parameter specifies the communication service availability requirement, expressed as a percentage. The communication service availability is defined in clause 3.1 of TS 22.261 [28]. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: True |
| serviceProfileId | A unique identifier of property of network slice related requirement should be supported by the network slice instance. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| sliceProfileId | A unique identifier of the property of network slice subnet related requirement should be supported by the network slice subnet instance. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| operationalState | It indicates the operational state of the network slice instance or the network slice subnet instance. It describes whether or not the resource is physically installed and working.allowedValues: "ENABLED", "DISABLED".The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| administrativeState | It indicates the administrative state of the network slice instance or the network slice subnet instance. It describes the permission to use or prohibition against using the instance, imposed through the OAM services.allowedValues: “LOCKED”, “UNLOCKED”, SHUTTINGDOWN” The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| nsInfo | This attribute contains the NsInfo of the NS instance corresponding to the network slice subnet instance. The NsInfo is described in clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: NsInfomultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| nSInstanceId | This attribute specifies the identifier of NS instance corresponding to the network slice subnet instance.See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| nsName | This attribute specifies the name of NS instance corresponding to the network slice subnet instance.See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| description | This attribute specifies the description of NS instance corresponding to the network slice subnet instance.See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| category | This attribute specifies the category of a service requirement/attribute of GST (see GSMA NG.116 [50]).allowedValues: character, scalability | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| tagging | This attribute specifies the tagging of a service requirement/attribute of GST in character catogary (see GSMA NG.116 [50]).allowedValues: performance, function, operation | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| exposure | This attribute specifies exposure mode of a service requirement/attribute of GST (see GSMA NG.116 [50]).allowedValues: API, KPI | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| sNSSAIList | This parameter specifies the S-NSSAI list to be supported by the new NSI to be created or the existing NSI to be re-used.sNSSAList is defined in subclause 4.4.1 |  |
| perfReq | This parameter specifies the requirements to the network slice subnet in terms of the scenarios defined in the TS 22.261 [28] and TS 22.104 [51], i.e. the "performance requirements for high data rate and traffic density scenarios" in TS 22.261 [28], "periodic deterministic communication, aperiodic deterministic communication, non-deterministic communication, and mixed traffic" in TS 22.104 [51].It is a structure containing the following elements:- list of perfReqDepending on the sST value, the list of perfReq will be- list of eMBBPerfReqor- list of uRLLCPerfReqor- list of mIoTPerfReqNOTE 1: the list of mIoTPerfReq is not addressed in the present document.allowedValues:- list of eMBBPerfReq is a list of entries where an entry identifies the performance requirements to the network slice subnet in terms of the scenarios defined in the Table 7.1-1 of TS 22.261 [28]. An entry has the following attributes: expDataRateDL (Integer), expDataRateUL (Integer), areaTrafficCapDL (Integer), areaTrafficCapUL (Integer), overallUserDensity (Integer), activityFactor (Integer), (see table 7.1-1 of TS 22.261 [28]).- list of uRLLCPerfReq is a list of entries where an entry identifies the performance requirements to the network slice subnet in terms of the scenarios defined in clauses 5.2 through 5.5 of TS 22.104 [51]. An entry has the following attributes: cSAvailabilityTarget (Float), cSReliabilityMeanTime (String), , expDataRate (Integer), msgSizeByte (String), transferIntervalTarget (String), survivalTime (String), , , (see table 5.2-1, table 5.3-1, table 5.4-1 and table 5.5-1 of TS 22.104 [51]).NOTE 2: Limitation on attribute values in instances of SliceProfile is not addressed in the present document.NOTE 3: The attributes inside perfReq here need further breaking down to define requirements for each subnetwork under different SST values. | type: PerfReqmultiplicity: \*1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxNumberofUEs | An attribute specifies the maximum number of UEs may simultaneously access the network slice instance. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| coverageAreaTAList | An attribute specifies a list of TrackingAreas where the NSI can be selected.allowedValues:Legacy TAC and Extended TAC are defined in clause 9.3.3.10 of TS 38.413 [5]. | type: Integermultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| latency | An attribute specifies the packet transmission latency (millisecond) through the RAN, CN, and TN part of 5G network and is used to evaluate utilization performance of the end-to-end network slice instance. See clause 6.3.1 of 28.554 [27]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| topSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through all domains of the network slice and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| CNSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through CN domain of the network slice and is used to evaluate the delay in CN domain, e.g. time between received UL/DL packet on N3/N6 interface of UPF and successfully sent out the packet on N6/N3 interface.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| RANSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through RAN domain of the network slice and is used to evaluate the delay in RAN domain, e.g. time between received UL/DL packet on air interface/NgU of gNB and successfully sent out the packet on NgU/air interface of the gNB.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| topSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through all domains of the network slice and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| uEMobilityLevel | An attribute specifies the mobility level of UE accessing the network slice instance. See 6.2.1 of TS 22.261 [28].allowedValues: stationary, nomadic, restricted mobility, fully mobility. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: True |
| serviceProfile.resourceSharingLevel | An attribute specifies whether the resources to be allocated to the network slice instance may be shared with another network slice instance(s).allowedValues: shared, non-shared. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: YesisNullable: True |
| sliceProfile.resourceSharingLevel | An attribute specifies whether the resources to be allocated to the network slice subnet instance may be shared with another network slice subnet instance(s).allowedValues: shared, non-shared. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: YesisNullable: True |
| serviceProfileList | An attribute specifies a list of ServiceProfile (see clause 6.3.3) supported by the network slice instance | type: ServiceProfilemultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sliceProfileList | An attribute specifies a list of SliceProfile (see clause 6.3.4) supported by the network slice subnet instance | type: SliceProfilemultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sST | This parameter specifies the slice/service type for a ServiceProfile.See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| delayTolerance | An attribute specifies the properties of service delivery flexibility, especially for the vertical services that are not chasing a high system performance. See clause 4.3 of TS 22.104 [51]. | type: DelayTolerancemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| DelayTolerance.support | An attribute specifies whether or not the NSI supports service delivery flexibility, especially for the vertical services that are not chasing a high system performance.allowedValues:"NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| deterministicComm | An attribute specifies the properties of the deterministic communication for periodic user traffic, see clause 4.3 of TS 22.104 [51]. | type: <<DeterminComm>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| DeterminComm.availability | An attribute specifies whether or not the NSI supports deterministic communication for period user traffic.allowedValues:"NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| DeterminComm.periodicityList | An attribute specifies a list of periodicities supported by the NSI or NSSI for deterministic communication. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| dLThptPerSlice | This attribute defines achievable data rate of the network slice or network slice subnet in downlink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50]. | type: DLThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| dLThptPerUE | This attribute defines data rate supported by the network slice or network slice subnet per UE, refer NG.116 [50].  | type: DLThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| guaThpt | This attribute describes the guaranteed data rate. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| maxThpt | This attribute describes the maximum data rate. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| uLThptPerSlice | This attribute defines achievable data rate of the network slice or network slice subnet in uplink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50].  | type: ULThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| uLThptPerUE | This attribute defines data rate supported by the network slice or network slice subnet per UE, refer NG.116 [50].  | type: ULThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxPktSize | This parameter specifies the maximum packet size supported by the network slice or network slice subnet, refer NG.116 [50].  | type: MaxPktSizemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| MaxPktSize.maxsize | This parameter specifies the maximum packet size supported by the network slice, refer NG.116 [50].  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxNumberofConns | This parameter defines the maximum number of concurrent sessions supported by the network slice or network slice subnet, refer NG.116 [50].  | type: MaxNumberofConnsmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| MaxNumberofConns.nOofConn | This parameter defines the maximum number of concurrent sessions supported by the network slice, refer NG.116 [50].  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| kPIMonitoring | An attribute specifies the name list of KQIs and KPIs available for performance monitoring. | type: KPIMonitoringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| KPIMonitoring. kPIList | An attribute specifies the name list of KQIs and KPIs available for performance monitoring. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| supportedAccessTech | An attribute specifies which access technologies are supported by the NSI. | type: SupportedAccessTechmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| SupportedAccessTech.accTechList | An attribute specifies which access technologies are supported by the NSI.allowedValues:1: NR2: NB-IoT3: WI-Fi4: Fixed access (e.g. DSL, Fibre) | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| userMgmtOpen | An attribute specifies whether or not the NSI supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements. | type: UserMgmtOpenmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| UserMgmtOpen.support | An attribute specifies whether or not the NSI supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements.allowedValues:"NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| v2XCommModels | An attribute specifies whether or not the V2X communication mode is supported by the NSI. | type: V2XCommModemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| V2XCommMode.v2XMode | An attribute specifies whether or not the V2X communication mode is supported by the NSI.allowedValues:"NOT SUPPORTED", "SUPPORTED BY NR". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| coverageArea | An attribute specifies the coverage area of the network slice, i.e. the geographic region where a 3GPP communication service is accessible, see Table 7.1-1 of TS 22.261 [28]) and NG.116 [50]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| termDensity | An attribute specifies the overall user density over the coverage area of the network slice or network slice subnet. See Table 7.1-1 of TS 22.261 [28]). | type: TermDensitymultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| TermDensity.density | An attribute specifies the overall user density over the coverage area of the network slice or network slice subnet. See Table 7.1-1 of TS 22.261 [28]). | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| activityFactor | An attribute specfies the percentage value of the amount of simultaneous active UEs to the total number of UEs where active means the UEs are exchanging data with the network. See Table 7.1-1 of TS 22.261 [28]). | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| uESpeed | An attribute specifies the maximum speed (in km/hour) supported by the network slice or network slice subnet at which a defined QoS can be achieved. See Table 7.1-1 of TS 22.261 [28]). | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| jitter | An attribute specifies the deviation from the desired value to the actual value when assessing time parameters, see clause C.4.1 of TS 22.104 [51]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| survivalTime | An attribute specifies the time that an application consuming a communication service may continue without an anticipated message. See clause 5 of TS 22.104 [51]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| reliability | An attribute specifies in the context of network layer packet transmissions, percentage value of the amount of sent network layer packets successfully delivered to a given system entity within the time constraint required by the targeted service, divided by the total number of sent network layer packets, see TS 22.261 [28] and TS 22.104 [51]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| NetworkSlice.networkSliceSubnetRef | This holds a DN of NetworkSliceSubnet relating to the NetworkSlice instance. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| NetworkSliceSubnet.networkSliceSubnetRef | This holds a list of DN of constituent NetworkSliceSubnet supporting NetworkSliceSubnet instance  | type: DNmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| managedFunctionRef | This holds a list of DN of ManagedFunction instances supporting the NetworkSliceSubnet instance. | type: DNmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| ipAddress | This parameter specifies the IP address assigned to a logical transport interface/endpoint. It can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| logicInterfaceId | This parameter specifies the identify of a logical transport interface. It could be VLAN ID, MPLS Tag or Segment ID. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nextHopInfo | This parameter is used to identify ingress transport nodes identification. This can be any of combination of IP address of next-hop router of transport network, system name, port name, IP management address of transport nodes. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| qosProfile | This parameter specifies an QoS Profile for a logical transport interface. It is a reference to the set of profile parameters which are locally provisioned on both sides of a logical transport interface. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: True |
| coverageAreaGeoPolygon | An attribute specifies a geographic coverage area described in the form a polygon where the NSI can be selected. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| serviceType | An attribute specifies the standardized network slice type.allowedValues: eMBB, URLLC, MIoT, V2X. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: True |
|  |  |  |

## 6.5 Common notifications

### 6.5.1 Alarm notifications

This clause presents a list of notifications, defined in TS 28.532 [35], that an MnS consumer may receive. The notification header attribute objectClass/objectInstance shall capture the DN of an instance of a class defined in the present document.

| Name | Qualifier | Notes |
| --- | --- | --- |
| notifyNewAlarm | M | -- |
| notifyClearedAlarm | M | -- |
| notifyAckStateChanged | M | -- |
| notifyAlarmListRebuilt | M | -- |
| notifyChangedAlarm | O | -- |
| notifyCorrelatedNotificationChanged | O | -- |
| notifyChangedAlarmGeneral | O | -- |
| notifyComments | O | -- |
| notifyPotentialFaultyAlarmList | O | -- |

### 6.5.2 Configuration notifications

 This clause presents a list of notifications, defined in TS 28.532 [35], that an MnS consumer may receive. The notification header attribute objectClass/objectInstance shall capture the DN of an instance of a class defined in the present document.

| Name | Qualifier | Notes |
| --- | --- | --- |
| notifyMOICreation | O | -- |
| notifyMOIDeletion | O | -- |
| notifyMOIAttributeValueChanges | O | -- |
| notifyEvent | O | -- |