3GPP TSG SA WG5 Meeting 135-e TDoc S5-211148

electronic meeting, online, 25 January - 3 February 2021

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **-** | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Adding IMS Information in converged charging | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | IMS nodes are missing in Nchf\_ConvergedCharging service. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add iMSNodeType in IMS information to indicate the explicit type of IMS node. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | IMS cannot use converged charging. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 5.1, 6.1.6.2.x (new), 6.1.6.3.x (new), A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This is input to the Rel-17 32.291 DraftCR for 5GSIMSCH | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **First change** |

2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.240: "Telecommunication management; Charging management; Charging architecture and principles".

[2] - [13] Void.

[14] 3GPP TS 32.254: "Telecommunication management; Charging management; Exposure function Northbound Application Program Interfaces (APIs) charging ".

[15] - [28] Void.

[29] 3GPP TS 32.274: "Telecommunication management; Charging management;Short Message Service (SMS) charging".

[30] 3GPP TS 32.255: "Telecommunication management; Charging management; 5G Data connectivity domain charging; stage 2".

[31] 3GPP TS 32.256: "Telecommunication management; Charging management; 5G connection and mobility domain charging; stage 2".

[32] 3GPP TS 32.260: "Telecommunication management; Charging management; IP Multimedia Subsystem (IMS) charging".

[33]- [49] Void.

[50] - [57] Void.

[58] 3GPP TS 32.290: "Telecommunication management; Charging management; 5G system; Services, operations and procedures of charging using Service Based Interface (SBI).

[59] - [69] Void.[70] 3GPP TS 28.201: "Charging management; Network slice performance and analytics charging in the 5G System (5GS); Stage 2".

[71] 3GPP TS 28.202: "Charging management; Network slice management charging in the 5G System (5GS); Stage 2".

[72] - [99] Void.

[100] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[101] 3GPP TR 21.900: "Technical Specification Group working methods".

[102] - [199] Void

[200] - [252] Void

[253] 3GPP TS 28.532: "Management and orchestration; Management services".

[254] 3GPP TS 28.541: "Management and orchestration; 5G Network Resource Model (NRM); Stage 2 and stage 3".

[255] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects".

[256] 3GPP TS 28.554: "Management and orchestration;5G end to end Key Performance Indicators (KPI)".

[257] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[258] - [298] Void

[299] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[300] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[301] 3GPP TS 29.594: "5G System; Spending Limit Control Service; Stage 3".

[302] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[303] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[304] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[305] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[306] 3GPP TS 29.520: "5G System; Network Data Analytics Services;Stage 3".

[307] - [370] Void

[371] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[372] - [389] Void

[390] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[391] - [399] Void

[400] Void.

[401] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2) ".

[402] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format ".

[403] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[404] - [499] Void.

[500] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[501] - [599] Void.

|  |
| --- |
| **Next change** |

5.1 Introduction

The following services are provided by the CHF.

**Table 5.1-1: NF Services provided by CHF**

| **Service Name** | **Description** | **Consumer** |
| --- | --- | --- |
| Nchf\_ConvergedCharging service | This service provides a converged charging for session and event based NF services, with and without quota management, as well as charging information record generation | SMF, SMSF, AMF, NEF, PGW-C+SMF, IMS-Node, CEF,  MnS Producer |
| Nchf\_OfflineOnlyCharging service | This service provides an offline only charging for session based NF service. | SMF |
| Nchf\_SpendingLimitControl | This service enables the PCF to retrieve policy counter status information per UE from the CHF by subscribing to spending limit reporting (i.e. notifications of policy counter status changes). | PCF |

The "Nchf\_SpendingLimitControl" service is defined in 29.594 [301].

|  |
| --- |
| **Next change** |

6.1.6.2.x IMS Specified Data Type

6.1.6.2.x.1 Type ChargingDataRequest

This clause is additional attributes of the type ChargingDataRequest defined in clause 6.1.6.2.x.1 for IMS charging described in 3GPP TS 32.260[32].

**Table 6.1.6.2.x.1-1: IMS Specified attribute of type ChargingDataRequest**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
| iMSChargingInformation | IMSChargingInformation | OM | 0..1 | This field holds the IMS specific information. |  |

6.1.6.2.x.2 Type ChargingDataResponse

This clause is additional attributes of the type ChargingDataResponse defined in clause 6.1.6.2.x.2 for IMS charging described in 3GPP TS 32.260[32].

**Table 6.1.6.2.x.2-1: IMS Specified attribute of type ChargingDataResponse**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
|  |  |  |  |  |  |

6.1.6.2.x.3 Type IMSChargingInformation

**Table 6.1.6.2.x.3-1: Definition of type IMSChargingInformation**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
| iMSNodeType | IMSNodeFunctionality | OM | 0..1 | This field contains the function of IMS node. |  |

|  |
| --- |
| **Next change** |

6.1.6.3.x Enumeration: IMSNodeFunctionality

**Table 6.1.6.3.x-1: Enumeration IMSNodeFunctionality**

|  |  |  |
| --- | --- | --- |
| **Enumeration value** | **Description** | **Applicability** |
| SIP\_AS | This field identifies that NF is a SIP AS. |  |
| MRFC | This field identifies that NF is a MRFC. |  |
| IMS\_GWF | This field identifies that NF is a IMS-GWF. |  |

|  |
| --- |
| **Next change** |

A.2 Nchf\_ConvergedCharging API

openapi: 3.0.0

info:

title: Nchf\_ConvergedCharging

version: 3.0.1

description: |

ConvergedCharging Service © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 32.291 V16.6.0: Telecommunication management; Charging management;

5G system, charging service; Stage 3.

url: 'http://www.3gpp.org/ftp/Specs/archive/32\_series/32.291/'

servers:

- url: '{apiRoot}/nchf-convergedcharging/v3'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

- {}

- oAuth2ClientCredentials:

- nchf-convergedcharging

paths:

/chargingdata:

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

responses:

'201':

description: Created

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataResponse'

'400':

description: Bad request

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

'404':

description: Not Found

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

chargingNotification:

'{$request.body#/notifyUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingNotifyRequest'

responses:

'204':

description: 'No Content, Notification was succesfull'

'400':

description: Bad request

content:

application/problem+json:

schema:

$ref: >-

TS29571\_CommonData.yaml#/components/schemas/ProblemDetails

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

'/chargingdata/{ChargingDataRef}/update':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

parameters:

- name: ChargingDataRef

in: path

description: a unique identifier for a charging data resource in a PLMN

required: true

schema:

type: string

responses:

'200':

description: OK. Updated Charging Data resource is returned

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataResponse'

'400':

description: Bad request

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

'404':

description: Not Found

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

'/chargingdata/{ChargingDataRef}/release':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

parameters:

- name: ChargingDataRef

in: path

description: a unique identifier for a charging data resource in a PLMN

required: true

schema:

type: string

responses:

'204':

description: No Content.

'404':

description: Not Found

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nchf-convergedcharging: Access to the Nchf\_ConvergedCharging API

schemas:

ChargingDataRequest:

type: object

properties:

subscriberIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

tenantIdentifier:

type: string

chargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

mnSConsumerIdentifier:

type: string

nfConsumerIdentification:

$ref: '#/components/schemas/NFIdentification'

invocationTimeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

invocationSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

retransmissionIndicator:

type: boolean

oneTimeEvent:

type: boolean

oneTimeEventType:

$ref: '#/components/schemas/oneTimeEventType'

notifyUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

serviceSpecificationInfo:

type: string

multipleUnitUsage:

type: array

items:

$ref: '#/components/schemas/MultipleUnitUsage'

minItems: 0

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

pDUSessionChargingInformation:

$ref: '#/components/schemas/PDUSessionChargingInformation'

roamingQBCInformation:

$ref: '#/components/schemas/RoamingQBCInformation'

sMSChargingInformation:

$ref: '#/components/schemas/SMSChargingInformation'

nEFChargingInformation:

$ref: '#/components/schemas/NEFChargingInformation'

registrationChargingInformation:

$ref: '#/components/schemas/RegistrationChargingInformation'

n2ConnectionChargingInformation:

$ref: '#/components/schemas/N2ConnectionChargingInformation'

locationReportingChargingInformation:

$ref: '#/components/schemas/LocationReportingChargingInformation'

nSPAChargingInformation:

$ref: '#/components/schemas/NSPAChargingInformation'

nSMChargingInformation:

$ref: '#/components/schemas/NSMChargingInformation'

iMSChargingInformation:

$ref: '#/components/schemas/IMSChargingInformation'

required:

- nfConsumerIdentification

- invocationTimeStamp

- invocationSequenceNumber

ChargingDataResponse:

type: object

properties:

invocationTimeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

invocationSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

invocationResult:

$ref: '#/components/schemas/InvocationResult'

sessionFailover:

$ref: '#/components/schemas/SessionFailover'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

multipleUnitInformation:

type: array

items:

$ref: '#/components/schemas/MultipleUnitInformation'

minItems: 0

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

pDUSessionChargingInformation:

$ref: '#/components/schemas/PDUSessionChargingInformation'

roamingQBCInformation:

$ref: '#/components/schemas/RoamingQBCInformation'

required:

- invocationTimeStamp

- invocationSequenceNumber

ChargingNotifyRequest:

type: object

properties:

notificationType:

$ref: '#/components/schemas/NotificationType'

reauthorizationDetails:

type: array

items:

$ref: '#/components/schemas/ReauthorizationDetails'

minItems: 0

required:

- notificationType

ChargingNotifyResponse:

type: object

properties:

invocationResult:

$ref: '#/components/schemas/InvocationResult'

NFIdentification:

type: object

properties:

nFName:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

nFIPv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

nFIPv6Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

nFPLMNID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

nodeFunctionality:

$ref: '#/components/schemas/NodeFunctionality'

nFFqdn:

type: string

required:

- nodeFunctionality

MultipleUnitUsage:

type: object

properties:

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

requestedUnit:

$ref: '#/components/schemas/RequestedUnit'

usedUnitContainer:

type: array

items:

$ref: '#/components/schemas/UsedUnitContainer'

minItems: 0

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

multihomedPDUAddress:

$ref: '#/components/schemas/PDUAddress'

required:

- ratingGroup

InvocationResult:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

failureHandling:

$ref: '#/components/schemas/FailureHandling'

Trigger:

type: object

properties:

triggerType:

$ref: '#/components/schemas/TriggerType'

triggerCategory:

$ref: '#/components/schemas/TriggerCategory'

timeLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

volumeLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

volumeLimit64:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

maxNumberOfccc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

tariffTimeChange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

required:

- triggerType

- triggerCategory

MultipleUnitInformation:

type: object

properties:

resultCode:

$ref: '#/components/schemas/ResultCode'

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

grantedUnit:

$ref: '#/components/schemas/GrantedUnit'

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

validityTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

quotaHoldingTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

finalUnitIndication:

$ref: '#/components/schemas/FinalUnitIndication'

timeQuotaThreshold:

type: integer

volumeQuotaThreshold:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

unitQuotaThreshold:

type: integer

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

required:

- ratingGroup

RequestedUnit:

type: object

properties:

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

UsedUnitContainer:

type: object

properties:

serviceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

quotaManagementIndicator:

$ref: '#/components/schemas/QuotaManagementIndicator'

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

triggerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

eventTimeStamps:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

minItems: 0

localSequenceNumber:

type: integer

pDUContainerInformation:

$ref: '#/components/schemas/PDUContainerInformation'

nSPAContainerInformation:

$ref: '#/components/schemas/NSPAContainerInformation'

required:

- localSequenceNumber

GrantedUnit:

type: object

properties:

tariffTimeChange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

FinalUnitIndication:

type: object

properties:

finalUnitAction:

$ref: '#/components/schemas/FinalUnitAction'

restrictionFilterRule:

$ref: '#/components/schemas/IPFilterRule'

filterId:

type: string

redirectServer:

$ref: '#/components/schemas/RedirectServer'

required:

- finalUnitAction

RedirectServer:

type: object

properties:

redirectAddressType:

$ref: '#/components/schemas/RedirectAddressType'

redirectServerAddress:

type: string

required:

- redirectAddressType

- redirectServerAddress

ReauthorizationDetails:

type: object

properties:

serviceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

quotaManagementIndicator:

$ref: '#/components/schemas/QuotaManagementIndicator'

PDUSessionChargingInformation:

type: object

properties:

chargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

homeProvidedChargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

mAPDUNon3GPPUserLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

pduSessionInformation:

$ref: '#/components/schemas/PDUSessionInformation'

unitCountInactivityTimer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'  
 rANSecondaryRATUsageReport:

$ref: '#/components/schemas/RANSecondaryRATUsageReport'

UserInformation:

type: object

properties:

servedGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

servedPEI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

unauthenticatedFlag:

type: boolean

roamerInOut:

$ref: '#/components/schemas/RoamerInOut'

PDUSessionInformation:

type: object

properties:

networkSlicingInfo:

$ref: '#/components/schemas/NetworkSlicingInfo'

pduSessionID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

pduType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

sscMode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

hPlmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

servingNetworkFunctionID:

$ref: '#/components/schemas/ServingNetworkFunctionID'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

mAPDUNon3GPPRATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

dnnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

dnnSelectionMode:

$ref: '#/components/schemas/dnnSelectionMode'

chargingCharacteristics:

type: string

pattern: '^[0-9a-fA-F]{1,4}$'

chargingCharacteristicsSelectionMode:

$ref: '#/components/schemas/ChargingCharacteristicsSelectionMode'

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

stopTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

sessionStopIndicator:

type: boolean

pduAddress:

$ref: '#/components/schemas/PDUAddress'

diagnostics:

$ref: '#/components/schemas/Diagnostics'

authorizedQoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AuthorizedDefaultQos'

subscribedQoSInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

authorizedSessionAMBR:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

subscribedSessionAMBR:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

servingCNPlmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

mAPDUSessionInformation:

$ref: '#/components/schemas/MAPDUSessionInformation'

enhancedDiagnostics:

$ref: '#/components/schemas/EnhancedDiagnostics5G'

required:

- pduSessionID

- dnnId

PDUContainerInformation:

type: object

properties:

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

afChargingIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

afChargingIdString:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNodeID:

type: array

items:

$ref: '#/components/schemas/ServingNetworkFunctionID'

minItems: 0

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

sponsorIdentity:

type: string

applicationserviceProviderIdentity:

type: string

chargingRuleBaseName:

type: string

mAPDUSteeringFunctionality:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

mAPDUSteeringMode:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringMode'

NSPAContainerInformation:

type: object

properties:

latency:

type: integer

throughput:

$ref: '#/components/schemas/Throughput'

maximumPacketLossRate:

type: string

serviceExperienceStatisticsData:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ServiceExperienceInfo'

theNumberOfPDUSessions:

type: integer

theNumberOfRegisteredSubscribers:

type: integer

loadLevel:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiLoadLevelInfo'

NSPAChargingInformation:

type: object

properties:

singleNSSAI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- singleNSSAI

NetworkSlicingInfo:

type: object

properties:

sNSSAI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- sNSSAI

PDUAddress:

type: object

properties:

pduIPv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

pduIPv6AddresswithPrefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

pduAddressprefixlength:

type: integer

iPv4dynamicAddressFlag:

type: boolean

iPv6dynamicPrefixFlag:

type: boolean

ServingNetworkFunctionID:

type: object

properties:

servingNetworkFunctionInformation:

$ref: '#/components/schemas/NFIdentification'

aMFId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AmfId'

required:

- servingNetworkFunctionInformation

RoamingQBCInformation:

type: object

properties:

multipleQFIcontainer:

type: array

items:

$ref: '#/components/schemas/MultipleQFIcontainer'

minItems: 0

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

roamingChargingProfile:

$ref: '#/components/schemas/RoamingChargingProfile'

MultipleQFIcontainer:

type: object

properties:

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

triggerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

localSequenceNumber:

type: integer

qFIContainerInformation:

$ref: '#/components/schemas/QFIContainerInformation'

required:

- localSequenceNumber

QFIContainerInformation:

type: object

properties:

qFI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

reportTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNetworkFunctionID:

type: array

items:

$ref: '#/components/schemas/ServingNetworkFunctionID'

minItems: 0

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

3gppChargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

diagnostics:

$ref: '#/components/schemas/Diagnostics'

enhancedDiagnostics:

type: array

items:

type: string

required:

- reportTime

RoamingChargingProfile:

type: object

properties:

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

partialRecordMethod:

$ref: '#/components/schemas/PartialRecordMethod'

SMSChargingInformation:

type: object

properties:

originatorInfo:

$ref: '#/components/schemas/OriginatorInfo'

recipientInfo:

type: array

items:

$ref: '#/components/schemas/RecipientInfo'

minItems: 0

userEquipmentInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

roamerInOut:

$ref: '#/components/schemas/RoamerInOut'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

sMSCAddress:

type: string

sMDataCodingScheme:

type: integer

sMMessageType:

$ref: '#/components/schemas/SMMessageType'

sMReplyPathRequested:

$ref: '#/components/schemas/ReplyPathRequested'

sMUserDataHeader:

type: string

sMStatus:

type: string

pattern: '^[0-7]?[0-9a-fA-F]$'

sMDischargeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

numberofMessagesSent:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

sMServiceType:

$ref: '#/components/schemas/SMServiceType'

sMSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

sMSresult:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

submissionTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

sMPriority:

$ref: '#/components/schemas/SMPriority'

messageReference:

type: string

messageSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

messageClass:

$ref: '#/components/schemas/MessageClass'

deliveryReportRequested:

$ref: '#/components/schemas/DeliveryReportRequested'

OriginatorInfo:

type: object

properties:

originatorSUPI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

originatorGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

originatorOtherAddress:

$ref: '#/components/schemas/SMAddressInfo'

originatorReceivedAddress:

$ref: '#/components/schemas/SMAddressInfo'

originatorSCCPAddress:

type: string

sMOriginatorInterface:

$ref: '#/components/schemas/SMInterface'

sMOriginatorProtocolId:

type: string

RecipientInfo:

type: object

properties:

recipientSUPI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

recipientGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

recipientOtherAddress:

$ref: '#/components/schemas/SMAddressInfo'

recipientReceivedAddress:

$ref: '#/components/schemas/SMAddressInfo'

recipientSCCPAddress:

type: string

sMDestinationInterface:

$ref: '#/components/schemas/SMInterface'

sMrecipientProtocolId:

type: string

SMAddressInfo:

type: object

properties:

sMaddressType:

$ref: '#/components/schemas/SMAddressType'

sMaddressData:

type: string

sMaddressDomain:

$ref: '#/components/schemas/SMAddressDomain'

RecipientAddress:

type: object

properties:

recipientAddressInfo:

$ref: '#/components/schemas/SMAddressInfo'

sMaddresseeType:

$ref: '#/components/schemas/SMAddresseeType'

MessageClass:

type: object

properties:

classIdentifier:

$ref: '#/components/schemas/ClassIdentifier'

tokenText:

type: string

SMAddressDomain:

type: object

properties:

domainName:

type: string

3GPPIMSIMCCMNC:

type: string

SMInterface:

type: object

properties:

interfaceId:

type: string

interfaceText:

type: string

interfacePort:

type: string

interfaceType:

$ref: '#/components/schemas/InterfaceType'

RANSecondaryRATUsageReport:

type: object

properties:

rANSecondaryRATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

qosFlowsUsageReports:

type: array

items:

$ref: '#/components/schemas/QosFlowsUsageReport'

Diagnostics:

type: integer

IPFilterRule:

type: string

QosFlowsUsageReport:

type: object

properties:

qFI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

startTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

endTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

NEFChargingInformation:

type: object

properties:

groupIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

aPIDirection:

$ref: '#/components/schemas/APIDirection'

aPITargetNetworkFunction:

$ref: '#/components/schemas/NFIdentification'

aPIResultCode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

aPIName:

type: string

aPIReference:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

aPIContent:

type: string

required:

- aPIName

RegistrationChargingInformation:

type: object

properties:

registrationMessagetype:

$ref: '#/components/schemas/RegistrationMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

5GMMCapability:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

mICOModeIndication:

$ref: '#/components/schemas/MICOModeIndication'

smsIndication:

$ref: '#/components/schemas/SmsIndication'

taiList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 0

serviceAreaRestriction:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

minItems: 0

requestedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

allowedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

rejectedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

required:

- registrationMessagetype

N2ConnectionChargingInformation:

type: object

properties:

n2ConnectionMessageType:

$ref: '#/components/schemas/N2ConnectionMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

amfUeNgapId:

type: integer

ranUeNgapId:

type: integer

ranNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

restrictedRatList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

minItems: 0

forbiddenAreaList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Area'

minItems: 0

serviceAreaRestriction:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

minItems: 0

restrictedCnList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/CoreNetworkType'

minItems: 0

allowedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

rrcEstCause:

type: string

pattern: '^[0-9a-fA-F]+$'

required:

- n2ConnectionMessageType

LocationReportingChargingInformation:

type: object

properties:

locationReportingMessageType:

$ref: '#/components/schemas/LocationReportingMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

required:

- locationReportingMessageType

N2ConnectionMessageType:

type: integer

LocationReportingMessageType:

type: integer

NSMChargingInformation:

type: object

properties:

managementOperation:

$ref: '#/components/schemas/ManagementOperation'

idNetworkSliceInstance:

type: string

listOfserviceProfileChargingInformation:

type: array

items:

$ref: '#/components/schemas/ServiceProfileChargingInformation'

minItems: 0

managementOperationStatus:

$ref: '#/components/schemas/ManagementOperationStatus'

# To be introduced once the reference to 'generic.yaml is resolved

# managementOperationalState:

# $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

# managementAdministrativeState:

# $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

required:

- managementOperation

ServiceProfileChargingInformation:

type: object

properties:

serviceProfileIdentifier:

type: string

sNSSAIList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

# To be introduced once the reference to 'nrNrm.yaml is resolved

# sST:

# $ref: 'nrNrm.yaml#/components/schemas/Sst'

latency:

type: integer

availability:

type: number

# To be introduced once the reference to sliceNrm.yaml is resolved

# resourceSharingLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/SharingLevel'

jitter:

type: integer

reliability:

type: string

maxNumberofUEs:

type: integer

coverageArea:

type: string

# To be introduced once the reference to sliceNrm.yaml is resolved

# uEMobilityLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/MobilityLevel'

# delayToleranceIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

dLThptPerSlice:

$ref: '#/components/schemas/Throughput'

dLThptPerUE:

$ref: '#/components/schemas/Throughput'

uLThptPerSlice:

$ref: '#/components/schemas/Throughput'

uLThptPerUE:

$ref: '#/components/schemas/Throughput'

maxNumberofPDUsessions:

type: integer

kPIMonitoringList:

type: string

supportedAccessTechnology:

type: integer

# To be introduced once the reference to sliceNrm.yaml is resolved

# v2XCommunicationModeIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

addServiceProfileInfo:

type: string

Throughput:

type: object

properties:

guaranteedThpt:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

maximumThpt:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

IMSChargingInformation:

type: object

properties:

iMSNodeFunctionality:

$ref: '#/components/schemas/IMSNodeFunctionality'

MAPDUSessionInformation:

type: object

properties:

mAPDUSessionIndicator:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MaPduIndication'

aTSSSCapability:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AtsssCapability'

EnhancedDiagnostics5G:

$ref: '#/components/schemas/RanNasCauseList'

RanNasCauseList:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

NotificationType:

anyOf:

- type: string

enum:

- REAUTHORIZATION

- ABORT\_CHARGING

- type: string

NodeFunctionality:

anyOf:

- type: string

enum:

- AMF

- SMF

- SMS

- PGW\_C\_SMF

- NEFF

- SGW

- I\_SMF

- ePDG

- CEF

- type: string

ChargingCharacteristicsSelectionMode:

anyOf:

- type: string

enum:

- HOME\_DEFAULT

- ROAMING\_DEFAULT

- VISITING\_DEFAULT

- type: string

TriggerType:

anyOf:

- type: string

enum:

- QUOTA\_THRESHOLD

- QHT

- FINAL

- QUOTA\_EXHAUSTED

- VALIDITY\_TIME

- OTHER\_QUOTA\_TYPE

- FORCED\_REAUTHORISATION

- UNUSED\_QUOTA\_TIMER # Included for backwards compatibility, shall not be used

- UNIT\_COUNT\_INACTIVITY\_TIMER

- ABNORMAL\_RELEASE

- QOS\_CHANGE

- VOLUME\_LIMIT

- TIME\_LIMIT

- EVENT\_LIMIT

- PLMN\_CHANGE

- USER\_LOCATION\_CHANGE

- RAT\_CHANGE

- SESSION\_AMBR\_CHANGE

- UE\_TIMEZONE\_CHANGE

- TARIFF\_TIME\_CHANGE

- MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS

- MANAGEMENT\_INTERVENTION

- CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA

- CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS

- SERVING\_NODE\_CHANGE

- REMOVAL\_OF\_UPF

- ADDITION\_OF\_UPF

- INSERTION\_OF\_ISMF

- REMOVAL\_OF\_ISMF

- CHANGE\_OF\_ISMF

- START\_OF\_SERVICE\_DATA\_FLOW

- ECGI\_CHANGE

- TAI\_CHANGE

- HANDOVER\_CANCEL

- HANDOVER\_START

- HANDOVER\_COMPLETE

- GFBR\_GUARANTEED\_STATUS\_CHANGE

- ADDITION\_OF\_ACCESS

- REMOVAL\_OF\_ACCESS

- START\_OF\_SDF\_ADDITIONAL\_ACCESS

- type: string

FinalUnitAction:

anyOf:

- type: string

enum:

- TERMINATE

- REDIRECT

- RESTRICT\_ACCESS

- type: string

RedirectAddressType:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- URL

- type: string

TriggerCategory:

anyOf:

- type: string

enum:

- IMMEDIATE\_REPORT

- DEFERRED\_REPORT

- type: string

QuotaManagementIndicator:

anyOf:

- type: string

enum:

- ONLINE\_CHARGING

- OFFLINE\_CHARGING

- QUOTA\_MANAGEMENT\_SUSPENDED

- type: string

FailureHandling:

anyOf:

- type: string

enum:

- TERMINATE

- CONTINUE

- RETRY\_AND\_TERMINATE

- type: string

SessionFailover:

anyOf:

- type: string

enum:

- FAILOVER\_NOT\_SUPPORTED

- FAILOVER\_SUPPORTED

- type: string

3GPPPSDataOffStatus:

anyOf:

- type: string

enum:

- ACTIVE

- INACTIVE

- type: string

ResultCode:

anyOf:

- type: string

enum:

- SUCCESS

- END\_USER\_SERVICE\_DENIED

- QUOTA\_MANAGEMENT\_NOT\_APPLICABLE

- QUOTA\_LIMIT\_REACHED

- END\_USER\_SERVICE\_REJECTED

- USER\_UNKNOWN

- RATING\_FAILED

- QUOTA\_MANAGEMENT

- type: string

PartialRecordMethod:

anyOf:

- type: string

enum:

- DEFAULT

- INDIVIDUAL

- type: string

RoamerInOut:

anyOf:

- type: string

enum:

- IN\_BOUND

- OUT\_BOUND

- type: string

SMMessageType:

anyOf:

- type: string

enum:

- SUBMISSION

- DELIVERY\_REPORT

- SM\_SERVICE\_REQUEST

- DELIVERY

- type: string

SMPriority:

anyOf:

- type: string

enum:

- LOW

- NORMAL

- HIGH

- type: string

DeliveryReportRequested:

anyOf:

- type: string

enum:

- YES

- NO

- type: string

InterfaceType:

anyOf:

- type: string

enum:

- UNKNOWN

- MOBILE\_ORIGINATING

- MOBILE\_TERMINATING

- APPLICATION\_ORIGINATING

- APPLICATION\_TERMINATING

- type: string

ClassIdentifier:

anyOf:

- type: string

enum:

- PERSONAL

- ADVERTISEMENT

- INFORMATIONAL

- AUTO

- type: string

SMAddressType:

anyOf:

- type: string

enum:

- EMAIL\_ADDRESS

- MSISDN

- IPV4\_ADDRESS

- IPV6\_ADDRESS

- NUMERIC\_SHORTCODE

- ALPHANUMERIC\_SHORTCODE

- OTHER

- IMSI

- type: string

SMAddresseeType:

anyOf:

- type: string

enum:

- TO

- CC

- BCC

- type: string

SMServiceType:

anyOf:

- type: string

enum:

- VAS4SMS\_SHORT\_MESSAGE\_CONTENT\_PROCESSING

- VAS4SMS\_SHORT\_MESSAGE\_FORWARDING

- VAS4SMS\_SHORT\_MESSAGE\_FORWARDING\_MULTIPLE\_SUBSCRIPTIONS

- VAS4SMS\_SHORT\_MESSAGE\_FILTERING

- VAS4SMS\_SHORT\_MESSAGE\_RECEIPT

- VAS4SMS\_SHORT\_MESSAGE\_NETWORK\_STORAGE

- VAS4SMS\_SHORT\_MESSAGE\_TO\_MULTIPLE\_DESTINATIONS

- VAS4SMS\_SHORT\_MESSAGE\_VIRTUAL\_PRIVATE\_NETWORK(VPN)

- VAS4SMS\_SHORT\_MESSAGE\_AUTO\_REPLY

- VAS4SMS\_SHORT\_MESSAGE\_PERSONAL\_SIGNATURE

- VAS4SMS\_SHORT\_MESSAGE\_DEFERRED\_DELIVERY

- type: string

ReplyPathRequested:

anyOf:

- type: string

enum:

- NO\_REPLY\_PATH\_SET

- REPLY\_PATH\_SET

- type: string

oneTimeEventType:

anyOf:

- type: string

enum:

- IEC

- PEC

- type: string

dnnSelectionMode:

anyOf:

- type: string

enum:

- VERIFIED

- UE\_DNN\_NOT\_VERIFIED

- NW\_DNN\_NOT\_VERIFIED

- type: string

APIDirection:

anyOf:

- type: string

enum:

- INVOCATION

- NOTIFICATION

- type: string

RegistrationMessageType:

anyOf:

- type: string

enum:

- INITIAL

- MOBILITY

- PERIODIC

- EMERGENCY

- DEREGISTRATION

- type: string

MICOModeIndication:

anyOf:

- type: string

enum:

- MICO\_MODE

- NO\_MICO\_MODE

- type: string

SmsIndication:

anyOf:

- type: string

enum:

- SMS\_SUPPORTED

- SMS\_NOT\_SUPPORTED

- type: string

ManagementOperation:

anyOf:

- type: string

enum:

- CreateMOI

- ModifyMOIAttributes

- DeleteMOI

- type: string

ManagementOperationStatus:

anyOf:

- type: string

enum:

- OPERATION\_SUCCEEDED

- OPERATION\_FAILED

- type: string

IMSNodeFunctionality:

anyOf:

- type: string

enum:

- SIP\_AS

- MRFC

- IMS\_GWF

- type: string

|  |
| --- |
| **End of changes** |