3GPP TSG SA WG5 Meeting 135-e TDoc S5-211159rev1

electronic meeting, online, 25 January - 3 February 2021

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Rel-17 Input to draftCR 28.541 Add new attributes in CNSliceSubnetProfile and RANSliceSubnetProfile |
|  |  |
| ***Source to WG:*** | China Mobile, Huawei, China Southern Power Grid |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | EMA5SLA |  | ***Date:*** | 2021-01-15 |
|  |  |  |  |  |
| ***Category:*** | C |  | ***Release:*** | *Rel-17* |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The attributes defined in CNSliceSubnetProfile and RANSliceSubnetProfile need to be added. And the latency defined in different domains of the network slice also needs to be relected in different profile. |
|  |  |
| ***Summary of change:*** | * Two new attributes are introduced in CNSliceSubnetProfile
* One new attributes is introduced in RANSliceSubnetProfile
* The existed attributes of latency is corrected
 |
|  |  |
| ***Consequences if not approved:*** | The solution will not be completed. |
|  |  |
| ***Clauses affected:*** | 6.3.c.2, 6.3.d.2, 6.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Input to draftCR 28.541 to add new attributes in CNSliceSubnetProfile and RANSliceSubnetProfile |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st modified section** |

# 6 Information model definitions for network slice NRM

#### 6.3.3.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| serviceProfileId | M | T | F | T | T |
| sNSSAIList | M | T | T | F | T |
| pLMNIdList | M | T | T | F | T |
| maxNumberofUEs | O | T | T | F | T |
| coverageArea | O | T | T | F | T |
| latency | O | T | T | F | T |
| uEMobilityLevel | O | T | T | F | T |
| resourceSharingLevel | O | T | T | F | T |
| sST | M | T | T | F | T |
| availability | O | T | T | F | T |
| delayTolerance | O | T | T | F | T |
| deterministicComm | O | T | T | F | T |
| dLThptPerSlice | O | T | T | F | T |
| dLThptPerUE | O | T | T | F | T |
| uLThptPerSlic | O | T | T | F | T |
| uLThptPerUE | O | T | T | F | T |
| maxPktSize | O | T | T | F | T |
| maxNumberofPDUSessions | O | T | T | F | T |
| kPIMonitoring | O | T | T | F | T |
| userMgmtOpen | O | T | T | F | T |
| v2XCommModels | O | T | T | F | T |
| termDensity | O | T | T | F | T |
| activityFactor | O | T | T | F | T |
| uESpeed | O | T | T | F | T |
| jitter | O | T | T | F | T |
| survivalTime | O | T | T | F | T |
| reliability | O | T | T | F | T |
| maxDLDataVolume | O | T | T | F | T |
| maxULDataVolume | O | T | T | F | T |
| nBIoT | O | T | T | F | T |
| synchronicity | O | T | T | F | T |
| positioning | O | T | T | F | T |

NOTE: The attributes in ServiceProfile represent mapped requirements from an NSC (e.g. an enterprise) to an NSP

|  |
| --- |
| **Next Change** |

### 6.3.4 SliceProfile <<dataType>>

#### 6.3.4.1 Definition

This data type represents the properties of network slice subnet related requirement that should be supported by the network slice subnet instance in a 5G network.

#### 6.3.4.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| sliceProfileId | M | T | F | T | T |
| sNSSAIList | M | T | T | F | T |
| pLMNIdList | M | T | T | F | T |
| perfReq | M | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| CNSliceSubnetProfile | CM | T | T | F | T |
| RANSliceSubnetProfile | CM | T | T | F | T |
| TopSliceSubnetProfile | CM | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

#### 6.3.4.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| CNSliceSubnetProfile Support Qualifier | Condition: It shall be present when the slice profile for CN domain is needed. |
| RANSliceSubnetProfile Support Qualifier | Condition: It shall be present when the slice profile for RAN domain is needed. |
| tOPSliceSubnetProfileSupport Qualifier | Condition: It shall be present when the slice profile is for top/root network slice subnet |

Editors Note 1: Need for specific slice profile for TN domain is FFS.

Editor's NOTE 2: Analysis on clashes/inconsistencies between perfReq attribute from SliceProfile (cf. Section 6.3.4.2) and attributes from domain-specific SliceProfiles is FFS.

Editor's NOTE 3: The common attributes of the three types of SliceProfile may be extracted out and put into the common part of the SliceProfile

Editor's NOTE 4: Whether SliceProfile is dataType or IOC is FFS.

Editor's NOTE 5: Whether RANSliceSubnetProfile is inherited from or contained by SliceProfile is FFS.

Editor's NOTE 6: Whether CNSliceSubnetProfile is inherited from or contained by SliceProfile is FFS.

Editor's NOTE 7: Whether tOPSliceSubnetProfile is inherited from or contained by SliceProfile is FFS.

Editor's NOTE 8: All the attributes of SliceProfile, CNSliceSubnetProfile, RANSliceSubnetProfile and topSliceSubnetProfile will be revisited later

|  |
| --- |
| **Next modified section** |

### 6.3.a DLThptSliceSubnet<<dataType>>

#### 6.3.a.1 Definition

This data type represents the downlink throughput per slice subnet or per UE.

#### 6.3.a.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| guaThpt | M | T | F | F | T |
| maxThpt | C | T | F | F | T |

#### 6.3.a.3 Attribute constraints

None.

#### 6.3.a.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Next modified section** |

### 6.3.b ULThptSliceSubnet<<dataType>>

#### 6.3.b.1 Definition

This data type represents the uplink throughput per slice subnet or per UE.

#### 6.3.b.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| guaThpt | M | T | F | F | T |
| maxThpt | C | T | F | F | T |

#### 6.3.b.3 Attribute constraints

None.

#### 6.3.b.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Next modified section** |

### 6.3.c CNSliceSubnetProfile<<dataType>>

#### 6.3.c.1 Definition

This data type represents the requirements for CN slice profile.

Editor's NOTE: Whether CNSliceSubnetProfile is an IOC or dataType is FFS.

#### 6.3.c.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| maxNumberofUEs | O | T | T | F | T |
| latency | O | T | T | F | T |
| dLThptPerSliceSubnet | O | T | T | F | T |
| dLThptPerUEPerSubnet | O | T | T | F | T |
| uLThptPerSliceSubnet | O | T | T | F | T |
| uLThptPerUEPerSubnet | O | T | T | F | T |
| maxNumberOfPDUSessions | O | T | T | F | T |
| coverageAreaTAList | O | T | T | F | T |
| resourceSharingLevel | O | T | T | F | T |

#### 6.3.c.3 Attribute constraints

None.

#### 6.3.c.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Next modified section** |

### 6.3.d RANSliceSubnetProfile<<dataType>>

#### 6.3.d.1 Definition

This data type represents the requirements for RAN slice profile.

Editor's NOTE 1: Whether the attributes of RANSliceSubnetProfile need to be modelled by one IOC or more than one IOC is FFS.

Editor's NOTE 2: Whether RANSliceSubnetProfile is an IOC or dataType is FFS.

#### 6.3.d.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| coverageAreaGeoPolygon | O | T | T | F | T |
| coverageAreaTAList | O | T | T | F | T |
| uEMobilityLevel | O | T | T | F | T |
| resourceSharingLevel | O | T | T | F | T |
| maxNumberofUEs | O | T | T | F | T |
| activityFactor | O | T | T | F | T |
| dLThptPerUEPerSubnet | O | T | T | F | T |
| uLThptPerUEPerSubnet | O | T | T | F | T |
| uESpeed | O | T | T | F | T |
| reliability | O | T | T | F | T |
| serviceType | O | T | T | F | T |
| latency | O | T | T | F | T |

#### 6.3.d.3 Attribute constraints

None.

#### 6.3.d.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Next modified section** |

### 6.3.e TopSliceSubnetProfile<<dataType>>

#### 6.3.e.1 Definition

This data type represents the requirements for the top slice associated with the network slice.

Editor's NOTE: Whether TopSliceSubnetProfile is an IOC or dataType is FFS.

#### 6.3.e.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| coverageArea | O | T | T | F | T |
| latency | O | T | T | F | T |
| maxNumberofUEs | O | T | T | F | T |
| dLThptPerSliceSubnet | O | T | T | F | T |
| dLThptPerUEPerSubnet | O | T | T | F | T |
| uLThptPerSliceSubnet | O | T | T | F | T |
| uLThptPerUEPerSubnet | O | T | T | F | T |
| maxPktSizePerSubnet | O | T | T | F | T |
| maxNumberOfPDUSessions | O | T | T | F | T |

#### 6.3.e.3 Attribute constraints

None.

#### 6.3.e.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Next modified section** |

### 6.3.f Positioning <<dataType>>

#### 6.3.f.1 Definition

This data type represents positioning support (see clause 3.4.20 of GSMA NG.116 [50]).

#### 6.3.f.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| availability | O | T | F | F | T |
| predictionfrequency | O | T | T | F | T |
| accuracy | O | T | T | F | T |

#### 6.3.f.3 Attribute constraints

None.

#### 6.3.f.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Next modified section** |

### 6.3.g Synchronicity <<dataType>>

#### 6.3.g.1 Definition

This data type represents synchronicity support (see clause 3.4.29 of GSMA NG.116 [50]).

#### 6.3.g.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| servAttrCom | M | T | F | F | T |
| availability | O | T | F | F | T |
| accuracy | O | T | T | F | T |

#### 6.3.g.3 Attribute constraints

None.

#### 6.3.g.4 Notifications

The subclause 6.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Next modified section** |

## 6.4 Attribute definition

### 6.4.1 Attribute properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| availability | This parameter specifies the communication service availability requirement, expressed as a percentage. The communication service availability is defined in clause 3.1 of TS 22.261 [28]. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: True |
| serviceProfileId | A unique identifier of property of network slice related requirement should be supported by the network slice instance. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| sliceProfileId | A unique identifier of the property of network slice subnet related requirement should be supported by the network slice subnet instance. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| operationalState | It indicates the operational state of the network slice instance or the network slice subnet instance. It describes whether or not the resource is physically installed and working.allowedValues: "ENABLED", "DISABLED".The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUM multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| administrativeState | It indicates the administrative state of the network slice instance or the network slice subnet instance. It describes the permission to use or prohibition against using the instance, imposed through the OAM services.allowedValues: “LOCKED”, “UNLOCKED”, SHUTTINGDOWN” The meaning of these values is as defined in 3GPP TS 28.625 [17] and ITU-T X.731 [18]. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| nsInfo | This attribute contains the NsInfo of the NS instance corresponding to the network slice subnet instance. The NsInfo is described in clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: NsInfomultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| nSInstanceId | This attribute specifies the identifier of NS instance corresponding to the network slice subnet instance.See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| nsName | This attribute specifies the name of NS instance corresponding to the network slice subnet instance.See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| description | This attribute specifies the description of NS instance corresponding to the network slice subnet instance.See clause 8.3.3.2.2 of ETSI GS NFV-IFA 013 [29]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No default valueisNullable: True |
| category | This attribute specifies the category of a service requirement/attribute of GST (see GSMA NG.116 [50]).allowedValues: character, scalability | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| tagging | This attribute specifies the tagging of a service requirement/attribute of GST in character catogary (see GSMA NG.116 [50]).allowedValues: performance, function, operation | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| exposure | This attribute specifies exposure mode of a service requirement/attribute of GST (see GSMA NG.116 [50]).allowedValues: API, KPI | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/A isNullable: False |
| sNSSAIList | This parameter specifies the S-NSSAI list to be supported by the new NSI to be created or the existing NSI to be re-used.sNSSAList is defined in subclause 4.4.1 |  |
| perfReq | This parameter specifies the requirements to the network slice subnet in terms of the scenarios defined in the TS 22.261 [28] and TS 22.104 [51], i.e. the "performance requirements for high data rate and traffic density scenarios" in TS 22.261 [28], "periodic deterministic communication, aperiodic deterministic communication, non-deterministic communication, and mixed traffic" in TS 22.104 [51].It is a structure containing the following elements:- list of perfReqDepending on the sST value, the list of perfReq will be- list of eMBBPerfReqor- list of uRLLCPerfReqor- list of mIoTPerfReqNOTE 1: the list of mIoTPerfReq is not addressed in the present document.allowedValues:- list of eMBBPerfReq is a list of entries where an entry identifies the performance requirements to the network slice subnet in terms of the scenarios defined in the Table 7.1-1 of TS 22.261 [28]. An entry has the following attributes: expDataRateDL (Integer), expDataRateUL (Integer), areaTrafficCapDL (Integer), areaTrafficCapUL (Integer), overallUserDensity (Integer), activityFactor (Integer), (see table 7.1-1 of TS 22.261 [28]).- list of uRLLCPerfReq is a list of entries where an entry identifies the performance requirements to the network slice subnet in terms of the scenarios defined in clauses 5.2 through 5.5 of TS 22.104 [51]. An entry has the following attributes: cSAvailabilityTarget (Float), cSReliabilityMeanTime (String), , expDataRate (Integer), msgSizeByte (String), transferIntervalTarget (String), survivalTime (String), , , (see table 5.2-1, table 5.3-1, table 5.4-1 and table 5.5-1 of TS 22.104 [51]).NOTE 2: Limitation on attribute values in instances of SliceProfile is not addressed in the present document.NOTE 3: The attributes inside perfReq here need further breaking down to define requirements for each subnetwork under different SST values. | type: PerfReqmultiplicity: \*1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxNumberofUEs | An attribute specifies the maximum number of UEs may simultaneously access the network slice or network slice subnet instance. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| coverageAreaTAList | An attribute specifies a list of TrackingAreas where the NSI can be selected.allowedValues:Legacy TAC and Extended TAC are defined in clause 9.3.3.10 of TS 38.413 [5]. | type: Integermultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| latency | An attribute specifies the packet transmission latency (millisecond) through the RAN, CN, and TN part of 5G network and is used to evaluate utilization performance of the end-to-end network slice instance. See clause 6.3.1 of 28.554 [27]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| topSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through all domains of the network slice and is used to evaluate utilization performance of the end-to-end network slice. See clause 6.3.1 of 28.554 [27]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| CNSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through CN domain of the network slice and is used to evaluate the delay in CN domain, e.g. time between received UL/DL packet on N3/N6 interface of UPF and successfully sent out the packet on N6/N3 interface.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| RANSliceSubnetProfile.latency | An attribute specifies the packet transmission latency (millisecond) through RAN domain of the network slice and is used to evaluate the delay in RAN domain, e.g. time between received UL/DL packet on air interface/NgU of gNB and successfully sent out the packet on NgU/air interface of the gNB.  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
|  |  |  |
| uEMobilityLevel | An attribute specifies the mobility level of UE accessing the network slice instance. See 6.2.1 of TS 22.261 [28].allowedValues: stationary, nomadic, restricted mobility, fully mobility.两点 | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: True |
| serviceProfile.resourceSharingLevel | An attribute specifies whether the resources to be allocated to the network slice instance may be shared with another network slice instance(s).allowedValues: shared, non-shared. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: YesisNullable: True |
| sliceProfile.resourceSharingLevel | An attribute specifies whether the resources to be allocated to the network slice subnet instance may be shared with another network slice subnet instance(s).allowedValues: shared, non-shared. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: YesisNullable: True |
| serviceProfileList | An attribute specifies a list of ServiceProfile (see clause 6.3.3) supported by the network slice instance | type: ServiceProfilemultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sliceProfileList | An attribute specifies a list of SliceProfile (see clause 6.3.4) supported by the network slice subnet instance | type: SliceProfilemultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| sST | This parameter specifies the slice/service type for a ServiceProfile.See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| delayTolerance | An attribute specifies the properties of service delivery flexibility, especially for the vertical services that are not chasing a high system performance. See clause 4.3 of TS 22.104 [51]. | type: DelayTolerancemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| DelayTolerance.support | An attribute specifies whether or not the NSI supports service delivery flexibility, especially for the vertical services that are not chasing a high system performance.allowedValues:"NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| deterministicComm | An attribute specifies the properties of the deterministic communication for periodic user traffic, see clause 4.3 of TS 22.104 [51]. | type: <<DeterminComm>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| DeterminComm.availability | An attribute specifies whether or not the NSI supports deterministic communication for period user traffic.allowedValues:"NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| DeterminComm.periodicityList | An attribute specifies a list of periodicities supported by the NSI for deterministic communication. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| dLThptPerSlice | This attribute defines achievable data rate of the network slice in downlink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50]. | type: DLThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| dLThptPerSliceSubnet | This attribute defines achievable data rate of the network slice subnet in downlink that is available ubiquitously across the coverage area of the slice. | type: DLThptSliceSubnetmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| dLThptPerUEPerSubnet | This attribute defines data rate supported by the network slice subnet per UE.  | type: DLThptSliceSubnetmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| dLThptPerUE | This attribute defines data rate supported by the network slice per UE, refer NG.116 [50].  | type: DLThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| guaThpt | This attribute describes the guaranteed data rate. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| maxThpt | This attribute describes the maximum data rate. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| uLThptPerSlice | This attribute defines achievable data rate of the network slice in uplink that is available ubiquitously across the coverage area of the slice, refer NG.116 [50].  | type: ULThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| uLThptPerUE | This attribute defines data rate supported by the network slice per UE, refer NG.116 [50].  | type: ULThptmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| uLThptPerSliceSubnet | This attribute defines achievable data rate of the network slice subnet in uplink that is available ubiquitously across the coverage area of the slice. | type: ULThptSliceSubnetmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| uLThptPerUEPerSubnet | This attribute defines data rate supported by the network slice subnet per UE.  | type: ULThptSliceSubnetmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxPktSize | This parameter specifies the maximum packet size supported by the network slice, refer NG.116 [50].  | type: MaxPktSizemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| MaxPktSize.maxsize | This parameter specifies the maximum packet size supported by the network slice, refer NG.116 [50].  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxPktSizePerSubnet | This parameter specifies the maximum packet size supported by the network slice subnet. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxNumberofPDUSessions | This parameter defines the maximum number of concurrent PDU sessions supported by the network slice, refer NG.116 [50].  | type: MaxNumberofPDUSessionsmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| MaxNumberofPDUSessions.nOofPDUSessions | This parameter defines the maximum number of concurrent PDU sessions supported by the network slice, refer NG.116 [50].  | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| kPIMonitoring | An attribute specifies the name list of KQIs and KPIs available for performance monitoring. | type: KPIMonitoringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| KPIMonitoring. kPIList | An attribute specifies the name list of KQIs and KPIs available for performance monitoring. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| nBIoT | An attribute specifies whether NB-IoT is supported in the RAN in the network slice, see NG.116 [50]. | type: NBIoTmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| NBIoT.support | An attribute specifies whether NB-IoT is supported in the RAN in the network slice, see NG.116 [50].allowedValues:"NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| synchronicity | An attribute specifies whether synchronicity of communication devices is supported, Two cases are most important in this context, see clause 3.4.29 of NG.116 [50]:- Synchronicity between a base station and a mobile device and- Synchronicity between mobile devices. | type: Synchronicitymultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| Synchronicity.availability | An attribute specifies whether synchronicity of communication devices is supported, see NG.116 [50].allowedValues:"NOT SUPPORTED", "BETWEEN BS AND UE", "BETWEEN BS AND UE & UE AND UE". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| Synchronicity.accuracy | An attribute specifies the accuracy of the synchronicity, see NG.116 [50]. | type: Realmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| userMgmtOpen | An attribute specifies whether or not the NSI supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements. | type: UserMgmtOpenmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| UserMgmtOpen.support | An attribute specifies whether or not the NSI supports the capability for the NSC to manage their users or groups of users’ network services and corresponding requirements.allowedValues:"NOT SUPPORTED", "SUPPORTED". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| v2XCommModels | An attribute specifies whether or not the V2X communication mode is supported by the NSI. | type: V2XCommModemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| V2XCommMode.v2XMode | An attribute specifies whether or not the V2X communication mode is supported by the NSI.allowedValues:"NOT SUPPORTED", "SUPPORTED BY NR". | type: <<enumeration>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| coverageArea | An attribute specifies the coverage area of the network slice, i.e. the geographic region where a 3GPP communication service is accessible, see Table 7.1-1 of TS 22.261 [28]) and NG.116 [50]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| termDensity | An attribute specifies the overall user density over the coverage area of the network slice. See Table 7.1-1 of TS 22.261 [28]). | type: TermDensitymultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| TermDensity.density | An attribute specifies the overall user density over the coverage area of the network slice. See Table 7.1-1 of TS 22.261 [28]). | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| positioning | An attribute specifies whether the network slice provides geo-localization methods or supporting methods, see clause 3.4.20 of NG.116 [50]. | type: Positioningmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| Positioning.availability | An attribute specifies if this attribute is provided by the network slice and contains a list of positioning methods provided by the slice. If the list is empty this attribute is not available in the network slice and the other parameters might be ignored, see NG.116 [50]. Comma separated multiple values are allowed:CIDE-CID (LTE and NR), OTDOA (LTE and NR), RF fingerprinting, AECID, Hybrid positioning, NET-RTK. | type: ENUMmultiplicity: 1..6isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| Positioning.predictionfrequency | An attribute specifies how often location information is provided. This parameter simply defines how often the customer is allowed to request location information. This is not related to the time it takes to determine the location, which is a characteristic of the positioning method, see NG.116 [50].allowedValues:"PERSEC", "PERMIN", "PERHOUR". | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| Positioning.accuracy | An attribute specifies the accuracy of the location information. Accuracy depends on the respective positioning solution applied in the network slice, see NG.116 [50]. | type: Realmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: False |
| activityFactor | An attribute specfies the percentage value of the amount of simultaneous active UEs to the total number of UEs where active means the UEs are exchanging data with the network. See Table 7.1-1 of TS 22.261 [28]). | type: Floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| uESpeed | An attribute specifies the maximum speed (in km/hour) supported by the network slice or network slice subnet at which a defined QoS can be achieved. See Table 7.1-1 of TS 22.261 [28]). | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| jitter | An attribute specifies the deviation from the desired value to the actual value when assessing time parameters, see clause C.4.1 of TS 22.104 [51]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| survivalTime | An attribute specifies the time that an application consuming a communication service may continue without an anticipated message. See clause 5 of TS 22.104 [51]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| reliability | An attribute specifies in the context of network layer packet transmissions, percentage value of the amount of sent network layer packets successfully delivered to a given system entity within the time constraint required by the targeted service, divided by the total number of sent network layer packets, see TS 22.261 [28] and TS 22.104 [51]. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| NetworkSlice.networkSliceSubnetRef | This holds a DN of NetworkSliceSubnet relating to the NetworkSlice instance. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| NetworkSliceSubnet.networkSliceSubnetRef | This holds a list of DN of constituent NetworkSliceSubnet supporting NetworkSliceSubnet instance  | type: DNmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| managedFunctionRef | This holds a list of DN of ManagedFunction instances supporting the NetworkSliceSubnet instance. | type: DNmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| ipAddress | This parameter specifies the IP address assigned to a logical transport interface/endpoint. It can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| logicInterfaceId | This parameter specifies the identify of a logical transport interface. It could be VLAN ID, MPLS Tag or Segment ID. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| nextHopInfoList | This parameter is used to identify ingress transport node. Each node can be identified by any of combination of IP address of next-hop router of transport network, system name, port name, IP management address of transport nodes. | type: Stringmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| qosProfileRefList | This parameter specifies reference to QoS Profile for a logical transport interface. A QoS profile includes a set of parameters which are locally provisioned on both sides of a logical transport interface. | type: Stringmultiplicity: \*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: True |
| maxDLDataVolume | An attribute specifies the maximum DL PDCP data volume supported by the network slice instance (performance measurement definition see in TS 28.552[69]). The unit is MByte/day. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| maxULDataVolume | An attribute specifies the maximum UL PDCP data volume supported by the network slice instance (performance measurement definition see in TS 28.552[69]). The unit is MByte/day. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| coverageAreaGeoPolygon | An attribute specifies a geographic coverage area described in the form a polygon where the NSI can be selected. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FalseisNullable: True |
| serviceType | An attribute specifies the standardized network slice type.allowedValues: eMBB, URLLC, MIoT, V2X. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: True |
| epApplicationRef | This parameter specifies a list of application level EPs associated with the logical transport interface.See note 2. | type: DNmultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| epTransportRef | This parameter specifies a list of transport level EPs associated with the application level EP | type: DNmultiplicity: \*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: True |
| NOTE 1: There is no direct relationship between localAddress/remoteAddress in EP\_RP and ipAddress in EP\_transport. While the localAddress/remoteAddress in EP\_RP could be exchanged as part of signalling between GTP-u tunnel end points, ipAddress in EP\_transport is used for transport routing. NOTE 2: Application level EP represents EP\_RP defined in TS 28.622 (see [30]). e.g. including EP\_NgC, EP\_N3, etc... |

|  |
| --- |
| **Next modified section** |

## J.4.3 OpenAPI document "sliceNrm.yaml"

openapi: 3.0.1

info:

 title: Slice NRM

 version: 16.5.0

 description: >-

 OAS 3.0.1 specification of the Slice NRM

 @ 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.541 V16.4.0; 5G NRM, Slice NRM

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

 schemas:

#------------ Type definitions ---------------------------------------------------

 Float:

 type: number

 format: float

 MobilityLevel:

 type: string

 enum:

 - STATIONARY

 - NOMADIC

 - RESTRICTED MOBILITY

 - FULLY MOBILITY

 SynAvailability:

 type: string

 enum:

 - NOT SUPPORTED

 - BETWEEN BS AND UE

 - BETWEEN BS AND UE & UE AND UE

 PositioningAvailability:

 type: array

 items:

 type: string

 enum:

 - CIDE-CID

 - OTDOA

 - RF FINGERPRINTING

 - AECID

 - HYBRID POSITIONING

 - NET-RTK

 Predictionfrequency:

 type: string

 enum:

 - PERSEC

 - PERMIN

 - PERHOUR

 SharingLevel:

 type: string

 enum:

 - SHARED

 - NON-SHARED

 ServiceType:

 type: string

 enum:

 - eMBB

 - RLLC

 - MIoT

 - V2X

PerfReqEmbb:

 type: object

 properties:

 expDataRateDL:

 type: number

 expDataRateUL:

 type: number

 areaTrafficCapDL:

 type: number

 areaTrafficCapUL:

 type: number

 userDensity:

 type: number

 activityFactor:

 type: number

 PerfReqEmbbList:

 type: array

 items:

 $ref: '#/components/schemas/PerfReqEmbb'

 PerfReqUrllc:

 type: object

 properties:

 cSAvailabilityTarget:

 type: number

 cSReliabilityMeanTime:

 type: string

 expDataRate:

 type: number

 msgSizeByte:

 type: string

 transferIntervalTarget:

 type: string

 survivalTime:

 type: string

 PerfReqUrllcList:

 type: array

 items:

 $ref: '#/components/schemas/PerfReqUrllc'

 PerfReq:

 oneOf:

 - $ref: '#/components/schemas/PerfReqEmbbList'

 - $ref: '#/components/schemas/PerfReqUrllcList'

 Category:

 type: string

 enum:

 - CHARACTER

 - SCALABILITY

 Tagging:

 type: string

 enum:

 - PERFORMANCE

 - FUNCTION

 - OPERATION

 Exposure:

 type: string

 enum:

 - API

 - KPI

 ServAttrCom:

 type: object

 properties:

 category:

 $ref: '#/components/schemas/Category'

 tagging:

 $ref: '#/components/schemas/Tagging'

 exposure:

 $ref: '#/components/schemas/Exposure'

 Support:

 type: string

 enum:

 - NOT SUPPORTED

 - SUPPORTED

 DelayTolerance:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 support:

 $ref: '#/components/schemas/Support'

 DeterministicComm:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 availability:

 $ref: '#/components/schemas/Support'

 periodicityList:

 type: string

 DLThptPerSlice:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 DLThptPerUE:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 ULThptPerSlice:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 ULThptPerUE:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 DLThptPerSliceSubnet:

 type: object

 properties:

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 DLThptPerUEPerSubnet:

 type: object

 properties:

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 ULThptPerSliceSubnet:

 type: object

 properties:

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 ULThptPerUEPerSubnet:

 type: object

 properties:

 guaThpt:

 $ref: '#/components/schemas/Float'

 maxThpt:

 $ref: '#/components/schemas/Float'

 MaxPktSize:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 maxsize:

 type: integer

 MaxNumberofPDUSessions:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 nOofPDUSessions:

 type: integer

 KPIMonitoring:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 kPIList:

 type: string

 NBIoT:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 support:

 $ref: '#/components/schemas/Support'

 Synchronicity:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 availability:

 $ref: '#/components/schemas/SynAvailability'

 accuracy:

 $ref: '#/components/schemas/Float'

 Positioning:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 availability:

 $ref: '#/components/schemas/PositioningAvailability'

 predictionfrequency:

 $ref: '#/components/schemas/Predictionfrequency'

 accuracy:

 $ref: '#/components/schemas/Float'

 UserMgmtOpen:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 support:

 $ref: '#/components/schemas/Support'

 V2XCommModels:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 v2XMode:

 $ref: '#/components/schemas/Support'

 TermDensity:

 type: object

 properties:

 servAttrCom:

 $ref: '#/components/schemas/ServAttrCom'

 density:

 type: integer

 NsInfo:

 type: object

 properties:

 nsInstanceId:

 type: string

 nsName:

 type: string

 CNSliceSubnetProfile:

 type: object

 properties:

 maxNumberofUEs:

 type: integer

 latency:

 type: integer

 dLThptPerSlice:

 $ref: '#/components/schemas/DLThptPerSliceSubnet'

 dLThptPerUEPerSubnet:

 $ref: '#/components/schemas/DLThptPerUEPerSubnet'

 uLThptPerSliceSubnet:

 $ref: '#/components/schemas/ULThptPerSliceSubnet'

 uLThptPerUEPerSubnet:

 $ref: '#/components/schemas/ULThptPerUEPerSubnet'

 maxNumberOfPDUSessions:

 type: integer

 RANSliceSubnetProfile:

 type: object

 properties:

 coverageAreaGeoPolygon:

 type: string

 coverageAreaTAList:

 type: integer

 MobilityLevel:

 $ref: '#/components/schemas/MobilityLevel'

 resourceSharingLevel:

 $ref: '#/components/schemas/SharingLevel'

 maxNumberofUEs:

 type: integer

 activityFactor:

 type: integer

 dLThptPerUE:

 $ref: '#/components/schemas/ULThptPerUEPerSubnet'

 uLThptPerUE:

 $ref: '#/components/schemas/ULThptPerUEPerSubnet'

 uESpeed:

 type: integer

 reliability:

 type: string

 serviceType:

 $ref: '#/components/schemas/ServiceType'

 TopSliceSubnetProfile:

 type: object

 properties:

 coverageArea:

 type: string

 latency:

 type: integer

 maxNumberofUEs:

 type: integer

 dLThptPerSlice:

 $ref: '#/components/schemas/DLThptPerSliceSubnet'

 dLThptPerUE:

 $ref: '#/components/schemas/DLThptPerUEPerSubnet'

 uLThptPerSlice:

 $ref: '#/components/schemas/ULThptPerSliceSubnet'

 uLThptPerUE:

 $ref: '#/components/schemas/ULThptPerUEPerSubnet'

 maxPktSize:

 type: integer

 maxNumberOfPDUSessions:

 type: integer

 ServiceProfileList:

 type: object

 additionalProperties:

 type: object

 properties:

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 maxNumberofUEs:

 type: number

 latency:

 type: number

 uEMobilityLevel:

 $ref: '#/components/schemas/MobilityLevel'

 sst:

 $ref: 'nrNrm.yaml#/components/schemas/Sst'

 resourceSharingLevel:

 $ref: '#/components/schemas/SharingLevel'

 availability:

 type: number

 delayTolerance:

 $ref: '#/components/schemas/DelayTolerance'

 deterministicComm:

 $ref: '#/components/schemas/DeterministicComm'

 dLThptPerSlice:

 $ref: '#/components/schemas/DLThptPerSlice'

 dLThptPerUE:

 $ref: '#/components/schemas/DLThptPerUE'

 uLThptPerSlice:

 $ref: '#/components/schemas/ULThptPerSlice'

 uLThptPerUE:

 $ref: '#/components/schemas/ULThptPerUE'

 maxPktSize:

 $ref: '#/components/schemas/MaxPktSize'

 maxNumberofPDUSessions:

 $ref: '#/components/schemas/MaxNumberofPDUSessions'

 kPIMonitoring:

 $ref: '#/components/schemas/KPIMonitoring'

 nBIoT:

 $ref: '#/components/schemas/NBIoT'

 synchronicity:

 $ref: '#/components/schemas/Synchronicity'

 positioning:

 $ref: '#/components/schemas/Positioning'

 userMgmtOpen:

 $ref: '#/components/schemas/UserMgmtOpen'

 v2XModels:

 $ref: '#/components/schemas/V2XCommModels'

 coverageArea:

 type: string

 termDensity:

 $ref: '#/components/schemas/TermDensity'

 activityFactor:

 $ref: '#/components/schemas/Float'

 uESpeed:

 type: integer

 jitter:

 type: integer

 survivalTime:

 type: string

 reliability:

 type: string

 maxDLDataVolume:

 type: string

 maxULDataVolume:

 type: string

 SliceProfileList:

 type: object

 additionalProperties:

 type: object

 properties:

 snssaiList:

 $ref: 'nrNrm.yaml#/components/schemas/SnssaiList'

 plmnIdList:

 $ref: 'nrNrm.yaml#/components/schemas/PlmnIdList'

 perfReq:

 $ref: '#/components/schemas/PerfReq'

 CNSliceSubnetProfile:

 $ref: '#/components/schemas/CNSliceSubnetProfile'

 RANSliceSubnetProfile:

 $ref: '#/components/schemas/RANSliceSubnetProfile'

 TopSliceSubnetProfile:

 $ref: '#/components/schemas/TopSliceSubnetProfile'

 IpAddress:

 oneOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

 - $ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

#------------ Definition of concrete IOCs ----------------------------------------

 NetworkSlice:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

 - type: object

 properties:

 networkSliceSubnetRef:

 $ref: 'genericNrm.yaml#/components/schemas/Dn'

 operationalState:

 $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

 administrativeState:

 $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

 serviceProfileList:

 $ref: '#/components/schemas/ServiceProfileList'

 NetworkSliceSubnet:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

 - type: object

 properties:

 managedFunctionRefList:

 $ref: 'genericNrm.yaml#/components/schemas/DnList'

 networkSliceSubnetRefList:

 $ref: 'genericNrm.yaml#/components/schemas/DnList'

 operationalState:

 $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

 administrativeState:

 $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

 nsInfo:

 $ref: '#/components/schemas/NsInfo'

 sliceProfileList:

 $ref: '#/components/schemas/SliceProfileList'

 EPTransport:

 $ref: '#/components/schemas/EP\_Transport-Multiple'

 EP\_Transport-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 ipAddress:

 $ref: '#/components/schemas/IpAddress'

 logicInterfaceId:

 type: string

 nextHopInfo:

 type: string

 qosProfile:

 type: string

 epApplicationRefs:

 $ref: 'genericNrm.yaml#/components/schemas/DnList'

 EP\_Transport-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/EP\_Transport-Single'

#------------ Definitions in TS 28.541 for TS 28.532 -----------------------------

 resources-sliceNrm:

 oneOf:

 - $ref: '#/components/schemas/NetworkSlice'

 - $ref: '#/components/schemas/NetworkSliceSubnet'

 - $ref: '#/components/schemas/EP\_Transport-Single'

|  |
| --- |
| **Next modified section** |

Annex L (normative):
Relation of GSMA GST, ServiceProfile and SliceProfile

# L.1 General

This annex describes the relation between GSMA GST [50] and information model ServiceProfile and SliceProfile.

# L.2 GSMA GST, ServiceProfile and SliceProfile

The GSMA GST is used as the SLA information for the communication between the vertical industry and the communication service provider. The SLA requirements can be fulfilled from management aspect and control aspect in a coordinated way. The SLS includes ServiceProfile information model.

As shown in figure L.2.1, the GST [50] is translated and used as input to NRM ServiceProfile, the ServiceProfile can be translated to corresponding requirements for dedicated domains. For example, 5GC SliceProfile is used to carry 5GC domain requirements, NG-RAN SliceProfile is used to carry NG-RAN domain requirements, and TN requirements are translated and provided to TN domain.

Some of the information (e.g maximum number of connection per slice, downlink throughput per slice) in 5GC SliceProfile and NG-RAN SliceProfile is translated to configurable parameters related to network function behaviour for the control plane SLA support purpose. While other information (e.g delay tolerance, determistic communication support) in 5GC SliceProfile and NG-RAN SliceProfile are kept at OAM domain and is used to determine the overall behaviour of the network slice.

Editors note: The list of configuration parameters is FFS and should be decided as per the requirements from SA2 and RAN WGs.



Figure L.2.1 Relation between GSMA GST, ServiceProfile and SliceProfile

|  |
| --- |
| **End of modified section** |