**3GPP TSG- Meeting #**

**, –**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **0295** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | TEI16 |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In clause 5.2.1.8 TS 32.255, 6 cases are defined related to termination action. The termination action can be provided by CHF. However, CHF can only provide FUA for “The final granted units have been used” case. For the other 5 cases, there’s no attribute for CHF to provide a termination action in ChargingDataReponse message. Also, the description of “The SMF Default Termination Action” is duplicated. In the next paragraph, we have similar definition that SMF shall pre-configure the default termination action. |
|  |  |
| ***Summary of change:*** | Limit the usage of CHF provided termination action to FUI scenario. Delete the duplicated description of “The SMF Default Termination Action”. |
|  |  |
| ***Consequences if not approved:*** | Charging implementation might be incorrect. |
|  |  |
| ***Clauses affected:*** | 5.2.1.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

#### 5.2.1.8 Termination action

The termination action applies only in case of online charging, i.e. quota management is active. It indicates the action, which the UPF should perform when no quota is granted. A packet for a specific rating group is subject to a termination action in the following cases:

- Zero units have been granted;

- The final granted units have been used;

- Quota limit reached;

- End user service rejected;

- End user service denied;

- Rating failed.

The defined termination actions include:

- Allowing the packets to pass through;

- Dropping the packets;

- The re-direction of packets to an application server (e.g. defined in the termination action).

NOTE Such a re-direction may trigger a new charging session to be initiated.

A Default Termination Action for all rating groups, for which no quota is granted and there is no specific termination action, shall be pre-configured in the SMF according to operator's policy. For instance, the default behaviour may consist of allowing packets of any terminated service to pass through the UPF.

When final units are granted, the CHF shall provide a termination action using finalUnitAction for each rating group. The SMF previously provided termination action shall be overwritten by the CHF.

|  |
| --- |
| **End of change** |