3GPP TSG SA WG5 Meeting 136-e S5-212294rev1

electronic meeting, online, 1 - 9 March 2021

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **TS28.535** | **CR** | 0034 | **rev** |  | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | **Add use case for goal translation** |
|  |  |
| ***Source to WG:*** | Lenovo, Motorola mobility |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** | 2021-02-22 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Adding a basic use case for translating goals within the 3GPP management system.  |
|  |  |
| ***Summary of change:*** | New use case |
|  |  |
| ***Consequences if not approved:*** | Basic functionality that may be required for the correct configuration of a ACCL goal may be ignored. |
|  |  |
| ***Clauses affected:*** | 6.1.X (new), 6.2  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**Start of Change 1**

### 6.1.x Translation of ACCL goal within a 3GPP management system

When the consumer of an assurance closed loop configures an assurance goal on to a managed entity (example: communication service or a network slice) in the 3GPP management, the goal may need to be translated or decomposed to tranlated goals or conditions (example: threshold notfications) over KPIs that are to be observed over *other* managed entities (example: NFs that form the Network slice) or the translated goals may be configured in other technology domains (example: transport, core or RAN management domain).

The 3GPP management system shall therefore have the ability to translate goals to other “composing goals” or conditions across technology domains that are a part of, or directly interact with, the 3GPP system. After translation, the 3GPP management system may then request configuration of the translated goals or conditions in the respective management service producers.

The MnS consumer provides the original ACCL goal to be configured on a particular managed entity. The 3GPP management system then translates this goal to translated goals or conditions on other related managed entities. When all translated goals or conditions are configured, the 3GPP management system notifies the MnS consumer of successful configuration.

**Start of Change 2**

## 6.2 Requirements

**REQ-CSA-CON-01** The 3GPP management system shall have the capability to take actions for a set of communication services serving certain group of UEs based on the target SLS.

**REQ-CSA-CON-02** The 3GPP management system shall have the capability to collect service experience information.

**REQ-CSA-CON-03** The 3GPP management system shall have the capability to analyse the performance information related to the set of communication services serving certain group of UEs.

**REQ-CSA-CON-04** The 3GPP management system shall have the capability to modify the configuration parameters related to the set of communication services serving certain group of UEs.

**REQ-CSA-CON-05** The 3GPP management system shall have the capability to collect NSI related data from one or more 5GC NF(s).

NOTE 1: An example for NSI related data may be QoE data.

**REQ-CSA-CON-06** The 3GPP management system shall have the capability to derive which communication service is associated to the QoE data from the collected NSI related QoE data.

**REQ-CSA-CON-07** The 3GPP management system shall have the capability to ascertain SLS breach.

**REQ-CSA-CON-08** The 3GPP management system shall have the capability to perform the root cause analysis (e.g., identifying the underlying reason) for an SLS breach.

**REQ-CSA-CON-09** The 3GPP management system shall have the capability to take corrective actions against the root cause identified.

**REQ-CSA-CON-10** The 3GPP management system shall have the capability to translate communicate service requirements to cross domain SLS goal and single domain SLS goal.

**REQ-CSA-CON-11** The 3GPP management system shall have the capability to collect single domain SLS analysis as input to cross domain SLS analysis.

**REQ-CSA-CON-12** The 3GPP management system shall have the capability to allow its authorized consumer to control the SLS assurance (e.g. specify the SLS to be assured, enable/disable, specify the assurance time and update the SLS assurance requirements).

**REQ-CSA-CON-13** The 3GPP management system shall have the capability to allow its authorized consumer to obtain the SLS assurance progress information and fulfil information.

NOTE 2: The management system refers to the producer of management service for SLS assurance.

**REQ-CSA-CON-14** The 3GPP management system shall have the capability to do network prediction (e.g. network resource usage and network performance) by analysing the network operation information in special scenarios.

**REQ-CSA-CON-15** The 3GPP management system shall have the capability to take actions such asnetwork configuration and perform network resource reallocation according to the network prediction results.

**REQ-CSA-CON-16** The 3GPP management system shall have the capability to allow its authorized consumer to limit the set of action capabilities executable by an assurance closed loop.

**REQ-CSA-CON-17** The 3GPP management system shall allow an authorized consumer to set a condition to enable/disable an ACCL.

REG-CSA-CON-X The 3GPP management system shall have the capability to translate or decompose goals to other “composing goals” or conditions in the network.

**End of Changes**