**3GPP TSG- Meeting #**

**, , - , 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | , NEC | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 1. In clause 5.8.15.3, Uu RSRP measurement of the cell on which RRC\_IDLE/INACTIVE U2N Remote UE camps or the PCell (for RRC\_CONNECTED L3 U2N Remote UE) is used to compare with the *threshHighRemote* within a field of *SL-RemoteUE-Config* ASN.1 IE type for triggering the NR sidelink U2N Relay UE selection and reselection procedure. For RRC\_IDLE/INACTIVE U2N Remote UE, it is the *sl-RemoteUE-ConfigCommon* field (of the *SL-RemoteUE-Config-r17* ASN.1 IE type) included in *SIB12*; for RRC\_CONNECTED U2N Remote UE, it is the *sl-RemoteUE-Config* field (of the *SL-RemoteUE-Config-r17* ASN.1 IE type) included in *sl-ConfigDedicatedNR* within *RRCReconfiguration*. In the current spec, “*sl-RemoteUE-Config*” is used so it only covers the case for RRC\_CONNECTED, and does not cover the case for RRC\_IDLE/INACTIVE. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. In clause 5.8.15.3, add “*sl-RemoteUE-ConfigCommon*/” before “*sl-RemoteUE-Config*” to cover the case for RRC\_IDLE/INACTIVE.   **Impact analysis**  Impacted 5G architecture options:  NR SA  Impacted functionality:  NR sidelink U2N Relay UE selection and reselection procedure  Inter-operability:  If the network implements this CR but not the UE, there is no interoperability issue.  If the UE implements this CR but not the network, there is no interoperabiilty issue. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | 1. UE will not use the right configuration parameter for NR SL U2N Relay UE selection and reselection procedure, which would cause interoperability issue of implementation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.8.15.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | * R2-2407272: initial version; * R2-2407727: rev1, implemeting the agreement at RAN2 #127 below:   + Change to add the sl-RemoteUE-ConfigCommon instead of the IE name | | | | | | | | |

*Start of Change*

#### 5.8.15.3 Selection and reselection of NR sidelink U2N Relay UE

A UE capable of NR sidelink U2N Remote UE operation that is configured by upper layers to search for a NR sidelink U2N Relay UE shall:

1> if the UE has no serving cell; or

1> if the RSRP measurement of the cell on which the UE camps (for L2 and L3 U2N Remote UE in RRC\_IDLE or RRC\_INACTIVE)/ the PCell (for L3 U2N Remote UE in RRC\_CONNECTED) is below *threshHighRemote* within *sl-RemoteUE-ConfigCommon* / *sl-RemoteUE-Config*:

2> if the UE does not have a selected NR sidelink U2N Relay UE; or

2> if the UE has a selected NR sidelink U2N Relay UE, and SL-RSRP of the currently selected NR sidelink U2N Relay UE is available and is below *sl-RSRP-Thresh*; or

2> if the UE has a selected NR sidelink U2N Relay UE, and SL-RSRP of the currently selected NR sidelink U2N Relay UE is not available, and SD-RSRP of the currently selected U2N Relay UE is below *sl-RSRP-Thresh*; or

NOTE 1: U2N Remote UE uses SL-RSRP measurements for relay reselection trigger evaluation when there is data transmission from U2N Relay UE to U2N Remote UE, and it is left to UE implementation whether to use SL-RSRP or SD-RSRP for relay reselection trigger evaluation in case of no data transmission from U2N Relay UE to U2N Remote UE. If SD-RSRP is used, the discovery procedure will be performed between the U2N Remote UE and the selected U2N Relay UE.

2> if the UE has a selected NR sidelink U2N Relay UE, and upper layers indicate not to use the currently selected NR sidelink U2N Relay UE; or

2> if the UE has a selected NR sidelink U2N Relay UE, and upper layers request the release of the PC5-RRC connection; or

2> if the UE has a selected NR sidelink U2N Relay UE, and sidelink radio link failure is detected on the PC5-RRC connection with the current U2N Relay UE as specified in clause 5.8.9.3:

3> perform NR sidelink discovery procedure as specified in clause 5.8.13 in order to search for candidate NR sidelink U2N Relay UEs;

4> when evaluating the one or more detected NR sidelink U2N Relay UEs, apply layer 3 filtering as specified in 5.5.3.2 across measurements that concern the same U2N Relay UE ID and using the *sl-FilterCoefficientRSRP* in *SIB12* (if in RRC\_IDLE/INACTIVE), the *sl-FilterCoefficientRSRP* in *sl-ConfigDedicatedNR* (if in RRC\_CONNECTED) or the preconfigured *sl-FilterCoefficientRSRP* as defined in 9.3 (out of coverage), before using the SD-RSRP measurement results;

4> consider a candidate NR sidelink U2N Relay UE for which SD-RSRP exceeds *sl-RSRP-Thresh* by *sl-HystMin* has met the AS criteria;

3> if the UE detects any suitable NR sidelink U2N Relay UE(s):

4> consider one of the available suitable NR sidelink U2N relay UE(s) can be selected;

NOTE 2: A candidate NR sidelink U2N Relay UE which meets all AS layer criteria defined in 5.8.15.3 and higher layer criteria defined in TS 23.304 [65] can be regarded as suitable NR sidelink U2N Relay UE by the NR sidelink U2N Remote UE. If multiple suitable NR sidelink U2N Relay UEs are available, it is up to Remote UE implementation to choose one NR sidelink U2N Relay UE. The details of the interaction with upper layers are up to UE implementation.

NOTE 3: For L2 U2N Remote UEs in RRC\_IDLE/INACTIVE and L3 U2N Remote UEs, the cell (re)selection procedure and relay (re)selection procedure run independently. If both suitable cells and suitable NR sidelink U2N Relay UEs are available, it is up to NR sidelink U2N Remote UE implementation to select either a cell or a NR sidelink U2N Relay UE. Furthermore, L3 U2N Remote UE's selection on both cell and NR sidelink U2N Relay UE is also based on UE implementation.

3> else:

4> consider no NR sidelink U2N Relay UE to be selected.

*End of Change*