**3GPP TSG CT WG3 Meeting #137 *C3-245xxx***

**Hefei, CN, 14th – 18th October, 2024 was C3-245175**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **0023** | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | |
| ***Title:*** | Naming alignment for the SDD\_DataStorage\_Query service operation | | | | | | | | |
|  |  | | | | | | | | |
| ***Source to WG:*** | Huawei, Nokia | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | |
|  |  | | | | | | | | |
| ***Work item code:*** | SEALDD\_Ph2 | | | | |  | ***Date:*** | | 2024-10-07 |
|  |  | | | |  | |  | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | |
| ***Reason for change:*** | | | Clause 9.5 of TS 23.433 was updated to change the "Query" service operation name to "Fetch" in the frame of resolving a pending Editor's Note.  It is hence needed to add a table NOTE in clause 5.3.2.1 to indicate that the stage 3 "Query" service operation corresponds to the stage 2 defined "Fetch" service operation. | | | | | | |
|  | | |  | | | | | | |
| ***Summary of change:*** | | | This CR proposes to:   * Address the above-detailed stage 2 requirements. | | | | | | |
|  | | |  | | | | | | |
| ***Consequences if not approved:*** | | | * The above-detailed stage 2 requirements are not specified in stage 3. | | | | | | |
|  | |  | | | | | | | |
| ***Clauses affected:*** | | 5.3.2.1 | | | | | | | |
|  | |  | | | | | | | |
|  | | **Y** | | **N** |  | | |  | |
| ***Other specs*** | |  | | **X** | Other core specifications | | | TS/TR ... CR ... | |
| ***affected:*** | |  | | **X** | Test specifications | | | TS/TR ... CR ... | |
| ***(show related CRs)*** | |  | | **X** | O&M Specifications | | | TS/TR ... CR ... | |
|  | |  | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible corrections to the OpenAPI description of the SDD\_DDContext API defined in this specification. | | | | | | | |
|  | |  | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | |

\* \* \* \* Start of changes \* \* \* \*

#### 5.3.2.1 Introduction

The service operations defined for the SDD\_DataStorage service are shown in table 5.3.2.1-1.

Table 5.3.2.1-1: SDD\_DataStorage Service Operations

|  |  |  |
| --- | --- | --- |
| Service Operation Name | Description | Initiated by |
| SDD\_DataStorage\_Create | This service operation enables a service consumer to request the creation of a SEALDD Data Storage and receive notifications on SEALDD Data Management and/or Status Information event(s). | e.g., VAL Server, SEALDD Server |
| SDD\_DataStorage\_Manage | This service operation enables a service consumer to request the update/modification/deletion of an existing SEALDD Data Storage. | e.g., VAL Server |
| SDD\_DataStorage\_Query | This service operation enables a service consumer to request the retrieval of one or several existing SEALDD Data Storage(s). | e.g., VAL Server, SEALDD Server |
| SDD\_DataStorage\_DelRequest | This service operation enables a service consumer to request for one-time SEALDD Data Storage Delivery. | e.g., VAL Server |
| SDD\_DataStorage\_EstablishDelConn | This service operation enables a service consumer to request for one-time SEALDD Data Storage Delivery connection establishment. | e.g., SEALDD Server |
| SDD\_DataStorage\_DelSubscribe | This service operation enables a service consumer to request the creation/update/deletion of a SEALDD Data Storage Delivery Subscription. | e.g., VAL Server |
| SDD\_DataStorage\_DelNotify | This service operation enables a service consumer to receive SEALDD Data Storage Delivery Notifications. | SEALDD Server |
| NOTE: The names of the service operations in this table are not always identical to the corresponding names in 3GPP TS 23.433 [7], e.g., SDD\_DataStorage\_Query vs SDD\_DataStorage\_Fetch, SDD\_DataStorage\_DelSubscribe vs SDD\_DataStorage\_Delivery\_Subscription, etc. | | |

\* \* \* \* End of changes \* \* \* \*