**3GPP TSG RAN WG1 #118bis *R1-2409xxx***

**Hefei, China, October 14th – 18th, 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.211** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **18.4.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on antenna port description for DMRS associated with a PSBCH in TS 38.211 (mirror on Rel-18) |
|  |  |
| ***Source to WG:*** | Moderator (ZTE Corporation), Sanechips, OPPO, Huawei, HiSilicon |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_SL\_enh-Core |  | ***Date:*** | 2024-10-16 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | For DM-RS associated with PSBCH, the reference to clause 8.4.3.1 for ‘the same block index’ is cited wrongly, there is no block index in clause 8.4.3.1. |
|  |  |
| ***Summary of change:*** | The description of “according to clause 8.4.3.1” is removed.  |
|  |  |
| ***Consequences if not approved:*** | Current spec includes wrongly cited clause number. |
|  |  |
| ***Clauses affected:*** | 8.2.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Impact Analysis:The CR can be implemented by a UE of an earlier release without interoperability issue. |
|  |  |
| ***This CR's revision history:*** |  |

### 8.2.4 Antenna ports

<Unchanged parts are omitted>

For DM-RS associated with a PSBCH, the channel over which a PSBCH symbol on one antenna port is conveyed can be inferred from the channel over which a DM-RS symbol on the same antenna port is conveyed only if the two symbols are within a S-SS/PSBCH block transmitted within the same slot, and with the same block index.

For DM-RS associated with a PSSCH, the channel over which a PSSCH symbol on one antenna port is conveyed can be inferred from the channel over which a DM-RS symbol on the same antenna port is conveyed only if the two symbols are within the same frequency resource as the scheduled PSSCH and in the same slot.

For DM-RS associated with a PSCCH, the channel over which a PSCCH symbol on one antenna port is conveyed can be inferred from the channel over which a DM-RS symbol on the same antenna port is conveyed only if the two symbols are within the same frequency resource as the transmitted PSCCH and in the same slot.

<Unchanged parts are omitted>