**3GPP T****SG-RAN WG4 Meeting #113 revision of R4-2419465**

**Orlando, US, November 18 – 22, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **.106** | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to TS 38.106 with terminology alignment for Rel-17 |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_netcon\_repeater-Core |  | ***Date:*** | 2024-11-08 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | This is CR to TS 38.106 Rel-17 with terminology aligment for repeaters discussed during RAN4#112 meeting and agreed in R4-2413502. * Agreement from R4-2413502
* Following terminology should be used to align repeater Rel-17 and Rel-18 specifications:

|  |  |
| --- | --- |
| **Term**  | **Repeater type**  |
| RF repeater (Rel-17)  | RF Repeater type 1-C (RFR type 1-C) RF Repeater type 2-O (RFR type 2-O)  |
| NCR (Rel-18)  | NCR type 1-C NCR type 1-H NCR type 2-O  |
| Repeater  | **Includes all repeaters in Rel-18:** RF Repeater type 1-C (RFR type 1-C) RF Repeater type 2-O (RFR type 2-O) NCR type 1-C NCR type 1-H NCR type 2-O  |
| NR repeater  | Term to be removed and not used as a name of any type of repeater.   |

 |
|  |  |
| ***Summary of change:*** | Updates of terminology in afftect claueses listed below. |
|  |  |
| ***Consequences if not approved:*** | Specification will include terminology which is not align. |
|  |  |
| ***Clauses affected:*** | 1, 3, 4.2, 4.3, 4.4, 4.5, 6.2, 6.7.2, 6.7.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | This is revision of R4-2419465. |

<Start of changes>

1 Scope

The present document establishes the minimum RF characteristics of RF repeater.

<Next change>

3 Definitions of terms, symbols and abbreviations

3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**Antenna connector:** connector at the conducted interface of the *repeater type 1-C*

**Beam:** beam (of the antenna) is the main lobe of the radiation pattern of an *antenna array*

**Beam centre direction:** direction equal to the geometric centre of the half-power contour of the beam

**Beam direction pair:** data set consisting of the *beam centre direction* and the related *beam peak direction*

**Beam peak direction:** direction where the maximum EIRP is found

**Beamwidth:** beam which has a half-power contour that is essentially elliptical, the half-power beamwidths in the two pattern cuts that respectively contain the major and minor axis of the ellipse

**directional requirement:** requirement which is applied in a specific direction within the *OTA coverage range*.

**Equivalent isotropic radiated power:** equivalent power radiated from an isotropic directivity device producing the same field intensity at a point of observation as the field intensity radiated in the direction of the same point of observation by the discussed device

**Fractional bandwidth:** *fractional bandwidth* FBW is defined as $FBW=200∙\frac{F\_{FBWhigh}-F\_{FBWlow}}{F\_{FBWhigh}+F\_{FBWlow}}\%$

**gap between passbands:** frequency gap between two consecutive passbands that belong to the same *operating band*, where the RF requirements in the gap are based on co-existence for un-coordinated operation

**Inter-passband gap**: The frequency gap between two supported consecutive *passbands* that belong to different operating bands.

**Maximum passband output power:** mean power level measured per *passband* at the *antenna connector*, during the *transmitter ON state* in a specified reference condition

**Maximum passband TRP output power:** mean power level measured perpassband during the *transmitter ON state* in a specified reference condition and corresponding to the declared *rated passband TRP output* power (Prated,p,,TRP)

**Measurement bandwidth**: RF bandwidth in which an emission level is specified

**multi-band connector**: *Antenna Connector* for a *Multi-band repeater*.

**Multi-band repeater:** *Repeater Type 1-C* whose *antenna connector* is associated with a transmitter and/or receiver that is characterized by the ability to process two or more *passband(s)* in common active RF components simultaneously, where at least one *passband* is configured at a different operating band than the other *passband(s)* and where this different operating band is not a sub-band or superseding-band of another supported operating band

**Nominal channel bandwidth:** Bandwidth calculated as min(100MHz, BWpassband) in FR1 or min(400MHz, BWpassband) in FR2. If this bandwidth is not defined for BS channel bandwidth for the operating band, *nominal channel bandwidth* shall be defined as the widest BS channel bandwidth for the operating band which is narrower than BWpassband.

**Non-contiguous spectrum**: spectrum consisting of two or more *passbands* separated by *inter-passband gap*(s).

**Operating band:** frequency range in which NR operates (paired or unpaired), that is defined with a specific set of technical requirements

**OTA coverage range**: a common range of directions within which OTA requirements that are neither specified in the *OTA peak directions sets* nor as *TRP requirement* are intended to be met

**OTA peak directions set:** set(s) of *beam peak directions* within which certain OTA requirements are intended to be met, where all *OTA peak directions set(s)* are subsets of the *OTA coverage range*

**Passband:** The frequency range in which the repeater operates in with operational configuration, this frequency range can correspond to one or several consecutive nominal channels, if they are not consecutive each subset of channels shall be considered as an individual *passband*, a repeater can have one or several *passbands*, all channels within the *passband(s)* shall belong to a single operator or collaborating operators.

**passband edge:** Frequency at the edge of the passband

**Radiated interface boundary:** *operating band* specific radiated requirements reference where the radiated requirements apply

**Rated beam EIRP:** For a declared beam and *beam direction pair*, the *rated beam EIRP* level is the maximum power that the repeater is declared to radiate at the associated *beam peak direction* during the *transmitter ON state*

**Rated passband output power:** mean power level associated with a *passband* the manufacturer has declared to be available at the *antenna connector*, during the *transmitter ON state*in a specified reference condition

**Rated passband TRP output power:** mean power level declared by the manufacturer per passband, that the manufacturer has declared to be available at the RIB during the *transmitter ON state*

**Rated total output power:** mean power level associated with a particular *operating band* the manufacturer has declared to be available at the *antenna connector*, during the *transmitter ON state* in a specified reference condition

**Rated total TRP output power:** mean power level associated with a particular *operating band*, that the manufacturer has declared to be available at the RIB during the *transmitter ON state* in a specified reference condition

**Reference beam direction pair:** Beam direction pair in the reference direction declared by the manufacturer.

**RF repeater type 1-C (RFR type 1-C):** Repeater operating at FR1 with a requirement set consisting only of conducted requirements defined at individual *antenna connectors*.

**RF repeater type 2-O (RFR type 2-O):** Repeater operating at FR2 with a requirement set consisting only of OTA requirements defined at the RIB

**Requirement set:** one of the NR requirements set as defined for *repeater*

**single-band connector:** *Repeater type 1-C* *antenna connector* supporting operation either in a single *operating band* only, or in multiple *operating bands* but does not meet the conditions for a *multi-band connector*.

**Sub-band:** A *sub-band* of an operating band contains a part of the uplink and downlink frequency range of the operating band.

**sub-block:** one contiguous allocated block of spectrum for transmission and reception by the repeater.

**Superseding-band:** A *superseding-band* of an operating band includes the whole of the uplink and downlink frequency range of the operating band.

**Total radiated power:** is the total power radiated by the antenna

NOTE: The *total radiated power* is the power radiating in all direction for two orthogonal polarizations. *Total radiated power* is defined in both the near-field region and the far-field region

**Transmitter OFF state:** Time period during which the repeater downlink or uplink is not allowed to transmit in the corresponding direction.

**Transmitter ON state:** Time period during which the repeater is transmitting downlink or uplink signals in the corresponding direction.

**Transmitter transient period:** Time period during which the repeater is changing from the OFF state to the ON state or vice versa.

<Next change>

3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

ACLR Adjacent Channel Leakage Ratio

AoA Angle of Arrival

BW Bandwidth

CACLR Cumulative ACLR

CP-OFDM Cyclic Prefix-OFDM

DFT-s-OFDM Discrete Fourier Transform-spread-OFDM

DL Downlink

EIRP Effective Isotropic Radiated Power

EVM Error Vector Magnitude

FBW Fractional Bandwidth

FR Frequency Range

ITU‑R Radiocommunication Sector of the International Telecommunication Union

LA Local Area

MR Medium Range

NR New Radio

OBUE Operating Band Unwanted Emissions

OOB Out-of-band

OTA Over-The-Air

QAM Quadrature Amplitude Modulation

RF Radio Frequency

RFR RF repeater

RIB Radiated Interface Boundary

RX Receiver

SCS Sub-Carrier Spacing

TX Transmitter

TRP Total Radiated Power

UL Uplink

WA Wide Area

<Next change>

4.2 Conducted and radiated requirement reference points

4.2.1 *RF repeater type 1-C*

For *RF* *repeater type 1-C*, the requirements are applied at the repeater *antenna connector* (BS-side connector or UE-side connector) for downlink or uplink for the configuration in normal operating conditions.

Downlink

Uplink

UE-side connector

BS-side connector

**Figure 4.2.1-1: *RF repeater type 1-C* downlink and uplink interface**

4.2.2 *RF repeater type 2-O*

For *RF* *repeater type 2-O*, the radiated characteristics are defined over the air (OTA), where the operating band specific radiated interface is referred to as the Radiated Interface Boundary (RIB). Radiated requirements are also referred to as OTA requirements. The (spatial) characteristics in which the OTA requirements apply are detailed for each requirement.

****

**Figure 4.2.2-1: Radiated reference points for *RF repeater type 2-O***

4.3 Repeater classes

4.3.1 Repeater class for downlink

The requirements in this specification apply to downlink Wide Area repeaters, downlink Medium Range repeaters and downlink Local Area repeaters unless otherwise stated. The associated deployment scenarios for each class are exactly the same for repeater with and without connectors.

For *RF repeater type 1-C* and *type 2-O*, repeater downlink classes are defined as indicated below:

- Wide Area repeaters are characterised by requirements derived from Macro Cell scenarios with a repeater to UE minimum distance along the ground equal to 35 m.

- Medium Range repeaters are characterised by requirements derived from Micro Cell scenarios with a repeater to UE minimum distance along the ground equal to 5 m.

- Local Area repeaters are characterised by requirements derived from Pico Cell scenarios with a repeater to UE minimum distance along the ground equal to 2 m or from Femto Cell scenarios.

- Note: The requirements in this specification for LA 1-C repeaters apply to 1-C repeaters with declared output power less than or equal to LA rated output power limits as in table 6.2.1-1.

4.3.2 Repeater class for uplink

The requirements in this specification apply to uplink Wide Area repeaters and uplink Local Area repeaters unless otherwise stated. The associated deployment scenarios for each class are exactly the same for repeater with and without connectors.

For *RF* *repeater type 1-C* and *type 2-O*, repeater uplink classes are defined as indicated below:

- Wide Area repeaters are characterised by requirements derived from Macro Cell and/or Micro Cell scenarios.

- Local Area repeaters are characterised by requirements derived from Pico Cell and/or Micro Cell scenarios.

4.4 Regional requirements

Some requirements in the present document may only apply in certain regions either as optional requirements, or as mandatory requirements set by local and regional regulation. It is normally not stated in the 3GPP specifications under what exact circumstances the regional requirements apply, since this is defined by local or regional regulation.

Table 4.4-1 lists all requirements in the present specification that may be applied differently in different regions.

**Table 4.4-1: List of regional requirements**

| **Clause number** | **Requirement** | **Comments** |
| --- | --- | --- |
| 5.2 | *Operating bands* | Some NR *operating bands* may be applied regionally. |
| 6.2 | Repeater output power  | For Band n41 and n90 operation in Japan, additional output power limits shall be applied. |
| 6.2.4,7.3.4 | Repeater output power,OTA repeater output power:Additional requirements | These requirements may be applied regionally as additional repeater output power requirements. |
| 6.5.2 | Adjacent Channel Leakage Power Ratio | For Band n41 and n90 operation in Japan, absolute ACLR limits shall be applied to the sum of the absolute ACLR power over all *antenna connectors* for *repeater type 1-C*. |
| 6.5.3.2,7.5.3.2 | Operating band unwanted emission,OTA operating band unwanted emissions | Category A or Category B operating band unwanted emissions limits may be applied regionally. |
| 6.5.3.2.5.1 | Operating band unwanted emission | The repeater may have to comply with the additional requirements, when deployed in regions where those limits are applied, and under the conditions declared by the manufacturer. |
| 6.5.3.2.5.2 | Operating band unwanted emission | The repeater operating in Band n20 may have to comply with the additional requirements for protection of DTT, when deployed in certain regions. |
| 6.5.3.2 | Operating band unwanted emissions | For Band n41 and n90 operation in Japan, the operating band unwanted emissions limits shall be applied to the sum of the emission power over all *antenna connectors* for *repeater type 1-C.* |
| 6.5.4.2.1,7.5.4.2 | Tx spurious emissions,OTA Tx spurious emissions | Category A or Category B spurious emission limits, as defined in ITU-R Recommendation SM.329 [5], may apply regionally. |
| 6.5.4.2.2,7.5.4.2.3 | Tx spurious emissions: additional requirements,OTA Tx spurious emissions: additional requirements | These requirements may be applied for the protection of system operating in frequency ranges other than the repeater *operating band*. |
| 6.5.4.2 | Transmitter spurious emissions | For Band n41 and n90 operation in Japan, the sum of the spurious emissions over all *antenna connectors* for *repeater type 1-C* shall not exceed the *basic limits*. |
| 6.5.5.1 | Receiver spurious emissions | For Band n41 and n90 operation in Japan, the sum of receiver spurious emissions requirements over all *antenna connectors* for *repeater type 1-C* shall not exceed *minimum requirements* defined in clause 6.5.5.2. |
| 6.7.2 | Input intermodulation | Interfering signal positions that are partially or completely outside of any downlink *operating band* of the repeater are not excluded from the requirement in Japan in Band n77, n78, n79. |
| 6.8 | Output intermodulation | For Band n41 and n90 operation in Japan, the repeater may have to comply with the additional requirements, when deployed in certain regions. |

4.5 Applicability of requirements

In table 4.5-1, the requirement applicability for each requirement set is defined. For each requirement, the applicable requirement clause in the specification is identified. Requirements not included in a requirement set is marked not applicable (NA).

**Table 4.5-1: *Requirement set* applicability**

|  |  |
| --- | --- |
| **Requirement** | **Requirement set** |
|  | ***RFR type 1-C*** | ***RFR type 2-O*** |
| Repeater output power | 6.2 |  |
| Frequency stability | 6.3 |  |
| Out of band gain | 6.4 |  |
| Unwanted emissions | 6.5 |  |
| Error Vector Magnitude | 6.6 | NA |
| Input intermodulation | 6.7 |  |
| Output intermodulation | 6.8 |  |
| Adjacent Channel Rejection Ratio (ACRR) | 6.9 |  |
| Transmit ON/OFF power | 6.10 |  |
| Repeater output power |  | 7.2 |
| OTA frequency stability |  | 7.3 |
| OTA out of band gain |  | 7.4 |
| OTA unwanted emissions |  | 7.5 |
| OTA Error Vector Magnitude | NA | 7.6 |
| OTA input intermodulation |  | 7.7 |
|  |  |  |
| OTA Adjacent Channel Rejection Ratio (ACRR) |  | 7.8 |
| OTA transmit ON/OFF power |  | 7.9 |

<Next change>

6.2 Repeater output power

6.2.1 General

The repeater conducted output power requirement is at the *antenna connector*.

The *rated passband output power* of the *RF* *repeater type 1-C* shall be as specified in table 6.2.1-1 and table 6.2.1-2.

**Table 6.2.1-1: *RF repeater type 1-C* DL transmission classes rated output power limits for repeater classes**

|  |  |
| --- | --- |
| **Repeater class** | **Prated,p,AC** |
| Wide Area repeater | Note 1 |
| Medium Range repeater | ≤ 38 dBm + X, Note 2 |
| Local Area repeater | ≤ 24 dBm + X, Note 2 |
| NOTE 1: There is no upper limit for the Prated,p,AC *rated passband output power* of the Wide Area repeaterNOTE 2: X = 10\*log (ceil (*passband* bandwidth/20MHz)) |

**Table 6.2.1-2: *RF repeater type 1-C* UL transmission classes rated output power limits for repeater classes**

|  |  |
| --- | --- |
| **Repeater class** | **Prated,p,AC** |
| Wide Area repeater | Note 1 |
| Local Area repeater | ≤ 24 dBm+ X, Note 2 |
| NOTE 1: There is no upper limit for the Prated,p,AC *rated passband output power* of the Wide Area repeater.NOTE 2: X = 10\*log (ceil (*passband* bandwidth/20MHz)) |

<Next change>

6.5.4.2.2 Additional spurious emissions requirements

These requirements may be applied for the protection of system operating in other frequency ranges. The limits may apply as an optional protection of such systems that are deployed in the same geographical area as the repeater-Node, or they may be set by local or regional regulation as a mandatory requirement for an NR *operating band*. It is in some cases not stated in the present document whether a requirement is mandatory or under what exact circumstances that a limit applies, since this is set by local or regional regulation. An overview of regional requirements in the present document is given in clause 4.5.

Some requirements may apply for the protection of specific equipment (UE, MS and/or BS) or equipment operating in specific systems (GSM, CDMA, UTRA, E-UTRA, NR, etc.) as listed below.

The spurious emission *minimum requirements* are provided in table 6.5.4.2.2-1 where requirements for co-existence with the system listed in the first column apply for *repeater type 1-C*. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.5.4.2.2-1 apply for each supported *operating band*.

**Table 6.5.4.2.2-1: *Repeater type 1-C* spurious emissions minimum requirements for co-existence with systems operating in other frequency bands**

| **System type to co-exist with** | **Frequency range for co-existence requirement** | ***Minimum requirements*** | ***Measurement bandwidth*** | **Note** |
| --- | --- | --- | --- | --- |
| GSM900 | 921 – 960 MHz | -57 dBm | 100 kHz | This requirement does not apply to repeater operating in band n8 |
|  | 876 – 915 MHz | -61 dBm | 100 kHz | For the frequency range 880-915 MHz, this requirement does not apply to repeater operating in band n8, since it is already covered by the requirement in clause 6.5.5.2.2. |
| DCS1800 | 1805 – 1880 MHz | -47 dBm | 100 kHz | This requirement does not apply to repeater operating in band n3.  |
|  | 1710 – 1785 MHz | -61 dBm | 100 kHz | This requirement does not apply to repeater operating in band n3, since it is already covered by the requirement in clause 6.5.5.2.2. |
| PCS1900 | 1930 – 1990 MHz | -47 dBm | 100 kHz | This requirement does not apply to repeater operating in band n2, n25 or band n70.  |
|  | 1850 – 1910 MHz | -61 dBm | 100 kHz | This requirement does not apply to repeater operating in band n2 or n25 since it is already covered by the requirement in clause 6.6.5.2.2.  |
| GSM850 or  | 869 – 894 MHz | -57 dBm | 100 kHz | This requirement does not apply to repeater operating in band n5 or n26.  |
| CDMA850 | 824 – 849 MHz | -61 dBm | 100 kHz | This requirement does not apply to repeater operating in band n5 or n26, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD  | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n1 or n65 |
| Band I or E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n1 or n65, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD  | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n2 or n70.  |
| Band II or E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n2, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD  | 1805 – 1880 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n3. |
| Band III orE-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2.  |
| UTRA FDD Band IV orE-UTRA Band 4 | 2110 – 2155 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n66 |
|  | 1710 – 1755 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band V orE-UTRA Band 5 or NR Band n5 | 869 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n5 or n26.  |
|  | 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n5 or n26, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD  | 860 – 890 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n18. |
| Band VI, XIX or | 815 – 830 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n18, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 6, 18, 19 or NR Band n18 | 830 – 845 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band VII orE-UTRA Band 7 or NR Band n7 | 2620 – 2690 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n7. |
|  | 2500 – 2570 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n7, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band VIII orE-UTRA Band 8 or NR Band n8 | 925 – 960 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n8. |
|  | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band IX orE-UTRA Band 9 | 1844.9 – 1879.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n3. |
|  | 1749.9 – 1784.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band X orE-UTRA Band 10 | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n66 |
|  | 1710 – 1770 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XI or XXI orE-UTRA Band 11 or 21 | 1475.9 – 1510.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n50, n74, n75, n92 or n94. |
|  | 1427.9 – 1447.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
|  | 1447.9 – 1462.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n50, n74, n75, n92 or n94. |
| UTRA FDD Band XII orE-UTRA Band 12 or NR Band n12 | 729 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n12 or n85. |
|  | 699 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n12 or n85, since it is already covered by the requirement in clause 6.6.5.2.2.For repeater operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XIII orE-UTRA Band 13 | 746 – 756 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n13. |
|  | 777 – 787 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n13, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XIV orE-UTRA Band 14 or NR band n14 | 758 – 768 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n14. |
|  | 788 – 798 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n14, since it is already covered by the requirement in clause 6.6.5.2.2. |
|  E-UTRA Band 17 | 734 – 746 MHz | -52 dBm | 1 MHz |  |
|  | 704 – 716 MHz | -49 dBm | 1 MHz | For repeater operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XX or E-UTRA Band 20 or NR Band n20 | 791 – 821 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n20 or n28. |
|  | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XXII or E-UTRA Band 22 | 3510 – 3590 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n48, n77 or n78. |
|  | 3410 – 3490 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n77 or n78. |
| E-UTRA Band 24 | 1525 – 1559 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n24. |
|  | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n24, since it is already covered by the requirement in clause 6.6.5.2.2. |
| UTRA FDD Band XXV orE-UTRA Band 25 or NR band n25 | 1930 – 1995 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n2, n25 or n70. |
|  | 1850 – 1915 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n25 since it is already covered by the requirement in clause 6.6.5.2.2. For repeater operating in Band n2, it applies for 1910 MHz to 1915 MHz, while the rest is covered in clause 6.6.5.2.2. |
| UTRA FDD Band XXVI orE-UTRA Band 26 or NR Band n26 | 859 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n5 or n26.  |
|  | 814 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n26 since it is already covered by the requirement in clause 6.6.5.2.2. For repeater operating in Band n5, it applies for 814 MHz to 824 MHz, while the rest is covered in clause 6.6.5.2.2. |
| E-UTRA Band 27 | 852 – 869 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n5. |
|  | 807 – 824 MHz | -49 dBm | 1 MHz | This requirement also applies to repeater operating in Band n28, starting 4 MHz above the Band n28 downlink operating band (Note 5). |
| E-UTRA Band 28 or NR Band n28 | 758 – 803 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n20, n67 or n28. |
|  | 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n28, since it is already covered by the requirement in clause 6.6.5.2.2.For repeater operating in band n67, it applies for 703 MHz to 736 MHz. |
| E-UTRA Band 29 or NR Band n29 | 717 – 728 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n29 or n85 |
| E-UTRA Band 30 or NR Band n30 | 2350 – 2360 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n30 |
|  | 2305 – 2315 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n30, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 31 | 462.5 – 467.5 MHz | -52 dBm | 1 MHz |  |
|  | 452.5 – 457.5 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD band XXXII or E-UTRA band 32 | 1452 – 1496 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n50, n74, n75, n92 or n94. |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n34. |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n2 or n25. |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n38.  |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n39. |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n41, n53 or [n90]. |
| E-UTRA Band 42 | 3400 – 3600 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n48, n77 or n78. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n48, n77 or n78. |
| E-UTRA Band 44 | 703 – 803 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n28. |
| E-UTRA Band 45 | 1447 – 1467 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 46 | 5150 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 47 | 5855 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n48, n77 or n78. |
| E-UTRA Band 50 or NR band n50  | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 53 or NR Band n53 | 2483.5 - 2495 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n41, n53 or n90. |
| E-UTRA Band 65 or NR Band n65 | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n1 or n65.  |
|  | 1920 – 2010 MHz | -49 dBm | 1 MHz | For repeater operating in Band n1, it applies for 1980 MHz to 2010 MHz, while the rest is covered in clause 6.6.5.2.2. This requirement does not apply to repeater operating in band n65, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 66 or NR Band n66 | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n66. |
|  | 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 67 | 738 – 758 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n28 or n67. |
| E-UTRA Band 68 | 753 -783 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n28. |
|  | 698-728 MHz | -49 dBm | 1 MHz | For repeater operating in Band n28, this requirement applies between 698 MHz and 703 MHz, while the rest is covered in clause 6.6.5.2.2. |
| E-UTRA Band 69 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n38. |
| E-UTRA Band 70 or NR Band n70 | 1995 – 2020 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n2, n25 or n70 |
|  | 1695 – 1710 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n70, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 71 or NR Band n71 | 617 – 652 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n71 |
|  | 663 – 698 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n71, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 72 | 461 – 466 MHz | -52 dBm | 1 MHz |  |
|  | 451 – 456 MHz | -49 dBm | 1 MHz |  |
| E-UTRA Band 74 or NR Band n74 | 1475 – 1518 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n50, n74, n75, n92 or n94. |
|  | 1427 – 1470 MHz | -49 dBm | 1MHz | This requirement does not apply to repeater operating in band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 75 or NR Band n75 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n74, n75, n76, n91, n92, n93 or n94. |
| E-UTRA Band 76 or NR Band n76 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n75, n76, n91, n92, n93 or n94. |
| NR Band n77 | 3.3 – 4.2 GHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n79 |
| NR Band n80 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n3, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n81 | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n8, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n82 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n20, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n83 | 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n28, since it is already covered by the requirement in clause 6.6.5.2.2.For repeater operating in Band n67, it applies for 703 MHz to 736 MHz. |
| NR Band n84 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n1, since it is already covered by the requirement in clause 6.6.5.2.2. |
| E-UTRA Band 85 or NR Band n85 | 728 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in band n12 or n85.For repeater operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
|  | 698 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n12 or n85, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n86 | 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n66, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n89 | 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n5, since it is already covered by the requirement in clause 6.6.5.2.2. |
| NR Band n91 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n75 or n76. |
|  | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n20, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n92 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n74, n75 or n76. |
|  | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n20, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n93 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n75 or n76. |
|  | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n8, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n94 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n50, n51, n74, n75 or n76. |
|  | 880 – 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n8, since it is already covered by the requirement in clause 6.6.5.5.1.2. |
| NR Band n95 | 2010 – 2025 MHz | -52 dBm | 1 MHz |  |
| NR Band n96 | 5925 – 7125 MHz | -52 dBm | 1 MHz |  |
| NR Band n97 | 2300 – 2400MHz | -52 dBm | 1 MHz |  |
| NR Band n98 | 1880 – 1920MHz | -52 dBm | 1 MHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This requirement does not apply to repeater operating in band n24, since it is already covered by the requirement in clause 6.5.5.2.2. |
| NR band n101 | 1900 – 1910 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n101. |
| NR Band n102 | 5925 – 6425 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 103 | 757 – 758 MHz | -52 dBm | 1 MHz |  |
|  | 787 – 788 MHz | -49 dBm | 1 MHz |  |
| NR Band n104 | 6425 – 7125 MHz | -52 dBm | 1 MHz | This requirement does not apply to repeater operating in Band n104 |

NOTE 1: As defined in the scope for spurious emissions in this clause, except for the cases where the noted requirements apply to a repeater operating in Band n28, the co-existence requirements in table 6.5.4.2.3 -1 do not apply for the ΔfOBUE frequency range immediately outside the downlink *operating band* (see table 5.2-1). Emission limits for this excluded frequency range may be covered by local or regional requirements.

NOTE 2: Table 6.5.5.2.3 -1 assumes that two *operating bands*, where the frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: For unsynchronized operation, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 4: For NR Band n28 repeater, specific solutions may be required to fulfil the spurious emissions limits for repeater for co-existence with E-UTRA Band 27 UL *operating band*.

NOTE 5: For NR Band n29 repeater, specific solutions may be required to fulfil the spurious emissions limits for repeater for co-existence with UTRA Band XII, E-UTRA Band 12 or NR Band n12 UL operating band, E-UTRA Band 17 UL operating band or E-UTRA Band 85 UL or NR Band n85 UL operating band.

The following requirement may be applied for the protection of PHS. This requirement is also applicable at specified frequencies falling between ΔfOBUE below the lowest repeater transmitter frequency of the downlink *operating band* and ΔfOBUE above the highest repeater transmitter frequency of the downlink *operating band*. ΔfOBUE is defined in clause 6.5.1.

The spurious emission *minimum requirements* for this requirement are:

**Table 6.5.4.2.3-2: Repeater spurious emissions minimum requirements for repeater for co-existence with PHS for DL**

|  |  |  |  |
| --- | --- | --- | --- |
| **Frequency range** | ***minimum requirements*** | ***Measurement Bandwidth*** | **Note** |
| 1884.5 – 1915.7 MHz | -41 dBm | 300 kHz | Applicable when co-existence with PHS system operating in 1884.5 – 1915.7 MHz  |

In certain regions, the following requirement may apply to repeater operating in Band n50 and n75 within the 1432 – 1452 MHz, and in Band n51 and Band n76. The *minimum requirements are* specified in table 6.5.4.2.3-4. This requirement is also applicable at the frequency range from ΔfOBUE below the lowest frequency of the repeater downlink *operating band* up to ΔfOBUE above the highest frequency of the repeater downlink *operating band*.

**Table 6.5.4.2.3-4: Additional operating band unwanted emission minimum requirement for repeater operating in Band n50 and n75 within 1432 – 1452 MHz, and in Band n51 and n76**

|  |  |  |
| --- | --- | --- |
| **Filter centre frequency, Ffilter** | ***Minimum requirements*** | ***Measurement Bandwidth*** |
| Ffilter = 1413.5 MHz | -42 dBm | 27 MHz |

In certain regions, the following requirement may apply to repeater operating in NR Band n50 and n75 within 1492-1517 MHz and in Band n74 within 1492-1518 MHz. The maximum level of emissions, measured on centre frequencies Ffilter with filter bandwidth according to table 6.5.4.2.3-5, shall be defined according to the *minimum requirements* PEM,n50/n75,a nor PEM,n50/n75,b declared by the manufacturer.

**Table 6.5.4.2.3-5: *Operating band* n50, n74 and n75 declared emission above 1518 MHz**

|  |  |  |
| --- | --- | --- |
| **Filter centre frequency, Ffilter** | **Declared *minimum requirements* (dBm)** | ***Measurement bandwidth*** |
| 1518.5 MHz ≤ Ffilter ≤ 1519.5 MHz | PEM, n50/n75,a | 1 MHz |
| 1520.5 MHz ≤ Ffilter ≤ 1558.5 MHz | PEM,n50/n75,b | 1 MHz |

In certain regions, the following requirement shall be applied to repeater operating in Band n13 and n14 to ensure that appropriate interference protection is provided to 700 MHz public safety operations. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the repeater downlink operating band up to 10 MHz above the highest frequency of the repeater downlink operating band.

The power of any spurious emission shall not exceed:

**Table 6.5.4.2.3-6: Repeater spurious emissions limits for protection of 700 MHz public safety operations**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operating Band** | **Frequency range** | **Maximum Level** | ***Measurement Bandwidth*** |
| n13 | 763 - 775 MHz | -46 dBm | 6.25 kHz |
| n13 | 793 - 805 MHz | -46 dBm | 6.25 kHz |
| n14 | 769 - 775 MHz | -46 dBm | 6.25 kHz |
| n14 | 799 - 805 MHz | -46 dBm | 6.25 kHz |

In certain regions, the following requirement may apply to repeater operating in Band n30. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the repeater downlink operating band up to 10 MHz above the highest frequency of the repeater downlink operating band.

The power of any spurious emission shall not exceed:

**Table 6.5.4.2.3-7: Additional repeater spurious emissions minimum requirements for Band n30**

|  |  |  |  |
| --- | --- | --- | --- |
| **Frequency range** | ***Minimum requirements*** | ***Measurement Bandwidth*** | **Note** |
| 2200 – 2345 MHz | -45 dBm | 1 MHz |  |
| 2362.5 – 2365 MHz | -25 dBm | 1 MHz |  |
| 2365 – 2367.5 MHz | -40 dBm | 1 MHz |  |
| 2367.5 – 2370 MHz | -42 dBm | 1 MHz |  |
| 2370 – 2395 MHz | -45 dBm | 1 MHz |  |

The following requirement may apply to repeater operating in Band n48 in certain regions. The power of any spurious emission shall not exceed:

**Table 6.5.4.2.3-8: Additional repeater spurious emissions limits for Band n48**

|  |  |  |  |
| --- | --- | --- | --- |
| **Frequency range** | **Maximum Level** | ***Measurement Bandwidth* (NOTE)** | **Note** |
| 3530 MHz – 3720 MHz | -25 dBm | 1 MHz | Applicable 10 MHz from the assigned *passband edge*  |
| 3100 MHz – 3530 MHz3720 MHz – 4200 MHz | -40 dBm | 1 MHz |  |

NOTE: The resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. However, to improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

NOTE: The regional requirement, included in [12], is defined in terms of EIRP, which is dependent on both the repeater emissions at the *antenna connector* and the deployment (including antenna gain and feeder loss). The requirement defined above provides the characteristics of the base station needed to verify compliance with the regional requirement. The assessment of the EIRP level is described in Annex F.

The following requirement shall be applied to repeater operating in Band n26 to ensure that appropriate interference protection is provided to 800 MHz public safety operations. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the repeater downlink operating band up to 10 MHz above the highest frequency of the repeater downlink operating band.

The power of any spurious emission shall not exceed:

**Table 6.5.4.2.3-9: Repeater spurious emissions limits for protection of 800 MHz public safety operations**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Operating Band** | **Frequency range** | **Maximum Level** | **Measurement Bandwidth** | **Note** |
| n26 | 851 - 859 MHz | -13 dBm | 100 kHz | Applicable for offsets > 37.5kHz from the *passband* edge |

The following requirement may apply to Repeater for Band n41 and n90 operation in Japan. This requirement is also applicable at the frequency range from ΔfOBUE below the lowest frequency of the Repeater downlink operating band up to ΔfOBUE above the highest frequency of the Repeater downlink operating band.

The power of any spurious emission shall not exceed:

**Table 6.5.4.2.3-10: Additional repeater spurious emissions minimum requirements for Band n41 and n90**

|  |  |  |
| --- | --- | --- |
| **Frequency range** | ***Minimum requirement*** | ***Measurement Bandwidth*** |
| 2505 MHz – 2535 MHz | -42 dBm | 1 MHz |
| NOTE: This requirement applies for carriers allocated within 2545-2645 MHz. |

The following requirement may apply to repeater operating in 3.45-3.55 GHz in Band n77 in certain regions. Emissions shall not exceed the maximum levels specified in table 6.5.4.2.3-11.

**Table 6.5.4.2.3-11: Additional repeater spurious emissions limits for Band n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Channel bandwidth [MHz]** | **Frequency range [MHz]** | **Filter centre frequency, Ffilter [MHz]** | **Minimum requirement [dBm]** | ***Measurement bandwidth* [MHz]** |
| All | 3430 – 34403560 – 3570 | 3430.5 ≤ Ffilter < 3439.53560.5 ≤ Ffilter < 3569.5 | -25 | 1 |
| All | ≤ 3430> 3570 | Ffilter < 3429.53570.5 ≤ Ffilter | -40 | 1 |

NOTE: The resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. However, to improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

<Next change>

6.7.2 Co-location with BS/repeater in other systems

6.7.2.1 General

This additional input intermodulation requirement may be applied for the protection of RF repeater receivers when GSM, CDMA, UTRA, E-UTRA, NR BS or repeater operating in a different frequency band are co-located with a RF repeater.

The following requirement applies for interfering signals depending on the repeaters *passband*.

This requirement applies to the uplink and downlink of the repeater. If the BS side is declared to meet co-location requirements, then it should meet input intermodulation co-location requirements for the downlink. If the UE side is declared to meet co-location requirements, then it should meet input intermodulation co-location requirements for the uplink.

6.7.2.2 Minimum requirement

For the parameters specified in table 6.7.2.2-1 for DL and 6.7.2.2-2 for UL, the power in the *passband* shall not increase with more than 10 dB at the output of the repeater as measured with 1MHz measurement bandwidth, compared to the level obtained without interfering signals applied.

The core requirement is applicable for all frequency separation possibilities between the two interfering signals that cause the 3rd order intermodulation product to fall into the *passband*.

**Table 6.7.2.2-1: input intermodulation requirement for RF repeater DL when co-located with BS/repeater in other frequency bands.**

| **Frequency range of interfering signal** | **Interfering signal mean power for repeater with WA UE side (dBm)** | **Interfering signal mean power for repeater with MR UE side(dBm)** | **Interfering signal mean power for repeater with LA UE side(dBm)** | **Type of interfering signals** |
| --- | --- | --- | --- | --- |
| Frequency range of co-located BS’s downlink operating band or located repeater’s *passband* | +16 | +8 | x (Note 1) | 2 CW carriers |
| NOTE 1: x = -7 dBm for RF repeater co-located with Pico GSM850 or Pico CDMA850 x = -4 dBm for RF repeater co-located with Pico DCS1800 or Pico PCS1900 x = -6 dBm for RF repeater co-located with UTRA bands or E-UTRA bands or NR bandsNOTE 2: The requirement does not apply when the interfering signal falls within the *passband*.NOTE 3: For unsynchronized base stations (except in band n46, n96, and n102) or repeaters, special co-location requirements may apply that are not covered by the 3GPP specifications. |

**Table 6.7.2.2-2: input intermodulation requirement for RF repeater UL when co-located with BS/repeater in other frequency bands.**

| **Frequency range of interfering signal** | **Interfering signal mean power for repeater with WA BS side(dBm)** | **Interfering signal mean power for repeater with LA BS side(dBm)** | **Type of interfering signals** |
| --- | --- | --- | --- |
| Frequency range of co-located BS’s downlink operating band or located repeater’s *passband* | +16 | Prated,p,AC -30 | 2 CW carriers |
| NOTE 1: The requirement does not apply when the interfering signal falls within the *passband*.NOTE 2: For unsynchronized base stations (except in band n46, n96, and n102) or repeaters, special co-location requirements may apply that are not covered by the 3GPP specifications. |

6.7.3 Co-existence with other systems

6.7.3.1 General

This input intermodulation existence requirement may be applied for the protection of RF repeater receivers when GSM, CDMA, UTRA, E-UTRA, NR BS or repeater operating in another frequency band co-exist with a RF repeater.

6.7.3.2 Minimum requirement

For the parameters specified in table 6.7.3.2-1, the power in the *passband* shall not increase with more than 10 dB at the output of the repeater as measured with 1MHz measurement bandwidth, compared to the level obtained without interfering signals applied.

The core requirement is applicable for all frequency separation possibilities between the two interfering signals that cause the 3rd order intermodulation product to fall into the *passband*.

**Table 6.7.3.2-1: input intermodulation requirement for RF repeater when co-exist with BS/repeater in other non-overlapping frequency bands**

| **Frequency range of interfering signal** | **Interfering signal mean power (dBm)** | **Type of interfering signals** | **Measurement bandwidth** |
| --- | --- | --- | --- |
| Frequency range of co-existence system operating band | -15 | 2 CW carriers | 1MHz |
| NOTE 1: All the interfering signals should be limited into the frequency ranges that are either X MHz higher than FUL,high or X MHz lower than FUL,low, where X equals to 20MHz when FUL,high - FUL,low is not larger than 200MHz, otherwise X equals to 60MHz  |

<End of changes>