**3GPP TSG-RAN4 Meeting #113**

**Orlando, United States, 18th Nov 2024 - 22nd Nov 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-4** | **CR** | **0694** | **rev** | 1 | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to 38.101-4: Editorial correction of eRedCap UE demodulation and CSI reporting requirements |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_redcap\_enh-Perf |  | ***Date:*** | 2024-11-22 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Editorial correction.  |
|  |  |
| ***Summary of change:*** | 1. Clarified the HD-FDD mode configuration is applicable for eRedCap.
2. Correction from RedCap to eRedCap.
3. Rename ‘RedCap enhancements’ to ‘eRedCap’ in CQI test to align the section title with other eRedCap requiremets.

Table number correction in 6.2.2.2.2.5. |
|  |  |
| ***Consequences if not approved:*** | Reader may misunderstand the specification.  |
|  |  |
| ***Clauses affected:*** | 5.5.1, 6.2.1.1.1.2, 6.2.1.1.2.2, 6.2.1.2.1.2, 6.2.1.2.2.2, 6.2.2.1.1.5, 6.2.2.1.2.5, 6.2.2.2.1.6, 6.2.2.2.2.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS 38.521-4 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of R4-2418990 |

----------------------------------------------------- Beginning of Change ------------------------------------------------------------

### 5.5.1 FR1 single carrier requirements

The requirements in this clause are applicable to the FR1 single carrier case.

The requirements and procedure defined in Clause 5.5A.1 apply using operating band instead of CA configuration, and bandwidth instead of bandwidth combination.

For RedCap and eRedCap, the requirements and procedure are defined in Clause 5.5A.1 except that the MIMO layers are configured to 2 for UE supporting 2 MIMO layers and 1 for UE supporting 1 MIMO layers for all operating band. Antenna configuration is 1x1 for UE supporting 1 layer and 2x2 for UE supporting 2 layers.

For eRedCap with reduced peak date rate and reduced baseband bandwidth in FR1, only 25 PRBs for 15kHz SCS and 12RBs for 30kHz SCS are allocated for PDSCH transmission.

For RedCap and eRedCap with HD-FDD mode, the additional test parameters are specified in Table 5.5.1-1.

Table 5.5.1-1: Additional test parameters for HD-FDD single carrier

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value** |
| Duplex mode |  | HD-FDD |
| PDSCH configuration | Starting symbol (S)  |  | 1 |
| Length (L) |  | 13 |
| Number of HARQ Processes |  | 4 |
| Full DL slots (Note 1, Note 2) |  | For slots i, if mod(i, 5) = {0,1,2} |
| K1 value (Note 2) |  | 4 if mod(i, 5) = 03 if mod(i, 5) = 12 if mod(i, 5) = 2 |
| Note 1: PDSCH is scheduled only on full DL slots.Note 2: i is the slot index per frame; i = {1, 2, …, 19}. |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

6.2.1.1.1.2 Minimum requirement for periodic CQI reporting for eRedCap

For the parameters specified in Table 6.2.1.1.1.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements for the eRedCap are specified by the following:

a) The reported CQI value according to the reference channel shall be in the range of ±1 of the reported median more than 90% of the time.

b) If the PDSCH BLER using the transport format indicated by median CQI is less than or equal to 0.1, then the BLER using the transport format indicated by the (median CQI+1) shall be greater than 0.1. If the PDSCH BLER using the transport format indicated by the median CQI is greater than 0.1, then the BLER using transport format indicated by (median CQI-1) shall be less than or equal to 0.1.

**Table 6.2.1.1.1.2-1: CQI reporting definition test**

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** | **Test 2** |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
| SNR | dB | 5 | 6 | 11 | 12 |
| Propagation channel |  | AWGN |
| Antenna configuration |  | 2×1 with static channel specified in Annex B.1 |
| Beamforming Model |  | As specified in Annex B.4.1 |
| BWP size  | RB | 52 (PRB 0 to 51) |
| PDSCH BW | RB  | 15 (PRB 0 to 14) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/5 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/5 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/5 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
| CodebookSubsetRestriction |  | 000001 |
| RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 10 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-1 |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

###### 6.2.1.1.2.2 Minimum requirement for wideband CQI reporting for eRedCap

The purpose of the requirements is to verify that the eRedCap is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the wideband CQI reporting under frequency selective fading conditions is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.1.1.2.2-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least *α*% of the time where *α*% is specified in Table 6.2.1.1.2.2-2;

b) The ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ *γ*, where *γ* is specified in Table 6.2.1.1.2.2-2;

c) When transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater than or equal to 0.02.

Table 6.2.1.1.2.2-1: Wideband CQI reporting test under frequency non-selective fading conditions

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test 1 | Test 2 |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
|  SNR | dB | 9 | 10 | 15 | 16 |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | 2×1 |
| Correlation configuration |  | ULA high |
| Beamforming Model |  | As specified in Annex B.4.1 |
| BWP size  | RB | 52 (PRB 0 to 51) |
| PDSCH BW | RB  | 15 (PRB 0 to 14) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/5 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/5 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/5 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
| CodebookSubsetRestriction |  | 000001 |
| RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 10 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-1 |

Table 6.2.1.1.2.2-2: Minimum requirements

|  |  |  |
| --- | --- | --- |
| Parameters | Test 1 | Test 2 |
| ** [%] | 20 | 20 |
| **  | 1.05 | 1.05 |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

6.2.1.2.1.2 Minimum requirement for periodic CQI reporting for eRedCap

The purpose of the requirements for the eRedCap is to verify that the reported CQI values are in accordance with the CQI definition given in TS 38.214 [12]. The reporting accuracy of CQI under AWGN condition is determined by the reporting variance and BLER performance using the transport format indicated by the reported CQI median. To account for sensitivity of the input SNR the reporting definition is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.1.2.1.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) The reported CQI value according to the reference channel shall be in the range of ±1 of the reported median more than 90% of the time.

b) If the PDSCH BLER using the transport format indicated by median CQI is less than or equal to 0.1, then the BLER using the transport format indicated by the (median CQI+1) shall be greater than 0.1. If the PDSCH BLER using the transport format indicated by the median CQI is greater than 0.1, then the BLER using transport format indicated by (median CQI-1) shall be less than or equal to 0.1.

**Table 6.2.1.2.1.2-1: CQI reporting definition test**

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** | **Test 2** |
| Bandwidth | MHz | 20 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD UL-DL pattern |  | FR1.30-1 |
| SNR |  dB | 5 | 6 | 11 | 12 |
| Propagation channel |  | AWGN |
| Antenna configuration |  | 2×1 with static channel specified in Annex B.1 |
| Beamforming Model |  | As specified in Annex B.4.1 |
| BWP size  | RB | 51 (PRB 0 to 50) |
| PDSCH BW | RB  | 7 (PRB 0 to 6) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/1 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/1 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
| CodebookSubsetRestriction |  | 000001 |
| RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 9.5 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-2 |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

###### 6.2.1.2.2.2 Minimum requirement for wideband CQI reporting for eRedCap

The purpose of the requirements is to verify that the eRedCap is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the reporting definition is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.1.2.2.2-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least *α*% of the time where *α*% is specified in Table 6.2.1.2.2.2-2;

b) The ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ *γ*, where *γ* is specified in Table 6.2.1.2.2.2-2;

c) When transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater than or equal to 0.02.

Table 6.2.1.2.2.2-1: Wideband CQI reporting test under frequency non-selective fading conditions

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test 1 | Test 2 |
| Bandwidth | MHz | 20 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD UL-DL pattern |  | FR1.30-1 |
| SNR |  dB | 9 | 10 | 15 | 16 |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | 2×1  |
| Correlation configuration |  | ULA high |
| Beamforming Model |  | As specified in Annex B.4.1  |
| BWP size  | RB | 51 (PRB 0 to 50) |
| PDSCH BW | RB  | 7 (PRB 0 to 6) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/1 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/1 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
| CodebookSubsetRestriction |  | 000001 |
| RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 9.5 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-2 |

Table 6.2.1.2.2.2-2: Minimum requirements

|  |  |  |
| --- | --- | --- |
| Parameters | Test 1 | Test 2 |
| ** [%] | 20 | 20 |
| **  | 1.05 | 1.05 |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

6.2.2.1.1.5 Minimum requirement for periodic CQI reporting for eRedCap

For the parameters specified in Table 6.2.2.1.1.5-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements for the eRedCap are specified by the following:

a) The reported CQI value according to the reference channel shall be in the range of ±1 of the reported median more than 90% of the time.

b) If the PDSCH BLER using the transport format indicated by median CQI is less than or equal to 0.1, then the BLER using the transport format indicated by the (median CQI+1) shall be greater than 0.1. If the PDSCH BLER using the transport format indicated by the median CQI is greater than 0.1, then the BLER using transport format indicated by (median CQI-1) shall be less than or equal to 0.1.

**Table 6.2.2.1.1.5-1: CQI reporting definition test**

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test 1** | **Test 2** |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
| SNR | dB | 8 | 9 | 14 | 15 |
| Propagation channel |  | AWGN |
| Antenna configuration |  | 2×2 with static channel specified in Annex B.1 |
| Beamforming Model |  | As specified in Annex B.4.1 |
| BWP size  | RB | 52 (PRB 0 to 51) |
| PDSCH BW | RB  | 15 (PRB 0 to 14) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/5 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/5 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/5 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
| CodebookSubsetRestriction |  | 010000 |
| RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 10 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-1 |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

###### 6.2.2.1.2.5 Minimum requirement for wideband CQI reporting for eRedCap

The purpose of the requirements is to verify that the eRedCap is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the wideband CQI reporting under frequency selective fading conditions is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.2.1.2.5-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least *α*% of the time where *α*% is specified in Table 6.2.2.1.2.5-2;

b) The ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ *γ*, where *γ* is specified in Table 6.2.2.1.2.5-2;

c) When transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater than or equal to 0.02.

Table 6.2.2.1.2.5-1: Wideband CQI reporting test under frequency non-selective fading conditions

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Test 1 |
| Bandwidth | MHz | 10 |
| Subcarrier spacing | kHz | 15 |
| Duplex Mode |  | FDD |
| SNR | dB | 6 | 7 |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | 2×2  |
| Correlation configuration |  | ULA high |
| Beamforming Model |  | As specified in Annex B.4.1 |
| BWP size  | RB | 52 (PRB 0 to 51) |
| PDSCH BW | RB  | 15 (PRB 0 to 14) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/5 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/5 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/5 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
|  | Codebook Mode |  | 1 |
|  | (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
|  | CodebookSubsetRestriction |  | 000001 |
|  | RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 10 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-1 |

Table 6.2.2.1.2.5-2: Minimum requirements

|  |  |
| --- | --- |
| Parameters | Test 1 |
| ** [%] | 20 |
| **  | 1.05 |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

6.2.2.2.1.6 Minimum requirement for periodic CQI reporting for eRedCap

The purpose of the requirements for the eRedCap is to verify that the reported CQI values are in accordance with the CQI definition given in TS 38.214 [12]. The reporting accuracy of CQI under AWGN condition is determined by the reporting variance and BLER performance using the transport format indicated by the reported CQI median. To account for sensitivity of the input SNR the reporting definition is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.2.2.1.6-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) The reported CQI value according to the reference channel shall be in the range of ±1 of the reported median more than 90% of the time.

b) If the PDSCH BLER using the transport format indicated by median CQI is less than or equal to 0.1, then the BLER using the transport format indicated by the (median CQI+1) shall be greater than 0.1. If the PDSCH BLER using the transport format indicated by the median CQI is greater than 0.1, then the BLER using transport format indicated by (median CQI-1) shall be less than or equal to 0.1.

Table 6.2.2.2.1.6-1: CQI reporting definition test

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test 1 | Test 2 |
| Bandwidth | MHz | 20 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD UL-DL pattern |  | FR1.30-1 |
| SNR |  dB | 8 | 9 | 14 | 15 |
| Propagation channel |  | AWGN |
| Antenna configuration |  | 2×2 with static channel specified in Annex B.1 |
| Beamforming Model |  | As specified in Annex B.4.1 |
| BWP size  | RB | 51 (PRB 0 to 50) |
| PDSCH BW | RB  | 7 (PRB 0 to 6) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/1 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/1 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
|  | Codebook Mode |  | 1 |
|  | (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
|  | CodebookSubsetRestriction |  | 010000 |
|  | RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 9.5 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-2 |

------------------------------------------------- Unchanged sections omitted --------------------------------------------------------

###### 6.2.2.2.2.5 Minimum requirement for wideband CQI reporting for eRedCap

The purpose of the requirements is to verify that the eRedCap is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the reporting definition is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.2.2.2.5-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least *α*% of the time where *α*% is specified in Table 6.2.2.2.2.5-2;

b) The ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ *γ*, where *γ* is specified in Table 6.2.2.2.2.5-2;

c) When transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater than or equal to 0.02.

Table 6.2.2.2.2.5-1: Wideband CQI reporting test under frequency non-selective fading conditions

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Test 1 |
| Bandwidth | MHz | 20 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD UL-DL pattern |  | FR1.30-1 |
| SNR | dB | 6 | 7 |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | 2×2  |
| Correlation configuration |  | ULA high |
| Beamforming Model |  | As specified in Annex B.4.1  |
| BWP size  | RB | 51 (PRB 0 to 50) |
| PDSCH BW | RB  | 7 (PRB 0 to 6) |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,4 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 9 |
| Frequency Occupation | RB | 0 to 23  |
| CSI-RSperiodicity and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 3,(6) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | 13 |
| Frequency Occupation | RB | 0 to 23  |
| NZP CSI-RS-timeConfigperiodicity and offset | slot | 10/1 |
| CSI-IM configuration | CSI-IM resource Type |  | Periodic |
| CSI-IM RE pattern |  | 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4, 9) |
| CSI-IM timeConfigperiodicity and offset | slot | 10/1 |
| ReportConfigType |  | Periodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 8 |
| Csi-ReportingBand |  | 1111111 |
| CSI-Report periodicity and offset | slot | 10/9 |
| aperiodicTriggeringOffset |  | Not configured |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
|  | Codebook Mode |  | 1 |
|  | (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured |
|  | CodebookSubsetRestriction |  | 000001 |
|  | RI Restriction |  | N/A |
| Physical channel for CSI report |  | PUCCH |
| CQI/RI/PMI delay  | ms | 9.5 |
| Maximum number of HARQ transmission |  | 1 |
| Measurement channel |  | As specified in Table A.4-6, TBS.6-2 |

Table 6.2.2.2.2.5-2: Minimum requirements

|  |  |
| --- | --- |
| Parameters | Test 1 |
| ** [%] | 20 |
| **  | 1.05 |

------------------------------------------------------------- End of change ------------------------------------------------------------