**3GPP TSG- Meeting #*****R4-2419892***

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **3** | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR for Rel-18 TS38.101-4, alignments on the expression of CSI-RS conigurations for RedCap enhancement requirements | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Taking the following table as an exampe, in TS38.101-4, the expression for configuraitons of ZP CSI-RS and NZP CSI-RS are differnet in CQI, PMI and RI requirements.   |  |  |  |  | | --- | --- | --- | --- | | Table 6.2.2.1.1.3-1 (CQI requirement) | ZP CSI-RS configuration | First subcarrier index in the PRB used for CSI-RS (k0) | Row 5,4 | | First OFDM symbol in the PRB used for CSI-RS (l0) | 9 | | NZP CSI-RS for CSI acquisition | First subcarrier index in the PRB used for CSI-RS (k0) | Row 3,(6) | | First OFDM symbol in the PRB used for CSI-RS (l0) | 13 | | Table 6.3.2.1.3-1 (PMI requirement) | ZP CSI-RS configuration | First subcarrier index in the PRB used for CSI-RS (k0, k1) | Row 5, (4,-) | | First OFDM symbol in the PRB used for CSI-RS (l0, l1) | (9,-) | | NZP CSI-RS for CSI acquisition | First subcarrier index in the PRB used for CSI-RS (k0, k1, k2, k3) | Row 12, (2, 4, 6, 8) | | First OFDM symbol in the PRB used for CSI-RS (l0, l1) | (5, -) | | Table 6.4.2.1-1 (RI requirement) | ZP CSI-RS configuration | First subcarrier index in the PRB used for CSI-RS (k0) | Row 5,(4) | | First OFDM symbol in the PRB used for CSI-RS (l0) | (9) | | NZP CSI-RS for CSI acquisition | First subcarrier index in the PRB used for CSI-RS (k0) | Row 3 (6) | | First OFDM symbol in the PRB used for CSI-RS (l0) | (13) | | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Align the expression for configuraitons of ZP CSI-RS and NZP CSI-RS in Caluse 6.2.4 with that in other Clauses 2. Add row configuration for the “First OFDM symbol in the PRB used for CSI-RS” to be aligned with “First subcarrier index in the PRB used for CSI-RS” | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The expression for configuraitons of ZP CSI-RS and NZP CSI-RS are not aligned | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.1.1.1.2, 6.2.1.1.2.2, 6.2.1.2.1.2, 6.2.1.2.2.2, 6.2.2.1.1.5, 6.2.2.1.2.5, 6.3.1.1.2, 6.3.1.2.2, 6.3.2.1.10 and 6.3.2.2.10 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS38.521-4 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Revision of R4-2419547 | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**START OF CHANGE 1**

6.2.1.1.1.2 Minimum requirement for periodic CQI reporting for RedCap enhancements

For the parameters specified in Table 6.2.1.1.1.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements for the eRedCap UE are specified by the following:

a) The reported CQI value according to the reference channel shall be in the range of ±1 of the reported median more than 90% of the time.

b) If the PDSCH BLER using the transport format indicated by median CQI is less than or equal to 0.1, then the BLER using the transport format indicated by the (median CQI+1) shall be greater than 0.1. If the PDSCH BLER using the transport format indicated by the median CQI is greater than 0.1, then the BLER using transport format indicated by (median CQI-1) shall be less than or equal to 0.1.

**Table 6.2.1.1.1.2-1: CQI reporting definition test**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Parameter** | | | **Unit** | **Test 1** | | **Test 2** | |
| Bandwidth | | | MHz | 10 | | | |
| Subcarrier spacing | | | kHz | 15 | | | |
| Duplex Mode | | |  | FDD | | | |
| SNR | | | dB | 5 | 6 | 11 | 12 |
| Propagation channel | | |  | AWGN | | | |
| Antenna configuration | | |  | 2×1 with static channel specified in Annex B.1 | | | |
| Beamforming Model | | |  | As specified in Annex B.4.1 | | | |
| BWP size | | | RB | 52 (PRB 0 to 51) | | | |
| PDSCH BW | | | RB | 15 (PRB 0 to 14) | | | |
| ZP CSI-RS configuration | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 4 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 5,(4) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 5,(9) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| CSI-RS  periodicity and offset | | slot | 10/5 | | | |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 2 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 3,(6) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 3,(13) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| NZP CSI-RS-timeConfig  periodicity and offset | | slot | 10/5 | | | |
| CSI-IM configuration | CSI-IM resource Type | |  | Periodic | | | |
| CSI-IM RE pattern | |  | 0 | | | |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) | |  | (4, 9) | | | |
| CSI-IM timeConfig  periodicity and offset | | slot | 10/5 | | | |
| ReportConfigType | | |  | Periodic | | | |
| CQI-table | | |  | Table 1 | | | |
| reportQuantity | | |  | cri-RI-PMI-CQI | | | |
| timeRestrictionForChannelMeasurements | | |  | Not configured | | | |
| timeRestrictionForInterferenceMeasurements | | |  | Not configured | | | |
| cqi-FormatIndicator | | |  | Wideband | | | |
| pmi-FormatIndicator | | |  | Wideband | | | |
| Sub-band Size | | | RB | 8 | | | |
| Csi-ReportingBand | | |  | 1111111 | | | |
| CSI-Report periodicity and offset | | | slot | 10/9 | | | |
| aperiodicTriggeringOffset | | |  | Not configured | | | |
| Codebook configuration | | Codebook Type |  | typeI-SinglePanel | | | |
| Codebook Mode |  | 1 | | | |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured | | | |
| CodebookSubsetRestriction |  | 000001 | | | |
| RI Restriction |  | N/A | | | |
| Physical channel for CSI report | | |  | PUCCH | | | |
| CQI/RI/PMI delay | | | ms | 10 | | | |
| Maximum number of HARQ transmission | | |  | 1 | | | |
| Measurement channel | | |  | As specified in Table A.4-6,  TBS.6-1 | | | |

**END OF CHANGE 1**

**START OF CHANGE 2**

###### 6.2.1.1.2.2 Minimum requirement for wideband CQI reporting for RedCap enhancements

The purpose of the requirements is to verify that the RedCap UE is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the wideband CQI reporting under frequency selective fading conditions is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.1.1.2.2-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least *α*% of the time where *α*% is specified in Table 6.2.1.1.2.2-2;

b) The ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ *γ*, where *γ* is specified in Table 6.2.1.1.2.2-2;

c) When transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater than or equal to 0.02.

Table 6.2.1.1.2.2-1: Wideband CQI reporting test under frequency non-selective fading conditions

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | | | Unit | Test 1 | | Test 2 | |
| Bandwidth | | | MHz | 10 | | | |
| Subcarrier spacing | | | kHz | 15 | | | |
| Duplex Mode | | |  | FDD | | | |
| SNR | | | dB | 9 | 10 | 15 | 16 |
| Propagation channel | | |  | TDLA30-5 | | | |
| Antenna configuration | | |  | 2×1 | | | |
| Correlation configuration | | |  | ULA high | | | |
| Beamforming Model | | |  | As specified in Annex B.4.1 | | | |
| BWP size | | | RB | 52 (PRB 0 to 51) | | | |
| PDSCH BW | | | RB | 15 (PRB 0 to 14) | | | |
| ZP CSI-RS configuration | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 4 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 5,(4) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 5,(9) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| CSI-RS  periodicity and offset | | slot | 10/5 | | | |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 2 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 3,(6) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 3,(13) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| NZP CSI-RS-timeConfig  periodicity and offset | | slot | 10/5 | | | |
| CSI-IM configuration | CSI-IM resource Type | |  | Periodic | | | |
| CSI-IM RE pattern | |  | 0 | | | |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) | |  | (4, 9) | | | |
| CSI-IM timeConfig  periodicity and offset | | slot | 10/5 | | | |
| ReportConfigType | | |  | Periodic | | | |
| CQI-table | | |  | Table 1 | | | |
| reportQuantity | | |  | cri-RI-PMI-CQI | | | |
| timeRestrictionForChannelMeasurements | | |  | Not configured | | | |
| timeRestrictionForInterferenceMeasurements | | |  | Not configured | | | |
| cqi-FormatIndicator | | |  | Wideband | | | |
| pmi-FormatIndicator | | |  | Wideband | | | |
| Sub-band Size | | | RB | 8 | | | |
| Csi-ReportingBand | | |  | 1111111 | | | |
| CSI-Report periodicity and offset | | | slot | 10/9 | | | |
| aperiodicTriggeringOffset | | |  | Not configured | | | |
| Codebook configuration | | Codebook Type |  | typeI-SinglePanel | | | |
| Codebook Mode |  | 1 | | | |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured | | | |
| CodebookSubsetRestriction |  | 000001 | | | |
| RI Restriction |  | N/A | | | |
| Physical channel for CSI report | | |  | PUCCH | | | |
| CQI/RI/PMI delay | | | ms | 10 | | | |
| Maximum number of HARQ transmission | | |  | 1 | | | |
| Measurement channel | | |  | As specified in Table A.4-6,  TBS.6-1 | | | |

Table 6.2.1.1.2.2-2: Minimum requirements

|  |  |  |
| --- | --- | --- |
| Parameters | Test 1 | Test 2 |
| *a* [%] | 20 | 20 |
| *g* | 1.05 | 1.05 |

**END OF CHANGE 2**

**START OF CHANGE 3**

6.2.1.2.1.2 Minimum requirement for periodic CQI reporting for RedCap enhancements

The purpose of the requirements for the eRedCap UE is to verify that the reported CQI values are in accordance with the CQI definition given in TS 38.214 [12]. The reporting accuracy of CQI under AWGN condition is determined by the reporting variance and BLER performance using the transport format indicated by the reported CQI median. To account for sensitivity of the input SNR the reporting definition is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.1.2.1.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) The reported CQI value according to the reference channel shall be in the range of ±1 of the reported median more than 90% of the time.

b) If the PDSCH BLER using the transport format indicated by median CQI is less than or equal to 0.1, then the BLER using the transport format indicated by the (median CQI+1) shall be greater than 0.1. If the PDSCH BLER using the transport format indicated by the median CQI is greater than 0.1, then the BLER using transport format indicated by (median CQI-1) shall be less than or equal to 0.1.

**Table 6.2.1.2.1.2-1: CQI reporting definition test**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Parameter** | | | **Unit** | **Test 1** | | **Test 2** | |
| Bandwidth | | | MHz | 20 | | | |
| Subcarrier spacing | | | kHz | 30 | | | |
| Duplex Mode | | |  | TDD | | | |
| TDD UL-DL pattern | | |  | FR1.30-1 | | | |
| SNR | | | dB | 5 | 6 | 11 | 12 |
| Propagation channel | | |  | AWGN | | | |
| Antenna configuration | | |  | 2×1 with static channel specified in Annex B.1 | | | |
| Beamforming Model | | |  | As specified in Annex B.4.1 | | | |
| BWP size | | | RB | 51 (PRB 0 to 50) | | | |
| PDSCH BW | | | RB | 7 (PRB 0 to 6) | | | |
| ZP CSI-RS configuration | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 4 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 5,(4) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 5,(9) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| CSI-RS  periodicity and offset | | slot | 10/1 | | | |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 2 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 3,(6) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 3,(13) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| NZP CSI-RS-timeConfig  periodicity and offset | | slot | 10/1 | | | |
| CSI-IM configuration | CSI-IM resource Type | |  | Periodic | | | |
| CSI-IM RE pattern | |  | 0 | | | |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) | |  | (4, 9) | | | |
| CSI-IM timeConfig  periodicity and offset | | slot | 10/1 | | | |
| ReportConfigType | | |  | Periodic | | | |
| CQI-table | | |  | Table 1 | | | |
| reportQuantity | | |  | cri-RI-PMI-CQI | | | |
| timeRestrictionForChannelMeasurements | | |  | Not configured | | | |
| timeRestrictionForInterferenceMeasurements | | |  | Not configured | | | |
| cqi-FormatIndicator | | |  | Wideband | | | |
| pmi-FormatIndicator | | |  | Wideband | | | |
| Sub-band Size | | | RB | 8 | | | |
| Csi-ReportingBand | | |  | 1111111 | | | |
| CSI-Report periodicity and offset | | | slot | 10/9 | | | |
| aperiodicTriggeringOffset | | |  | Not configured | | | |
| Codebook configuration | | Codebook Type |  | typeI-SinglePanel | | | |
| Codebook Mode |  | 1 | | | |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured | | | |
| CodebookSubsetRestriction |  | 000001 | | | |
| RI Restriction |  | N/A | | | |
| Physical channel for CSI report | | |  | PUCCH | | | |
| CQI/RI/PMI delay | | | ms | 9.5 | | | |
| Maximum number of HARQ transmission | | |  | 1 | | | |
| Measurement channel | | |  | As specified in Table A.4-6,  TBS.6-2 | | | |

**END OF CHANGE 3**

**START OF CHANGE 4**

###### 6.2.1.2.2.2 Minimum requirement for wideband CQI reporting for RedCap enhancements

The purpose of the requirements is to verify that the RedCap UE is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the reporting definition is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.1.2.2.2-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least *α*% of the time where *α*% is specified in Table 6.2.1.2.2.2-2;

b) The ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ *γ*, where *γ* is specified in Table 6.2.1.2.2.2-2;

c) When transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater than or equal to 0.02.

Table 6.2.1.2.2.2-1: Wideband CQI reporting test under frequency non-selective fading conditions

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | | | Unit | Test 1 | | Test 2 | |
| Bandwidth | | | MHz | 20 | | | |
| Subcarrier spacing | | | kHz | 30 | | | |
| Duplex Mode | | |  | TDD | | | |
| TDD UL-DL pattern | | |  | FR1.30-1 | | | |
| SNR | | | dB | 9 | 10 | 15 | 16 |
| Propagation channel | | |  | TDLA30-5 | | | |
| Antenna configuration | | |  | 2×1 | | | |
| Correlation configuration | | |  | ULA high | | | |
| Beamforming Model | | |  | As specified in Annex B.4.1 | | | |
| BWP size | | | RB | 51 (PRB 0 to 50) | | | |
| PDSCH BW | | | RB | 7 (PRB 0 to 6) | | | |
| ZP CSI-RS configuration | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 4 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 5,(4) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 5,(9) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| CSI-RS  periodicity and offset | | slot | 10/1 | | | |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 2 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 3,(6) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 3,(13) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| NZP CSI-RS-timeConfig  periodicity and offset | | slot | 10/1 | | | |
| CSI-IM configuration | CSI-IM resource Type | |  | Periodic | | | |
| CSI-IM RE pattern | |  | 0 | | | |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) | |  | (4, 9) | | | |
| CSI-IM timeConfig  periodicity and offset | | slot | 10/1 | | | |
| ReportConfigType | | |  | Periodic | | | |
| CQI-table | | |  | Table 1 | | | |
| reportQuantity | | |  | cri-RI-PMI-CQI | | | |
| timeRestrictionForChannelMeasurements | | |  | Not configured | | | |
| timeRestrictionForInterferenceMeasurements | | |  | Not configured | | | |
| cqi-FormatIndicator | | |  | Wideband | | | |
| pmi-FormatIndicator | | |  | Wideband | | | |
| Sub-band Size | | | RB | 8 | | | |
| Csi-ReportingBand | | |  | 1111111 | | | |
| CSI-Report periodicity and offset | | | slot | 10/9 | | | |
| aperiodicTriggeringOffset | | |  | Not configured | | | |
| Codebook configuration | | Codebook Type |  | typeI-SinglePanel | | | |
| Codebook Mode |  | 1 | | | |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured | | | |
| CodebookSubsetRestriction |  | 000001 | | | |
| RI Restriction |  | N/A | | | |
| Physical channel for CSI report | | |  | PUCCH | | | |
| CQI/RI/PMI delay | | | ms | 9.5 | | | |
| Maximum number of HARQ transmission | | |  | 1 | | | |
| Measurement channel | | |  | As specified in Table A.4-6,  TBS.6-2 | | | |

Table 6.2.1.2.2.2-2: Minimum requirements

|  |  |  |
| --- | --- | --- |
| Parameters | Test 1 | Test 2 |
| *a* [%] | 20 | 20 |
| *g* | 1.05 | 1.05 |

**END OF CHANGE 4**

**END OF CHANGE 5**

6.2.2.1.1.5 Minimum requirement for periodic CQI reporting for RedCap enhancements

For the parameters specified in Table 6.2.2.1.1.5-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements for the eRedCap UE are specified by the following:

a) The reported CQI value according to the reference channel shall be in the range of ±1 of the reported median more than 90% of the time.

b) If the PDSCH BLER using the transport format indicated by median CQI is less than or equal to 0.1, then the BLER using the transport format indicated by the (median CQI+1) shall be greater than 0.1. If the PDSCH BLER using the transport format indicated by the median CQI is greater than 0.1, then the BLER using transport format indicated by (median CQI-1) shall be less than or equal to 0.1.

**Table 6.2.2.1.1.5-1: CQI reporting definition test**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Parameter** | | | **Unit** | **Test 1** | | **Test 2** | |
| Bandwidth | | | MHz | 10 | | | |
| Subcarrier spacing | | | kHz | 15 | | | |
| Duplex Mode | | |  | FDD | | | |
| SNR | | | dB | 8 | 9 | 14 | 15 |
| Propagation channel | | |  | AWGN | | | |
| Antenna configuration | | |  | 2×2 with static channel specified in Annex B.1 | | | |
| Beamforming Model | | |  | As specified in Annex B.4.1 | | | |
| BWP size | | | RB | 52 (PRB 0 to 51) | | | |
| PDSCH BW | | | RB | 15 (PRB 0 to 14) | | | |
| ZP CSI-RS configuration | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 4 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 5,(4) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 5,(9) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| CSI-RS  periodicity and offset | | slot | 10/5 | | | |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type | |  | Periodic | | | |
| Number of CSI-RS ports (*X*) | |  | 2 | | | |
| CDM Type | |  | FD-CDM2 | | | |
| Density (ρ) | |  | 1 | | | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 3,(6) | | | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 3,(13) | | | |
| Frequency Occupation | | RB | 0 to 23 | | | |
| NZP CSI-RS-timeConfig  periodicity and offset | | slot | 10/5 | | | |
| CSI-IM configuration | CSI-IM resource Type | |  | Periodic | | | |
| CSI-IM RE pattern | |  | 0 | | | |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) | |  | (4, 9) | | | |
| CSI-IM timeConfig  periodicity and offset | | slot | 10/5 | | | |
| ReportConfigType | | |  | Periodic | | | |
| CQI-table | | |  | Table 1 | | | |
| reportQuantity | | |  | cri-RI-PMI-CQI | | | |
| timeRestrictionForChannelMeasurements | | |  | Not configured | | | |
| timeRestrictionForInterferenceMeasurements | | |  | Not configured | | | |
| cqi-FormatIndicator | | |  | Wideband | | | |
| pmi-FormatIndicator | | |  | Wideband | | | |
| Sub-band Size | | | RB | 8 | | | |
| Csi-ReportingBand | | |  | 1111111 | | | |
| CSI-Report periodicity and offset | | | slot | 10/9 | | | |
| aperiodicTriggeringOffset | | |  | Not configured | | | |
| Codebook configuration | | Codebook Type |  | typeI-SinglePanel | | | |
| Codebook Mode |  | 1 | | | |
| (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured | | | |
| CodebookSubsetRestriction |  | 010000 | | | |
| RI Restriction |  | N/A | | | |
| Physical channel for CSI report | | |  | PUCCH | | | |
| CQI/RI/PMI delay | | | ms | 10 | | | |
| Maximum number of HARQ transmission | | |  | 1 | | | |
| Measurement channel | | |  | As specified in Table A.4-6,  TBS.6-1 | | | |

**END OF CHANGE 5**

**START OF CHANGE 6**

###### 6.2.2.1.2.5 Minimum requirement for wideband CQI reporting for RedCap enhancements

The purpose of the requirements is to verify that the RedCap UE is tracking the channel variations and selecting the largest transport format possible according to the prevailing channel state for the frequency non-selective scheduling.

The reporting accuracy of CQI under frequency non-selective fading conditions is determined by the reporting variance, the relative increase of the throughput obtained when the transport format is indicated by the reported CQI compared to the throughput obtained when a fixed transport format is configured according to the reported median CQI, and a minimum BLER using the transport formats indicated by the reported CQI. To account for sensitivity of the input SNR the wideband CQI reporting under frequency selective fading conditions is considered to be verified if the reporting accuracy is met for at least one of two SNR levels separated by an offset of 1 dB.

For the parameters specified in Table 6.2.2.1.2.5-1 and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified by the following:

a) A CQI index not in the set {median CQI -1, median CQI, median CQI +1} shall be reported at least *α*% of the time where *α*% is specified in Table 6.2.2.1.2.5-2;

b) The ratio of the throughput obtained when transmitting the transport format indicated by each reported wideband CQI index and that obtained when transmitting a fixed transport format configured according to the wideband CQI median shall be ≥ *γ*, where *γ* is specified in Table 6.2.2.1.2.5-2;

c) When transmitting the transport format indicated by each reported wideband CQI index, the average BLER for the indicated transport formats shall be greater than or equal to 0.02.

Table 6.2.2.1.2.5-1: Wideband CQI reporting test under frequency non-selective fading conditions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | | | Unit | Test 1 | |
| Bandwidth | | | MHz | 10 | |
| Subcarrier spacing | | | kHz | 15 | |
| Duplex Mode | | |  | FDD | |
| SNR | | | dB | 6 | 7 |
| Propagation channel | | |  | TDLA30-5 | |
| Antenna configuration | | |  | 2×2 | |
| Correlation configuration | | |  | ULA high | |
| Beamforming Model | | |  | As specified in Annex B.4.1 | |
| BWP size | | | RB | 52 (PRB 0 to 51) | |
| PDSCH BW | | | RB | 15 (PRB 0 to 14) | |
| ZP CSI-RS configuration | CSI-RS resource Type | |  | Periodic | |
| Number of CSI-RS ports (*X*) | |  | 4 | |
| CDM Type | |  | FD-CDM2 | |
| Density (ρ) | |  | 1 | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 5,(4) | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 5,(9) | |
| Frequency Occupation | | RB | 0 to 23 | |
| CSI-RS  periodicity and offset | | slot | 10/5 | |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type | |  | Periodic | |
| Number of CSI-RS ports (*X*) | |  | 2 | |
| CDM Type | |  | FD-CDM2 | |
| Density (ρ) | |  | 1 | |
| First subcarrier index in the PRB used for CSI-RS (k0) | |  | Row 3,(6) | |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | Row 3,(13) | |
| Frequency Occupation | | RB | 0 to 23 | |
| NZP CSI-RS-timeConfig  periodicity and offset | | slot | 10/5 | |
| CSI-IM configuration | CSI-IM resource Type | |  | Periodic | |
| CSI-IM RE pattern | |  | 0 | |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) | |  | (4, 9) | |
| CSI-IM timeConfig  periodicity and offset | | slot | 10/5 | |
| ReportConfigType | | |  | Periodic | |
| CQI-table | | |  | Table 1 | |
| reportQuantity | | |  | cri-RI-PMI-CQI | |
| timeRestrictionForChannelMeasurements | | |  | Not configured | |
| timeRestrictionForInterferenceMeasurements | | |  | Not configured | |
| cqi-FormatIndicator | | |  | Wideband | |
| pmi-FormatIndicator | | |  | Wideband | |
| Sub-band Size | | | RB | 8 | |
| Csi-ReportingBand | | |  | 1111111 | |
| CSI-Report periodicity and offset | | | slot | 10/9 | |
| aperiodicTriggeringOffset | | |  | Not configured | |
| Codebook configuration | | Codebook Type |  | typeI-SinglePanel | |
|  | | Codebook Mode |  | 1 | |
|  | | (CodebookConfig-N1,CodebookConfig-N2) |  | Not configured | |
|  | | CodebookSubsetRestriction |  | 000001 | |
|  | | RI Restriction |  | N/A | |
| Physical channel for CSI report | | |  | PUCCH | |
| CQI/RI/PMI delay | | | ms | 10 | |
| Maximum number of HARQ transmission | | |  | 1 | |
| Measurement channel | | |  | As specified in Table A.4-6,  TBS.6-1 | |

Table 6.2.2.1.2.5-2: Minimum requirements

|  |  |
| --- | --- |
| Parameters | Test 1 |
| *a* [%] | 20 |
| *g* | 1.05 |

**END OF CHANGE 6**

**START OF CHANGE 7**

##### 6.3.1.1.2 Single PMI with 4TX TypeI-SinglePanel Codebook for eRedCap

For the parameters specified in Table 6.3.1.1.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.1.1.2-2.

Table 6.3.1.1.2-1: Test parameters (single layer)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | | Unit | Test 1 |
| Bandwidth | | MHz | 10 |
| Subcarrier spacing | | kHz | 15 |
| Duplex Mode | |  | FDD |
| Propagation channel | |  | TDLA30-5 |
| Antenna configuration | |  | High ULA 4 x 1 |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,(4) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | Row 5,(9) |
| Frequency Occupation | RB | 0 to 27 |
| CSI-RS  periodicity and offset | slot | 5/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 4,(0) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | Row 4,(13) |
| Frequency Occupation | RB | 0 to 27 |
| CSI-RS  periodicity and offset |  | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  periodicity and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Wideband |
| Sub-band Size | | RB | 8 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report periodicity and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 3 |
| CSI request | |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 6 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel (Note 4) | |  | R.PDSCH.1-6.5 FDD  R.PDSCH.1-3.2 HD-FDD |
| PDSCH & PDSCH DMRS Precoding configuration for random Precoding | |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, and with Wideband granularity |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-3), this reported PMI cannot be applied at the gNB downlink before slot#(n+3).  Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3.  Note 4: Applied reference channel depends on the supported operation mode: FDD or HD-FDD | | | |

Table 6.3.1.1.2-2: Minimum requirement

|  |  |
| --- | --- |
| Parameter | Test 1 |
| *g* | 1.3 |

**END OF CHANGE 7**

**START OF CHANGE 8**

##### 6.3.1.2.2 Single PMI with 4TX TypeI-SinglePanel Codebook for eRedCap

For the parameters specified in Table 6.3.1.2.2-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.1.2.2-2.

Table 6.3.1.2.2-1: Test parameters (single layer)

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Test 1** |
| Bandwidth | | MHz | 20 |
| Subcarrier spacing | | kHz | 30 |
| Duplex Mode | |  | TDD |
| TDD DL-UL configuration | |  | FR1.30-1 as specified in Annex A |
| Propagation channel | |  | TDLA30-5 |
| Antenna configuration | |  | High ULA 4 x 1 |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,(4) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | Row 5,(9) |
| Frequency Occupation |  | 0 to 23 |
| CSI-RS  periodicity and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 4,(0) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | Row 4,(13) |
| Frequency Occupation |  | 0 to 23 |
| CSI-RS  periodicity and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  periodicity and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Wideband |
| Sub-band Size | | RB | 8 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report periodicity and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 8 |
| CSI request | |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 5.5 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel | |  | R.PDSCH.2-8.6 TDD |
| PDSCH & PDSCH DMRS Precoding configuration for random Precoding | |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, and with Wideband granularity |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot #n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).  Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. | | | |

Table 6.3.1.2.2-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| *g* | 1.3 |

**END OF CHANGE 8**

**START OF CHANGE 9**

##### 6.3.2.1.10 Single PMI with 4TX TypeI-SinglePanel Codebook for eRedCap

For the parameters specified in Table 6.3.2.1.10-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.1.10-2.

Table 6.3.2.1.10-1: Test parameters (single layer)

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Test 1** |
| Bandwidth | | MHz | 10 |
| Subcarrier spacing | | kHz | 15 |
| Duplex Mode | |  | FDD |
| Propagation channel | |  | TDLA30-5 |
| Antenna configuration | |  | High XP 4 x 2  (N1,N2) = (2,1) |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,(4) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | Row 5,(9) |
| Frequency Occupation | RB | 0 to 27 |
| CSI-RS  periodicity and offset | slot | 5/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 4,(0) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | Row 4,(13) |
| Frequency Occupation | RB | 0 to 27 |
| CSI-RS  periodicity and offset |  | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  periodicity and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Wideband |
| Sub-band Size | | RB | 8 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report periodicity and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 4 for FDD  3 for HD-FDD |
| CSI request | |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 6 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel (Note 4) | |  | R.PDSCH.1-6.5 FDD  R.PDSCH.1-3.2 HD-FDD |
| PDSCH & PDSCH DMRS Precoding configuration for random Precoding | |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, and with Wideband granularity |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-3), this reported PMI cannot be applied at the gNB downlink before slot#(n+3).  Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3.  Note 4: Applied reference channel depends on the supported operation mode: FDD or HD-FDD. | | | |

Table 6.3.2.1.10-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| *g* | 1.3 |

**END OF CHANGE 9**

**START OF CHANGE 10**

##### 6.3.2.2.10 Single PMI with 4TX TypeI-SinglePanel Codebook for eRedCap

For the parameters specified in Table 6.3.2.2.10-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.2.10-2.

Table 6.3.2.2.10-1: Test parameters (single layer)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | | Unit | Test 1 |
| Bandwidth | | MHz | 20 |
| Subcarrier spacing | | kHz | 30 |
| Duplex Mode | |  | TDD |
| TDD DL-UL configuration | |  | FR1.30-1 as specified in Annex A |
| Propagation channel | |  | TDLA30-5 |
| Antenna configuration | |  | High XP 4 x 2  (N1,N2) = (2,1) |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 5,(4) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | Row 5,(9) |
| Frequency Occupation | RB | 0 to 23 |
| CSI-RS  periodicity and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0) |  | Row 4,(0) |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | Row 4,(13) |
| Frequency Occupation | RB | 0 to 23 |
| CSI-RS  periodicity and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  periodicity and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Wideband |
| Sub-band Size | | RB | 8 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report periodicity and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 8 |
| CSI request | |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 5.5 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel | |  | R.PDSCH.2-8.6 TDD |
| PDSCH & PDSCH DMRS Precoding configuration for random Precoding | |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, and with Wideband granularity |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot #n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).  Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. | | | |

Table 6.3.2.2.10-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| *g* | 1.3 |

**END OF CHANGE 10**