# Comments for final CRs

Please check the final CRs in ftp folder, and provide comments below.

## R1-240xxxx CR#3-3, Correction on guardband PRB handling

If you want to co-source, please add your company name in the list below:

|  |  |
| --- | --- |
| ***Source to WG:*** | Moderator (Huawei), vivo, Samsung |

If you have comments on the cover page, please provide in box below:

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Please add OPPO to co-source company |
| Samsung | Please add Samsung as a co-source company |

## R1-240xxxx CR#3-4, Correction on the determination of intra-cell guard band for SL-U

If you want to co-source, please add your company name in the list below:

|  |  |
| --- | --- |
| ***Source to WG:*** | Moderator (Huawei), CATT, CICTCI, Samsung |

If you have comments on the cover page, please provide in box below:

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Samsung | Please add Samsung as a co-source company. Also, the following change is needed for cover page “Reason for Change”. Intra-cell guard band can be determined according to the nominal manner as specified in TS 38.101-1 in addition to being configured by higher layer parameter. |
|  |  |

## R1-240xxxx CR#3-5, Correction on the frequency resource of a resource pool for SL-U

If you want to co-source, please add your company name in the list below:

|  |  |
| --- | --- |
| ***Source to WG:*** | Moderator (Huawei), CATT, CICTCI, NEC |

If you have comments on the cover page, please provide in box below:

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Please add OPPO to co-source company |
|  |  |

## R1-240xxxx CR#3-6, Correction on the highest sub-channel of PSSCH

If you want to co-source, please add your company name in the list below:

|  |  |
| --- | --- |
| ***Source to WG:*** | Moderator (Huawei), ZTE, Sanechips, Samsung |

If you have comments on the cover page, please provide in box below:

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Please add OPPO to co-source company |
| Samsung | Please add Samsung as a co-source company.Also the following changes are needed for the cover page “Reason for change”: If the higher layer parameter sl-TransmissionStructureForPSCCHandPSSCH is set to ‘contiguousRB', and if more than 1 sub-channel is used for PSSCH transmission, there are two cases as depicted in the figure below: |

## R1-240xxxx CR#4-2, Corrections on determination of PSFCH resources for a PSSCH

If you want to co-source, please add your company name in the list below:

|  |  |
| --- | --- |
| ***Source to WG:*** | Moderator (Huawei), Sharp, NEC, Samsung |

If you have comments on the cover page, please provide in box below:

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Please add OPPO to co-source company |
| Samsung | Please add Samsung as a co-source company The following changes are needed for cover page: Every sl-PSFCH-Type should be replaced by sl-TransmissionStructureForPSFCH |