**3GPP TSG-SA5 Meeting #155 *S5-242701rev1***

**Jeju, South Korea, 27 - 31 May 2024**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **32.271** | **CR** | **0023** | **rev** | **1** | **Current version:** | **18.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Add CDR generation and handling for converged charging of Ranging and Sidelink Positioning |
|  |  |
| ***Source to WG:*** | China Telecom |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | DUMMY |  | ***Date:*** | 2024-05-16 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | To support Ranging and Sidelink Positioning Charging, CDR generation and handling needs to be introduced. |
|  |  |
| ***Summary of change:*** | Add CDR generation and handling for Ranging and Sidelink Positioning |
|  |  |
| ***Consequences if not approved:*** | Charging for Ranging and Sidelink Positioning will not be supported |
|  |  |
| ***Clauses affected:*** | 5.x.3 (new), 5.x.4 (new), 5.x.5 (new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

### 5.x.3 CDR generation

#### 5.x.3.1 Introduction

The CHF CDRs for Ranging and Sidelink Positioning charging are generated by the CHF to collect charging information that they subsequently transfer to the Charging Gateway Function (CGF).

The following clauses describe in details the conditions for generating, opening and closing the CHF CDR, which shall be supported by the CHF.

#### 5.x.3.2 Triggers for CHF CDR

##### 5.x.3.2.1 General

A CHF CDR is used to collect charging information related to Ranging and Sidelink Positioning chargeable events for PEC.

##### 5.x.3.2.2 Triggers for CHF CDR generation

A CHF CDR is generated by the CHF for each received Charging Data Request[Event].

### 5.x.4 Ga record transfer flows

Details of the Ga protocol application are specified in TS 32.295 [54].

### 5.x.5 Bl CDR file transfer

Details of the Bl protocol application are specified in TS 32.297 [52].

|  |
| --- |
| **End of changes** |