**3GPP TSG-SA5 Meeting #155 *S5-243038***

**Jeju, South Korea, 27 - 31 May 2024**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **32.254** | **CR** | **0051** | **rev** | **1** | **Current version:** | **18.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |
| --- | --- |
| ***Title:***  | Rel-18 CR 32.254 Correction of charging information applicability |
|  |  |
| ***Source to WG:*** | Ericsson LM |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | TEI18 |  | ***Date:*** | 2024-05-17 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The charging data request doesn’t contain all applicable information elements |
|  |  |
| ***Summary of change:*** | Adding missing information elements and removing not applicable. |
|  |  |
| ***Consequences if not approved:*** | Not included information elements may be interpreted as not applicable and which may lead to interoperability issues. |
|  |  |
| ***Clauses affected:*** | 6.2a.1.2.1 and 6.2a.1.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of S5-242789 |

|  |
| --- |
| **First change** |

##### 6.2a.1.2.1 Charging Data Request message

Table 6.2a.1.2.1.1 illustrates the basic structure of a Charging Data Request message as used for NEF converged charging.

Table 6.2a.1.2.1.1: Charging Data Request message contents

|  |  |  |
| --- | --- | --- |
| **Information Element** | **Category** | **Description** |
| Session Identifier | OC | Described in TS 32.290 [57] |
| Subscriber Identifier | OM | Described in TS 32.290 [57], and holds the identifier of the AF |
| NF Consumer Identification | M | Described in TS 32.290 [57] |
| NF Functionality | M | Described in 3GPP TS 32.290 [6]. |
| NF Name | OC | Described in 3GPP TS 32.290 [6]. |
| NF Address | OC | Described in 3GPP TS 32.290 [6]. |
| NF PLMN ID | OC | Described in 3GPP TS 32.290 [6]. |
| Charging Identifier | OM | Described in TS 32.290 [57] |
| Invocation Timestamp | M | Described in TS 32.290 [57] |
| Invocation Sequence Number | M | Described in TS 32.290 [57] |
| One-time Event | OC | Described in TS 32.290 [57]. |
| One-time Event Type | OC | Described in TS 32.290 [57]. |
|  |  |  |
|  |  |  |
|  |  |  |
| Notify URI | - | This field is only applicable for the notification of abort charging. |
| Supported Features | OC | Described in TS 32.290 [57] |
| Service Specification Information | OC | Described in TS 32.290 [57] |
| Triggers | OC | This field is described in TS 32.290 [57] and holds the NEF specific triggers described in clause 5.4.1.2  |
| Multiple Unit Usage | OC | This field contains the parameters for the quota management request and/or usage reporting. |
| Rating Group | M | Described in TS 32.290 [57] |
| Requested Unit | OC | Described in TS 32.290 [57] |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| Used Unit Container | OC | Described in TS 32.290 [57] |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| Total Volume | OC | Described in TS 32.290 [57] |
| Uplink Volume | OC | Described in TS 32.290 [57] |
| Downlink Volume | OC | Described in TS 32.290 [57] |
|  |  |  |
|  |  |  |
|  |  |  |
| NEF API Charging Information | OM | This field holds the NEF API specific information described in clause 6.3.1.4 |

##### 6.2a.1.2.2 Charging Data Response message

Table 6.2a.1.2.2.1 illustrates the basic structure of a Charging Data Response message as used for NEF converged charging.

Table 6.2a.1.2.2.1: Charging Data Response message content

|  |  |  |
| --- | --- | --- |
| **Information Element** | **Category** | **Description** |
| Session Identifier | OC | Described in TS 32.290 [57] |
| Invocation Timestamp | M | Described in TS 32.290 [57] |
| Invocation Result | OC | Described in TS 32.290 [57] |
| Invocation Result Code | OC | Described in TS 32.290 [57] |
| Failed parameter | OC | Described in TS 32.290 [57] |
| Failure Handling | OC | Described in TS 32.290 [57] |
| Invocation Sequence Number | M | Described in TS 32.290 [57] |
| Session Failover | OC | Described in TS 32.290 [57] |
| Supported Features | OC | Described in TS 32.290 [57] |
|  |  |  |
| Multiple Unit Information | OC | This field holds the parameters for the quota management information. |
| Result Code | OC | Described in TS 32.290 [57] |
| Rating Group | OM | Described in TS 32.290 [57] |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| Validity Time | OC | Described in TS 32.290 [57] |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |
| --- |
| **End of changes** |