**3GPP TSG-SA5 Meeting #155 *S5-242852rev1***

**Jeju, South Korea, 27 - 31 May 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Rel-18 CR TS 32.255 Update scenario of clause 5.2.2.22 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | MATRIXX Software | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NETSLICE\_CH\_Ph2 | | | | |  | ***Date:*** | | | 2024-05-13 |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Clause 5.2.2.22 describes a scenario of UE PDU session charging based on Business converged charging. In this scenario, charging information are exchanged between the C-CHF and the B-CHF for the purpose of UE PDU session charging. However using Charging Data Request/Response between the C-CHF and the B-CHF implies additional charging for the UE PDU session. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Remove Charging Data Request/Response between C-CHF and B-CHF in flow of Figure 5.2.2.22.2-1, and leave the exchange unspecified for this release. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Charging UE PDU session twice. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2.2.22.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Revision of S5-242852 | | | | | | | | |

|  |
| --- |
| **First change** |

##### 5.2.2.22.2 PDU session establishment

The following figure 5.2.2.22.2-1 describes a UE PDU session converged influenced by business converged charging:



Figure 5.2.2.22.2-1: UE PDU session converged Charging influenced by business charging

0ch. Business charging information obtained by B-CHF from NWDAF, MnS Producer, NSACF, which could be e.g:

- S-NSSAI service profile: e.g. "Max nb of PDU sessions", "Max nb of UEs”, "Duration of the slice"…

- S-NSSAI KPIs;

- load level.

1 to 9ch-b. PDU session establishment for individual UE per Figure 5.2.2.2.2-1.

9ch-aa. UE PDU session charging needs input from business charging

9ch-ab. C-CHF sends a request to B-CHF, and receives charging information from B-CHF.

The messages exchange between C-CHF and B-CHF for this scenario is not specified in this release of the specification.

9ch-ac. Account, Rating and reservation control for individual UE based on "business charging information" received from B-CHF.

9ch-c. C-CHF provides appropriate answer for the individual UE.

|  |
| --- |
| **End of change** |