**3GPP TSG CT WG3 Meeting #135 *C3-243160r1***

**Hyderabad, IN, 27 - 31 May, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **29.122** | **CR** | **0843** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Completion of re-used data types table |
|  |  |
| ***Source to WG:*** | ZTE, Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | XRM |  | ***Date:*** | 2024-05-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | The following data types are missing in Table 5.14.2.1.1-1:* DurationMilliSec
* DurationMilliSecRm
* ProtocolDescriptionRm
 |
|  |  |
| ***Summary of change:*** | Add the missing data types above to Table 5.14.2.1.1-1. |
|  |  |
| ***Consequences if not approved:*** | Table 5.14.2.1.1-1 is incomplete. |
|  |  |
| ***Clauses affected:*** | 5.14.2.1.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not have any impact in the OpenAPI specification. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.14.2.1.1 Introduction

This clause defines data structures to be used in resource representations, including subscription resources.

Table 5.14.2.1.1-1 specifies data types re-used by the AsSessionWithQoS API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the AsSessionWithQoS API.

Table 5.14.2.1.1-1: AsSessionWithQoS API re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AcceptableServiceInfo | 3GPP TS 29.514 [52] | Acceptable maximum requested bandwidth. |  |
| AlternativeServiceRequirementsData | 3GPP TS 29.514 [52] | Contains alternative QoS related parameters and a reference to them. |  |
| AverWindow | 3GPP TS 29.571 [45] | Averaging Window. | EnQoSMon |
| AverWindowRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "AverWindow" data type, but with the OpenAPI "nullable: true" property. | EnQoSMon |
| BatOffsetInfo | 3GPP TS 29.514 [52] | Contains the offset of the BAT and the optionally adjusted periodicity. | EnTSCAC |
| BitRate | 3GPP TS 29.571 [45] | String representing a bit rate that shall be formatted as follows:Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$'Examples:"125 Mbps", "0.125 Gbps", "125000 Kbps" | EnQoSMon, ListUE\_5G |
| BitRateRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "BitRate" data type, but with the OpenAPI "nullable: true" property. |  |
| Dnn | 3GPP TS 29.571 [45] | Identifies a DNN. |  |
| DurationMilliSec | 3GPP TS 29.514 [52] | Indicates the time interval in units of milliseconds. | PowerSaving |
| DurationMilliSecRm | 3GPP TS 29.514 [52] | This data type is defined in the same way as the "DurationMilliSec" data type, but with the OpenAPI "nullable: true" property. | PowerSaving |
| EthFlowDescription | 3GPP TS 29.514 [52] | Defines a packet filter for an Ethernet flow.(NOTE 1) | EthAsSessionQoS\_5G, GMEC\_5G |
| EventsSubscReqData | 3GPP TS 29.514 [52] | Identifies the events the application subscribes to. | EnQoSMon |
| EventsSubscReqDataRm | 3GPP TS 29.514 [52] | This data type is defined in the same way as the "EventsSubscReqData" data type, but with the OpenAPI "nullable: true" property | EnQoSMon |
| ExtMaxDataBurstVol | 3GPP TS 29.571 [45] | Unsigned integer indicating Maximum Data Burst Volume (see clauses 5.7.3.7 and 5.7.4 of 3GPP TS 23.501 [8]), expressed in Bytes.Minimum = 4096. Maximum = 2000000. |  |
| ExtMaxDataBurstVolRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "ExtMaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. |  |
| ExternalGroupId | 5.2.1.3.2 | Represents an external group identifier. | GMEC\_5G |
| Gpsi | 3GPP TS 29.571 [45] | Represents a GPSI. | GMEC\_5G |
| IpAddr | 3GPP TS 29.571 [45] | UE IP Address. | ListUE\_5G |
| MacAddr48 | 3GPP TS 29.571 [45] | MAC Address. | EthAsSessionQoS\_5G, enNB |
| MediaType | 3GPP TS 29.514 [52] | Indicates the media type of a single-modal data flow of a multi-modal service. | MultiMedia |
| MultiModalId | 3GPP TS 29.514 [52] | Represents multi-modal service identifier.  | MultiMedia |
| PacketDelBudget | 3GPP TS 29.571 [45] | Unsigned integer indicating Packet Delay Budget (see clauses 5.7.3.4 and 5.7.4 of 3GPP TS 23.501 [8])), expressed in milliseconds.Minimum = 1. | TSC\_5G, XRM\_5G |
| PacketDelBudgetRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "PacketDelBudget" data type, but with the OpenAPI "nullable: true" property. | TSC\_5G, MultiMedia |
| PacketErrRate | 3GPP TS 29.571 [45] | String representing Packet Error Rate (see clauses 5.7.3.5 and 5.7.4 of 3GPP TS 23.501 [8]), expressed as a "*scalar* x 10-k" where the scalar and the *exponent k are each encoded as one decimal digit*.Pattern: '^([0-9]E-[0-9])$'Examples:Packer Error Rate 4x10-6 shall be encoded as "4E-6".Packer Error Rate 10-2 shall be encoded as "1E-2". | ExtQoS\_5G |
| PacketErrRateRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "PacketErrRate" data type, but with the OpenAPI "nullable: true" property. | ExtQoS\_5G |
| PdvMonitoringReport | 3GPP TS 29.514 [52] | Represents a PDV monitoring report. | EnQoSMon |
| PeriodicityInfo | 3GPP TS 29.514 [52] | Indicates the time period between the start of the two data bursts in Uplink and/or Downlink direction. | PowerSaving |
| PduSetQosPara | 3GPP TS 29.571 [45] | Represents the PDU Set level QoS parameters. | PDUSetHandling |
| PduSetQosParaRm | 3GPP TS 29.571 [45] | Represents the PDU Set level QoS parameters to be modified. | PDUSetHandling |
| PlmnIdNid | 3GPP TS 29.571 [45] | Identifies the network: the PLMN Identifier (the mobile country code and the mobile network code) or the SNPN Identifier (the PLMN Identifier and the NID). | enNB\_5G |
| Port | 5.2.1.3.2 | Unsigned integer with valid values between 0 and 65535 representing a port. | ListUE\_5G |
| ProblemDetails | 5.2.1.2.12 | Problem Details when returning an error response. |  |
| ProtocolDescription | 3GPP TS 29.571 [45] | Represents Protocol description of the media flow | PDUSetHandlingPowerSaving |
| ProtocolDescriptionRm | 3GPP TS 29.571 [45] | Represents the same as the "ProtocolDescription" data type, but with the OpenAPI "nullable: true" property. | PDUSetHandlingPowerSaving |
| RatType | 3GPP TS 29.571 [45] | Identifies the RAT Type. | enNB\_5G |
| ReportingFrequency | 3GPP TS 29.512 [8] | Indicates the frequency for the reporting, such as event triggeredand/or periodic. (NOTE 2) |  |
| RequestedQosMonitoringParameter | 3GPP TS 29.512 [8] | Indicates the QoS information to be measured, e.g.UL packet delay, DL packet delay or round trip packet delay between the UE and the UPF is to be monitored when the QoS Monitoring for packet delay is enabled for the service data flow. (NOTE 2) |  |
| ServAuthInfo | 3GPP TS 29.514 [52] | The authorization result of a request for QoS / QoS monitoring. | EnQoSMon |
| Snssai | 3GPP TS 29.571 [45] | Identifies the S-NSSAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [45] | Used to negotiate the applicability of the optional features defined in table 5.14.4-1. |  |
| TemporalInValidity | 3GPP TS 29.565 [72] | Represents the temporal invalidity related information. | GMEC\_5G |
| TscaiInputContainer | 3GPP TS 29.514 [52] | TSCAI Input information container. | TSC\_5G, MultiMedia, GMEC\_5G |
| TscPriorityLevel | 3GPP TS 29.514 [52] | Represents priority of TSC Flows. | TSC\_5G, MultiMedia, GMEC\_5G |
| TscPriorityLevelRm | 3GPP TS 29.514 [52] | Represents the same as the TscPriorityLevel data type, but with the OpenAPI "nullable: true" property. | TSC\_5G, MultiMedia, GMEC\_5G |
| TsnQosContainer | 3GPP TS 29.514 [52] | Represents individual QoS parameters  | MultiMedia |
| TsnQosContainerRm | 3GPP TS 29.514 [52] | Represents the same as the TsnQosContainer data type, but with the OpenAPI "nullable: true" property. | MultiMedia |
| Uinteger | 3GPP TS 29.571 [45] | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible.Minimum = 0. |  |
| UintegerRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "Uinteger" data type, but with the OpenAPI "nullable: true" property. |  |
| UplinkDownlinkSupport | 3GPP TS 29.514 [52] | Provides L4S support information. | L4S, GMEC\_5G |
| NOTE 1: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange\_5G as specified in clause 5.14.4 shall be supported.NOTE 2: In order to support QoS Monitoring, feature QoSMonitoring\_5G as specified in clause 5.14.4 shall be supported. |  |

Table 5.14.2.1.1-2 specifies the data types defined for the AsSessionWithQoS API.

Table 5.14.2.1.1-2: AsSessionWithQoS API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| AdditionalInfoAsSessionWithQos | 5.14.2.1.10 | Describes additional error information specific for this API. |  |
| AsSessionWithQoSSubscription | 5.14.2.1.2 | Represents an individual AS session with required QoS subscription resource. |  |
| AsSessionWithQoSSubscriptionPatch | 5.14.2.1.3 | Represents parameters to modify an AS session with specific QoS subscription. |  |
| AsSessionMediaComponent | 5.14.2.1.13 | Represents media component data for a multi-modal service. It contains service data flow information for a single modal data flow of a multi-modal service. | MultiMedia |
| AsSessionMediaComponentRm | 5.14.2.1.14 | Represents the same as the AsSessMediaComponent data type but with the "nullable: true" property. | MultiMedia |
| MultiModalFlows | 5.14.2.1.15 | Represents flow information within a single-modal data flow for a multi-modal service. | MultiMedia |
| ProblemDetailsAsSessionWithQos | 5.14.2.1.11 | ProblemDetails as defined in clause 5.2.12.12 extended with specific error information for this API, as described in AdditionalInfoAsSessionWithQos. |  |
| QosMonitoringInformation | 5.14.2.1.6 | Represents QoS monitoring information. | QoSMonitoring\_5G |
| QosMonitoringInformationRm | 5.14.2.1.7 | Represents the same as the QosMonitoringInformation data type but with the "nullable: true" property. | QoSMonitoring\_5G |
| QosMonitoringReport | 5.14.2.1.8 | Represents a QoS monitoring report. | QoSMonitoring\_5G |
| TscQosRequirement | 5.14.2.1.9 | Represents QoS requirements for time sensitive communication. | TSC\_5G, XRM\_5G, GMEC\_5G |
| TscQosRequirementRm | 5.14.2.1.10 | Represents the same as the TscQosRequirement data type but with the "nullable: true" property. | TSC\_5G, XRM\_5G, GMEC\_5G |
| UserPlaneEvent | 5.14.2.2.3 | Represents the user plane event. | enNB, GMEC\_5G |
| UserPlaneEventReport | 5.14.2.1.5 | Represents an event report for user plane. | enNB, GMEC\_5G |
| UserPlaneNotificationData | 5.14.2.1.4 | Represents the parameters to be conveyed in a user plane event(s) notification. | enNB, GMEC\_5G |
| UeAddInfo | 5.14.2.1.16 | Represents the UE address information. | ListUE\_5G |

\*\*\* End of Changes \*\*\*