**3GPP TSG RAN WG1 #118 R1-24nnnnn**

**Maastricht, NL, August 19th – 23rd, 2024**

**Source: Ad-Hoc Chair (AT&T)**

**Title: Session Notes of AI 8.2.2**

**Agenda Item:** **8.2.2**

**Document for:** **Endorsement**

### 8.2.2 UE features for other Rel-18 work items (Topics B)

*Including UE features for NR MIMO, expanded and improved NR positioning, NES, mobility enhancement, NCR, IoT-NTN, NR-NTN, and BWP without restriction.*

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 42. Netw\_Energy\_NR | 42-1 | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for periodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35 | Yes |  | UE does not support spatial domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2b and components 3~6 in FG 42-2a and 42-2c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1a | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUSCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUSCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35, 2-32b | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUSCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1a and 42-1c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1a and 42-1c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1a and 42-1c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1c | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUCCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35, 2-32a | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations.  Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1a and 42-1c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1a and 42-1c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1a and 42-1c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1b | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35 | Yes |  | UE does not support spatial domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11,12}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2 | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35 | Yes |  | UE does not support power domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 2 candidate value: {2,3,4}Component 4 candidate value: {1, 2, 3 … 32}Component 5 candidate value: {8, 16, 24, … 128 }Component 6 candidate value: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2a | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUSCH | Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for semi-persistent CSI reporting1. The max number of sub-configurations Lmax in one CSI report configuration on PUSCH2. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.3. Supported maximum number of simultaneous NZP-CSI-RS resources per CC4. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs6. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Support of single-panel type 1 codebook8. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35, 2-32b | Yes |  | UE does not support power domain adaptation for semi-persistent CSI reporting on PUSCH | Per band | No | No | N/A | Component 1 candidate values: {2,3,4,5,6,7,8}Component 2 candidate values: {2,3,4}Component 3 candidate values: {1, 2, 3 … 32}Component 4 candidate values: {8, 16, 24, … 128 }Component 5 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 6 candidate values: {8, 16, 24, …, 248, 256}Component 8 candidate values: {2, 3, 4,5,6,7,8,9,10,11,12}Note: Components 5 and 6 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-2a and 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-2a and 42-2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-2a and 42-2c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2c | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for semi-persistent CSI reporting on PUCCH1. The max number of sub-configurations Lmax in one CSI report configuration2. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.3. Supported maximum number of simultaneous NZP-CSI-RS resources per CC4. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs6. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Support of single-panel type 1 codebook8. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35, 2-32a | Yes |  | UE does not support power domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {2,3,4}Component 2 candidate values: {2,3,4}Component 3 candidate values: {1, 2, 3 … 32}Component 4 candidate values: {8, 16, 24, … 128}Component 5 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 6 candidate values: {8, 16, 24, …, 248, 256}Component 8 candidate values: {2, 3, 4}Note: Components 5 and 6 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-2a and 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-2a and 42-2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-2a and 42-2c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2b | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | ~~FFS~~ 2-35 | Yes |  | UE does not support power domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128 }Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-8 | simultaneousCSI-SubReportsPerCC-r18 | Indicates the number of CSI report(s) for which the UE can measure and process reference signals simultaneously in a CC of the band for which this capability is provided. The CSI report comprises periodic, semi-persistent and aperiodic CSI and any latency classes and codebook types. The CSI report in *simultaneousCSI-SubReportsPerCC-r18* includes the beam report, and CSI report without sub-configurations plus CSI sub-report across CSI reports | ~~FFS~~ 2-35 | Yes |  | UE does not support spatial or power domain adaptation for CSI reporting | Per Band | No | No | N/A | Component 1 candidate values: {1, 2, 3, 4, 5, 6, 7, 8}Note: UE shall report the value in this feature group being equal to or larger than that in *simultaneousCSI-ReportsPerCC*Note: UE supporting at least one of FG 42-1/1a/1b/1c/2/2a/2b/2c shall report this FG | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-9 | simultaneousCSI-SubReportsAllCC-r18 | Indicates whether the UE supports CSI report framework and the number of CSI report(s) which the UE can simultaneously process across all CCs, and across MCG and SCG in case of NR-DC. The CSI report comprises periodic, semi-persistent and aperiodic CSI and any latency classes and codebook types. The CSI report in *simultaneousCSI-SubReportsAllCC-r18* includes the beam report, and CSI report without sub-configurations plus CSI sub-report across CSI reports. This parameter may further limit *simultaneousCSI-SubReportsPerCC-r18* in MIMO-ParametersPerBand and Phy-ParametersFRX-Diff for each band in a given band combination | ~~FFS~~ 2-35 | Yes |  | UE does not support spatial or power domain adaptation for CSI reporting | Per BC | No | No | N/A | Component 1 candidate values: {5, 6, 7, ..., 32}Note: UE shall report the value in this feature group being equal to or larger than that in *simultaneousCSI-ReportsAllCC*Note: UE supporting at least one of FG 42-1/1a/1b/1c/2/2a/2b/2c shall report this FG | Optional with capability signaling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 42. Netw\_Energy\_NR | 42-1 | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for periodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support spatial domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2b and components 3~6 in FG 42-2a and 42-2c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FG 42-1 and FG 42-2, and if the UE is configured with CSI report settings with sub-configurations corresponding to both FG 42-1 and 42-2, then the supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1 and 42-2. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1b | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support spatial domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11,12}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1b and FG 42-2b, and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1b and 42-2b, then the supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1b and 42-2b. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2 | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support power domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 2 candidate value: {2,3,4}Component 4 candidate value: {1, 2, 3 … 32}Component 5 candidate value: {8, 16, 24, … 128 }Component 6 candidate value: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FG 42-1 and FG 42-2, and if the UE is configured with CSI report settings with sub-configurations corresponding to both FG 42-1 and 42-2, then the supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1 and 42-2. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2b | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support power domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128 }Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1b and FG 42-2b, and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1b and 42-2b, then the supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1b and 42-2b. | Optional with capability signaling |

**Agreement: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 42. Netw\_Energy\_NR | 42-1 | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for periodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support spatial domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to all sub-configuration that contain~~s~~ one port subsetNote: SD-type2 refers to all sub-configuration that contain~~s~~ list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2b and components 3~6 in FG 42-2a and 42-2c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1a | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUSCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUSCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUSCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to all sub-configuration that contain~~s~~ one port subsetNote: SD-type2 refers to all sub-configuration that contain~~s~~ list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1a and 42-1c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1a and 42-1c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1a and 42-1c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1c | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUCCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to all sub-configuration that contain~~s~~ one port subsetNote: SD-type2 refers to all sub-configuration that contain~~s~~ list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations.  Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1a and 42-1c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1a and 42-1c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1a and 42-1c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1b | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | FFS | Yes |  | UE does not support spatial domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to all sub-configuration that contain~~s~~ one port subsetNote: SD-type2 refers to all sub-configuration that contain~~s~~ list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11,12}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset. | Optional with capability signaling |



**Proposal: With regards to FG 41-1-7a and FG 41-1-7b, consider the following options:**

* **Option 1: Remove component 3 from both FGs, since there is no corresponding feature specified in SLPP**
* **Option 2: Send an LS to RAN2 to inform them that this UE capability component has been specified, but there is no corresponding report specified in the ProvideLocationInformation message of TDOA and TOA methods.**

**Proposal: To address the absence of a number of ARP-IDs the device supports, introduce a new component in FG 41-1-19a:**

* **Add a new component in FG 41-1-19a, “Maximum number of Rx ARP-IDs it supports”, with values {1,2,3,4}**

**Proposal: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 41. NR\_pos\_enh2 | 41-5-2a | Support of positioning SRS with Tx frequency hopping in RRC\_INACTIVE for RedCap UEs | 1. Maximum SRS bandwidth across all hops2. Maximum number of hops3. RF Tx retuning time between consecutive hops4. Switching time between active BWP and frequency hop5. Overlapping PRB(s) between adjacent hops6. Support of {0,1,2,4} overlapping PRB(s) between adjacent hops7. Maximum number of positioning SRS resources with Tx frequency hopping | 27-15b~~, one of {28-1,48-1}~~ | Yes | n/a | Positioning SRS with Tx hopping in RRC\_INACTIVE is not supported | Per band | n/a | n/a | n/a | Component 1 candidate values:FR1: {40, 50, 80, 100, 200, 300}FR2: {100, 200, 400}Component 2 candidate values: {2,3,4,5,6}Component 3 candidate values:FR1: {70us, 140us, 210us}FR2: {35us, 70us, 140us}Component 4 candidate values:{100us, 140us, 200us, 300us, 500us}Component 7 candidate values:Periodic: {1,2,4,8,16,32,64}Semi-persistent: {0,1,2,4,8,16,32,64}Note: No additional UE requirements shall be specified for the case of Tx hopping with non-overlapping hops compared to the case of Tx hopping with overlapping hops, e.g., a UE is not responsible for keeping phase continuity across the hops in either case of overlapping or non-overlapping hopsNeed for location server to know if the feature is supported | Optional with capability signalling |

**Proposal: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 42. Netw\_Energy\_NR | 42-1a | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUSCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUSCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32b | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUSCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports ~~both~~ more than one FG from FGs 42-1a/1c and 42-~~1~~2a/2c and if the UE is configured with CSI report settings with sub-configurations corresponding to ~~both~~ a subset of the reported FGs 42-1a/1c and 42-~~1~~2a/2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from that subset ~~both FGs 42-1a and 42-1c~~. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1c | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUCCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32a | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations.  Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports ~~both~~ more than one FG from FGs 42-1a/1c and 42-~~1~~2a/2c and if the UE is configured with CSI report settings with sub-configurations corresponding to ~~both~~ a subset of the reported FGs 42-1a/1c and 42-~~1~~2a/2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from that subset ~~both FGs 42-1a and 42-1c~~. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2a | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUSCH | Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for semi-persistent CSI reporting1. The max number of sub-configurations Lmax in one CSI report configuration on PUSCH2. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.3. Supported maximum number of simultaneous NZP-CSI-RS resources per CC4. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs6. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Support of single-panel type 1 codebook8. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32b | Yes |  | UE does not support power domain adaptation for semi-persistent CSI reporting on PUSCH | Per band | No | No | N/A | Component 1 candidate values: {2,3,4,5,6,7,8}Component 2 candidate values: {2,3,4}Component 3 candidate values: {1, 2, 3 … 32}Component 4 candidate values: {8, 16, 24, … 128 }Component 5 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 6 candidate values: {8, 16, 24, …, 248, 256}Component 8 candidate values: {2, 3, 4,5,6,7,8,9,10,11,12}Note: Components 5 and 6 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports ~~both~~ more than one FG from FGs 42-~~2~~1a/1c and 42-2a/2c and if the UE is configured with CSI report settings with sub-configurations corresponding to ~~both~~ a subset of the reported FGs 42-~~2~~1a/1c and 42-2a/2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from that subset ~~both FGs 42-2a and 42-2c~~. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2c | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for semi-persistent CSI reporting on PUCCH1. The max number of sub-configurations Lmax in one CSI report configuration2. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.3. Supported maximum number of simultaneous NZP-CSI-RS resources per CC4. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs6. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Support of single-panel type 1 codebook8. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32a | Yes |  | UE does not support power domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {2,3,4}Component 2 candidate values: {2,3,4}Component 3 candidate values: {1, 2, 3 … 32}Component 4 candidate values: {8, 16, 24, … 128}Component 5 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 6 candidate values: {8, 16, 24, …, 248, 256}Component 8 candidate values: {2, 3, 4}Note: Components 5 and 6 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports ~~both~~ more than one FG from FGs 42-~~2~~1a/1c and 42-2a/2c and if the UE is configured with CSI report settings with sub-configurations corresponding to ~~both~~ a subset of the reported FGs 42-~~2~~1a/1c and 42-2a/2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from that subset ~~both FGs 42-2a and 42-2c~~. | Optional with capability signaling |

**Proposal: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 42. Netw\_Energy\_NR | 42-1c | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUCCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32a | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations.  Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1a and 42-1c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1a and 42-1c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1a and 42-1c.Note: The value reported for Components 2 and 3 is no larger than the value reported for Components 2 and 3 in FG 42-1a (if supported), respectively. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2c | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for semi-persistent CSI reporting on PUCCH1. The max number of sub-configurations Lmax in one CSI report configuration2. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.3. Supported maximum number of simultaneous NZP-CSI-RS resources per CC4. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs6. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Support of single-panel type 1 codebook8. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32a | Yes |  | UE does not support power domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {2,3,4}Component 2 candidate values: {2,3,4}Component 3 candidate values: {1, 2, 3 … 32}Component 4 candidate values: {8, 16, 24, … 128}Component 5 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 6 candidate values: {8, 16, 24, …, 248, 256}Component 8 candidate values: {2, 3, 4}Note: Components 5 and 6 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-2a and 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-2a and 42-2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-2a and 42-2c.Note: The value reported for Components 2 and 3 is no larger than the value reported for Components 2 and 3 in FG 42-2a (if supported), respectively. | Optional with capability signaling |

**Proposal: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 42. Netw\_Energy\_NR | 42-1 | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for periodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | 2-35 | Yes |  | UE does not support spatial domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2b and components 3~6 in FG 42-2a and 42-2c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE does not report only type 1 or only type 2 for components 4~7 in both FGs 42-1 and 42-1b and if the UE is configured with CSI report settings with sub-configurations corresponding to both SD-type 1 and SD-type 2, then the supported total number of NZP-CSI-RS resources/ports is determined by the minimum of the reported values for both SD-type 1 and SD-type 2. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1b | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | 2-35 | Yes |  | UE does not support spatial domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11,12}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports is determined by the minimum of the reported values from that subset.Note: If a UE does not report only type 1 or only type 2 for components 4~7 in both FGs 42-1 and 42-1b and if the UE is configured with CSI report settings with sub-configurations corresponding to both SD-type 1 and SD-type 2, then the supported total number of NZP-CSI-RS resources/ports is determined by the minimum of the reported values for both SD-type 1 and SD-type 2. | Optional with capability signaling |

**Proposal: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 42. Netw\_Energy\_NR | 42-1 | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for periodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | 2-35 | Yes |  | UE does not support spatial domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2b and components 3~6 in FG 42-2a and 42-2c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1a | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUSCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUSCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32b | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUSCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1a and 42-1c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1a and 42-1c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1a and 42-1c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1c | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for semi-persistent CSI reporting on PUCCH2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32a | Yes |  | UE does not support spatial domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128}Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations.  Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-1a and 42-1c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-1a and 42-1c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-1a and 42-1c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-1b | Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one port subset configuration/list of CSI-RS resource IDs for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | 2-35 | Yes |  | UE does not support spatial domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 1 candidate values: {SD-type1, SD-type2, SD-type1and2}Note: SD-type1 refers to configuration contains one port subsetNote: SD-type2 refers to configuration contains list of CSI-RS resource IDsComponent 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values {2,3,4}Component 4 candidate values: SD Type 1: {1, 2, 3 … 32}SD Type 2: {1, 2, 3 … 32}Component 5 candidate values: SD Type 1: {8, 16, 24, … 128 }SD Type 2: {8, 16, 24, … 128 }Component 6 candidate values: SD Type 1: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}SD Type 2: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: SD Type 1: {8, 16, 24, …, 248, 256}SD Type 2: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11,12}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2 | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of periodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across periodic CSI report settings with sub-configurations per BWP | 2-35 | Yes |  | UE does not support power domain adaptation for periodicCSI reporting | Per band | No | No | N/A | Component 2 candidate value: {2,3,4}Component 4 candidate value: {1, 2, 3 … 32}Component 5 candidate value: {8, 16, 24, … 128 }Component 6 candidate value: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate value: {8, 16, 24, …, 248, 256}Note: Components 6 and 7 are signaled per BCComponent 9 candidate values: {2, 3, 4}Note: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2a | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUSCH | Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for semi-persistent CSI reporting1. The max number of sub-configurations Lmax in one CSI report configuration on PUSCH2. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.3. Supported maximum number of simultaneous NZP-CSI-RS resources per CC4. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs6. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Support of single-panel type 1 codebook8. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32b | Yes |  | UE does not support power domain adaptation for semi-persistent CSI reporting on PUSCH | Per band | No | No | N/A | Component 1 candidate values: {2,3,4,5,6,7,8}Component 2 candidate values: {2,3,4}Component 3 candidate values: {1, 2, 3 … 32}Component 4 candidate values: {8, 16, 24, … 128 }Component 5 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 6 candidate values: {8, 16, 24, …, 248, 256}Component 8 candidate values: {2, 3, 4,5,6,7,8,9,10,11,12}Note: Components 5 and 6 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-2a and 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-2a and 42-2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-2a and 42-2c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2c | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI reporting on PUCCH | Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for semi-persistent CSI reporting on PUCCH1. The max number of sub-configurations Lmax in one CSI report configuration2. Report of N CSI sub-report(s) included in one SP-CSI report where each CSI sub-report corresponds to one sub-configuration.3. Supported maximum number of simultaneous NZP-CSI-RS resources per CC4. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs6. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Support of single-panel type 1 codebook8. Supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP | 2-35, 2-32a | Yes |  | UE does not support power domain adaptation for semi-persistent CSI reporting on PUCCH | Per band | No | No | N/A | Component 1 candidate values: {2,3,4}Component 2 candidate values: {2,3,4}Component 3 candidate values: {1, 2, 3 … 32}Component 4 candidate values: {8, 16, 24, … 128}Component 5 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 6 candidate values: {8, 16, 24, …, 248, 256}Component 8 candidate values: {2, 3, 4}Note: Components 5 and 6 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset.Note: If a UE reports both FGs 42-2a and 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to both FGs 42-2a and 42-2c, then the supported total number of semi-persistent CSI reporting settings without sub-configurations plus the total number of sub-configurations across semi-persistent CSI report settings with sub-configurations per BWP is determined by the minimum of the reported values from both FGs 42-2a and 42-2c. | Optional with capability signaling |
| 42. Netw\_Energy\_NR | 42-2b | Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting | 1. Support of CSI feedback based on CSI report sub-configuration(s), each containing one power offset for aperiodic CSI reporting2. The max number of sub-configurations Lmax in one CSI report configuration3. Report of N CSI sub-report(s) included in one CSI report where each CSI sub-report corresponds to one sub-configuration4. Supported maximum number of simultaneous NZP-CSI-RS resources per CC5. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources per CC6. Supported maximum number of simultaneous NZP-CSI-RS resources in active BWPs across all CCs7. Supported maximum number of total CSI-RS ports in simultaneous NZP-CSI-RS resources in active BWPs across all CCs8. Support of single-panel type 1 codebook9. Supported total number of aperiodic CSI reporting settings without sub-configurations plus the total number of sub-configurations across aperiodic CSI report settings with sub-configurations per BWP | 2-35 | Yes |  | UE does not support power domain adaptation for aperiodic CSI reporting | Per band | No | No | N/A | Component 2 candidate values: {2,3,4,5,6,7,8}Component 3 candidate values: {2,3,4}Component 4 candidate values: {1, 2, 3 … 32}Component 5 candidate values: {8, 16, 24, … 128 }Component 6 candidate values: {5, 6, 7, 8, 9, 10, 12, 14, 16, …, 62, 64}Component 7 candidate values: {8, 16, 24, …, 248, 256}Component 9 candidate values: {2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12}Note: Components 6 and 7 are signaled per BCNote: For components 4~7 in FG42-1, 42-1a/b/c, 42-2, 42-2b and components 3~6 in FG42-2a/c, NZP-CSI-RS resource and CSI-RS ports are counted for reporting settings with and without sub-configurations. Note: If a UE reports more than one FG from FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c and if the UE is configured with CSI report settings with sub-configurations corresponding to a subset of the reported FGs 42-1, 42-1a, 42-1b, 42-1c, 42-2, 42-2a, 42-2b, 42-2c, then the supported maximum of NZP-CSI-RS resources/ports across all periodic, semi-persistent, aperiodic CSI report settings with sub-configurations corresponding to all of spatial and power domain adaptations and without sub-configurations is determined by the minimum of the reported values from that subset. | Optional with capability signaling |

**Proposal: Adopt the following changes highlighted in chromatic fonts, while keeping the yellow highlighting, if any, as shown**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 2. IoT\_NTN\_enh | 2-4a | GNSS position fix in RRC Connected state for eMTC—autonomous | 1. UE re-acquires GNSS autonomously (when configured by the network) if it does not receive eNB GNSS measurement trigger2. UE reports GNSS position fix time duration for measurement at least during the initial access stage and in connected mode via RRCConnectionReestablishmentComplete and RRCConnectionReconfigurationComplete for HO case3. UE reports the remaining GNSS validity duration with MAC CE in connected mode | ~~[Rel. 18 2-3a,]~~ Rel. 17 2-1 | Yes | N/A | Release 18 eMTC UE cannot get autonomous GNSS position fix in RRC Connected state | Per UE | No  | No | Note: This applies to non-DRXNote: For a UE that supports this FG in NGSO, it must also support Rel. 18 2-3a  | Optional with capability signalling |
| 2. IoT\_NTN\_enh | 2-4b | GNSS position fix in RRC Connected state for NB-IoT—autonomous | 1. UE re-acquires GNSS autonomously (when configured by the network) if it does not receive eNB GNSS measurement trigger2. UE reports GNSS position fix time duration for measurement at least during the initial access stage and in connected mode via RRCConnectionReestablishmentComplete-NB3. UE reports the remaining GNSS validity duration with MAC CE in connected mode | ~~[Rel. 18 2-3b],~~ Rel. 17 2-1b |  |  | Release 18 NB-IoT UE cannot get autonomous GNSS position fix in RRC Connected state | Per UE | No | No | Note: This applies to non-DRX | Optional with capability signalling |

[R1-2405835](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2405835.zip) UE features for other Rel-18 work items (Topics B) Huawei, HiSilicon

[R1-2406352](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2406352.zip) Remaining issues on UE features for Rel-18 LTM CATT

[R1-2406636](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2406636.zip) UE features for other Rel-18 work items (Topics B) Samsung

[R1-2406798](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2406798.zip) UE Features for Other Topics B (NES, MobEnh, IoT-NTN) Nokia

[R1-2406825](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2406825.zip) Views on UE features for other Rel-18 work items (Topics B) Apple

[R1-2406919](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2406919.zip) Discussion on UE features for other Rel-18 work items (Topics B) NTT DOCOMO, INC.

[R1-2406961](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2406961.zip) UE features for other Rel-18 work items (Topics B) ZTE Corporation, Sanechips

[R1-2407018](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2407018.zip) UE features for other Rel-18 work items (Topics B) Qualcomm Incorporated

[R1-2407055](file:///C%3A%5CUsers%5Cyouns%5COneDrive%5CDocuments%5C3GPP%5CRAN1%5CTSGR1_118%5CDocs%5CR1-2407055.zip) Rel-18 UE features topics set B Ericsson