**3GPP TSG RAN WG1 #118 R1-240XXXX**

**Maastricht, NL, August 19th – 23rd, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.214** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR on CBSR configuration for CJT in TS38.214 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung, NEC | | | | | | | | | |
| ***Source to TSG:*** | RAN1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_MIMO\_evo\_DL\_UL-Core | | | | |  | ***Date:*** | | | 2024-08-19 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | TS38.214 describes Rel-18 Type-II CJT CBSR based on an agreement in RAN1#112bis-e (that a UE must be configured with at least 1 CBSR), which was later superseded by RAN2 decision allowing no CBSR configuration (since N1,N2 configuration is taken out from CBSR IE). | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Updating the description in TS 38.214 following CBSR configuration structure in TS 38.331. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Misaligned configuration/description in TS 38.214 and TS 38.331. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2.2.2.8 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | |  | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | This is the first version of the CR. | | | | | | | | |

5.2.2.2.8 Enhanced Type II codebook for CJT

<Unchanged part omitted>

The bitmap parameter *n1-n2-codebookSubsetRestrictionList-r18* is configured for the CSI-RS resources, and it is configured as described in Clause 5.2.2.2.5, where only the bit values '00' or '11' of Table 5.2.2.2.5-6 are configurable. If parameter *cbsr-list-r18* does not include an element associated with a CSI-RS resource, no restriction is applied to the selection of vectors corresponding to that resource. If parameter *no-cbsr-r18* is configured, no restriction is applied to the selection of vectors corresponding to any of the CSI-RS resources.

<Unchanged part omitted>