**3GPP TSG- Meeting #126**

**Fukuoka, Japan, 20th – 24th May 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **4803** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  [meas\_report\_enh] |
|  |  |
| ***Source to WG:*** | Ericsson, T-Mobile USA, Turkcell, Rakuten Mobile, BT Plc., NTT Docomo, Deutsche Telekom, MediaTek Inc., Verizon, AT&T, Vodafone, Continental Automotive, KDDI, Charter, NEC, Telecom Italia, CATT, Reliance Jio, Qualcomm Incorporated. ZTE Corporation, Apple |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** | 2024-05-10 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In NR, for each measurement event there is the opportunity to use the reportOnLeave indication, so the network can identify for example, a neighbor cells are still in good condition compared to the serving cell.However, even with such indication available, it has been seen in real-life deployments that it is still difficult for the network to know whether the UE has entered an event or exited an event just by looking at the received measurement report from the UE.In fact, the network has to keep track of the historical measurement reports from the UE to understand if there is any cell that was included in the past measurement report but missing in the current measurement report sent by the UE. Since this unnecessarily increases the network overhead, a simple solution would be for the UE to just indicate for each cell in the cell triggered list whether it has entered an event or exited an event.Further, this new flag would allow an early preparation of target cells with better accuracy. For example, If a PCI is indicated as leaving and another is entering, the leaving PCI should not be considered as a valid candidate if NW want to manage resources in an effective. |
|  |  |
| ***Summary of change:*** | Section 5.5.4.1- Added procedural text to clarify how the UE should handle reportOnBestCellChangeSection 5.5.5.1- Added procedural text to clarify how the UE should handle the fields firstEntering, cellsMetReportOnLeaveList, and reportOnBestCellChangeSection 6.3.2- Added new fields firstEntering, cellsMetReportOnLeaveList, and reportOnBestCellChangeSection 6.3.3- Added new UE capabilities for the introduced fieldsSection 7.4- Add new field currentBestNeighbourCell |
|  |  |
| ***Consequences if not approved:*** | If the CR is not agreed, it would be difficult for the network to know whether the UE has entered an event or exited an event just by looking at the received measurement report from the UE. Further, if these changes are approved it would be allowed an early preparation of target cells with better accuracy/predictability. For example, If a PCI is indicated as leaving and another is entering, the leaving PCI should not be considered as a valid candidate if NW want to manage resources in an effective. |
|  |  |
| ***Clauses affected:*** | 5.5.4.1, 5.5.5.1, 6.3.2, 6.3.3, 7.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 38.306 CR 1110  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*START OF CHANGES*

### 5.5.4 Measurement report triggering

#### 5.5.4.1 General

If AS security has been activated successfully, the UE shall:

1> for each *measId* included in the *measIdList* within *VarMeasConfig*:

2> if the corresponding *reportConfig* includes a *reportType* set to *eventTriggered* or *periodical*:

3> if the corresponding *measObject* concerns NR:

4> if the corresponding *reportConfig* includes *measRSSI-ReportConfig*:

5> consider the resource indicated by the *rmtc-Config* on the associated frequency to be applicable;

4> if the *eventA1* or *eventA2* is configured in the corresponding *reportConfig*:

5> consider only the serving cell to be applicable;

4> if the *eventA3* or *eventA5* or *eventA3H1* or *eventA3H2* or *eventA5H1* or *eventA5H2* is configured in the corresponding *reportConfig*:

5> if a serving cell is associated with a *measObjectNR* and neighbours are associated with another *measObjectNR*, consider any serving cell associated with the other *measObjectNR* to be a neighbouring cell as well;

4> if the *eventX2* is configured in the corresponding *reportConfig*:

5> consider only the serving L2 U2N Relay UE to be applicable;

4> if corresponding *reportConfig* includes *reportType* set to *periodical*; or

4> for measurement events other than *eventA1,* *eventA2, eventD1*, *eventD2*, *eventX2*, *eventH1* or *eventH2*:

5> if *useAllowedCellList* is set to *true*:

6> consider any neighbouring cell detected based on parameters in the associated *measObjectNR* to be applicable when the concerned cell is included in the *allowedCellsToAddModList* defined within the *VarMeasConfig* for this *measId*;

5> else:

6> consider any neighbouring cell detected based on parameters in the associated *measObjectNR* to be applicable when the concerned cell is not included in the *excludedCellsToAddModList* defined within the *VarMeasConfig* for this *measId*;

4> if the *eventH1* or *eventH2* is configured in the corresponding *reportConfig*:

5> for all the events with the same *eventID* for which *simulMultiTriggerSingleMeasReport* is set to *true* and the entry condition applicable for the event has been satisfied:

6> consider only the event for which the difference between the corresponding altitude threshold and the altitude of the UE is the smallest to be applicable;

4> else if the *eventA3H1* or *eventA3H2* or *eventA4H1* or *eventA4H2* or *eventA5H1* or *eventA5H2* is configured in the corresponding *reportConfig*:

5> for all the events with the same *eventID* associated with the same *measObjectNR* for which *simulMultiTriggerSingleMeasReport* is set to *true* and the entry conditions applicable for the event has been satisfied:

6> consider only the event for which the difference between the corresponding altitude threshold and the altitude of the UE is the smallest to be applicable;

3> else if the corresponding *measObject* concerns E-UTRA:

4> if *eventB1* or *eventB2* is configured in the corresponding *reportConfig*:

5> consider a serving cell, if any, on the associated E-UTRA frequency as neighbour cell;

4> consider any neighbouring cell detected on the associated frequency to be applicable when the concerned cell is not included in the *excludedCellsToAddModListEUTRAN* defined within the *VarMeasConfig* for this *measId*;

3> else if the corresponding *measObject* concerns UTRA-FDD:

4> if *eventB1-UTRA-FDD* or *eventB2-UTRA-FDD* is configured in the corresponding *reportConfig*; or

4> if corresponding *reportConfig* includes *reportType* set to *periodical*:

5> consider a neighbouring cell on the associated frequency to be applicable when the concerned cell is included in the *cellsToAddModList* defined within the *VarMeasConfig* for this *measId*;

3> else if the corresponding *measObject* concerns L2 U2N Relay UE:

4> if *eventY1-Relay* or *eventY2-Relay* or *eventZ1-Relay* is configured in the corresponding *reportConfig*; or

4> if corresponding *reportConfig* includes *reportType* set to *periodical*:

5> consider any L2 U2N Relay UE fulfilling upper layer criteria detected on the associated frequency to be applicable for this *measId*;

2> else if the corresponding *reportConfig* includes a *reportType* set to *reportCGI*:

3> consider the cell detected on the associated *measObject* which has a physical cell identity matching the value of the *cellForWhichToReportCGI* included in the corresponding *reportConfig* within the *VarMeasConfig* to be applicable;

2> else if the corresponding *reportConfig* includes a *reportType* set to *reportSFTD*:

3> if the corresponding *measObject* concerns NR:

4> if the *reportSFTD-Meas* is set to *true*:

5> consider the NR PSCell to be applicable;

4> else if the *reportSFTD-NeighMeas* is included:

5> if *cellsForWhichToReportSFTD* is configured in the corresponding *reportConfig*:

6> consider any NR neighbouring cell detected on the associated *measObjectNR* which has a physical cell identity that is included in the *cellsForWhichToReportSFTD* to be applicable;

5> else:

6> consider up to 3 strongest NR neighbouring cells detected based on parameters in the associated *measObjectNR* to be applicable when the concerned cells are not included in the *excludedCellsToAddModList* defined within the *VarMeasConfig* for this *measId*;

3> else if the corresponding *measObject* concerns E-UTRA:

4> if the *reportSFTD-Meas* is set to *true*:

5> consider the E-UTRA PSCell to be applicable;

2> else if the corresponding *reportConfig* includes a *reportType* set to *cli-Periodical or cli-EventTriggered*:

3> consider all CLI measurement resources included in the corresponding *measObject* to be applicable;

2> else if the corresponding *reportConfig* includes a *reportType* set to *rxTxPeriodical*:

3> consider all Rx-Tx time difference measurement resources included in the corresponding *measObject* to be applicable;

2> if the corresponding *reportConfig* concerns the reporting for NR sidelink communication/discovery (i.e. *reportConfigNR-SL*):

3> consider the transmission resource pools indicated by the *tx-PoolMeasToAddModList* defined within the *VarMeasConfig* for this *measId* to be applicable;

2> if the *reportType* is set to *eventTriggered*, and if the corresponding *reportConfig* does not include *numberOfTriggeringCells*, and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable cells for all measurements after layer 3 filtering taken during *timeToTrigger* defined for this event within the *VarMeasConfig*, while the *VarMeasReportList* does not include a measurement reporting entry for this *measId* (a first cell triggers the event):

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned cell(s) in the *cellsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> if *useT312* is set to *true* in *reportConfig* for this event:

4> if T310 for the corresponding SpCell is running; and

4> if T312 is not running for corresponding SpCell:

5> start timer T312 for the corresponding SpCell with the value of T312 configured in the corresponding *measObjectNR*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> else if the *reportType* is set to *eventTriggered*, and if the corresponding *reportConfig* does not include *numberOfTriggeringCells*,and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable cells not included in the *cellsTriggeredList* for all measurements after layer 3 filtering taken during *timeToTrigger* defined for this event within the *VarMeasConfig* (a subsequent cell triggers the event):

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned cell(s) in the *cellsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> if *useT312* is set to *true* in *reportConfig* for this event:

4> if T310 for the corresponding SpCell is running; and

4> if T312 is not running for corresponding SpCell:

5> start timer T312 for the corresponding SpCell with the value of T312 configured in the corresponding *measObjectNR*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> if the *reportType* is set to *eventTriggered*, and if the corresponding *reportConfig* includes *numberOfTriggeringCells*, and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable cells for all measurements after layer 3 filtering taken during *timeToTrigger* defined for this event within the *VarMeasConfig*:

3> if the *VarMeasReportList* does not include a measurement reporting entry for this *measId* (a first cell triggers the event):

4> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> if the number of cell(s) in the *cellsTriggeredList* is larger than or equal to *numberOfTriggeringCells*:

4> include the concerned cell(s) in the *cellsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> else:

4> include the concerned cell(s) in the *cellsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

4> if the number of cell(s) in the *cellsTriggeredList* is larger than or equal to *numberOfTriggeringCells*:

5> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

5> initiate the measurement reporting procedure, as specified in 5.5.5;

2> if the *reportType* is set to *eventTriggered* and if the leaving condition applicable for this event is fulfilled for one or more of the cells included in the *cellsTriggeredList* defined within the *VarMeasReportList* for this *measId* for all measurements after layer 3 filtering taken during *timeToTrigger* defined within the *VarMeasConfig* for this event:

3> remove the concerned cell(s) in the *cellsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> if *reportOnLeave* is set to *true* for the corresponding reporting configuration:

4> if the corresponding *reportConfig* does not include *numberOfTriggeringCells*; or

4> if the corresponding *reportConfig* includes *numberOfTriggeringCells* and a measurement report was previously sent to the network for at least one of the concerned cell(s):

5> initiate the measurement reporting procedure, as specified in 5.5.5;

3> if the *cellsTriggeredList* defined within the *VarMeasReportList* for this *measId* is empty:

4> remove the measurement reporting entry within the *VarMeasReportList* for this *measId*;

4> stop the periodical reporting timer for this *measId*, if running;

2> if the *reportType* is set to *eventTriggered* and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable L2 U2N Relay UEs for all measurements after layer 3 filtering taken during *timeToTrigger* defined for this event within the *VarMeasConfig*, while the *VarMeasReportList* does not include a measurement reporting entry for this *measId* (a first L2 U2N Relay UE triggers the event):

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned L2 U2N Relay UE(s) in the *relaysTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> else if the *reportType* is set to *eventTriggered* and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable L2 U2N Relay UEs not included in the *relaysTriggeredList* for all measurements after layer 3 filtering taken during *timeToTrigger* defined for this event within the *VarMeasConfig* (a subsequent L2 U2N Relay UE triggers the event):

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned L2 U2N Relay UE(s) in the *relaysTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> else if the *reportType* is set to *eventTriggered* and if the leaving condition applicable for this event is fulfilled for one or more of the L2 U2N Relay UEs included in the *relaysTriggeredList* defined within the *VarMeasReportList* for this *measId* for all measurements after layer 3 filtering taken during *timeToTrigger* defined within the *VarMeasConfig* for this event:

3> remove the concerned L2 U2N Relay UE(s) in the *relaysTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> if *reportOnLeave* is set to *true* for the corresponding reporting configuration:

4> initiate the measurement reporting procedure, as specified in 5.5.5;

3> if the *relaysTriggeredList* defined within the *VarMeasReportList* for this *measId* is empty:

4> remove the measurement reporting entry within the *VarMeasReportList* for this *measId*;

4> stop the periodical reporting timer for this *measId*, if running;

2> else if the *reportType* is set to *eventTriggered* and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable transmission resource pools for all measurements taken during *timeToTrigger* defined for this event within the *VarMeasConfig*, while the *VarMeasReportList* does not include an measurement reporting entry for this *measId* (a first transmission resource pool triggers the event):

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned transmission resource pool(s) in the *poolsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> else if the *reportType* is set to *eventTriggered* and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable transmission resource pools not included in the *poolsTriggeredList* for all measurements taken during *timeToTrigger* defined for this event within the *VarMeasConfig* (a subsequent transmission resource pool triggers the event):

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned transmission resource pool(s) in the *poolsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> if the *reportType* is set to *eventTriggered* and if the leaving condition applicable for this event is fulfilled for one or more applicable transmission resource pools included in the *poolsTriggeredList* defined within the *VarMeasReportList* for this *measId* for all measurements taken during *timeToTrigger* defined within the *VarMeasConfig* for this event:

3> remove the concerned transmission resource pool(s) in the *poolsTriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> if the *poolsTriggeredList* defined within the *VarMeasReportList* for this *measId* is empty:

4> remove the measurement reporting entry within the *VarMeasReportList* for this *measId*;

4> stop the periodical reporting timer for this *measId*, if running

2> else if the *reportType* is set to *eventTriggered* and if the *eventId* is set to *eventD1* or *eventD2* or *eventH1* or *eventH2* and if the entering condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled during *timeToTrigger* defined for this event within the *VarMeasConfig*, while the *VarMeasReportList* does not include a measurement reporting entry for this *measId*:

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> else if the *reportType* is set to *eventTriggered* and if the *eventId* is set to *eventD1* or *eventD2* or *eventH1* or *eventH2* and if the leaving condition applicable for this event is fulfilled for the associated *VarMeasReport* within the *VarMeasReportList* for this *measId* during *timeToTrigger* defined within the *VarMeasConfig* for this event:

3> if *reportOnLeave* is set to *true* for the corresponding reporting configuration:

4> initiate the measurement reporting procedure, as specified in 5.5.5;

3> remove the measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> stop the periodical reporting timer for this *measId*, if running;

NOTE 1: Void.

2> if *reportType* is set to *periodical* and if a (first) measurement result is available:

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> if the corresponding *reportConfig* includes *measRSSI-ReportConfig*:

4> initiate the measurement reporting procedure as specified in 5.5.5 immediately when RSSI sample values are reported by the physical layer after the first L1 measurement duration;

3> else if the corresponding *reportConfig* includes the *ul-DelayValueConfig*:

4> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after a first measurement result is provided from lower layers of the associated DRB identity;

3> else if the corresponding *reportConfig* includes the *ul-ExcessDelayConfig*:

4> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after a first measurement result is provided from lower layers of the associated DRB identity(ies) according to the configured threshold per DRB identity(ies);

3> else if the *reportAmount* exceeds 1:

4> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after the quantity to be reported becomes available for the NR SpCell or for the serving L2 U2N Relay UE (if the UE is a L2 U2N Remote UE);

3> else (i.e. the *reportAmount* is equal to 1):

4> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after the quantity to be reported becomes available for the NR SpCell and for the strongest cell among the applicable cells, or for the NR SpCell and for the strongest L2 U2N Relay UEs among the applicable L2 U2N Relay UEs; or initiate the measurement reporting procedure, as specified in 5.5.5, immediately after the quantity to be reported becomes available for the serving L2 U2N Relay UE and for the strongest cell among the applicable cells, or for the serving L2 U2N Relay UE and for the strongest L2 U2N Relay UEs among the applicable L2 U2N Relay UEs (if the UE is a L2 U2N Remote UE);

2> if, in case the corresponding *reportConfig* concerns the reporting for NR sidelink communication/discovery, *reportType* is set to *periodical* and if a (first) measurement result is available:

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after the quantity to be reported becomes available for the NR SpCell and CBR measurement results become available;

2> if the *reportType* is set to *cli-EventTriggered* and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more applicable CLI measurement resources for all measurements after layer 3 filtering taken during *timeToTrigger* defined for this event within the *VarMeasConfig*, while the *VarMeasReportList* does not include a measurement reporting entry for this *measId* (a first CLI measurement resource triggers the event):

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned CLI measurement resource(s) in the *cli-TriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> else if the *reportType* is set to *cli-EventTriggered* and if the entry condition applicable for this event, i.e. the event corresponding with the *eventId* of the corresponding *reportConfig* within *VarMeasConfig*, is fulfilled for one or more CLI measurement resources not included in the *cli-TriggeredList* for all measurements after layer 3 filtering taken during *timeToTrigger* defined for this event within the *VarMeasConfig* (a subsequent CLI measurement resource triggers the event):

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> include the concerned CLI measurement resource(s) in the *cli-TriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> if the *reportType* is set to *cli-EventTriggered* and if the leaving condition applicable for this event is fulfilled for one or more of the CLI measurement resources included in the *cli-TriggeredList* defined within the *VarMeasReportList* for this *measId* for all measurements after layer 3 filtering taken during *timeToTrigger* defined within the *VarMeasConfig* for this event:

3> remove the concerned CLI measurement resource(s) in the *cli-TriggeredList* defined within the *VarMeasReportList* for this *measId*;

3> if *reportOnLeave* is set to *true* for the corresponding reporting configuration:

4> initiate the measurement reporting procedure, as specified in 5.5.5;

3> if the *cli-TriggeredList* defined within the *VarMeasReportList* for this *measId* is empty:

4> remove the measurement reporting entry within the *VarMeasReportList* for this *measId*;

4> stop the periodical reporting timer for this measId, if running;

2> if *reportType* is set to *cli-Periodical* and if a (first) measurement result is available:

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after the quantity to be reported becomes available for at least one CLI measurement resource;

2> if *reportType* is set to *rxTxPeriodical* and if a (first) measurement result is available:

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> initiate the measurement reporting procedure, as specified in 5.5.5;

2> upon expiry of the periodical reporting timer for this *measId*:

3> if *reportType* is set to *eventTriggered* and *reportOnBestCellChange* is configured for this *measId*

4> if *reportOnBestCellChange* is set to *n1*, and the best measured neighbouring cell among cells within *cellsTriggeredList* according to the sorting quantity is the same as the first cell in *reportedBestNeighbourCell* defined within the *VarMeasReportList* for this *measId*, or

4> if *reportOnBestCellChange* is set to *n2* and there is only one cell included in the *cellsTriggeredList* for this *measId*, and the best measured neighbouring cell according to the sorting quantity in the *cellsTriggeredList* is the same as the first cell in *reportedBestNeighbourCell* defined within the *VarMeasReportList* for this *measId*, or

4> if *reportOnBestCellChange* is set to *n2* and there are more than one cells included in the *cellsTriggeredList* for this *measId*, and the best measured neighbouring cell among cells within *cellsTriggeredList* according to the sorting quantity is the same as the first cell in *reportedBestNeighbourCell* defined within the *VarMeasReportList* for this *measId*, and the second best measured neighbouring cell among cells within *cellsTriggeredList* according to the sorting quantity is the same as the second cell in *reportedBestNeighbourCell* defined within the *VarMeasReportList* for this *measId*:

5> increment the *numberOfReportsSent* as defined within the *VarMeasReportList* for this *measId* by 1;

5> if the *numberOfReportsSent* as defined within the *VarMeasReportList* for this *measId* is less than the *reportAmount* as defined within the corresponding reportConfig for this *measId*:

6> restart the periodical reporting timer with the value of *reportInterval* as defined within the corresponding *reportConfig* for this *measId*;

5> else:

6> initiate the measurement reporting procedure, as specified in 5.5.5.3> else:

4> initiate the measurement reporting procedure, as specified in 5.5.5.

2> if the corresponding *reportConfig* includes a *reportType* is set to *reportSFTD*:

3> if the corresponding *measObject* concerns NR:

4> if the *drx-SFTD-NeighMeas* is included:

5> if the quantity to be reported becomes available for each requested pair of PCell and NR cell:

6> stop timer T322;

6> initiate the measurement reporting procedure, as specified in 5.5.5;

4> else

5> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after the quantity to be reported becomes available for each requested pair of PCell and NR cell or the maximal measurement reporting delay as specified in TS 38.133 [14];

3> else if the corresponding *measObject* concerns E-UTRA:

4> initiate the measurement reporting procedure, as specified in 5.5.5, immediately after the quantity to be reported becomes available for the pair of PCell and E-UTRA PSCell or the maximal measurement reporting delay as specified in TS 38.133 [14];

2> if *reportType* is set to *reportCGI*:

3> if the UE acquired the *SIB1* or *SystemInformationBlockType1* for the requested cell; or

3> if the UE detects that the requested NR cell is not transmitting *SIB1* (see TS 38.213 [13], clause 13):

4> stop timer T321;

4> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

4> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

4> initiate the measurement reporting procedure, as specified in 5.5.5;

2> upon the expiry of T321 for this *measId*:

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*;

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

3> initiate the measurement reporting procedure, as specified in 5.5.5.

2> upon the expiry of T322 for this *measId*:

3> initiate the measurement reporting procedure, as specified in 5.5.5.

If AS security has been activated successfully and if SCell activation(s) indication is received from lower layer, the UE shall:

1> if *reportType* is set to *reportOnActivation* for any *measId* included in the *measIdList* within *VarMeasConfig*:

2> if the activated SCell(s) fulfills the measurement requirement as specified in TS 38.133 [14]:

3> include a measurement reporting entry within the *VarMeasReportList* for this *measId*:

3> set the *numberOfReportsSent* defined within the *VarMeasReportList* for this *measId* to 0;

4> initiate the measurement reporting procedure, as specified in 5.5.5.

*END OF CHANGES*

*START OF CHANGES*

### 5.5.5 Measurement reporting

#### 5.5.5.1 General

Figure 5.5.5.1-1: Measurement reporting

The purpose of this procedure is to transfer measurement results from the UE to the network. The UE shall initiate this procedure only after successful AS security activation.

For the *measId* for which the measurement reporting procedure was triggered, the UE shall set the *measResults* within the *MeasurementReport* message as follows:

1> set the *measId* to the measurement identity that triggered the measurement reporting;

1> for each serving cell configured with *servingCellMO*:

2> if the *reportConfig* associated with the *measId* that triggered the measurement reporting includes *rsType*:

3> if the serving cell measurements based on the *rsType* included in the *reportConfig* that triggered the measurement report are available:

4> set the *measResultServingCell* within *measResultServingMOList* to include RSRP, RSRQ and the available SINR of the serving cell, derived based on the *rsType* included in the *reportConfig* that triggered the measurement report;

2> else:

3> if SSB based serving cell measurements are available:

4> set the *measResultServingCell* within *measResultServingMOList* to include RSRP, RSRQ and the available SINR of the serving cell, derived based on SSB;

3> else if CSI-RS based serving cell measurements are available:

4> set the *measResultServingCell* within *measResultServingMOList* to include RSRP, RSRQ and the available SINR of the serving cell, derived based on CSI-RS;

1> set the *servCellId* within *measResultServingMOList* to include each NR serving cell that is configured with *servingCellMO*, if any;

1> if the *reportConfig* associated with the *measId* that triggered the measurement reporting includes *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport*:

2> for each serving cell configured with *servingCellMO*, include beam measurement information according to the associated *reportConfig* as described in 5.5.5.2;

1> if the *reportConfig* associated with the *measId* that triggered the measurement reporting includes *reportAddNeighMeas*:

2> for each *measObjectId* referenced in the *measIdList* which is also referenced with *servingCellMO*, other than the *measObjectId* corresponding with the *measId* that triggered the measurement reporting:

3> if the *measObjectNR* indicated by the *servingCellMO* includes the RS resource configuration corresponding to the *rsType* indicated in the *reportConfig*:

4> set the *measResultBestNeighCell* within *measResultServingMOList* to include the *physCellId* and the available measurement quantities based on the *reportQuantityCell* and *rsType* indicated in *reportConfig* of the non-serving cell corresponding to the concerned *measObjectNR* with the highest measured RSRP if RSRP measurement results are available for cells corresponding to this *measObjectNR*, otherwise with the highest measured RSRQ if RSRQ measurement results are available for cells corresponding to this *measObjectNR*, otherwise with the highest measured SINR;

4> if the *reportConfig* associated with the *measId* that triggered the measurement reporting includes *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport:*

5> for each best non-serving cell included in the measurement report:

6> include beam measurement information according to the associated *reportConfig* as described in 5.5.5.2;

1> if the *reportConfig* associated with the *measId* that triggered the measurement reporting is set to *eventTriggered* and *eventID* is set to *eventA3*, or *eventA4*, or *eventA5*, or *eventB1*, or *eventB2,* or *eventA3H1,* or *eventA3H2,* or *eventA4H1,* or *eventA4H2,* or *eventA5H1,* or *eventA5H2*:

2> if the UE is in NE-DC and the measurement configuration that triggered this measurement report is associated with the MCG:

3> set the *measResultServFreqListEUTRA-SCG* to include an entry for each E-UTRA SCG serving frequency with the following:

4> include *carrierFreq* of the E-UTRA serving frequency;

4> set the *measResultServingCell* to include the available measurement quantities that the UE is configured to measure by the measurement configuration associated with the SCG;

4> if *reportConfig* associated with the *measId* that triggered the measurement reporting includes *reportAddNeighMeas*:

5> set the *measResultServFreqListEUTRA-SCG* to include within *measResultBestNeighCell* the quantities of the best non-serving cell, based on RSRP, on the concerned serving frequency;

1> if *reportConfig* associated with the *measId* that triggered the measurement reporting is set to *eventTriggered* and *eventID* is set to *eventA3*, or *eventA4*, or *eventA5,* or *eventA3H1,* or *eventA3H2,* or *eventA4H1,* or *eventA4H2,* or *eventA5H1,* or *eventA5H2*:

2> if the UE is in NR-DC and the measurement configuration that triggered this measurement report is associated with the MCG:

3> set the *measResultServFreqListNR-SCG* to include for each NR SCG serving cell that is configured with *servingCellMO*, if any, the following:

4> if the *reportConfig* associated with the *measId* that triggered the measurement reporting includes *rsType*:

5> if the serving cell measurements based on the *rsType* included in the *reportConfig* that triggered the measurement report are available according to the measurement configuration associated with the SCG:

6> set the *measResultServingCell* within *measResultServFreqListNR-SCG* to include RSRP, RSRQ and the available SINR of the serving cell, derived based on the *rsType* included in the *reportConfig* that triggered the measurement report;

4> else:

5> if SSB based serving cell measurements are available according to the measurement configuration associated with the SCG:

6> set the *measResultServingCell* within *measResultServFreqListNR-SCG* to include RSRP, RSRQ and the available SINR of the serving cell, derived based on SSB;

5> else if CSI-RS based serving cell measurements are available according to the measurement configuration associated with the SCG:

6> set the *measResultServingCell* within *measResultServFreqListNR-SCG* to include RSRP, RSRQ and the available SINR of the serving cell, derived based on CSI-RS;

4> if results for the serving cell derived based on SSB are included:

5> include the *ssbFrequency* to the value indicated by ssbFrequency as included in the *MeasObjectNR* of the serving cell;

4> if results for the serving cell derived based on CSI-RS are included:

5> include the *refFreqCSI-RS* to the value indicated by *refFreqCSI-RS* as included in the *MeasObjectNR* of the serving cell;

4> if the *reportConfig* associated with the *measId* that triggered the measurement reporting includes *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport*:

5> for each serving cell configured with *servingCellMO*, include beam measurement information according to the associated *reportConfig* as described in 5.5.5.2, where availability is considered according to the measurement configuration associated with the SCG;

4> if *reportConfig* associated with the *measId* that triggered the measurement reporting includes *reportAddNeighMeas*:

5> if the *measObjectNR* indicated by the *servingCellMO* includes the RS resource configuration corresponding to the *rsType* indicated in the *reportConfig*:

6> set the *measResultNeighCellListNR* within *measResultServFreqListNR-SCG* to include one entry with the *physCellId* and the available measurement quantities based on the *reportQuantityCell* and *rsType* indicated in *reportConfig* of the non-serving cell corresponding to the concerned *measObjectNR* with the highest measured RSRP if RSRP measurement results are available for cells corresponding to this *measObjectNR*, otherwise with the highest measured RSRQ if RSRQ measurement results are available for cells corresponding to this *measObjectNR*, otherwise with the highest measured SINR, where availability is considered according to the measurement configuration associated with the SCG;

7> if the *reportConfig* associated with the *measId* that triggered the measurement reporting includes *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport:*

8> for each best non-serving cell included in the measurement report:

9> include beam measurement information according to the associated *reportConfig* as described in 5.5.5.2, where availability is considered according to the measurement configuration associated with the SCG;

1> if the *measRSSI-ReportConfig* is configured within the corresponding *reportConfig* for this *measId*:

2> set the *rssi-Result* to the linear average of sample value(s) provided by lower layers in the *reportInterval;*

2> set the *channelOccupancy* to the rounded percentage of sample values which are beyond the *channelOccupancyThreshold* within all the sample values in the *reportInterval;*

1> if the UE is acting as L2 U2N Remote UE:

2> set the *sl-MeasResultServingRelay* in accordance with the following:

3> set the *cellIdentity* to include the *cellAccessRelatedInfo* contained in the discovery message received from the serving L2 U2N Relay UE;

3> set the *sl-RelayUE-Identity* to include the Source L2 ID of the serving L2 U2N Relay;

3> if the measurement of serving L2 U2N Relay UE is based on SL-RSRP:

4> set the *sl-MeasResult* to include the SL-RSRP of the serving L2 U2N Relay UE;

4> set the *sl-MeasQuantity* to *sl-rsrp*, if supported by the UE;

3> else:

4> set the *sl-MeasResult* to include the SD-RSRP of the serving L2 U2N Relay UE;

4> set the *sl-MeasQuantity* to *sd-rsrp*, if supported by the UE;

NOTE 1: In case of no data transmission from L2 U2N Relay UE to L2 U2N Remote UE, it is left to UE implementation whether to use SL-RSRP or SD-RSRP when setting the *sl-MeasResultServingRelay* of the serving L2 U2N Relay UE.

1> if *reportConfig* associated with the *measId* that triggered the measurement reporting is set to *eventTriggered* and if *enteringLeavingReport* is configured:

2> for each cell that is included in *measResultNeighCells*:

3> if the *measObject* associated with this *measId* concerns NR:

4> if the event leaving condition for the event that triggered the measurement report has been fulfilled by one or more cells:

5> set *cellsMetReportOnLeaveList* to include the cell(s) which met the event leaving condition;

4> if event entry condition for the event that triggered this measurement report has been fulfilled for the first time (the cell has just been included to *cellsTriggeredList*) since the *measID* has been configured for the cell:

5> set *firstEntering* to *true* for the concerned NR cell;

1> if there is at least one applicable neighbouring cell or candidate L2 U2N Relay UE to report:

2> if the *reportType* is set to *eventTriggered* or *periodical*:

3> if the measurement report concerns the candidate L2 U2N Relay UE:

4> set the *sl-MeasResultsCandRelay* in *measResultNeighCells* to include the best candidate L2 U2N Relay UEs up to *maxNrofRelayMeas* in accordance with the following:

5> if the *reportType* is set to *eventTriggered*:

6> include the L2 U2N Relay UEs included in the *relaysTriggeredList* as defined within the *VarMeasReportList* for this *measId*;

5> else:

6> include the applicable L2 U2N Relay UEs for which the new measurement results became available since the last periodical reporting or since the measurement was initiated or reset;

5> for each L2 U2N Relay UE that is included in the *sl-MeasResultsCandRelay*:

6> set the *cellIdentity* to include the *cellAccessRelatedInfo* contained in the discovery message received from the concerned L2 U2N Relay UE;

6> set the *sl-RelayUE-Identity* to include the Source L2 ID of the concerned L2 U2N Relay UE;

6> set the *sl-MeasResult* to include the SD-RSRP of the concerned L2 U2N Relay UE;

5> for each included L2 U2N Relay UE, include the layer 3 filtered measured results in accordance with the *reportConfig* for this *measId*, ordered as follows:

6> set the *sl-MeasResult* to include the quantity(ies) indicated in the *reportQuantityRelay* within the concerned *reportConfigRelay* in decreasing order of the sorting quantity, determined as specified in 5.5.5.3, i.e. the best L2 U2N Relay UE is included first;

6> if the UE supports *multipathRemoteUE-PC5L2* and idle/inactive relay UE reporting, and if the *sl-RelayIndicationMP* is contained in the discovery message received from the concerned L2 U2N Relay UE:

7> set the *sl-RelayIndicationMP* in the *sl-MeasResultsCandRelay*;

3> else:

4> set the *measResultNeighCells* to include the best neighbouring cells up to *maxReportCells* in accordance with the following:

5> if the *reportType* is set to *eventTriggered* and *eventId* is not set to *eventD1* or *eventD2* or *eventH1* or *eventH2*:

6> include the cells included in the *cellsTriggeredList* as defined within the *VarMeasReportList* for this *measId*;

5> else:

6> include the applicable cells for which the new measurement results became available since the last periodical reporting or since the measurement was initiated or reset;

5> for each cell that is included in the *measResultNeighCells*, include the *physCellId*;

5> if the reportType is set to eventTriggered or periodical:

6> for each included cell, include the layer 3 filtered measured results in accordance with the *reportConfig* for this *measId*, ordered as follows:

7> if the *measObject* associated with this *measId* concerns NR:

8> if *rsType* in the associated *reportConfig* is set to *ssb*:

9> set *resultsSSB-Cell* within the *measResult* to include the SS/PBCH block based quantity(ies) indicated in the *reportQuantityCell* within the concerned *reportConfig*, in decreasing order of the sorting quantity, determined as specified in 5.5.5.3, i.e. the best cell is included first;

9> if *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport* are configured, include beam measurement information as described in 5.5.5.2;

8> else if *rsType* in the associated *reportConfig* is set to *csi-rs*:

9> set *resultsCSI-RS-Cell* within the *measResult* to include the CSI-RS based quantity(ies) indicated in the *reportQuantityCell* within the concerned *reportConfig*, in decreasing order of the sorting quantity, determined as specified in 5.5.5.3, i.e. the best cell is included first;

9> if *reportQuantityRS-Indexes* and *maxNrofRS-IndexesToReport* are configured, include beam measurement information as described in 5.5.5.2;

7> if the *measObject* associated with this *measId* concerns E-UTRA:

8> set the *measResult* to include the quantity(ies) indicated in the *reportQuantity* within the concerned *reportConfigInterRAT* in decreasing order of the sorting quantity, determined as specified in 5.5.5.3, i.e. the best cell is included first;

7> if the *measObject* associated with this *measId* concerns UTRA-FDD and if *ReportConfigInterRAT* includes the *reportQuantityUTRA-FDD*:

8> set the *measResult* to include the quantity(ies) indicated in the *reportQuantityUTRA-FDD* within the concerned *reportConfigInterRAT* in decreasing order of the sorting quantity, determined as specified in 5.5.5.3, i.e. the best cell is included first;

6> if *reportType* is set to *eventTriggered* and *reportOnBestCellChange* is configured:

7> if *reportOnBestCellChange* is set to *n1*:

8> set the *reportedBestNeighbourCell* defined within the *VarMeasReportList* for this *measId* to the first cell listed in the *measResultNeighCells*;

7> if *reportOnBestCellChange* is set to *n2*:

8> set the first cell in *reportedBestNeighbourCell* defined within the *VarMeasReportList* for this *measId* to the first cell listed in the *measResultNeighCells* and the second cell in *reportedBestNeighbourCell* defined within the *VarMeasReportList* for this *measId* to the second cell listed in the *measResultNeighCells*;

2> else:

3> if the cell indicated by *cellForWhichToReportCGI* is an NR cell:

4> if *plmn-IdentityInfoList* of the *cgi-Info* for the concerned cell has been obtained:

5> include the *plmn-IdentityInfoList* including *plmn-IdentityList*, *trackingAreaCode* (if available), *trackingAreaList* (if available)*, ranac* (if available), *cellIdentity* and *cellReservedForOperatorUse* for each entry of the *plmn-IdentityInfoList*;

5> include *frequencyBandList* if available;

5> for each *PLMN-IdentityInfo* in *plmn-IdentityInfoList*:

6> if the *gNB-ID-Length* is broadcast:

7> include *gNB-ID-Length*;

4> if *nr-CGI-Reporting-NPN* is supported by the UE and *npn-IdentityInfoList* of the *cgi-Info* for the concerned cell has been obtained:

5> include the *npn-IdentityInfoList* including *npn-IdentityList*, *trackingAreaCode*, *ranac* (if available), *cellIdentity* and *cellReservedForOperatorUse* for each entry of the *npn-IdentityInfoList*;

5> for each *NPN-IdentityInfo* in *NPN-IdentityInfoList*:

6> if the *gNB-ID-Length* is broadcast:

7> include *gNB-ID-Length*;

5> include *cellReservedForOtherUse* if available;

4> else if *MIB* indicates the *SIB1* is not broadcast:

5> include the *noSIB1* including the *ssb-SubcarrierOffset* and *pdcch-ConfigSIB1* obtained from *MIB* of the concerned cell;

3> if the cell indicated by *cellForWhichToReportCGI* is an E-UTRA cell:

4> if all mandatory fields of the *cgi-Info-EPC* for the concerned cell have been obtained:

5> include in the *cgi-Info-EPC* the fields broadcasted in E-UTRA *SystemInformationBlockType1* associated to EPC;

4> if the UE is E-UTRA/5GC capable and all mandatory fields of the *cgi-Info-5GC* for the concerned cell have been obtained:

5> include in the *cgi-Info-5GC* the fields broadcasted in E-UTRA *SystemInformationBlockType1* associated to 5GC;

4> if the mandatory present fields of the *cgi-Info* for the cell indicated by the *cellForWhichToReportCGI* in the associated *measObject* have been obtained:

5> include the *freqBandIndicator*;

5> if the cell broadcasts the *multiBandInfoList*, include the *multiBandInfoList*;

5> if the cell broadcasts the *freqBandIndicatorPriority*, include the *freqBandIndicatorPriority*;

1> if the corresponding *measObject* concerns NR:

2> if the *reportSFTD-Meas* is set to *true* within the corresponding *reportConfigNR* for this *measId*:

3> set the *measResultSFTD-NR* in accordance with the following:

4> set *sfn-OffsetResult* and *frameBoundaryOffsetResult* to the measurement results provided by lower layers;

4> if the *reportRSRP* is set to *true*;

5> set *rsrp-Result* to the RSRP of the NR PSCell derived based on SSB;

2> else if the *reportSFTD-NeighMeas* is included within the corresponding *reportConfigNR* for this *measId*:

3> for each applicable cell which measurement results are available, include an entry in the *measResultCellListSFTD-NR* and set the contents as follows:

4> set *physCellId* to the physical cell identity of the concerned NR neighbour cell.

4> set *sfn-OffsetResult* and *frameBoundaryOffsetResult* to the measurement results provided by lower layers;

4> if the *reportRSRP* is set to *true*:

5> set *rsrp-Result* to the RSRP of the concerned cell derived based on SSB;

1> else if the corresponding *measObject* concerns E-UTRA:

2> if the *reportSFTD-Meas* is set to *true* within the corresponding *reportConfigInterRAT* for this *measId*:

3> set the *measResultSFTD-EUTRA* in accordance with the following:

4> set *sfn-OffsetResult* and *frameBoundaryOffsetResult* to the measurement results provided by lower layers;

4> if the *reportRSRP* is set to *true*;

5> set *rsrpResult-EUTRA* to the RSRP of the EUTRA PSCell;

1> if average uplink PDCP delay values are available:

2> set the *ul-PDCP-DelayValueResultList* to include the corresponding average uplink PDCP delay values;

1> if PDCP excess delay measurements are available:

2> set the *ul-PDCP-ExcessDelayResultList* to include the corresponding PDCP excess delay measurements;

1> if the *includeCommonLocationInfo* is configured in the corresponding *reportConfig* for this *measId* and detailed location information that has not been reported is available, set the content of *commonLocationInfo* of the *locationInfo* as follows:

2> include the *locationTimestamp*;

2> include the *locationCoordinate*, if available;

2> include the *velocityEstimate*, if available;

2> include the *locationError*, if available;

2> include the *locationSource*, if available;

2> if available, include the *gnss-TOD-msec*,

1> if the *coarseLocationRequest* is set to *true* in the corresponding *reportConfig* for this *measId*:

2> include *coarseLocationInfo,* if available;

1> if the *includeWLAN-Meas* is configured in the corresponding *reportConfig* for this *measId*, set the *wlan-LocationInfo* of the *locationInfo* in the *measResults* as follows:

2> if available, include the *LogMeasResultWLAN*, in order of decreasing RSSI for WLAN APs;

1> if the *includeBT-Meas* is configured in the corresponding *reportConfig* for this *measId*, set the *BT-LocationInfo* of the *locationInfo* in the *measResults* as follows:

2> if available, include the *LogMeasResultBT*, in order of decreasing RSSI for Bluetooth beacons;

1> if the *includeSensor-Meas* is configured in the corresponding *reportConfig* for this *measId*, set the *sensor-LocationInfo* of the *locationInfo* in the *measResults* as follows:

2> if available, include the *sensor-MeasurementInformation*;

2> if available, include the *sensor-MotionInformation*;

1> if the *includeAltitudeUE* is set to *true* in the corresponding *reportConfig* for this *measId*:

2> set the *altitudeUE* to include the altitude of the UE;

1> if there is at least one applicable transmission resource pool for NR sidelink communication/discovery (for *measResultsSL*):

2> set the *measResultsListSL* to include the CBR measurement results in accordance with the following:

3> if the *reportType* is set to *eventTriggered*:

4> include the transmission resource pools included in the *poolsTriggeredList* as defined within the *VarMeasReportList* for this *measId*;

3> else:

4> include the applicable transmission resource pools for which the new measurement results became available since the last periodical reporting or since the measurement was initiated or reset;

3> if the corresponding *measObject* concerns NR sidelink communication/discovery, then for each transmission resource pool to be reported:

4> set the *sl-poolReportIdentity* to the identity of this transmission resource pool;

4> set the *sl-CBR-ResultsNR* to the CBR measurement results on PSSCH and PSCCH of this transmission resource pool provided by lower layers, if available;

NOTE 1: Void.

1> if there is at least one applicable CLI measurement resource to report:

2> if the *reportType* is set to *cli-EventTriggered* or *cli-Periodical*:

3> set the *measResultCLI* to include the most interfering SRS resources or most interfering CLI-RSSI resources up to *maxReportCLI* in accordance with the following:

4> if the *reportType* is set to *cli-EventTriggered*:

5> if trigger quantity is set to *srs-RSRP* i.e. *i1-Threshold* is set to *srs-RSRP*:

6> include the SRS resource included in the *cli-TriggeredList* as defined within the *VarMeasReportList* for this *measId*;

5> if trigger quantity is set to *cli-RSSI* i.e. *i1-Threshold* is set to *cli-RSSI*:

6> include the CLI-RSSI resource included in the *cli-TriggeredList* as defined within the *VarMeasReportList* for this *measId*;

4> else:

5> if *reportQuantityCLI* is set to *srs-rsrp*:

6> include the applicable SRS resources for which the new measurement results became available since the last periodical reporting or since the measurement was initiated or reset;

5> else:

6> include the applicable CLI-RSSI resources for which the new measurement results became available since the last periodical reporting or since the measurement was initiated or reset;

4> for each SRS resource that is included in the *measResultCLI*:

5> include the *srs-ResourceId*;

5> set *srs-RSRP-Result* to include the layer 3 filtered measured results in decreasing order, i.e. the most interfering SRS resource is included first;

4> for each CLI-RSSI resource that is included in the *measResultCLI*:

5> include the *rssi-ResourceId*;

5> set *cli-RSSI-Result* to include the layer 3 filtered measured results in decreasing order, i.e. the most interfering CLI-RSSI resource is included first;

1> if there is at least one applicable UE Rx-Tx time difference measurement to report:

2> set *measResultRxTxTimeDiff* to the latest measurement result;

1> increment the *numberOfReportsSent* as defined within the *VarMeasReportList* for this *measId* by 1;

1> stop the periodical reporting timer, if running;

1> if the *numberOfReportsSent* as defined within the *VarMeasReportList* for this *measId* is less than the *reportAmount* as defined within the corresponding *reportConfig* for this *measId*:

2> start the periodical reporting timer with the value of *reportInterval* as defined within the corresponding *reportConfig* for this *measId*;

1> else:

2> if the *reportType* is set to *periodical* or *cli-Periodical* or *rxTxPeriodical*:

3> remove the entry within the *VarMeasReportList* for this *measId*;

3> remove this *measId* from the *measIdList* within *VarMeasConfig*;

1> if the measurement reporting was configured by a *sl-ConfigDedicatedNR* received within the *RRCConnectionReconfiguration*:

2> submit the *MeasurementReport* message to lower layers for transmission via SRB1, embedded in E-UTRA RRC message *ULInformationTransferIRAT* as specified TS 36.331 [10], clause 5.6.28;

1> else if the UE is in (NG)EN-DC:

2> if SRB3 is configured and the SCG is not deactivated:

3> submit the *MeasurementReport* message via SRB3 to lower layers for transmission, upon which the procedure ends;

2> else:

3> submit the *MeasurementReport* message via E-UTRA embedded in E-UTRA RRC message *ULInformationTransferMRDC* as specified in TS 36.331 [10].

1> else if the UE is in NR-DC:

2> if the measurement configuration that triggered this measurement report is associated with the SCG:

3> if SRB3 is configured and the SCG is not deactivated:

4> submit the *MeasurementReport* message via SRB3 to lower layers for transmission, upon which the procedure ends;

3> else:

4> submit the *MeasurementReport* message via SRB1 embedded in NR RRC message *ULInformationTransferMRDC* as specified in5.7.2a.3;

2> else:

3> submit the *MeasurementReport* message via SRB1 to lower layers for transmission, upon which the procedure ends;

1> else:

2> submit the *MeasurementReport* message to lower layers for transmission, upon which the procedure ends.

*END OF CHANGES*

*START OF CHANGES*

### 6.3.2 Radio resource control information elements

#### – *MeasResults*

The IE *MeasResults* covers measured results for intra-frequency, inter-frequency, inter-RAT mobility and measured results for NR sidelink communication/discovery.

*MeasResults* information element

-- ASN1START

-- TAG-MEASRESULTS-START

MeasResults ::= SEQUENCE {

 measId MeasId,

 measResultServingMOList MeasResultServMOList,

 measResultNeighCells CHOICE {

 measResultListNR MeasResultListNR,

 ...,

 measResultListEUTRA MeasResultListEUTRA,

 measResultListUTRA-FDD-r16 MeasResultListUTRA-FDD-r16,

 sl-MeasResultsCandRelay-r17 OCTET STRING -- Contains PC5 SL-MeasResultListRelay-r17

 } OPTIONAL,

 ...,

 [[

 measResultServFreqListEUTRA-SCG MeasResultServFreqListEUTRA-SCG OPTIONAL,

 measResultServFreqListNR-SCG MeasResultServFreqListNR-SCG OPTIONAL,

 measResultSFTD-EUTRA MeasResultSFTD-EUTRA OPTIONAL,

 measResultSFTD-NR MeasResultCellSFTD-NR OPTIONAL

 ]],

 [[

 measResultCellListSFTD-NR MeasResultCellListSFTD-NR OPTIONAL

 ]],

 [[

 measResultForRSSI-r16 MeasResultForRSSI-r16 OPTIONAL,

 locationInfo-r16 LocationInfo-r16 OPTIONAL,

 ul-PDCP-DelayValueResultList-r16 UL-PDCP-DelayValueResultList-r16 OPTIONAL,

 measResultsSL-r16 MeasResultsSL-r16 OPTIONAL,

 measResultCLI-r16 MeasResultCLI-r16 OPTIONAL

 ]],

 [[

 measResultRxTxTimeDiff-r17 MeasResultRxTxTimeDiff-r17 OPTIONAL,

 sl-MeasResultServingRelay-r17 OCTET STRING OPTIONAL,

 -- Contains PC5 SL-MeasResultRelay-r17

 ul-PDCP-ExcessDelayResultList-r17 UL-PDCP-ExcessDelayResultList-r17 OPTIONAL,

 coarseLocationInfo-r17 OCTET STRING OPTIONAL

 ]],

 [[

 altitudeUE-r18 Altitude-r18 OPTIONAL,

 cellsMetReportOnLeaveList-r18 SEQUENCE (SIZE (1..maxCellReport)) OF PhysCellId OPTIONAL

 ]]

}

MeasResultServMOList ::= SEQUENCE (SIZE (1..maxNrofServingCells)) OF MeasResultServMO

MeasResultServMO ::= SEQUENCE {

 servCellId ServCellIndex,

 measResultServingCell MeasResultNR,

 measResultBestNeighCell MeasResultNR OPTIONAL,

 ...

}

MeasResultListNR ::= SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultNR

MeasResultNR ::= SEQUENCE {

 physCellId PhysCellId OPTIONAL,

 measResult SEQUENCE {

 cellResults SEQUENCE{

 resultsSSB-Cell MeasQuantityResults OPTIONAL,

 resultsCSI-RS-Cell MeasQuantityResults OPTIONAL

 },

 rsIndexResults SEQUENCE{

 resultsSSB-Indexes ResultsPerSSB-IndexList OPTIONAL,

 resultsCSI-RS-Indexes ResultsPerCSI-RS-IndexList OPTIONAL

 } OPTIONAL

 },

 ...,

 [[

 cgi-Info CGI-InfoNR OPTIONAL

 ]],

 [[

 choCandidate-r17 ENUMERATED {true} OPTIONAL,

 choConfig-r17 SEQUENCE (SIZE (1..2)) OF CondTriggerConfig-r16 OPTIONAL,

 triggeredEvent-r17 SEQUENCE {

 timeBetweenEvents-r17 TimeBetweenEvent-r17 OPTIONAL,

 firstTriggeredEvent-r17 ENUMERATED {condFirstEvent, condSecondEvent} OPTIONAL

 } OPTIONAL

 ]],

 [[

 firstEntering-r18 ENUMERATED {true} OPTIONAL

 ]]

}

MeasResultListEUTRA ::= SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultEUTRA

MeasResultEUTRA ::= SEQUENCE {

 eutra-PhysCellId PhysCellId,

 measResult MeasQuantityResultsEUTRA,

 cgi-Info CGI-InfoEUTRA OPTIONAL,

 ...

}

MultiBandInfoListEUTRA ::= SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicatorEUTRA

MeasQuantityResults ::= SEQUENCE {

 rsrp RSRP-Range OPTIONAL,

 rsrq RSRQ-Range OPTIONAL,

 sinr SINR-Range OPTIONAL

}

MeasQuantityResultsEUTRA ::= SEQUENCE {

 rsrp RSRP-RangeEUTRA OPTIONAL,

 rsrq RSRQ-RangeEUTRA OPTIONAL,

 sinr SINR-RangeEUTRA OPTIONAL

}

ResultsPerSSB-IndexList::= SEQUENCE (SIZE (1..maxNrofIndexesToReport2)) OF ResultsPerSSB-Index

ResultsPerSSB-Index ::= SEQUENCE {

 ssb-Index SSB-Index,

 ssb-Results MeasQuantityResults OPTIONAL

}

ResultsPerCSI-RS-IndexList::= SEQUENCE (SIZE (1..maxNrofIndexesToReport2)) OF ResultsPerCSI-RS-Index

ResultsPerCSI-RS-Index ::= SEQUENCE {

 csi-RS-Index CSI-RS-Index,

 csi-RS-Results MeasQuantityResults OPTIONAL

}

MeasResultServFreqListEUTRA-SCG ::= SEQUENCE (SIZE (1..maxNrofServingCellsEUTRA)) OF MeasResult2EUTRA

MeasResultServFreqListNR-SCG ::= SEQUENCE (SIZE (1..maxNrofServingCells)) OF MeasResult2NR

MeasResultListUTRA-FDD-r16 ::= SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultUTRA-FDD-r16

MeasResultUTRA-FDD-r16 ::= SEQUENCE {

 physCellId-r16 PhysCellIdUTRA-FDD-r16,

 measResult-r16 SEQUENCE {

 utra-FDD-RSCP-r16 INTEGER (-5..91) OPTIONAL,

 utra-FDD-EcN0-r16 INTEGER (0..49) OPTIONAL

 }

}

MeasResultForRSSI-r16 ::= SEQUENCE {

 rssi-Result-r16 RSSI-Range-r16,

 channelOccupancy-r16 INTEGER (0..100)

}

MeasResultCLI-r16 ::= SEQUENCE {

 measResultListSRS-RSRP-r16 MeasResultListSRS-RSRP-r16 OPTIONAL,

 measResultListCLI-RSSI-r16 MeasResultListCLI-RSSI-r16 OPTIONAL

}

MeasResultListSRS-RSRP-r16 ::= SEQUENCE (SIZE (1.. maxCLI-Report-r16)) OF MeasResultSRS-RSRP-r16

MeasResultSRS-RSRP-r16 ::= SEQUENCE {

 srs-ResourceId-r16 SRS-ResourceId,

 srs-RSRP-Result-r16 SRS-RSRP-Range-r16

}

MeasResultListCLI-RSSI-r16 ::= SEQUENCE (SIZE (1.. maxCLI-Report-r16)) OF MeasResultCLI-RSSI-r16

MeasResultCLI-RSSI-r16 ::= SEQUENCE {

 rssi-ResourceId-r16 RSSI-ResourceId-r16,

 cli-RSSI-Result-r16 CLI-RSSI-Range-r16

}

UL-PDCP-DelayValueResultList-r16 ::= SEQUENCE (SIZE (1..maxDRB)) OF UL-PDCP-DelayValueResult-r16

UL-PDCP-DelayValueResult-r16 ::= SEQUENCE {

 drb-Id-r16 DRB-Identity,

 averageDelay-r16 INTEGER (0..10000),

 ...

}

UL-PDCP-ExcessDelayResultList-r17 ::= SEQUENCE (SIZE (1..maxDRB)) OF UL-PDCP-ExcessDelayResult-r17

UL-PDCP-ExcessDelayResult-r17 ::= SEQUENCE {

 drb-Id-r17 DRB-Identity,

 excessDelay-r17 INTEGER (0..31),

 ...

}

TimeBetweenEvent-r17 ::= INTEGER (0..1023)

-- TAG-MEASRESULTS-STOP

-- ASN1STOP

|  |
| --- |
| *MeasResultEUTRA* field descriptions |
| ***eutra-PhysCellId***Identifies the physical cell identity of the E-UTRA cell for which the reporting is being performed. The UE reports a value in the range 0..503, other values are reserved. |

|  |
| --- |
| *MeasResultNR* field descriptions |
| ***averageDelay***Indicates average delay for the packets during the reporting period, as specified in TS 38.314 [53]. Value 0 corresponds to 0 millisecond, value 1 corresponds to 0.1 millisecond, value 2 corresponds to 0.2 millisecond, and so on. |
| ***cellResults***Cell level measurement results. |
| ***cellsMetReportOnLeaveList***This field indicates the list of cells which met the event leaving condition. |
| ***choCandidate***This field indicates whether the associated cell is a candidate target cell for conditional handover or conditional PSCell change or addition. This field may be included only in the *SuccessHO-Report* or *SuccessPSCell-Report* within *UEInformationResponse* message. |
| ***choConfig***If the associated cell is a candidate target cell for conditional handover, this field indicates the conditional handover execution condition for each *measId* within *condTriggerConfig* associated to the cell. This field may be included only in the *rlf-report* within *UEInformationResponse* message. |
| ***drb-Id***Indicates DRB value for which uplink PDCP delay ratio or value is provided, according to TS 38.314 [53]. |
| ***firstEntering***This field indicates if the event entering condition for the cell is satisfied for the first time (the cell has been just added within *cellsTriggeredList*). |
| ***firstTriggeredEvent***This field is set to *condFirstEvent* if the execution condition associated to the first entry of *choConfig* was fulfilled first in time. This field is set to *condSecondEvent* if the execution condition associated to the second entry of *choConfig* was fulfilled first in time. This field may be included in *rlf-report* within *UEInformationResponse* message or in *SCGFailureInformation* message. |
| ***locationInfo***Positioning related information and measurements. |
| ***physCellId***The physical cell identity of the NR cell for which the reporting is being performed. |
| ***resultsSSB-Cell***Cell level measurement results based on SS/PBCH related measurements. |
| ***resultsSSB-Indexes***Beam level measurement results based on SS/PBCH related measurements. |
| ***resultsCSI-RS-Cell***Cell level measurement results based on CSI-RS related measurements. |
| ***resultsCSI-RS-Indexes***Beam level measurement results based on CSI-RS related measurements. |
| ***rsIndexResults***Beam level measurement results. |
| ***timeBetweenEvents***Indicates the time elapsed between fulfilling the conditional execution conditions included in *choConfig*. Value in milliseconds. The maximum value 1023 means 1023ms or longer. This field may be included in the reports associated to *UEInformationResponse* message, e.g., *rlf-Report* or in the *SCGFailureInformation* message. |

|  |
| --- |
| *MeasResultUTRA-FDD* field descriptions |
| ***physCellId***The physical cell identity of the UTRA-FDD cell for which the reporting is being performed. |
| ***utra-FDD-EcN0***According to CPICH\_Ec/No in TS 25.133 [46] for FDD. |
| ***utra-FDD-RSCP***According to CPICH\_RSCP in TS 25.133 [46] for FDD. |

| *MeasResults* field descriptions |
| --- |
| ***coarseLocationInfo***This field indicates the coarse location information reported by the UE. This field is coded as the *Ellipsoid-Point* defined in TS 37.355 [49]. The first/leftmost bit of the first octet contains the most significant bit. The least significant bits of *degreesLatitude* and *degreesLongitude* are set to 0 to meet the accuracy requirement corresponds to a granularity of approximately 2 km.It is up to UE implementation how many LSBs are set to 0 to meet the accuracy requirement |
| ***excessDelay***Indicates the ratio of packets in UL per DRB exceeding the configured delay threshold among the UL PDCP SDUs, according to the UL PDCP Excess Packet Delay per DRB mapping table, as defined in TS 38.314 [53], Table 4.3.1.e-1. |
| ***measId***Identifies the measurement identity for which the reporting is being performed. |
| ***measQuantityResults***The value sinr is not included when it is used for *LogMeasReport-r16*. |
| ***measResultCellListSFTD-NR***SFTD measurement results between the PCell and the NR neighbour cell(s) in NR standalone. |
| ***measResultCLI***CLI measurement results. |
| ***measResultEUTRA***Measured results of an E-UTRA cell. |
| ***measResultForRSSI***Includes measured RSSI result in dBm (see TS 38.215 [9]) and *channelOccupancy* which is the percentage of samples when the RSSI was above the configured *channelOccupancyThreshold* for the associated *reportConfig*. |
| ***measResultListEUTRA***List of measured results for the maximum number of reported best cells for an E-UTRA measurement identity. |
| ***measResultListNR***List of measured results for the maximum number of reported best cells for an NR measurement identity. |
| ***measResultListUTRA-FDD***List of measured results for the maximum number of reported best cells for a UTRA-FDD measurement identity. |
| ***measResultNR***Measured results of an NR cell. |
| ***measResultServFreqListEUTRA-SCG***Measured results of the E-UTRA SCG serving frequencies: the measurement result of PSCell and each SCell, if any, and of the best neighbouring cell on each E-UTRA SCG serving frequency. |
| ***measResultServFreqListNR-SCG***Measured results of the NR SCG serving frequencies: the measurement result of PSCell and each SCell, if any, and of the best neighbouring cell on each NR SCG serving frequency. |
| ***measResultServingMOList***Measured results of measured cells with reference signals indicated in the serving cell measurement objects including measurement results of SpCell, configured SCell(s) and best neighbouring cell within measured cells with reference signals indicated in on each serving cell measurement object. If the sending of the *MeasurementReport* message is triggered by a measurement configured by the field *sl-ConfigDedicatedForNR* received within an E-UTRA *RRCConnectionReconfiguration* message (i.e. CBR measurements), this field is not applicable and its contents is ignored by the network. |
| ***measResultSFTD-EUTRA***SFTD measurement results between the PCell and the E-UTRA PScell in NE-DC. |
| ***measResultSFTD-NR***SFTD measurement results between the PCell and the NR PScell in NR-DC. |
| ***measResultsSL***CBR measurements results for NR sidelink communication/discovery. |
| ***measResultUTRA-FDD***Measured result of a UTRA-FDD cell. |
| ***sl-MeasResultsCandRelay***Measurement result(s) of candiate L2 U2N relay UE(s). |
| ***sl-MeasResultServingRelay***Measurement result of serving L2 U2N relay UE. |

#### – *ReportConfigNR*

The IE *ReportConfigNR* specifies criteria for triggering of an NR measurement reporting event or of a CHO, CPA or CPC event or of an L2 U2N relay measurement reporting event. For events labelled AN with N equal to 1, 2 and so on, measurement reporting events and CHO, CPA or CPC events are based on cell measurement results, which can either be derived based on SS/PBCH block or CSI-RS.

Event A1: Serving becomes better than absolute threshold;

Event A2: Serving becomes worse than absolute threshold;

Event A3: Neighbour becomes amount of offset better than PCell/PSCell;

Event A4: Neighbour becomes better than absolute threshold;

Event A5: PCell/PSCell becomes worse than absolute threshold1 AND Neighbour/SCell becomes better than another absolute threshold2;

Event A6: Neighbour becomes amount of offset better than SCell;

Event D1: Distance between UE and a reference location *referenceLocation1* becomes larger than configured threshold *distanceThreshFromReference1* and distance between UE and a reference location *referenceLocation2* becomes shorter than configured threshold *distanceThreshFromReference2*;

Event D2: Distance between UE and a moving reference location based on *movingReferenceLocation* and its corresponding satellite ephemeris and epoch time broadcast in *SIB19* for the serving cell becomes larger than configured threshold *distanceThreshFromReference1* and distance between UE and a moving reference location determined based on *referenceLocation2* becomes shorter than configured threshold *distanceThreshFromReference2*;

CondEvent A3: Conditional reconfiguration candidate becomes amount of offset better than PCell/PSCell;

CondEvent A4: Conditional reconfiguration candidate becomes better than absolute threshold where *condEventA4* can also be used for current PSCell (i.e., in case it is configured as candidate PSCell for CondEvent A4 evaluation) for CHO with candidate SCG(s) case;

CondEvent A5: PCell/PSCell becomes worse than absolute threshold1 AND Conditional reconfiguration candidate becomes better than another absolute threshold2;

CondEvent D1: Distance between UE and a reference location *referenceLocation1* becomes larger than configured threshold *distanceThreshFromReference1* and distance between UE and a reference location *referenceLocation2* of conditional reconfiguration candidate becomes shorter than configured threshold *distanceThreshFromReference2*;

CondEvent D2: Distance between UE and a moving reference location determined based on *movingReferenceLocation* and its corresponding satellite ephemeris and epoch time broadcast in *SIB19* for the serving cell becomes larger than configured threshold *distanceThreshFromReference1* and distance between UE and a moving reference location determined based on *referenceLocation2* of conditional reconfiguration candidate becomes shorter than configured threshold *distanceThreshFromReference2*;

CondEvent T1: Time measured at UE becomes more than configured threshold *t1-Threshold* but is less than *t1-Threshold + duration*;

Event X1: Serving L2 U2N Relay UE becomes worse than absolute threshold1 AND NR Cell becomes better than another absolute threshold2;

Event X2: Serving L2 U2N Relay UE becomes worse than absolute threshold;

For event I1, measurement reporting event is based on CLI measurement results, which can either be derived based on SRS-RSRP or CLI-RSSI.

Event I1: Interference becomes higher than absolute threshold;

The reporting events concerning Aerial UE altitude are labelled H*N* with *N* equal to 1 and 2. Additionally, the reporting events concerning Aerial UE altitude and the neighboring cell measurements simultaneously are labelled A*M*H*N* with *M* equal to 3, 4, 5 and *N* equal to 1, 2.

Event H1: Aerial UE altitude becomes higher than a threshold;

Event H2: Aerial UE altitude becomes lower than a threshold;

Event A3H1: Neighbour becomes offset better than SpCell and the Aerial UE altitude becomes higher than a threshold;

Event A3H2: Neighbour becomes offset better than SpCell and the Aerial UE altitude becomes lower than a threshold;

Event A4H1: Neighbour becomes better than threshold1 and the Aerial UE altitude becomes higher than a threshold2;

Event A4H2: Neighbour becomes better than threshold1 and the Aerial UE altitude becomes lower than a threshold2;

Event A5H1: SpCell becomes worse than threshold1 and neighbour becomes better than threshold2 and the Aerial UE altitude becomes higher than a threshold3;

Event A5H2: SpCell becomes worse than threshold1 and neighbour becomes better than threshold2 and the Aerial UE altitude becomes lower than a threshold3.

*ReportConfigNR* information element

-- ASN1START

-- TAG-REPORTCONFIGNR-START

ReportConfigNR ::= SEQUENCE {

 reportType CHOICE {

 periodical PeriodicalReportConfig,

 eventTriggered EventTriggerConfig,

 ...,

 reportCGI ReportCGI,

 reportSFTD ReportSFTD-NR,

 condTriggerConfig-r16 CondTriggerConfig-r16,

 cli-Periodical-r16 CLI-PeriodicalReportConfig-r16,

 cli-EventTriggered-r16 CLI-EventTriggerConfig-r16,

 rxTxPeriodical-r17 RxTxPeriodical-r17,

 reportOnScellActivation-r18 ReportOnScellActivation-r18

 }

}

ReportCGI ::= SEQUENCE {

 cellForWhichToReportCGI PhysCellId,

 ...,

 [[

 useAutonomousGaps-r16 ENUMERATED {setup} OPTIONAL -- Need R

 ]]

}

ReportSFTD-NR ::= SEQUENCE {

 reportSFTD-Meas BOOLEAN,

 reportRSRP BOOLEAN,

 ...,

 [[

 reportSFTD-NeighMeas ENUMERATED {true} OPTIONAL, -- Need R

 drx-SFTD-NeighMeas ENUMERATED {true} OPTIONAL, -- Need R

 cellsForWhichToReportSFTD SEQUENCE (SIZE (1..maxCellSFTD)) OF PhysCellId OPTIONAL -- Need R

 ]]

}

CondTriggerConfig-r16 ::= SEQUENCE {

 condEventId CHOICE {

 condEventA3 SEQUENCE {

 a3-Offset MeasTriggerQuantityOffset,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger

 },

 condEventA5 SEQUENCE {

 a5-Threshold1 MeasTriggerQuantity,

 a5-Threshold2 MeasTriggerQuantity,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger

 },

 ...,

 condEventA4-r17 SEQUENCE {

 a4-Threshold-r17 MeasTriggerQuantity,

 hysteresis-r17 Hysteresis,

 timeToTrigger-r17 TimeToTrigger

 },

 condEventD1-r17 SEQUENCE {

 distanceThreshFromReference1-r17 INTEGER(0.. 65525),

 distanceThreshFromReference2-r17 INTEGER(0.. 65525),

 referenceLocation1-r17 ReferenceLocation-r17,

 referenceLocation2-r17 ReferenceLocation-r17,

 hysteresisLocation-r17 HysteresisLocation-r17,

 timeToTrigger-r17 TimeToTrigger

 },

 condEventT1-r17 SEQUENCE {

 t1-Threshold-r17 INTEGER (0..549755813887),

 duration-r17 INTEGER (1..6000)

 },

 condEventD2-r18 SEQUENCE {

 distanceThreshFromReference1-r18 INTEGER(0.. 65535),

 distanceThreshFromReference2-r18 INTEGER(0.. 65535),

 referenceLocation2-r18 ReferenceLocation-r17,

 hysteresisLocation-r18 HysteresisLocation-r17,

 timeToTrigger-r18 TimeToTrigger

 }

 },

 rsType-r16 NR-RS-Type,

 ...,

 [[

 nesEvent-r18 ENUMERATED {true} OPTIONAL -- Need R

 ]]

}

EventTriggerConfig ::= SEQUENCE {

 eventId CHOICE {

 eventA1 SEQUENCE {

 a1-Threshold MeasTriggerQuantity,

 reportOnLeave BOOLEAN,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger

 },

 eventA2 SEQUENCE {

 a2-Threshold MeasTriggerQuantity,

 reportOnLeave BOOLEAN,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger

 },

 eventA3 SEQUENCE {

 a3-Offset MeasTriggerQuantityOffset,

 reportOnLeave BOOLEAN,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger,

 useAllowedCellList BOOLEAN

 },

 eventA4 SEQUENCE {

 a4-Threshold MeasTriggerQuantity,

 reportOnLeave BOOLEAN,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger,

 useAllowedCellList BOOLEAN

 },

 eventA5 SEQUENCE {

 a5-Threshold1 MeasTriggerQuantity,

 a5-Threshold2 MeasTriggerQuantity,

 reportOnLeave BOOLEAN,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger,

 useAllowedCellList BOOLEAN

 },

 eventA6 SEQUENCE {

 a6-Offset MeasTriggerQuantityOffset,

 reportOnLeave BOOLEAN,

 hysteresis Hysteresis,

 timeToTrigger TimeToTrigger,

 useAllowedCellList BOOLEAN

 },

 ...,

 [[

 eventX1-r17 SEQUENCE {

 x1-Threshold1-Relay-r17 SL-MeasTriggerQuantity-r16,

 x1-Threshold2-r17 MeasTriggerQuantity,

 reportOnLeave-r17 BOOLEAN,

 hysteresis-r17 Hysteresis,

 timeToTrigger-r17 TimeToTrigger,

 useAllowedCellList-r17 BOOLEAN

 },

 eventX2-r17 SEQUENCE {

 x2-Threshold-Relay-r17 SL-MeasTriggerQuantity-r16,

 reportOnLeave-r17 BOOLEAN,

 hysteresis-r17 Hysteresis,

 timeToTrigger-r17 TimeToTrigger

 },

 eventD1-r17 SEQUENCE {

 distanceThreshFromReference1-r17 INTEGER(1.. 65525),

 distanceThreshFromReference2-r17 INTEGER(1.. 65525),

 referenceLocation1-r17 ReferenceLocation-r17,

 referenceLocation2-r17 ReferenceLocation-r17,

 reportOnLeave-r17 BOOLEAN,

 hysteresisLocation-r17 HysteresisLocation-r17,

 timeToTrigger-r17 TimeToTrigger

 }

 ]],

 [[

 eventH1-r18 SEQUENCE {

 h1-Threshold-r18 Altitude-r18,

 h1-Hysteresis-r18 HysteresisAltitude-r18,

 reportOnLeave-r18 BOOLEAN,

 timeToTrigger-r18 TimeToTrigger,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventH2-r18 SEQUENCE {

 h2-Threshold-r18 Altitude-r18,

 h2-Hysteresis-r18 HysteresisAltitude-r18,

 reportOnLeave-r18 BOOLEAN,

 timeToTrigger-r18 TimeToTrigger,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventA3H1-r18 SEQUENCE {

 a3-Offset-r18 MeasTriggerQuantityOffset,

 reportOnLeave-r18 BOOLEAN,

 a3-Hysteresis-r18 Hysteresis,

 timeToTrigger-r18 TimeToTrigger,

 useAllowedCellList-r18 BOOLEAN,

 h1-Threshold-r18 Altitude-r18,

 h1-Hysteresis-r18 HysteresisAltitude-r18,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventA3H2-r18 SEQUENCE {

 a3-Offset-r18 MeasTriggerQuantityOffset,

 reportOnLeave-r18 BOOLEAN,

 a3-Hysteresis-r18 Hysteresis,

 timeToTrigger-r18 TimeToTrigger,

 useAllowedCellList-r18 BOOLEAN,

 h2-Threshold-r18 Altitude-r18,

 h2-Hysteresis-r18 HysteresisAltitude-r18,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventA4H1-r18 SEQUENCE {

 a4-Threshold-r18 MeasTriggerQuantity,

 reportOnLeave-r18 BOOLEAN,

 a4-Hysteresis-r18 Hysteresis,

 timeToTrigger-r18 TimeToTrigger,

 useAllowedCellList-r18 BOOLEAN,

 h1-Threshold-r18 Altitude-r18,

 h1-Hysteresis-r18 HysteresisAltitude-r18,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventA4H2-r18 SEQUENCE {

 a4-Threshold-r18 MeasTriggerQuantity,

 reportOnLeave-r18 BOOLEAN,

 a4-Hysteresis-r18 Hysteresis,

 timeToTrigger-r18 TimeToTrigger,

 useAllowedCellList-r18 BOOLEAN,

 h2-Threshold-r18 Altitude-r18,

 h2-Hysteresis-r18 HysteresisAltitude-r18,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventA5H1-r18 SEQUENCE {

 a5-Threshold1-r18 MeasTriggerQuantity,

 a5-Threshold2-r18 MeasTriggerQuantity,

 reportOnLeave-r18 BOOLEAN,

 a5-Hysteresis-r18 Hysteresis,

 timeToTrigger-r18 TimeToTrigger,

 useAllowedCellList-r18 BOOLEAN,

 h1-Threshold-r18 Altitude-r18,

 h1-Hysteresis-r18 HysteresisAltitude-r18,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventA5H2-r18 SEQUENCE {

 a5-Threshold1-r18 MeasTriggerQuantity,

 a5-Threshold2-r18 MeasTriggerQuantity,

 reportOnLeave-r18 BOOLEAN,

 a5-Hysteresis-r18 Hysteresis,

 timeToTrigger-r18 TimeToTrigger,

 useAllowedCellList-r18 BOOLEAN,

 h2-Threshold-r18 Altitude-r18,

 h2-Hysteresis-r18 HysteresisAltitude-r18,

 includeAltitudeUE-r18 BOOLEAN,

 simulMultiTriggerSingleMeasReport-r18 BOOLEAN

 },

 eventD2-r18 SEQUENCE {

 distanceThreshFromReference1-r18 INTEGER(1.. 65535),

 distanceThreshFromReference2-r18 INTEGER(1.. 65535),

 referenceLocation2-r18 ReferenceLocation-r17,

 reportOnLeave-r18 BOOLEAN,

 hysteresisLocation-r18 HysteresisLocation-r17,

 timeToTrigger-r18 TimeToTrigger

 }

 ]]

 },

 rsType NR-RS-Type,

 reportInterval ReportInterval,

 reportAmount ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},

 reportQuantityCell MeasReportQuantity,

 maxReportCells INTEGER (1..maxCellReport),

 reportQuantityRS-Indexes MeasReportQuantity OPTIONAL, -- Need R

 maxNrofRS-IndexesToReport INTEGER (1..maxNrofIndexesToReport) OPTIONAL, -- Need R

 includeBeamMeasurements BOOLEAN,

 reportAddNeighMeas ENUMERATED {setup} OPTIONAL, -- Need R

 ...,

 [[

 measRSSI-ReportConfig-r16 MeasRSSI-ReportConfig-r16 OPTIONAL, -- Need R

 useT312-r16 BOOLEAN OPTIONAL, -- Need M

 includeCommonLocationInfo-r16 ENUMERATED {true} OPTIONAL, -- Need R

 includeBT-Meas-r16 SetupRelease {BT-NameList-r16} OPTIONAL, -- Need M

 includeWLAN-Meas-r16 SetupRelease {WLAN-NameList-r16} OPTIONAL, -- Need M

 includeSensor-Meas-r16 SetupRelease {Sensor-NameList-r16} OPTIONAL -- Need M

 ]],

 [[

 coarseLocationRequest-r17 ENUMERATED {true} OPTIONAL, -- Need R

 reportQuantityRelay-r17 SL-MeasReportQuantity-r16 OPTIONAL -- Need R

 ]],

 [[

 numberOfTriggeringCells-r18 INTEGER (2..maxCellReport) OPTIONAL, -- Need R

 cellIndividualOffsetList-r18 SEQUENCE (SIZE (1..maxNrofCellMeas)) OF CellIndividualOffsetList-r18 OPTIONAL, -- Need R

 eventX1-SD-Threshold1-r18 SL-MeasTriggerQuantity-r16 OPTIONAL, -- Need S

 eventX2-SD-Threshold-r18 SL-MeasTriggerQuantity-r16 OPTIONAL -- Need S

-- Editor’s Note: FFS if this is proper place for Event X1 thresolds.

 reportOnBestCellChange-r18 ENUMERATED {n1, n2} OPTIONAL -- Need R

 enteringLeavingReport-r18 ENUMERATED {true} OPTIONAL -- Need R

 ]]

}

PeriodicalReportConfig ::= SEQUENCE {

 rsType NR-RS-Type,

 reportInterval ReportInterval,

 reportAmount ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},

 reportQuantityCell MeasReportQuantity,

 maxReportCells INTEGER (1..maxCellReport),

 reportQuantityRS-Indexes MeasReportQuantity OPTIONAL, -- Need R

 maxNrofRS-IndexesToReport INTEGER (1..maxNrofIndexesToReport) OPTIONAL, -- Need R

 includeBeamMeasurements BOOLEAN,

 useAllowedCellList BOOLEAN,

 ...,

 [[

 measRSSI-ReportConfig-r16 MeasRSSI-ReportConfig-r16 OPTIONAL, -- Need R

 includeCommonLocationInfo-r16 ENUMERATED {true} OPTIONAL, -- Need R

 includeBT-Meas-r16 SetupRelease {BT-NameList-r16} OPTIONAL, -- Need M

 includeWLAN-Meas-r16 SetupRelease {WLAN-NameList-r16} OPTIONAL, -- Need M

 includeSensor-Meas-r16 SetupRelease {Sensor-NameList-r16} OPTIONAL, -- Need M

 ul-DelayValueConfig-r16 SetupRelease { UL-DelayValueConfig-r16 } OPTIONAL, -- Need M

 reportAddNeighMeas-r16 ENUMERATED {setup} OPTIONAL -- Need R

 ]],

 [[

 ul-ExcessDelayConfig-r17 SetupRelease { UL-ExcessDelayConfig-r17 } OPTIONAL, -- Need M

 coarseLocationRequest-r17 ENUMERATED {true} OPTIONAL, -- Need R

 reportQuantityRelay-r17 SL-MeasReportQuantity-r16 OPTIONAL -- Need R

 ]]

}

NR-RS-Type ::= ENUMERATED {ssb, csi-rs}

MeasTriggerQuantity ::= CHOICE {

 rsrp RSRP-Range,

 rsrq RSRQ-Range,

 sinr SINR-Range

}

MeasTriggerQuantityOffset ::= CHOICE {

 rsrp INTEGER (-30..30),

 rsrq INTEGER (-30..30),

 sinr INTEGER (-30..30)

}

MeasReportQuantity ::= SEQUENCE {

 rsrp BOOLEAN,

 rsrq BOOLEAN,

 sinr BOOLEAN

}

MeasRSSI-ReportConfig-r16 ::= SEQUENCE {

 channelOccupancyThreshold-r16 RSSI-Range-r16 OPTIONAL -- Need R

}

CLI-EventTriggerConfig-r16 ::= SEQUENCE {

 eventId-r16 CHOICE {

 eventI1-r16 SEQUENCE {

 i1-Threshold-r16 MeasTriggerQuantityCLI-r16,

 reportOnLeave-r16 BOOLEAN,

 hysteresis-r16 Hysteresis,

 timeToTrigger-r16 TimeToTrigger

 },

 ...

 },

 reportInterval-r16 ReportInterval,

 reportAmount-r16 ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},

 maxReportCLI-r16 INTEGER (1..maxCLI-Report-r16),

 ...

}

CLI-PeriodicalReportConfig-r16 ::= SEQUENCE {

 reportInterval-r16 ReportInterval,

 reportAmount-r16 ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},

 reportQuantityCLI-r16 MeasReportQuantityCLI-r16,

 maxReportCLI-r16 INTEGER (1..maxCLI-Report-r16),

 ...

}

RxTxPeriodical-r17 ::= SEQUENCE {

 rxTxReportInterval-r17 RxTxReportInterval-r17 OPTIONAL, -- Need R

 reportAmount-r17 ENUMERATED {r1, infinity, spare6, spare5, spare4, spare3, spare2, spare1},

 ...

}

RxTxReportInterval-r17 ::= ENUMERATED {ms80,ms120,ms160,ms240,ms320,ms480,ms640,ms1024,ms1280,ms2048,ms2560,ms5120,spare4,spare3,spare2,spare1}

MeasTriggerQuantityCLI-r16 ::= CHOICE {

 srs-RSRP-r16 SRS-RSRP-Range-r16,

 cli-RSSI-r16 CLI-RSSI-Range-r16

}

MeasReportQuantityCLI-r16 ::= ENUMERATED {srs-rsrp, cli-rssi}

ReportOnScellActivation-r18 ::= SEQUENCE {

 rsType NR-RS-Type,

 reportQuantityRS-Indexes MeasReportQuantity,

 maxNrofRS-IndexesToReport INTEGER (1..maxNrofIndexesToReport),

 includeBeamMeasurements BOOLEAN

}

CellIndividualOffsetList-r18 ::= SEQUENCE {

 physCellId-r18 PhysCellId,

 cellIndividualOffset-r18 Q-OffsetRangeList

}

-- TAG-REPORTCONFIGNR-STOP

-- ASN1STOP

|  |
| --- |
| *CondTriggerConfig* field descriptions |
| ***a3-Offset***Offset value(s) to be used in NR conditional reconfiguration triggering condition for cond event a3. The actual value is field value \* 0.5 dB. |
| ***a4-Threshold***Threshold value associated to the selected trigger quantity (e.g. RSRP, RSRQ, SINR) per RS Type (e.g. SS/PBCH block, CSI-RS) to be used in NR conditional reconfiguration triggering condition for cond event a4. |
| ***a5-Threshold1/ a5-Threshold2***Threshold value associated to the selected trigger quantity (e.g. RSRP, RSRQ, SINR) per RS Type (e.g. SS/PBCH block, CSI-RS) to be used in NR conditional reconfiguration triggering condition for cond event a5. In the same *condeventA5*, the network configures the same quantity for the *MeasTriggerQuantity* of the *a5-Threshold1* and for the *MeasTriggerQuantity* of the *a5-Threshold2*. |
| ***condEventId***Choice of NR conditional reconfiguration event triggered criteria. |
| ***distanceThreshFromReference1, distanceThreshFromReference2***Distance from a fixed reference location configured with *referenceLocation1* or *referenceLocation2* or a moving reference location determined by the UE based on the serving cell *movingReferenceLocation* broadcast in *SIB19* or *referenceLocation2* and their corresponding satellite ephemeris and epoch time. Each step represents 50m. |
| ***duration***This field is used for defining the leaving condition T1-2 for conditional HO event *condEventT1*. Each step represents 100ms. |
| ***nesEvent***Indicates the event is a NES-specific CHO event and the event is only considered to be satisfied if indication from lower layers is received indicating the applicability of NES-specific CHO event and the related entry condition(s) is fulfilled. This field can only be configured for *condEventA3*, *condEventA4* or *condEventA5*. This field cannot be configured for CPAC. |
| ***referenceLocation1, referenceLocation2***For *condEventD1*, the r*eferenceLocation1* is associated to serving cell and *referenceLocation2* is associated to candidate target cell. For *condEventD2*, the *refereceLocation2* is associated to candidate target cell. |
| ***t1-Threshold***The field counts the number of UTC seconds in 10 ms units since 00:00:00 on Gregorian calendar date 1 January, 1900 (midnight between Sunday, December 31, 1899 and Monday, January 1, 1900). |
| ***timeToTrigger***Time during which specific criteria for the event needs to be met in order to execute the conditional reconfiguration evaluation. |

|  |
| --- |
| *ReportConfigNR* field descriptions |
| ***reportType***Type of the configured measurement report. In MR-DC, network does not configure report of type *reportCGI* using SRB3. The *condTriggerConfig is* used for CHO, CPA or CPC configuration. |

|  |
| --- |
| *ReportCGI* field descriptions |
| ***useAutonomousGaps***Indicates whether or not the UE is allowed to use autonomous gaps in acquiring system information from the NR neighbour cell. When the field is included, the UE applies the corresponding value for T321. |

|  |
| --- |
| *EventTriggerConfig* field descriptions |
| ***a3-Offset/a6-Offset***Offset value(s) to be used in NR measurement report triggering condition for event a3/a6. The actual value is field value \* 0.5 dB. |
| ***aN-ThresholdM***Threshold value associated to the selected trigger quantity (e.g. RSRP, RSRQ, SINR) per RS Type (e.g. SS/PBCH block, CSI-RS) to be used in NR measurement report triggering condition for event number aN. If multiple thresholds are defined for event number aN, the thresholds are differentiated by M. In the same *eventA5*, *eventA5H1, eventA5H2,* the network configures the same quantity for the *MeasTriggerQuantity* of the *a5-Threshold1* and for the *MeasTriggerQuantity* of the *a5-Threshold2*. |
| ***channelOccupancyThreshold***RSSI threshold which is used for channel occupancy evaluation. |
| ***coarseLocationRequest***This field is used to request UE to report coarse location information. |
| ***distanceThreshFromReference1, distanceThreshFromReference2***Threshold value associated to the distance from a reference location configured with *referenceLocation1* or *referenceLocation2.* Each step represents 50m. |
| ***eventId***Choice of NR event triggered reporting criteria. |
| ***eventXN-SD-Threshold***Indicates the SD-RSRP threshold value for the serving L2 U2N Relay UE in event *XN* (*N* equals 1 or 2). If this field is not included, the UE considers the SD-RSRP threshold value equals to the one indicated by *x1-Threshold1-Relay*/ *x2-Threshold-Relay*. |
| ***includeAltitudeUE***This field is used to request UE to report altitude information. |
| ***maxNrofRS-IndexesToReport***Max number of RS indexes to include in the measurement report for A1-A6 events. |
| ***maxReportCells***Max number of non-serving cells to include in the measurement report. |
| ***numberOfTriggeringCells***Indicates the number of cells detected that are required to fulfill an event for a measurement report to be triggered. This field is applicable only for the events concerning neighbor cells, i.e. *eventA3*, *eventA4, eventA5, eventA3H1, eventA3H2, eventA4H1, eventA4H2, eventA5H1, eventA5H2*. |
| ***referenceLocation1, referenceLocation2***For *eventD1*, the *referenceLocation1* is associated to serving cell and *referenceLocation2* is associated to neighbour cell. For *eventD2*, the *refereceLocation2* is associated to neighbour cell. |
| ***reportAddNeighMeas***Indicates that the UE shall include the best neighbour cells per serving frequency. |
| ***reportAmount***Number of measurement reports applicable for *eventTriggered* as well as for *periodical* report types. |
| ***reportOnBestCellChange*** Indicates whether the UE shall only send measurement report if the measured best cell is changed. In this release of the specification, this field is applicable only for the events concerning neighbor cells. This field can only be configured when the value of the field *reportAmount* is set to any other value than *r1*. |
| ***reportOnLeave***Indicates whether or not the UE shall initiate the measurement reporting procedure when the leaving condition is met for a cell in *cellsTriggeredList*, as specified in 5.5.4.1.Indicates whether or not the UE shall initiate the measurement reporting procedure when the leaving condition is met if configured in *eventD1*, *eventD2*, *eventH1*, *eventH2* as specified in 5.5.4.1. |
| ***reportQuantityCell***The cell measurement quantities to be included in the measurement report. |
| ***reportQuantityRS-Indexes***Indicates which measurement information per RS index the UE shall include in the measurement report. |
| ***simulMultiTriggerSingleMeasReport***Indicates when multiple events with the same *eventID* satisfy the entering condition(s), whether to consider only the event with the smallest value between the altitude of the UE and the configured altitude threshold. |
| ***timeToTrigger***Time during which specific criteria for the event needs to be met in order to trigger a measurement report. |
| ***useAllowedCellList***Indicates whether only the cells included in the allow-list of the associated measObject are applicable as specified in 5.5.4.1. |
| ***useT312***If value *TRUE* is configured, the UE shall use the timer T312 with the value *t312* as specified in the corresponding *measObjectNR*. If value FALSE is configured, the timer T312 is considered as disabled. Network configures value *TRUE* only if *reportType* is set to *eventTriggered*. |
| ***xN-ThresholdM***Threshold value associated to the selected trigger quantity (e.g. RSRP, RSRQ, SINR) per RS Type (e.g. SS/PBCH block, CSI-RS) to be used in NR measurement report triggering condition for event xN. If multiple thresholds are defined for event number xN, the thresholds are differentiated by M. *x1-Threshold1* and *x2-Threshold* indicates the threshold value for the serving L2 U2N Relay UE, *x1-Threshold2* indicates the threshold value for the NR Cells. |

|  |
| --- |
| *CLI-EventTriggerConfig* field descriptions |
| ***i1-Threshold***Threshold value associated to the selected trigger quantity (e.g. SRS-RSRP, CLI-RSSI) to be used in CLI measurement report triggering condition for event i1. |
| ***eventId***Choice of CLI event triggered reporting criteria. |
| ***maxReportCLI***Max number of CLI measurement resource to include in the measurement report. |
| ***reportAmount****Number* of measurement reports. |
| ***reportOnLeave***Indicates whether or not the UE shall initiate the measurement reporting procedure when the leaving condition is met for a CLI measurement resource in *srsTriggeredList* or *rssiTriggeredList*, as specified in 5.5.4.1. |
| ***timeToTrigger***Time during which specific criteria for the event needs to be met in order to trigger a measurement report. |

|  |
| --- |
| *CLI-PeriodicalReportConfig* field descriptions |
| ***maxReportCLI***Max number of CLI measurement resource to include in the measurement report. |
| ***reportAmount****Number* of measurement reports. |
| ***reportQuantityCLI***The CLI measurement quantities to be included in the measurement report. |

|  |
| --- |
| *PeriodicalReportConfig* field descriptions |
| ***coarseLocationRequest***This field is used to request UE to report coarse location information. |
| ***maxNrofRS-IndexesToReport***Max number of RS indexes to include in the measurement report. |
| ***maxReportCells***Max number of non-serving cells to include in the measurement report. |
| ***reportAddNeighMeas***Indicates that the UE shall include the best neighbour cells per serving frequency. |
| ***reportAmount****Number* of measurement reports applicable for *eventTriggered* as well as for *periodical* report types |
| ***reportQuantityCell***The cell measurement quantities to be included in the measurement report. |
| ***reportQuantityRS-Indexes***Indicates which measurement information per RS index the UE shall include in the measurement report. |
| ***ul-DelayValueConfig***If the field is present, the UE shall perform the actual UL PDCP Packet Average Delay measurement per DRB as specified in TS 38.314 [53] and the UE shall ignore the fields *reportQuantityCell* and *maxReportCells*. The applicable values for the corresponding *reportInterval* are (one of the) {ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240, ms20480, ms40960, min1,min6, min12, min30}. The *reportInterval* indicates the periodicity for performing and reporting of UL PDCP Packet Average Delay per DRB measurement as specified in TS 38.314 [53]. |
| ***ul-ExcessDelayConfig***If the field is present, the UE shall perform the actual UL PDCP Excess Packet Delay per DRB measurement as specified in TS 38.314 [53] and the UE shall ignore the fields *reportQuantityCell* and *maxReportCells*. The applicable values for the corresponding *reportInterval* are (one of the) {ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240, ms20480, ms40960, min1,min6, min12, min30}. The *reportInterval* indicates the periodicity for performing and reporting of UL PDCP Excess Packet Delay per DRB measurement as specified in TS 38.314 [53]. |
| ***useAllowedCellList***Indicates whether only the cells included in the allow-list of the associated measObject are applicable as specified in 5.5.4.1. |

|  |
| --- |
| *ReportSFTD-NR* field descriptions |
| ***cellForWhichToReportSFTD***Indicates the target NR neighbour cells for SFTD measurement between PCell and NR neighbour cells. |
| ***drx-SFTD-NeighMeas***Indicates that the UE shall use available idle periods (i.e. DRX off periods) for the SFTD measurement in NR standalone. The network only includes *drx-SFTD-NeighMeas* field when *reprtSFTD-NeighMeas* is set to true. |
| ***reportSFTD-Meas***Indicates whether UE is required to perform SFTD measurement between PCell and NR PSCell in NR-DC. |
| ***reportSFTD-NeighMeas***Indicates whether UE is required to perform SFTD measurement between PCell and NR neighbour cells in NR standalone. The network does not include this field if *reportSFTD-Meas* is set to *true*. |
| ***reportRSRP***Indicates whether UE is required to include RSRP result of NR PSCell or NR neighbour cells in SFTD measurement result, derived based on SSB. If it is set to true, the network should ensure that *ssb-ConfigMobility* is included in the measurement object for NR PSCell or NR neighbour cells. |

|  |
| --- |
| *RxTxPeriodical field descriptions* |
| ***reportAmount***This field indicates the number of UE Rx-Tx time difference measurement reports. If configured to *r1,* the network does not configure *rxTxReportInterval* and only one measurement is reported. If configured to *infinity*, UE periodically reports measurements according to the periodicity configured by *rxTxReportInterval*. |
| ***rxTxReportInterval***This field indicates the measurement reporting periodicity of UE Rx-Tx time difference. |

|  |
| --- |
| otherfield descriptions |
| ***MeasTriggerQuantity***SINR is applicable only for CONNECTED mode events. |

|  |
| --- |
| *ReportOnScellActivation* field descriptions |
| ***rsType***Indicates which RS is used to provide the measurement result. Only value *ssb* can be set in this release. |
| ***reportQuantityRS-Indexes***Indicates which measurement information per RS index is used to sort the reported measurement results and is included in the measurement report. |
| ***maxNrofRS-IndexesToReport***Max number of RS indexes to include in the measurement report. |
| ***includeBeamMeasurements***Indicates whether to include the measurement result per RS index in the measurement report. |

|  |
| --- |
| *CellIndividualOffsetList* field descriptions |
| ***cellIndividualOffset***Cell individual offsets applicable to a specific measurement event. |
| ***physCellId***Physical cell identity of a cell in the cell list. |

*END OF CHANGES*

*START OF CHANGES*

### 6.3.3 UE capability information elements

#### – *MeasAndMobParameters*

The IE *MeasAndMobParameters* is used to convey UE capabilities related to measurements for radio resource management (RRM), radio link monitoring (RLM) and mobility (e.g. handover).

*MeasAndMobParameters* information element

-- ASN1START

-- TAG-MEASANDMOBPARAMETERS-START

MeasAndMobParameters ::= SEQUENCE {

 measAndMobParametersCommon MeasAndMobParametersCommon OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

MeasAndMobParameters-v1700 ::= SEQUENCE {

 measAndMobParametersFR2-2-r17 MeasAndMobParametersFR2-2-r17 OPTIONAL

}

MeasAndMobParametersCommon ::= SEQUENCE {

 supportedGapPattern BIT STRING (SIZE (22)) OPTIONAL,

 ssb-RLM ENUMERATED {supported} OPTIONAL,

 ssb-AndCSI-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 eventB-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFDD-TDD ENUMERATED {supported} OPTIONAL,

 eutra-CGI-Reporting ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting ENUMERATED {supported} OPTIONAL

 ]],

 [[

 independentGapConfig ENUMERATED {supported} OPTIONAL,

 periodicEUTRA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFR1-FR2 ENUMERATED {supported} OPTIONAL,

 maxNumberCSI-RS-RRM-RS-SINR ENUMERATED {n4, n8, n16, n32, n64, n96} OPTIONAL

 ]],

 [[

 nr-CGI-Reporting-ENDC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 eutra-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

 eutra-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 reportAddNeighMeasForPeriodic-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverParametersCommon-r16 SEQUENCE {

 condHandoverFDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverFR1-FR2-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 nr-NeedForGap-Reporting-r16 ENUMERATED {supported} OPTIONAL,

 supportedGapPattern-NRonly-r16 BIT STRING (SIZE (10)) OPTIONAL,

 supportedGapPattern-NRonly-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 maxNumberCLI-RSSI-r16 ENUMERATED {n8, n16, n32, n64} OPTIONAL,

 maxNumberCLI-SRS-RSRP-r16 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

 maxNumberPerSlotCLI-SRS-RSRP-r16 ENUMERATED {n2, n4, n8} OPTIONAL,

 mfbi-IAB-r16 ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting-NPN-r16 ENUMERATED {supported} OPTIONAL,

 idleInactiveEUTRA-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

 idleInactive-ValidityArea-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 eutra-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

 pcellT312-r16 ENUMERATED {supported} OPTIONAL,

 supportedGapPattern-r16 BIT STRING (SIZE (2)) OPTIONAL

 ]],

 [[

 -- R4 19-2 Concurrent measurement gaps

 concurrentMeasGap-r17 CHOICE {

 concurrentPerUE-OnlyMeasGap-r17 ENUMERATED {supported},

 concurrentPerUE-PerFRCombMeasGap-r17 ENUMERATED {supported}

 } OPTIONAL,

 -- R4 19-1 Network controlled small gap (NCSG)

 nr-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

 eutra-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-1-1 per FR Network controlled small gap (NCSG)

 ncsg-MeasGapPerFR-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-1-2 Network controlled small gap (NCSG) supported patterns

 ncsg-MeasGapPatterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

 -- R4 19-1-3 Network controlled small gap (NCSG) supported NR-only patterns

 ncsg-MeasGapNR-Patterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

 -- R4 19-3-2 pre-configured measurement gap

 preconfiguredUE-AutonomousMeasGap-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-3-1 pre-configured measurement gap

 preconfiguredNW-ControlledMeasGap-r17 ENUMERATED {supported} OPTIONAL,

 handoverFR1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

 handoverFR2-1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

 -- RAN4 14-1: per-FR MG for PRS measurement

 independentGapConfigPRS-r17 ENUMERATED {supported} OPTIONAL,

 rrm-RelaxationRRC-ConnectedRedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 25-3: Parallel measurements with multiple measurement gaps

 parallelMeasurementGap-r17 ENUMERATED {n2} OPTIONAL,

 condHandoverWithSCG-NRDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-ENDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-NEDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-NRDC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-LengthReporting-NPN-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R4 25-1: Parallel measurements on multiple SMTC-s for a single frequency carrier

 parallelSMTC-r17 ENUMERATED {n4} OPTIONAL,

 -- R4 19-2-1 Concurrent measurement gaps for EUTRA

 concurrentMeasGapEUTRA-r17 ENUMERATED {supported} OPTIONAL,

 serviceLinkPropDelayDiffReporting-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 19-1-4 Network controlled small gap (NCSG) performing measurement based on flag deriveSSB-IndexFromCellInter

 ncsg-SymbolLevelScheduleRestrictionInter-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 eventD1-MeasReportTrigger-r17 ENUMERATED {supported} OPTIONAL,

 independentGapConfig-maxCC-r17 SEQUENCE {

 fr1-Only-r17 INTEGER (1..32) OPTIONAL,

 fr2-Only-r17 INTEGER (1..32) OPTIONAL,

 fr1-AndFR2-r17 INTEGER (1..32) OPTIONAL

 } OPTIONAL

 ]],

 [[

 interSatMeas-r17 ENUMERATED {supported} OPTIONAL,

 deriveSSB-IndexFromCellInterNon-NCSG-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R4 31-1 Enhanced L3 measurement reporting for unknown SCell activation if the valid L3 measurement results are available

 l3-MeasUnknownSCellActivation-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 31-3 Shorter measurement interval for unknown SCell activation

 shortMeasInterval-r18 ENUMERATED {supported} OPTIONAL,

 nr-NeedForInterruptionReport-r18 ENUMERATED {supported} OPTIONAL,

 measSequenceConfig-r18 ENUMERATED {supported} OPTIONAL,

 cellIndividualOffsetPerMeasEvent-r18 ENUMERATED {supported} OPTIONAL,

 ltm-MCG-r18 ENUMERATED {supported} OPTIONAL,

 ltm-SCG-r18 ENUMERATED {supported} OPTIONAL,

 ltm-MCG-NRDC-r18 ENUMERATED {supported} OPTIONAL,

 ltm-RACH-LessDG-r18 ENUMERATED {supported} OPTIONAL,

 ltm-RACH-LessCG-r18 ENUMERATED {supported} OPTIONAL,

 ltm-Recovery-r18 ENUMERATED {supported} OPTIONAL,

 ltm-ReferenceConfig-r18 ENUMERATED {supported} OPTIONAL,

 eventD2-MeasReportTrigger-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 32-1: Concurrent gaps with Pre-MG in a FR

 concurrentMeasGapsPreMG-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 32-4: Concurrent gaps with NCSG in a FR

 concurrentMeasGapsNCSG-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 32-7: Inter-RAT EUTRAN measurement without gap

 eutra-NoGapMeasurement-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 32-8: Effective measurement window for inter-RAT EUTRAN measurements

 eutra-MeasEMW-r18 BIT STRING (SIZE(6)) OPTIONAL,

 -- R4 32-9: Simultaneous reception of NR data and EUTRAN CRS within BWP with different numerology

 concurrentMeasCRS-InsideBWP-EUTRA-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 39-2a: SSB based inter-frequency L1-RSRP measurements with measurement gaps

 ltm-InterFreqMeasGap-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 39-7: Faster UE processing time during cell switch

 ltm-FastUE-Processing-r18 SEQUENCE {

 fr1-r18 ENUMERATED {ms10, ms15},

 fr2-r18 ENUMERATED {ms10, ms15},

 fr1-AndFR2-r18 ENUMERATED {ms20, ms30}

 } OPTIONAL,

 -- R4 39-8: Measurement validation based on EMR measurement during connection setup/resume

 measValidationReportEMR-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 39-9: Measurement validation based on non-EMR measurement during connection setup/resume

 measValidationReportNonEMR-r18 ENUMERATED {supported} OPTIONAL,

 enterAndLeaveCellReport-r18 ENUMERATED {supported} OPTIONAL,

 bestCellChangeReport-r18 ENUMERATED {supported} OPTIONAL,

 secondBestCellChangeReport-r18 ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersXDD-Diff ::= SEQUENCE {

 intraAndInterF-MeasAndReport ENUMERATED {supported} OPTIONAL,

 eventA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 sftd-MeasNR-Neigh ENUMERATED {supported} OPTIONAL,

 sftd-MeasNR-Neigh-DRX ENUMERATED {supported} OPTIONAL

 ]],

 [[

 dummy ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersFRX-Diff ::= SEQUENCE {

 ss-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithSSB ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithoutSSB ENUMERATED {supported} OPTIONAL,

 csi-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxNumberResource-CSI-RS-RLM ENUMERATED {n2, n4, n6, n8} OPTIONAL

 ]],

 [[

 simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

 ]],

 [[

 nr-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-ENDC-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 cli-RSSI-Meas-r16 ENUMERATED {supported} OPTIONAL,

 cli-SRS-RSRP-Meas-r16 ENUMERATED {supported} OPTIONAL,

 interFrequencyMeas-NoGap-r16 ENUMERATED {supported} OPTIONAL,

 simultaneousRxDataSSB-DiffNumerology-Inter-r16 ENUMERATED {supported} OPTIONAL,

 idleInactiveNR-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 6-2: Support of beam level Early Measurement Reporting

 idleInactiveNR-MeasBeamReport-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 increasedNumberofCSIRSPerMO-r16 ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersFR2-2-r17 ::= SEQUENCE {

 handoverInterF-r17 ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC-r17 ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC-r17 ENUMERATED {supported} OPTIONAL,

 idleInactiveNR-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-MEASANDMOBPARAMETERS-STOP

-- ASN1STOP

*END OF CHANGES*

*START OF CHANGES*

## 7.4 UE variables

#### – *VarMeasReportList*

The UE variable *VarMeasReportList* includes information about the measurements for which the triggering conditions have been met.

*VarMeasReportList UE variable*

-- ASN1START

-- TAG-VARMEASREPORTLIST-START

VarMeasReportList ::= SEQUENCE (SIZE (1..maxNrofMeasId)) OF VarMeasReport

VarMeasReport ::= SEQUENCE {

 -- List of measurement that have been triggered

 measId MeasId,

 cellsTriggeredList CellsTriggeredList OPTIONAL,

 numberOfReportsSent INTEGER,

 cli-TriggeredList-r16 CLI-TriggeredList-r16 OPTIONAL,

 tx-PoolMeasToAddModListNR-r16 Tx-PoolMeasList-r16 OPTIONAL,

 relaysTriggeredList-r17 RelaysTriggeredList-r17 OPTIONAL,

 reportedBestNeighbourCell-r18 SEQUENCE (SIZE (1..2)) OF PhysCellId OPTIONAL

}

CellsTriggeredList ::= SEQUENCE (SIZE (1..maxNrofCellMeas)) OF CHOICE {

 physCellId PhysCellId,

 physCellIdEUTRA EUTRA-PhysCellId,

 physCellIdUTRA-FDD-r16 PhysCellIdUTRA-FDD-r16

 }

CLI-TriggeredList-r16 ::= CHOICE {

 srs-RSRP-TriggeredList-r16 SRS-RSRP-TriggeredList-r16,

 cli-RSSI-TriggeredList-r16 CLI-RSSI-TriggeredList-r16

 }

SRS-RSRP-TriggeredList-r16 ::= SEQUENCE (SIZE (1.. maxNrofCLI-SRS-Resources-r16)) OF SRS-ResourceId

CLI-RSSI-TriggeredList-r16 ::= SEQUENCE (SIZE (1.. maxNrofCLI-RSSI-Resources-r16)) OF RSSI-ResourceId-r16

RelaysTriggeredList-r17 ::= SEQUENCE (SIZE (1.. maxNrofRelayMeas-r17)) OF SL-SourceIdentity-r17

-- TAG-VARMEASREPORTLIST-STOP

-- ASN1STOP

*END OF CHANGES*