**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (NR\_CA\_R16\_intra-Core) CR to add notes for SCS restrictions on CBWs in CA configurations - TS38.101-1, Rel-16 |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_CA\_R16\_intra-Core |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Different tables in section 5.5A Configurations give channel bandwidths for carriers but do not mention or indicate what are the SCSs supported. It should be clearly indicated to readers (including RAN5) that the SCS of each channel bandwidth for NR band is in Table 5.3.5-1 and that for the same band, not all UE channel bandwidths support the same SCSs. This will avoid the testing of non required CA combinations with non-supported SCSs for some channel bandwidths.  |
|  |  |
| ***Summary of change:*** | The following notes - NOTE 1 in Table 5.5A.1-1- NOTE 3 in Table 5.5A.2-1are updated with the text “For each channel bandwidth of each component carrier, refer to Table 5.3.5-1 for the applicable SCSs. For a given band, not all UE channel bandwidths support the same SCSs.” |
|  |  |
| ***Consequences if not approved:*** | Non required CA combinations with non-supported SCSs will be tested for some channel bandwidths. |
|  |  |
| ***Clauses affected:*** | 5.5A |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-1  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | r1: Remove the text NOTE from table headers that were added in the previous version of this CR. |

<<Unchanged sections skipped>>

<<Start of change>>

### 5.5A.1 Configurations for intra-band contiguous CA

Table 5.5A.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |
| --- |
| NR CA configuration / Bandwidth combination set |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated bandwidth (MHz) | Bandwidth combination set |
| CA\_n1B | - | 10 | 10,15 |  |  |  | 40 | 0 |
|  |  | 15 | 15,20 |  |  |  |  |  |
|  |  | 20 | 20 |  |  |  |  |  |
| CA\_n7B | CA\_n7B | 10 | 10, 15, 20, 30, 40 |  |  |  | 50 | 0 |
|  |  | 15 | 15, 20, 30 |  |  |  |  |  |
|  |  | 20 | 20, 30 |  |  |  |  |  |
| CA\_n40B | - | 20 | 80 |  |  |  | 100 | 0 |
|  |  | 50 | 50 |  |  |  |  |  |
| CA\_n41B | CA\_n41B | 10, 20, 30, 40, 50 | 10, 20, 30, 40, 50 |  |  |  | 100 | 0 |
| CA\_n41C | CA\_n41C | 40 | 80, 100 |  |  |  | 180 | 0 |
|  |  | 50, 60, 80 | 60, 80, 100 |  |  |  |  |  |
|  |  | 10 | 100 |  |  |  | 190 | 1 |
|  |  | 15, 20 | 90, 100 |  |  |  |  |  |
|  |  | 40 | 80, 90, 100 |  |  |  |  |  |
|  |  | 50, 60, 80, 90 | 60, 80, 90, 100 |  |  |  |  |  |
| CA\_n46B | - | 20, 40, 60 | 20, 40 |  |  |  | 100 | 0 |
| CA\_n46C | - | 60, 80 | 60, 80 |  |  |  | 160 | 0 |
| CA\_n46D | - | 60, 80 | 80 | 80 |  |  | 240 | 0 |
| CA\_n46M | - | 20, 40, 60 | 20, 40 | 20, 40 |  |  | 140 | 0 |
| CA\_n46N | - | Void  |  |  |  |  |  | 0 |
|  | - | 20, 40, 60 | 20, 40 | 20, 40 | 20, 40 |  | 180 | 1 |
| CA\_n46O | - | 20, 60 | 20, 40 | 20, 40 | 20, 40 | 20, 40 | 220 | 0 |
| CA\_n48B | CA\_n48B | 5 | 15, 20 |  |  |  | 40 | 0 |
|  |  | 10, 15, 20 | 10, 15, 20 |  |  |  |  |  |
|  |  | 15, 20 | 15, 20 |  |  |  |  |  |
|  | - | 10 | 50, 60, 80, 90 |  |  |  | 100 | 1 |
|  |  | 15, 20 | 40, 50, 60, 80 |  |  |  |  |  |
|  |  | 40 | 40, 50, 60 |  |  |  |  |  |
| CA\_n48C | - | 10 | 100 |  |  |  | 140 | 0 |
|  |  | 15 | 90,100 |  |  |  |  |  |
|  |  | 20 | 90, 100 |  |  |  |  |  |
|  |  | 40 | 80, 90, 100 |  |  |  |  |  |
| CA\_n66B | - | 5 | 20, 40 |  |  |  | 50 | 0 |
|  |  | 10 | 15, 20, 40 |  |  |  |  |  |
|  |  | 15 | 15, 20 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| CA\_n71B | - | 5 | 20 |  |  |  | 25 | 0 |
|  |  | 10 | 15 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  | 10 | 20 |  |  |  | 35 | 1 |
|  |  | 15 | 15, 20 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| CA\_n77C | CA\_n77C | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
|  |  | 60 | 60, 80, 100 |  |  |  |  |  |
|  |  | 80 | 80, 100 |  |  |  |  |  |
|  |  | 100 | 100 |  |  |  |  |  |
|  |  | 10 |  100 |  |  |  | 200 | 1 |
|  |  | 15, 20 | 90, 100 |  |  |  |  |  |
|  |  | 25, 30 | 80, 90, 100 |  |  |  |  |  |
|  |  | 40 | 70, 80, 90, 100 |  |  |  |  |  |
|  |  | 50, 60, 70, 80, 90, 100 | 60, 70, 80, 90, 100 |  |  |  |  |  |
| CA\_n77D | - | 100 | 100 | 100 |  |  | 300 | 0 |
| CA\_n78B | - | 20 | 50 |  |  |  | 70 | 0 |
| CA\_n78C | CA\_n78C | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
|  |  | 60 | 60, 80, 100 |  |  |  |  |  |
|  |  | 80 | 80, 100 |  |  |  |  |  |
|  |  | 100 | 100 |  |  |  |  |  |
|  |  | 10 | 100 |  |  |  | 200 | 1 |
|  |  | 15, 20 | 90, 100 |  |  |  |  |  |
|  |  | 25, 30 | 80, 90, 100 |  |  |  |  |  |
|  |  | 40 | 70, 80, 90, 100 |  |  |  |  |  |
|  |  | 50, 60, 70, 80, 90, 100 | 60, 70, 80, 90, 100 |  |  |  |  |  |
| CA\_n78D | - | 100 | 100 | 100 |  |  | 300 | 0 |
| CA\_n79C | CA\_n79C | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
|  |  | 60 | 60, 80, 100 |  |  |  |  |  |
|  |  | 80 | 80, 100 |  |  |  |  |  |
|  |  | 100 | 100 |  |  |  |  |  |
| CA\_n79D | - | 100 | 100 | 100 |  |  | 300 | 0 |
| NOTE 1: For each channel bandwidth of each component carrier, refer to Table 5.3.5-1 for the applicable SCSs. For a given band, not all UE channel bandwidths support the same SCSs. |

Table 5.5A.1-2: Void

### 5.5A.2 Configurations for intra-band non-contiguous CA

Table 5.5A.2-1: NR CA configurations and bandwidth combination sets defined for intra-band non-contiguous CA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | MaximumAggregated bandwidth(MHz) | Bandwidth combination set |
| CA\_n3(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n7(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n25(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n41(2A) | CA\_n41(2A) | 40, 50, 60, 80 | 40, 50, 60, 80, 100 |  |  | 180 | 0 |
|  |  | 10, 15, 20, 40, 50, 60, 80, 90 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 190 | 1 |
| CA\_n48(2A) | - | 10, 15, 20, 40, 50, 60 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 1402 | 0 |
| CA\_n48(3A) | - | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 |  | 1402 | 0 |
| CA\_n48(4A) | - | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 1352 | 0 |
| CA\_n66(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20, 40 |  |  | 60 | 0 |
| CA\_n77(2A) | CA\_n77(2A) | 20, 40, 80, 100 | 20, 40, 80, 100 |  |  | 200 | 0 |
| CA\_n78(2A) | CA\_n78(2A) | 10, 20, 40, 50, 60, 80, 90, 100 | 10, 20, 40, 50, 60, 80, 90, 100 |  |  | 200 | 0 |
|  |  | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |  | 200 | 1 |
|  |  | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 200 | 2 |
| NOTE 1: Void.NOTE 2: Parameter value accounts for both, the maximum frequency range of band n48 (150 MHz), and the minimum frequency gaps in between NR non-contiguous component carriers.NOTE 3: For each channel bandwidth of each component carrier, refer to Table 5.3.5-1 for the applicable SCSs. For a given band, not all UE channel bandwidths support the same SCSs. |

<<Unchanged sections skipped>>

<<End of change>>