**3GPP TSG-RAN WG4 Meeting #111R4-24xxxxx**

**Fukuoka, Japan, 20th May - 24th May 2024**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **36.108** | **CR** | **0025** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (TEI18) CR to 36.108 In-band NB-IoT NTN deployment with NR from Rel-18 [TEI\_NTN] |
|  |  |
| ***Source to WG:*** | Inmarsat, Viasat, Omnispace, Terrestar Solutions, Thuraya, Ligado Networks, EchoStar, Thales, Skyworks, Apple  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | TEI18 |  | ***Date:*** | 2024-05-09 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | NB-IoT supports In-band and guard-band deployments with LTE carriers since Rel-13 and in-band with NR carriers since Rel-15. Based on the conclusions of TR 37.824 and of the approved TP in R4- 2220812, the current channel arrangement and offset values can already support in-band deployment with NR. However, clarification is required in the spec. |
|  |  |
| ***Summary of change:*** | Clarify support for in-band deployment of NB-IoT NTN with NR NTN carriers in the same SAN. |
|  |  |
| ***Consequences if not approved:*** | If not supported by UE: NB-IoT UE will not be able to access the network with carriers deployed in-band with NR NTNIf not supported by the Network: Operators will not be able to deploy NB-IoT NTN in-band with NR NTN |
|  |  |
| ***Clauses affected:*** | 5.4B.1, 5.4B.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

###

### << START OF CHANGE >>

## 5.4B Channel arrangement for category NB1 and NB2

### 5.4B.1 Channel spacing

Nominal channel spacing for UE category NB1 and NB2 in stand-alone mode is 200 kHz. For in-band case, the nominal channel spacing between two adjacent category NB1 or NB2 carriers is 180 kHz.

### 5.4B.2 Channel raster, carrier frequency and EARFCN

The channel raster of UE category NB1/NB2 shall be as defined in clause 5.4A.2, and the channel raster per-frequency band shall be as defined in table 5.4A.2-1.

The carrier frequency of UE category NB1/NB2 in the downlink is designated by the E-UTRA Absolute Radio Frequency Channel Number (EARFCN) as defined in Table 5.4A.2-1, and the Offset of category NB1/NB2 Channel Number to EARFCN in the range of {-10, -9, -8, -7, -6, -5, -4, -3, -2, -1, -0.5, 0, 1, 2, 3, 4, 5, 6, 7, 8, 9} for FDD. The relation between EARFCN, Offset of category NB1/NB2 Channel Number to EARFCN and the carrier frequency in MHz for the downlink is given by the following equation, where FDL is the downlink carrier frequency of category NB1/NB2, FDL\_low and NOffs-DL are given in table 5.4A.2-1, NDL is the downlink EARFCN, MDL is the Offset of category NB1/NB2 Channel Number to downlink EARFCN.

FDL = FDL\_low + 0.1(NDL – NOffs-DL) + 0.0025\*(2MDL)

The carrier frequency of UE category NB1/NB2 in the uplink is designated by the E-UTRA Absolute Radio Frequency Channel Number (EARFCN) as defined in Table 5.4A.2-1, and the Offset of category NB1/NB2 Channel Number to EARFCN in the range of {-10, -9, -8, -7, -6, -5, -4, -3, -2, -1, 0, 1, 2, 3, 4, 5, 6, 7, 8, 9} for FDD. The relation between EARFCN, Offset of category NB1/NB2 Channel Number to EARFCN and the carrier frequency in MHz for the uplink is given by the following equation, where FUL is the uplink carrier frequency of category NB1/NB2, FUL\_low and NOffs-UL are given in table 5.4A.2-1, NUL is the uplink EARFCN, MUL is the Offset of category NB1/NB2 Channel Number to uplink EARFCN.

FUL = FUL\_low + 0.1(NUL – NOffs-UL) + 0.0025\*(2MUL)

NOTE 1:

NOTE 2: For the carrier including NPSS/NSSS for stand-alone operation, MDL = 0.

### << END OF CHANGE >>