**3GPP TSG-RAN WG4 Meeting #111 R4-24xxxxx**

**Fukuoka, Japan, 20 – 24 May 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **-1** | **CR** |  | **rev** |  | **Current version:** | **0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draftCR 38.101-1 to add new NR CA 3BDL configurations | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, T-Mobile USA | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_3BDL\_xBUL | | | | |  | ***Date:*** | | | 2024-05-20 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To add new NR CA 3BDL configurations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | To add:  CA\_n25(2A)-n66(2A)-n71B  CA\_n25(2A)-n66A-n85A  CA\_n25(2A)-n71A-n85A  CA\_n25A-n66(2A)-n85A  CA\_n25A-n71(2A)-n85A  CA\_n25A-n71B-n85A  CA\_n66(2A)-n71A-n85A  CA\_n66A-n71(2A)-n85A  CA\_n66A-n71B-n85A | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | New NR CA 3BDL configurations are not included in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

#### 5.5A.3.2 Configurations for inter-band CA (three bands)

---Text omitted---

Table 5.5A.3.2-1b: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration  or single uplink carrier6 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n8A-n20A-n28A | CA\_n8A-n20A | n8 | 5, 10, 15, 20 | 0 |
|  | CA\_n8A-n28A | n20 | 5, 10, 15, 20 |  |
|  | CA\_n20A-n28A | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n8A-n20A-n75A | - | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n28A-n75A | - | n8 | n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n28A-n78A | - | n8 | 5, 10, 15, 20 | 0 |
|  | n28 | 5, 10, 15, 20 |
|  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
| CA\_n8A-n38A-n40A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n39A-n41A | CA\_n8A-n39A  CA\_n8A-n41A  CA\_n39A-n41A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  | - | n8 | 5, 10, 15, 20 | 1 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  | CA\_n8A-n39A  CA\_n8A-n41A  CA\_n39A-n41A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n39A-n41C | CA\_n8A-n39A  CA\_n8A-n41A  CA\_n39A-n41A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n8A-n39A-n79A | CA\_n8A-n39A  CA\_n8A-n79A  CA\_n39A-n79A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n40A-n41A | CA\_n8A-n40A  CA\_n8A-n41A  CA\_n40A-n41A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n40A-n41C | CA\_n41C  CA\_n8A-n40A  CA\_n8A-n41A  CA\_n40A-n41A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n8A-n40A-n78A | CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n41A-n79A | CA\_n8A-n41A  CA\_n8A-n79A  CA\_n41A-n79A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n8 | 5, 10, 15, 20 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n41C-n79A | CA\_n41C  CA\_n8A-n41A  CA\_n8A-n79A  CA\_n41A-n79A | n8 | See n8 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n8A-n78A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n78(2A)-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n12A-n25A-n41A | - | n12 | 5, 10, 15 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n12A-n25A-n66A | - | n12 | 5, 10, 15 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n12A-n30A-n66A | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n12A-n30A-n66(2A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n12A-n30A-n66(3A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n12A-n30A-n77A | n777,9  CA\_n12A-n30A,  CA\_n12A-n77A7  CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n77(2A) | n777,9  CA\_n12A-n30A  CA\_n12A-n77A7  CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n41A-n66A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n12A-n41A-n77A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66A-n77A | n777,9  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66(2A)-n77A | n777,9  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66A-n77(2A) | n777,9  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n66(2A)-n77(2A) | n777  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n66(3A)-n77A | n777  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66(3A)-n77(2A) | n777  CA\_n12A-n66A  CA\_n12A-n77A7  CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n71A-n77A | CA\_n12A-n77A  CA\_n71A-n77A | n12 | 5, 10, 15 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n25A-n66A | CA\_n13A-n25A  CA\_n13A-n66A  CA\_n25A-n66A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n25A-n77A | n777,9  CA\_n13A-n25A  CA\_n13A-n77A7  CA\_n25A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n25A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n13A-n25A  CA\_n13A-n77A7  CA\_n25A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n66A-n77A | n777, 9  CA\_n13A-n66A  CA\_n13A-n77A7  CA\_n66A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n66A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n13A-n66A  CA\_n13A-n77A7  CA\_n66A-n77A7 | n13 | 5, 10 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66A | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n14A-n30A-n66(2A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66(3A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n14A-n30A-n77A | n777,9  CA\_n14A-n30A  CA\_n14A-n77A7  CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n77(2A) | n777,9  CA\_n14A-n30A  CA\_n14A-n77A7  CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66A-n77A | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66(2A)-n77A | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66A-n77(2A) | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66(2A)-n77(2A) | n777,9  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66(3A)-n77A | n777  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66(3A)-n77(2A) | n777  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n28A-n41A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77A | n777  CA\_n18A-n28A  CA\_n18A-n77A7  CA\_n28A-n77A7 | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77(2A) | n777  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n41A-n77A | n417  n777  CA\_n18A-n41A7  CA\_n18A-n77A7  CA\_n41A-n77A7 | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n41A-n77(2A) | n777  CA\_n18A-n41A7  CA\_n18A-n77A7  CA\_n41A-n77A7 | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n20A-n28A-n75A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n75 | 5, 10, 15, 20 |  |
| CA\_n20A-n28A-n78A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n20A-n28A-n78C | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n20A-n67A-n78A | CA\_n20A-n78A | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | See n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n20A-n67A-n78(2A) | CA\_n20A-n78A  CA\_n78(2A) | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | See n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n24A-n41A-n48A | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
| CA\_n24A-n41(2A)-n48A | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
| CA\_n24A-n41A-n48(2A) | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n48(2A) | CA\_n24A-n41A  CA\_n24A-n48A  CA\_n41A-n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41A-n77A | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41(2A)-n77A | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41A-n77(2A) | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n77(2A) | CA\_n24A-n41A  CA\_n24A-n77A  CA\_n41A-n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48A-n77A | - | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48(2A)-n77A | - | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48A-n77(2A) | - | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48(2A)-n77(2A) | - | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n25A-n29A-n66A | CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41C-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7  CA\_n25A-n41C  CA\_n41C-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(3A)-n66A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n66A | n417,9  CA\_n25A-n41A7  CA\_n25A-n66A  CA\_n41A-n66A7  CA\_n41C7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n66(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(A-C)-n66A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A  CA\_n41C | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41A-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(3A)-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41(3A)-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41C-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7  CA\_n25A-n41C  CA\_n41C-n71A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41C-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41(A-C)-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71B | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n71(2A) | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(3A)-n71A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n71A | n417,9  CA\_n25A-n41A7  CA\_n25A-n71A  CA\_n41A-n71A7  CA\_n41C7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C-n71(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n71B | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(A-C)-n71A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n41A-n71A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(3A)-n77A | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77(2A) | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n77(2A) | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n77A | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n77(2A) | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(2A)-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77A | n417,9  n777,9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(A-C)-n77A | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77(2A) | n417,9  n777.9  CA\_n25A-n41A7  CA\_n25A-n77A7  CA\_n41A-n77A7  CA\_n41C7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41C-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A)-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41(3A)-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41(A-C)-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A  CA\_n41C | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n78A | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n41A-n78(2A) | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n85A | CA\_n25A-n41A  CA\_n25A-n85A  CA\_n41A-n85A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n48A-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48(2A)-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48C-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n66A-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66(2A)-n71B | CA\_n25A-n66A CA\_n25A-n71A CA\_n66A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n66A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n25A-n66(2A)-n77(2A) | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n77A | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n77(2A) | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66(2A)-n77(2A) | n777,9  CA\_n25A-n66A  CA\_n25A-n77A7  CA\_n66A-n77A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n66A-n78A | n787,9  CA\_n25A-n66A  CA\_n25A-n78A7  CA\_n66A-n78A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78A | n787,9  CA\_n25A-n66A CA\_n25A-n78A7 CA\_n66A-n78A7 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66A-n78(2A) | n787  CA\_n78(2A)7  CA\_n25A-n66A CA\_n25A-n78A7 CA\_n66A-n78A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66A-n85A | CA\_n25A-n66A  CA\_n25A-n85A  CA\_n66A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n85A | CA\_n25A-n66A CA\_n25A-n85A CA\_n66A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n85A | CA\_n25A-n66A CA\_n25A-n85A CA\_n66A-n85A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71A-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A) BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A) BCS1 |  |
| CA\_n25A-n71B-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71B-n77(2A) | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71(2A)-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71(2A)-n77(2A) | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n71A-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71A-n77(2A) | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n71B-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71B-n77(2A) | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n71(2A)-n77A | n777,9  CA\_n25A-n71A  CA\_n25A-n77A7  CA\_n71A-n77A7 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71(2A)-n77(2A) | n77  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n71A-n78A | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n71A-n78(2A) | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n71A-n85A | CA\_n25A-n71A  CA\_n25A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71B-n85A | CA\_n25A-n71A CA\_n25A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71(2A)-n85A | CA\_n25A-n71A CA\_n25A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71A-n85A | CA\_n25A-n71A CA\_n25A-n85A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n77A-n85A | CA\_n25A-n77A  CA\_n25A-n85A  CA\_n77A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n77(2A)-n85A | CA\_n25A-n77A  CA\_n25A-n85A  CA\_n77A-n85A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n77A-n85A | CA\_n25A-n77A  CA\_n25A-n85A  CA\_n77A-n85A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n26A-n29A-n66A | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n29A-n66(2A) | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n26A-n29A-n66(3A) | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n26A-n29A-n70A | CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
| CA\_n26A-n48A-n66A | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n48(2A)-n66A | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n48A-n66(2A) | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n26A-n48(2A)-n66(2A) | CA\_n26A-n48A  CA\_n26A-n66A  CA\_n48A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n26A-n48A-n70A | CA\_n26A-n48A  CA\_n26A-n70A  CA\_n48A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 5012, 6012, 8012, 9012, 10012 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
| CA\_n26A-n66A-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66(2A)-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66(3A)-n70A | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66A-n71A | CA\_n26A-n66A  CA\_n66A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n66(2A)-n71A | CA\_n26A-n66A  CA\_n66A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n66(3A)-n71A | CA\_n66A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n66A-n77A | CA\_n26A-n66A  CA\_n26A-n77A  CA\_n66A-n77A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n70A-n71A | CA\_n26A-n70A  CA\_n70A-n71A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n70A-n77A | CA\_n26A-n70A  CA\_n26A-n77A  CA\_n70A-n77A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n28A-n38A-n78A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n39A-n40A | CA\_n28A-n39A  CA\_n28A-n40A  CA\_n39A-n40A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
| CA\_n28A-n39A-n41A | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n39A-n41C | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n28A-n39A-n79A | CA\_n28A-n39A  CA\_n28A-n79A  CA\_n39A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n40A-n41A | CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n40A-n41C | CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C\_BCS0 |  |
| CA\_n28A-n40A-n78A | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n40A-n77A | CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n40A-n77(2A) | CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n28A-n40B-n78A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n40A-n79A | CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41A-n77A | n417,9  n777,9  CA\_n28A-n41A7 | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41B-n77A | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41A-n77(2A) | n417,9  n777,9  CA\_n28A-n41A7 | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n28A-n41A-n77(3A) | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n28A-n41A-n78A | CA\_n28A-n41A  CA\_n41A-n78A  CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n41A-n78(2A) | CA\_n78(2A) | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n41A-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n41A-n79C | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n28A-n41C-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n41C-n79C | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n28A-n46A-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46C-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46D-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46(2A)-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46(2A)-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46A-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46C-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n46D-n78(2A) | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n75A-n78A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n77A-n79A4 | n777,9  n797,9  CA\_n28A-n77A7  CA\_n28A-n79A7  CA\_n77A-n79A7 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n77(2A)-n79A4 | n777,9  n797,9  CA\_n28A-n77A7  CA\_n28A-n79A7  CA\_n77A-n79A7 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n77(3A)-n79A4 | CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n78A-n79A | n787,9  n797,9  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n78A-n102A | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n78A-n102B | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102B  CA\_n78A-n102A  CA\_n78A-n102B | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n78A-n102C | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102C  CA\_n78A-n102A  CA\_n78A-n102C | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n78A-n102D | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n78A-n102E | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n78A-n102(2A) | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n28A-n78(2A)-n102A | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n78(2A)-n102B | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102B  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n78(2A)-n102C | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n28A-n102C  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n78(2A)-n102D | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n78(2A)-n102E | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n78(2A)-n102(2A) | CA\_n28A-n78A  CA\_n28A-n102A  CA\_n78A-n102A  CA\_n78(2A) | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n29A-n30A-n66A | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n29A-n30A-n66(2A) | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n29A-n30A-n77A | n777,9  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n30A-n77(2A) | n777,9  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66A-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66B-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66(2A)-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66(3A)-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66A-n71A | CA\_n66A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n66(2A)-n71A | CA\_n66A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n66(3A)-n71A | CA\_n66A-n71A | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n66A-n77A | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66(2A)-n77A | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66A-n77(2A) | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66(3A)-n77A | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66(2A)-n77(2A) | n777,9  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66(3A)-n77(2A) | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n70A-n71A | CA\_n70A-n71A | n29 | 5, 10 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n30A-n66A-n77A | n777,9  CA\_n30A-n66A  CA\_n30A-n77A7  CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66(2A)-n77A | n777,9  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66A-n77(2A) | n777,9  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n30A-n66(2A)-n77(2A) | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n30A-n66(3A)-n77A | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66(3A)-n77(2A) | n777  CA\_n30A-n66A  CA\_n30A-n77A7  CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n34A-n39A-n40A | CA\_n34A-n39A  CA\_n34A-n40A  CA\_n39A-n40A | n34 | 5, 10, 15 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n39A-n41A | CA\_n34A-n39A  CA\_n34A-n41A  CA\_n39A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n39A-n41C | CA\_n34A-n39A  CA\_n34A-n41A  CA\_n39A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n34A-n40A-n41A | CA\_n34A-n40A  CA\_n34A-n41A  CA\_n40A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n40A-n41C | CA\_n34A-n40A  CA\_n34A-n41A  CA\_n40A-n41A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n34A-n41A-n79A | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41A-n79C | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n34A-n41C-n79A | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41C-n79C | CA\_n34A-n41A  CA\_n34A-n79A  CA\_n41A-n79A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n38A-n66A-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66A-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n38A-n66(2A)-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66(2A)-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n39A-n40A-n41A | CA\_n39A-n40A  CA\_n39A-n41A  CA\_n40A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n40A-n41C | CA\_n39A-n40A  CA\_n39A-n41A  CA\_n40A-n41A | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n39A-n40A-n79A | CA\_n39A-n40A  CA\_n40A-n79A  CA\_n39A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n40 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41A-n79C | CA\_n39A-n41A  CA\_n39A-n79A  CA\_n41A-n79A | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | CA\_n79C\_BCS 4 and 5 |  |
| CA\_n39A-n41A-n79A | CA\_n39A-n41A  CA\_n39A-n79A  CA\_n41A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n40A-n41A-n79A | CA\_n40A-n41A  CA\_n40A-n79A  CA\_n41A-n79A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n41C-n79A | CA\_n41C  CA\_n41A-n79A  CA\_n40A-n41A  CA\_n40A-n79A | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n78A-n105A | CA\_n40A-n78A  CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n41A-n66A-n70A | CA\_n41A-n66A  CA\_n41A-n70A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n41A-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71B | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41A-n66A-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71A | n417,9  CA\_n41A-n66A7  CA\_n66A-n71A  CA\_n41A-n71A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n71B | n417,9  CA\_n41A-n66A7  CA\_n66A-n71A  CA\_n41A-n71A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n66A-n71A  CA\_n41A-n71A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n66A-n71A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71B | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A)-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66(2A)-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A)-n71B | CA\_n41A-n71A  CA\_n41A-n66A CA\_n66A-n71A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66(2A)-n71A | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66A-n71B | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41C-n66A-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71B | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41C-n66A-n71(2A) | n417,9  CA\_n41A-n66A7  CA\_n41A-n71A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41C-n66(2A)-n71A | n417,9  CA\_n41A-n71A7  CA\_n41A-n66A7  CA\_n41C7  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A)-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n41C  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41C-n66(2A)-n71B | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n41C  CA\_n66A-n71A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n71A | n417,9  CA\_n41C7  CA\_n41A-n71A7  CA\_n41A-n66A7 CA\_n66A-n71A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n66A-n71B | CA\_n41A-n66A CA\_n41A-n71A CA\_n41C CA\_n66A-n71A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n71(2A) | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41C | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n66(2A)-n71A | CA\_n41A-n71A  CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41C | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77(2A) | n417,9  n777,9  CA\_n41A-n77A7  CA\_n41A-n66A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n77(2A) | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n77(2A) | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66(2A)-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n66A-n77A7 | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66(2A)-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n77(2A) | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n66(2A)-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A)-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n41C  CA\_n66A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A-n77A | n417,9  n777,9  CA\_n41A-n66A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n66A-n77A7 | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n66(2A)-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n41C  CA\_n66A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66(2A)-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66(2A)-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66A-n85A | CA\_n41A-n66A  CA\_n41A-n85A  CA\_n66A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n85A | CA\_n41A-n66A  CA\_n41A-n85A  CA\_n66A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n85A | CA\_n41A-n66A CA\_n41A-n85A CA\_n66A-n85A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n85A | CA\_n41A-n66A CA\_n41A-n85A CA\_n41C CA\_n66A-n85A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n70A-n78A | CA\_n41A-n70A  CA\_n41A-n78A  CA\_n70A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71A-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71A-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71(2A)-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n71A-n77A7 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n71B-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n71(2A)-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(3A)-n71B-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n71(2A)-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(3A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71B-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71(2A)-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71A-n77(2A) | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n71B-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n71(2A)-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(A-C)-n71A-n77A | n417,9  n777,9  CA\_n41A-n71A7  CA\_n41A-n77A7  CA\_n41C7  CA\_n71A-n77A7 | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n71B-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n71(2A)-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n41C  CA\_n71A-n77A | n41 | CA\_n41(A-C) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71A-n78A | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n78(2A) | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n71A-n85A | CA\_n41A-n71A  CA\_n41A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n85A | CA\_n41A-n71A  CA\_n41A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71(2A)-n85A | CA\_n41A-n71A  CA\_n41A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n77A-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77(2A)-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77(3A)-n79A | CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n41A-n77A-n85A | CA\_n41A-n77A  CA\_n41A-n85A  CA\_n77A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n77A-n85A | CA\_n41A-n77A CA\_n41A-n85A CA\_n77A-n85A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n77(2A)-n85A | CA\_n41A-n77A CA\_n41A-n85A CA\_n77A-n85A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n77A-n85A | CA\_n41A-n77A CA\_n41A-n85A CA\_n41C CA\_n77A-n85A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |

Table 5.5A.3.2-1c: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration  or single uplink carrier6 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n46A-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48A-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48B-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48C-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48C-n96A | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 1001 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48A-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48A-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48A-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48A-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48A-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48A-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48A-n96C | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48B-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48B-n96C | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48C-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48C-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48C-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48C-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48C-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48C-n96C | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48A-n96D | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48A-n96D | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48A-n96D | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48A-n96D | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48A-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48A-n96D | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48C-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48C-n96D | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48A-n96E | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48A-n96E | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48A-n96E | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48A-n96E | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48A-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48A-n96E | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48C-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48C-n96E | CA\_n46A-n48A  CA\_n46A-n48B  CA\_n48A-n96A  CA\_n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(2A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(2A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(2A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(2A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(2A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(3A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(3A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(3A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(3A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(3A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(4A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(4A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(4A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(4A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46A-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46A-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46A-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46A-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46A-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46(2A)-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46(2A)-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46(2A)-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46(2A)-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46(2A)-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46(2A)-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46C-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46C-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46C-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46C-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46C-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46C-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46D-n78A-n102A | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46D-n78A-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46D-n78A-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46D-n78A-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46D-n78A-n102E | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46D-n78A-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46A-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46A-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46A-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46A-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46A-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46A-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | 10,20, 40, 60, 80, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46(2A)-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  | CA\_n78(2A) | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46(2A)-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46C-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46C-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46C-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46C-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46C-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46C-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46D-n78(2A)-n102A | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46D-n78(2A)-n102B | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102B  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46D-n78(2A)-n102C | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78A-n102C  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46D-n78(2A)-n102D | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46D-n78(2A)-n102E | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46D-n78(2A)-n102(2A) | CA\_n46A-n78A  CA\_n78A-n102A  CA\_n78(2A) | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n48A-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66(2A)-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48(2A)-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48B-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66(2A)-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n66A-n71A | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66A-n71(2A) | CA\_n48A-n66A  CA\_n48A-n71A  CA\_n66A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48A-n66A-n77A | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66(2A)-n77A | CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66A-n77C | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7  CA\_n77C | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48B-n66A-n77C | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7  CA\_n77C | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48B-n66A-n77A | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77A | n777,9  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77C | n777,9  CA\_n77C  CA\_n48A-n66A  CA\_n66A-n77A7 | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 3 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48A-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n70A-n71A | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n70A-n71(2A) | CA\_n48A-n70A  CA\_n48A-n71A  CA\_n70A-n71A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48A-n70A-n77A | CA\_n48A-n70A  CA\_n70A-n77A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n70A-n77A | CA\_n48A-n70A  CA\_n70A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n71A-n77A | CA\_n48A-n71A  CA\_n71A-n77A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n71A-n77A | CA\_n48A-n71A  CA\_n71A-n77A | n48 | 5, 10, 15, 20, 30, 40, 5012, 6012, 7012, 8012, 9012, 10012 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A-n78A | CA\_n66A-n78A CA\_n70A-n78A | n66 | 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71(2A) | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n66B-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201,251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66(2A)-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66(3A)-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A-n77A | CA\_n66A-n77A  CA\_n70A-n77A | n66 | 5, 10, 15, 20, 25, 30, 35, 40 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n70A-n77A | CA\_n66A-n77A  CA\_n70A-n77A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n71A-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n77(2A) | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71(2A)-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71(2A)-n77(2A) | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71A-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71A-n77(2A) | n777,9  CA\_n77(2A)7  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71A-n77(3A) | n777,9  CA\_n77(2A)7  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n66(2A)-n71B-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71B-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71(2A)-n77A | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71A-n77(2A) | n777,9  CA\_n66A-n71A  CA\_n66A-n77A7  CA\_n71A-n77A7 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  | n71 | 5, 10, 15, 20 |  |
|  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71(2A)-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71A-n78A | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n71A-n78(2A) | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n66(2A)-n71A-n78A | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n71A-n78(2A) | CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n66A-n71A-n85A | CA\_n66A-n71A  CA\_n66A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n85A | CA\_n66A-n71A CA\_n66A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71(2A)-n85A | CA\_n66A-n71A CA\_n66A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71A-n85A | CA\_n66A-n71A CA\_n66A-n85A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n77A-n85A | CA\_n66A-n77A  CA\_n66A-n85A  CA\_n77A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n77(2A)-n85A | CA\_n66A-n77A CA\_n66A-n85A CA\_n77A-n85A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n77A-n85A | CA\_n66A-n77A  CA\_n66A-n85A  CA\_n77A-n85A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n85 | n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n70A-n71A-n77A | CA\_n70A-n71A  CA\_n70A-n77A  CA\_n71A-n77A | n70 | 5, 10, 15, 20, 25 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |

---End of changes---