**3GPP TSG-RAN WG4 Meeting #111 *R4-2407618***

**Fukuoka, Japan, May 20 – May 24, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** | **<CR#>** | **rev** | **<Rev#>** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR for TS 38.101-1 to introduce FR1 inter-band BCS 4 and 5 with two bands CA | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_2BDL\_xBUL-Core | | | | |  | ***Date:*** | | | 2024-04-27 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19) Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To introduce BCS4&5 for the following CA combos with two bands.  CA\_n40B-n78(2A): the fallback CA\_n40A-n78(2A) with BCS4&5 is supported in the specification, and CA\_n40B with BCS 4&5 is included in the endorsed CR R4-2405332 in RAN4#110bis.  CA\_n77A-n79A/CA\_n77(2A)-n79A with BCS4&5: No need to update MSD test configuration. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | To introduce BCS4&5 for the following CA combos with two bands.  CA\_n40B-n78(2A) and CA\_n77A-n79A/CA\_n77(2A)-n79A | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Current specification can’t support CA\_n40B-n78(2A) and CA\_n77A-n79A/CA\_n77(2A)-n79A. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## **<<Start of Change>>**

#### 5.5A.3.1 Configurations for inter-band CA (two bands)

**<<Uchanged part omitted>>**

##### Table 5.5A.3.1-1f ~ Table 5.5A.3.1-1j

Table 5.5A.3.1-1f: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n12A-n25A | CA\_n12A-n25A | n12 | 5, 10, 15 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n12A-n30A | CA\_n12A-n30A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
| CA\_n12A-n41A | - | n12 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n48A | - | n12 | 5, 10, 15 | 0 |
|  |  | n48 | 10, 15, 20, 30, 40 |  |
| CA\_n12A-n66A | CA\_n12A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n12A-n66(2A) | CA\_n12A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n12A-n66(3A) | CA\_n12A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n12A-n71A | - | n12 | 5, 10, 15 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n12A-n77A | n778, 9  CA\_n12A-n77A8 | n12 | 5, 10, 15 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n12A-n77B | - | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n12A-n77C | - | n12 | n12 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n12A-n77(2A) | n778, 9  CA\_n12A-n77A8 | n12 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n78A | CA\_n12A-n78A | n12 | 5, 10, 15 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n78(2A) | CA\_n12A-n78A | n12 | 5, 10, 15 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n13A-n25A | CA\_n13A-n25A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n66A | CA\_n13A-n66A | n13 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n13 | 5, 10, | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n77A | n778, 9  CA\_n13A-n77A8 | n13 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n77(2A) | n778,9  CA\_n77(2A)8  CA\_n13A-n77A8 | n13 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n77C | n778,9  CA\_n77C  CA\_n13A-n77A8 | n13 | 5, 10 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n14A-n30A | CA\_n14A-n30A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
| CA\_n14A-n66A | CA\_n14A-n66A | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n14A-n66(2A) | CA\_n14A-n66A | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n14A-n66(3A) | CA\_n14A-n66A | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n14A-n77A | n778, 9  CA\_n14A-n77A8 | n14 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n77(2A) | n778, 9  CA\_n14A-n77A8 | n14 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n28A | CA\_n18A-n28A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
| CA\_n18A-n40A | CA\_n18A-n40A | n18 | 5, 10, 15 | 0 |
|  |  | n40 | 10, 15, 20, 30, 40 |  |
| CA\_n18A-n41A | n418  CA\_n18A-n41A8 | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n74A | CA\_n18A-n74A | n18 | 5, 10, 15 | 0 |
|  |  | n74 | 5, 10, 15, 20 |  |
| CA\_n18A-n77A | n778  CA\_n18A-n77A8 | n18 | 5, 10, 15 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n18A-n77(2A) | n778  CA\_n18A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n18A-n77(3A) | CA\_n18A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n18A-n78A | CA\_n18A-n78A | n18 | 5, 10, 15 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n18A-n78(2A) | CA\_n18A-n78A | n18 | 5, 10, 15 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n18 | See n18 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |

Table 5.5A.3.1-1g: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n20A-n28A | CA\_n20A-n28A | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n20 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n20 | 5, 10, 15, 20 | 2 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n20A-n40A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n20A-n67A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n20A-n75A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
|  |  | n20 | 5, 10,15, 20 | 1 |
|  |  | n75 | 5, 10,15, 20, 25, 30, 40, 50 |  |
| CA\_n20A-n78A | CA\_n20A-n78A | n20 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n20A-n78C | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n20A-n78(2A) | CA\_n20A-n78A  CA\_n78(2A) | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n24A-n41A | CA\_n24A-n41A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n24 | See n24 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n24A-n41(2A) | CA\_n24A-n41A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n24 | See n24 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 |  |
| CA\_n24A-n48A | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n24A-n48B | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
| CA\_n24A-n48(2A) | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n24A-n48(3A) | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n24A-n77A | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n24 | See n24 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n24A-n77C | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n24A-n77(2A) | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n25A-n29A | - | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n29 | 5, 10 |  |
| CA\_n25A-n38A | CA\_n25A-n38A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A | CA\_n25A-n38A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n41A13,14 | n418,9  CA\_n25A-n41A8, 13,14 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A | n418,9  CA\_n25A-n41A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C | n418,9  CA\_n25A-n41A8  CA\_n25A-n41C  CA\_n41C8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | CA\_n41C\_BCS2 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A) | n418,9  CA\_n25A-n41A 8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS3 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41C | n418,9  CA\_n25A-n41A8  CA\_n41C8 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  | n418,9  CA\_n25A-n41A8  CA\_n41C8  CA\_n25A-n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
| CA\_n25A-n41(2A) | n418,9  CA\_n25A-n41A8 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS3 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(3A) | n418,9  CA\_n25A-n41A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(3A)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(A-C) | n418,9  CA\_n25A-n41A8  CA\_n41C8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(A-C)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(3A) | n418,9  CA\_n25A-n41A8 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(A-C) | n418,9  CA\_n41C8  CA\_n25A-n41A8 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 |  |
| CA\_n25A-n46A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
| CA\_n25A-n48A | CA\_n25A-n48A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n25A-n48(2A) | CA\_n25A-n48A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n25A-n48C | CA\_n25A-n48A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n25A-n66A | n25A8  n66A8  CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A) | CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A | CA\_n25A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 10, 15, 20, 30, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A) | CA\_n25A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 2 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n71A | CA\_n25A-n71A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71B | CA\_n25A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n71(2A) | CA\_n25A-n71A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n71A | CA\_n25A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71(2A) | CA\_n25A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n71B | CA\_n25A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n77A | n778,9  CA\_n25A-n77A8,13,14 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n77(2A) | n778,9  CA\_n77(2A)8  CA\_n25A-n77A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n77(3A) | n778,9  CA\_n77(2A)8  CA\_n25A-n77A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n25(2A)-n77A | n778,9  CA\_n25A-n77A8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n77(2A) | n778,9  CA\_n77(2A)8  CA\_n25A-n77A8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n77(3A) | n778,9  CA\_n25(2A)  CA\_n77(2A)8  CA\_n25A-n77A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n25A-n78A | n788,9  CA\_n25A-n78A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n78(2A) | n788,9  CA\_n25A-n78A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n78(2A)8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n25(2A)-n78A | n788,9  CA\_n25A-n78A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n78(2A) | n788,9  CA\_n25A-n78A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n25 | CA\_n25(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n25A-n85A | n258  CA\_n25A-n85A | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n85A | CA\_n25A-n85A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |

Table 5.5A.3.1-1h: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n26A-n28A | CA\_n26A-n28A16 | n26 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n26A-n29A | - | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n29 | 5, 10 |  |
| CA\_n26A-n48A | CA\_n26A-n48A | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 |  |
| CA\_n26A-n48(2A) | CA\_n26A-n48A | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n26A-n66A | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n66(2A) | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n26A-n66(3A) | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n26A-n70A | CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n71A | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n77A | CA\_n26A-n77A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n26A-n78A | CA\_n26A-n78A13 | n26 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n26(2A)-n78A | CA\_n26A-n78A | n26 | CA\_n26(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n26A-n78(2A) | CA\_n26A-n78A | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n26(2A)-n78(2A) | CA\_n26A-n78A | n26 | CA\_n26(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n28A-n34A | n348,9  CA\_n28A-n34A8 | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n34 | 5, 10, 15 |  |
| CA\_n28A-n38A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n28A-n39A | n398  CA\_n28A-n39A8 | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n40A | CA\_n28A-n40A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n40B | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
| CA\_n28A-n41A | n418,9  CA\_n28A-n41A8,13 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | 5, 10, 15, 20, 30 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n41B | CA\_n28A-n41A | n28 | 5, 10 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
| CA\_n28A-n41C | n418,9  CA\_n41C8  CA\_n28A-n41A8 | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  | CA\_n41C  CA\_n28A-n41A  CA\_n28A-n41C | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n28A-n46A | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
| CA\_n28A-n46C | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
| CA\_n28A-n46D | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
| CA\_n28A-n46(2A) | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
| CA\_n28A-n50A | CA\_n28A-n50A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n50 | 5, 10, 15, 20, 40, 50, 60, 801 |  |
| CA\_n28A-n71A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n28A-n74A | CA\_n28A-n74A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n74 | 5, 10, 15, 20 |  |
| CA\_n28A-n75A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20 | 1 |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 2 |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n28A-n77A | n778,9  CA\_n28A-n77A8 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n77C | CA\_n28A-n77A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n28A-n77(2A) | n778,9  CA\_n77(2A)8  CA\_n28A-n77A8 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n28A-n77(3A) | n778,9  CA\_n77(2A)  CA\_n28A-n77A8 | n28 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n28A-n78A | n788,9  CA\_n28A-n78A8,13 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | 5, 10, 15, 20, 30 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n78C | CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n28A-n78(2A) | CA\_n78(2A)  CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n28A-n79A | n798,9  CA\_n28A-n79A8 | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n79C | n798,9  CA\_n79C8 | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n28A-n94A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n94 | 5, 10, 15, 20 |  |
| CA\_n28A-n102A | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n102(2A) | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n28A-n102B | CA\_n28A-n102A  CA\_n28A-n102B | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n102C | CA\_n28A-n102A  CA\_n28A-n102C | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n102D | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n102E | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n105A | - | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n29A-n30A | - | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
| CA\_n29A-n48A | - | n29 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 |  |
| CA\_n29A-n66A | - | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n29 | 5, 10 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n29A-n66B | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n29A-n66(2A) | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n29 | 5, 10 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n29A-n66(3A) | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n29A-n70A | - | n29 | 5, 10 | 0 |
|  |  | n70 | 5, 10, 15, 201,, 251 |  |
| CA\_n29A-n71A | - | n29 | 5, 10 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n77A | n778, 9 | n29 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n77(2A) | n778, 9 | n29 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |

Table 5.5A.3.1-1i: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n30A-n66A | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n30A-n66(2A) | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n30A-n66(3A) | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n30A-n77A | n778, 9  CA\_n30A-n77A8 | n30 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n77(2A) | n778, 9  CA\_n77(2A)  CA\_n30A-n77A8 | n30 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n34A-n39A | n348,9  n398  CA\_n34A-n39A8 | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n40A | n348,9  n408,9  CA\_n34A-n40A8 | n34 | 5, 10, 15 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41A | n348,9  n418,9  CA\_n34A-n41A8 | n34 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30 ,40 ,50, 60, 70, 80, 90, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41C | CA\_n41C  CA\_n34A-n41A  CA\_n34A-n41C | n34 | 5, 10, 15 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n34A-n79A | n348,9  n798,9  CA\_n34A-n79A8 | n34 | 5, 10, 15 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n79C | CA\_n34A-n79A | n34 | 5, 10, 15 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n38A-n40A | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66A | CA\_n38A-n66A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n38A-n66(2A) | CA\_n38A-n66A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n38A-n71A | - | n38 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n38A-n78A | CA\_n38A-n78A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n38A-n78(2A) | CA\_n38A-n78A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n38A-n79A | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n38A-n79C | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n39A-n40A | n398  n408,9  CA\_n39A-n40A8 | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41A | CA\_n39A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41C | CA\_n41C  CA\_n39A-n41A  CA\_n39A-n41C | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n39A-n41(2A) | CA\_n39A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 |  |
| CA\_n39A-n79A | n398  n798,9  CA\_n39A-n79A8 | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n79C | CA\_n79C  CA\_n39A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n40A-n41A | n418  CA\_n40A-n41A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n41C | CA\_n41C12  CA\_n40A-n41A  CA\_n40A-n41C12 | n40 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n40A-n77A | CA\_n40A-n77A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 704,80, 904, 100 |  |
| CA\_n40A-n77(2A) | CA\_n40A-n77A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n40A-n77C | - | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n40B-n77A | n778  CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 704,80, 904, 100 |  |
| CA\_n40B-n77(2A) | CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n40B-n77C | CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n40A-n78A | CA\_n40A-n78A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n78(2A) | CA\_n40A-n78A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n40A-n78C | CA\_n40A-n78A | n40 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n40B-n78A | - | n40 | CA\_n40B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n40B-n78(2A) | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n40 | CA\_n40B\_BCS 4 and 5 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n40B-n78C | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n40A-n79A | n408,9  n798,9  CA\_n40A-n79A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n79C | n408,9  n798,9  CA\_n79C8  CA\_n40A-n79A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  | CA\_n79C  CA\_n40A-n79A  CA\_n40A-n79C | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n40A-n105A | CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |

Table 5.5A.3.1-1j: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n41A-n48A | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n48B | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n41A-n48C | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n48 | CA\_n48C\_BCS1 |  |
| CA\_n41A-n48(2A) | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n41C-n48A | CA\_n41A-n48A | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n41C-n48B | CA\_n41A-n48A | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n41C-n48C | CA\_n41A-n48A | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n48 | CA\_n48C\_BCS1 |  |
| CA\_n41(2A)-n48A | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n48B | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n41(2A)-n48C | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n48 | CA\_n48C\_BCS1 |  |
| CA\_n41(2A)-n48(2A) | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n41A-n50A | CA\_n41A-n50A | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n50 | 5, 10, 15, 20, 40, 50, 60, 801 |  |
| CA\_n41A-n66A13,14 | n418,9  CA\_n41A-n66A8, 13,14 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A | n418, 9  CA\_n41A-n66A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A) | n418, 9  CA\_n41A-n66A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n66A | n418, 9  CA\_n41A-n66A8  CA\_n41C | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | n418, 9  CA\_n41A-n66A8  CA\_n41C  CA\_n41C-n66A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A) | n418, 9  CA\_n41A-n66A8  CA\_n41C-n66A  CA\_n41C | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A) | n418, 9  CA\_n41A-n66A8 | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41(3A)-n66A | n418, 9  CA\_n41A-n66A8 | n41 | CA\_n41(3A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40, |  |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66(2A) | n418,9  CA\_n41A-n66A8 | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A | n418, 9  CA\_n41C8  CA\_n41A-n66A8 | n41 | CA\_n41(A-C)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n66(2A) | n418,9  CA\_n41C8  CA\_n41A-n66A8 | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n70A | CA\_n41A-n70A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n41A-n71A | n418,9  CA\_n41A-n71A8, 13, 14 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B | n418,9  CA\_n41A-n71A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41A-n71(2A) | n418,9  CA\_n41A-n71A8 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n71A | n418, 9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | n418, 9  CA\_n41A-n71A8  CA\_n41C8  CA\_n41C-n71A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71(2A) | n418,9  CA\_n41A-n71A8  CA\_n41C-n71A  CA\_n41C8 | n41 | CA\_n41C\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n71A | n418, 9  CA\_n41A-n71A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A)\_BCS3 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71(2A) | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n71B | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41(3A)-n71A | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(3A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n71B | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(3A)\_BCS4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS4 and 5 |  |
| CA\_n41(3A)-n71(2A) | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(3A)\_BCS4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS4 and 5 |  |
| CA\_n41(A-C)-n71A | n418,9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41(A-C)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n71B | n418,9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41(A-C)-n71(2A) | n418,9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n71B | n418,9  CA\_n41A-n71A8  CA\_n41C-n71A  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41A-n74A | CA\_n41A-n74A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n74 | 5, 10, 15, 20 |  |
| CA\_n41A-n77A | n418,9  n778,9  CA\_n41A-n77A8, 13 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41B-n77A | CA\_n41A-n77A | n41 | CA\_n41B\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41(2A)-n77A | n418,9  n778,9  CA\_n41A-n77A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n77A | n418,9  n778,9  CA\_n41A-n77A8 | n41 | CA\_n41(3A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n77A | n418,9  n778,9  CA\_n41C8  CA\_n41A-n77A8 | n41 | CA\_n41(A-C)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n77A | n418,9  n778,9  CA\_n41A-n77A8  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n418,9  n778,9  CA\_n41A-n77A8  CA\_n41C8  CA\_n41C-n77A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n77(2A) | n418,9  n778,9  CA\_n77(2A)  CA\_n41A-n77A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n418,9  n778,9  CA\_n41A-n77A8 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n77(2A) | n418,9  n778,9  CA\_n41A-n77A8  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n77(3A) | n418,9  n778,9  CA\_n41A-n77A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n77(2A) | - | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n418,9  n778,9  CA\_n41A-n77A8 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n77C | CA\_n41A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n41A-n78A | CA\_n41A-n78A | n41 | 10, 15, 20, 40, 50, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n78(2A) | CA\_n41A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n41A-n78C | CA\_n41A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n41A-n79A | n418,9  n798,9  CA\_n41A-n79A8 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60 | 1 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 2 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n79C | n418,9  n798,9  CA\_n41A-n79A8  CA\_n79C8 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n41C-n79A | n418,9  n798,9  CA\_n41A-n79A8  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n79C | CA\_n41C  CA\_n79C  CA\_n41A-n79A | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n41A-n85A | CA\_n41A-n85A | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n85A | CA\_n41A-n85A  CA\_n41C | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n85A | CA\_n41A-n85A | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n85A | CA\_n41A-n85A | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n85A | CA\_n41A-n85A  CA\_n41C | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |

Table 5.5A.3.1-1k ~ Table 5.5A.3.1-1n

**Table 5.5A.3.1-1k: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NR CA configuration** | **Uplink CA configuration or single uplink carrier10** | **NR Band** | **Channel bandwidth (MHz) (NOTE 3)** | **Bandwidth combination set** |
| CA\_n46A-n48A | CA\_n46A-n48A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | 20 |  |
|  |  | n46 | 20, 40, 60, 80 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n46A-n48(2A) | CA\_n46A-n48A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n46A-n48(3A) | CA\_n46A-n48A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n46A-n48(4A) | CA\_n46A-n48A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
| CA\_n46A-n48B | CA\_n46A-n48A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
| CA\_n46A-n48C | CA\_n46A-n48A  CA\_n46A-n48B | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n46B-n48A | CA\_n46A-n48A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 20 |  |
|  |  | n46 | CA\_n46B\_BCS0 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n46B-n48(2A) | CA\_n46A-n48A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n46B-n48(3A) | CA\_n46A-n48A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n46B-n48(4A) | CA\_n46A-n48A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
| CA\_n46B-n48B | CA\_n46A-n48A  CA\_n46A-n48B | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
| CA\_n46B-n48C | CA\_n46A-n48A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n46C-n48A | CA\_n46A-n48A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 20 |  |
|  |  | n46 | CA\_n46C\_BCS0 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n46C-n48(2A) | CA\_n46A-n48A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n46C-n48(3A) | CA\_n46A-n48A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n46C-n48(4A) | CA\_n46A-n48A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
| CA\_n46C-n48B | CA\_n46A-n48A  CA\_n46A-n48B | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
| CA\_n46C-n48C | CA\_n46A-n48A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n46D-n48A | CA\_n46A-n48A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 20 |  |
|  |  | n46 | CA\_n46D\_BCS0 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n46D-n48(2A) | CA\_n46A-n48A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n46D-n48(3A) | CA\_n46A-n48A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n46D-n48(4A) | CA\_n46A-n48A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
| CA\_n46D-n48B | CA\_n46A-n48A  CA\_n46A-n48B | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
| CA\_n46D-n48C | CA\_n46A-n48A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n46M-n48A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 20 |  |
| CA\_n46M-n48(2A) | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n46M-n48(3A) | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n46M-n48(4A) | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
| CA\_n46M-n48B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
| CA\_n46M-n48C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n46N-n48A | CA\_n46A-n48A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 |  |
| CA\_n46N-n48(2A) | CA\_n46A-n48A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n46N-n48(3A) | CA\_n46A-n48A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n46N-n48(4A) | CA\_n46A-n48A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
| CA\_n46N-n48B | CA\_n46A-n48A  CA\_n46A-n48B | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
| CA\_n46N-n48C | CA\_n46A-n48A | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n46A-n66A | - | n46 | 20, 40, 60, 80 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n46A-n77A | CA\_n46A-n77A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46C-n77A | CA\_n46A-n77A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46D-n77A | CA\_n46A-n77A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46A-n77(2A) | CA\_n77(2A)  CA\_n46A-n77A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n46C-n77(2A) | CA\_n77(2A)  CA\_n46A-n77A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n46D-n77(2A) | CA\_n77(2A)  CA\_n46A-n77A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n46(2A)-n77A | CA\_n46A-n77A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46(2A)-n77(2A) | CA\_n77(2A)  CA\_n46A-n77A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n46A-n78A | CA\_n46A-n78A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46C-n78A | CA\_n46A-n78A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46D-n78A | CA\_n46A-n78A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46A-n78(2A) | CA\_n78(2A)  CA\_n46A-n78A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n46C-n78(2A) | CA\_n78(2A)  CA\_n46A-n78A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n46D-n78(2A) | CA\_n78(2A)  CA\_n46A-n78A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n46(2A)-n78A | CA\_n46A-n78A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n46(2A)-n78(2A) | CA\_n78(2A)  CA\_n46A-n78A | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n46A-n96A | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n96A | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n96A | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n96A | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n96A | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n96B | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n96B | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n96B | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n96B | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n96B | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n96C | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n96D | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n96D | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n96D | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n96D | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n96D | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n96E | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n96E | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n96E | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n96E | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n96E | - | n46 | CA\_n46N\_BCS1 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n102A | - | n46 | 10, 20, 40, 60, 80, 100 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46A-n102(2A) | - | n46 | 10, 20, 40, 60, 80, 100 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46A-n102B | CA\_n102B | n46 | 10, 20, 40, 60, 80, 100 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46A-n102C | CA\_n102C | n46 | 10, 20, 40, 60, 80, 100 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46A-n102D | - | n46 | 10, 20, 40, 60, 80, 100 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46A-n102E | - | n46 | 10, 20, 40, 60, 80, 100 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46(2A)-n102A | - | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46(2A)-n102(2A) | - | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46(2A)-n102B | CA\_n102B | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46(2A)-n102C | CA\_n102C | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46(2A)-n102D | - | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46(2A)-n102E | - | n46 | CA\_n46(2A)\_BCS0 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46C-n102A | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46C-n102(2A) | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46C-n102B | CA\_n102B | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46C-n102C | CA\_n102C | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46C-n102D | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46C-n102E | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n46D-n102A | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n46D-n102(2A) | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n46D-n102B | CA\_n102B | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n46D-n102C | CA\_n102C | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n46D-n102D | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n46D-n102E | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |

**Table 5.5A.3.1-1l: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NR CA configuration** | **Uplink CA configuration or single uplink carrier10** | **NR Band** | **Channel bandwidth (MHz) (NOTE 3)** | **Bandwidth combination set** |
| CA\_n48A-n53A | - | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n53 | 5, 10 |  |
| CA\_n48(2A)-n53A | - | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n53 | 5, 10 |  |
| CA\_n48A-n66A | CA\_n48A-n66A | n48 | 5, 10, 15, 20, 40, 506,606, 806,906,1006 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 506, 606, 806, 906, 1006 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40, |  |
| CA\_n48A-n66B | CA\_n48A-n66A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n48A-n66(2A) | CA\_n48A-n66A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n48B-n66A | CA\_n48B  CA\_n48A-n66A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n48 | CA\_n48B\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48B-n66(2A) | CA\_n48B  CA\_n48A-n66A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n66 | CA\_n66(2A)\_BCS2 |  |
| CA\_n48C-n66A | CA\_n48B  CA\_n48A-n66A | n48 | CA\_n48C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n48 | CA\_n48C\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48(2A)-n66A | CA\_n48A-n66A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48(2A)-n66B | CA\_n48A-n66A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n48(2A)-n66(2A) | CA\_n48A-n66A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n48(A-B)-n66A | CA\_n48A-n66A | n48 | CA\_n48(A-B)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48(A-C)-n66A | CA\_n48A-n66A | n48 | CA\_n48(A-C)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n48 | CA\_n48(A-C)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n48A-n70A | CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48(2A)-n70A | CA\_n48A-n70A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
| CA\_n48B-n70A | CA\_n48A-n70A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n71A | CA\_n48A-n71A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n71(2A) | CA\_n48A-n71A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48(2A)-n71A | CA\_n48A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n71(2A) | CA\_n48A-n71A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48(3A)-n71A | CA\_n48A-n71A | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(4A)-n71A | CA\_n48A-n71A | n48 | CA\_n48(4A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n71A | CA\_n48A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n71(2A) | CA\_n48A-n71A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48C-n71A | CA\_n48A-n71A | n48 | CA\_n48C\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n77A | n778,9 | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n48A-n77C | n778,9  CA\_n77C | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48A-n77(2A) | - | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n48(2A)-n77A | n778,9 | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n48(2A)-n77C | n778,9  CA\_n77C | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 2 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 3 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48(2A)-n77(2A) | - | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n48(3A)-n77A | - | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48B-n77A | CA\_n48B  n778,9 | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS1 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48B-n77C | CA\_n48B  n778,9  CA\_n77C | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48B\_BCS0 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 3 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48(A-B)-n77A | n778,9 | n48 | CA\_n48(A-B)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(A-B)-n77C | n778,9  CA\_n48B  CA\_n77C | n48 | CA\_n48(A-B)\_BCS1 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48A-n96A | CA\_n48A-n96A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n48(2A)-n96A | CA\_n48A-n96A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n48(2A)-n96B | CA\_n48A-n96B | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n48(2A)-n96C | CA\_n48A-n96A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n48(2A)-n96D | CA\_n48A-n96A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n48(2A)-n96E | CA\_n48A-n96A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n48(3A)-n96A | CA\_n48A-n96A | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n48(3A)-n96B | CA\_n48A-n96B | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n48(3A)-n96C | CA\_n48A-n96A | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n48(3A)-n96D | CA\_n48A-n96A | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n48(3A)-n96E | CA\_n48A-n96A | n48 | CA\_n48(3A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n48(4A)-n96A | CA\_n48A-n96A | n48 | CA\_n48(4A)\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n48(4A)-n96B | CA\_n48A-n96A | n48 | CA\_n48(4A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n48(4A)-n96C | CA\_n48A-n96A | n48 | CA\_n48(4A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n48(4A)-n96D | CA\_n48A-n96A | n48 | CA\_n48(4A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n48(4A)-n96E | CA\_n48A-n96A | n48 | CA\_n48(4A)\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n48A-n96B | CA\_n48A-n96A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n48A-n96C | CA\_n48A-n96A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n48A-n96D | CA\_n48A-n96A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n48A-n96E | CA\_n48A-n96A | n48 | 5, 10, 15, 20, 30, 40, 506, 606, 706, 806, 906, 1006 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n48B-n96A | CA\_n48A-n96A CA\_n48B-n96A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n48B-n96B | CA\_n48A-n96A CA\_n48B-n96A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n48B-n96C | CA\_n48A-n96A CA\_n48B-n96A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n48B-n96D | CA\_n48A-n96A CA\_n48B-n96A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n48B-n96E | CA\_n48A-n96A CA\_n48B-n96A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n48C-n96A | CA\_n48A-n96A | n48 | CA\_n48C\_BCS0 | 0 |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n48C-n96B | CA\_n48A-n96A | n48 | CA\_n48C\_BCS0 | 0 |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n48C-n96C | CA\_n48A-n96A | n48 | CA\_n48C\_BCS0 | 0 |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n48C-n96D | CA\_n48A-n96A | n48 | CA\_n48C\_BCS0 | 0 |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n48C-n96E | CA\_n48A-n96A | n48 | CA\_n48C\_BCS0 | 0 |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n50A-n78A | CA\_n50A-n78A | n50 | 5, 10, 15, 20, 30, 40, 50, 60, 801 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |

**Table 5.5A.3.1-1m: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NR CA configuration** | **Uplink CA configuration or single uplink carrier10** | **NR Band** | **Channel bandwidth (MHz) (NOTE 3)** | **Bandwidth combination set** |
| CA\_n66A-n70A | - | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n66B-n70A | - | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66(2A)-n70A | - | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66(3A)-n70A | - | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n66A-n71A | n668  n718  CA\_n66A-n71A | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B | CA\_n66A-n71A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n66A-n71(2A) | CA\_n66A-n71A | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n66(2A)-n71A | CA\_n66A-n71A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71B | CA\_n66A-n71A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n66(2A)-n71(2A) | CA\_n66A-n71A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n66(3A)-n71A | CA\_n66A-n71A | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66B-n71A | CA\_n66A-n71A | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n77A | n778,9  CA\_n66A-n77A8,13,14 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n77B | CA\_n66A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n66(2A)-n77A | n778,9  CA\_n66A-n77A8 | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n77B | CA\_n66A-n77A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n66A-n77(2A) | n778,9  CA\_n66A-n77A8  CA\_n77(2A)8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n66(3A)-n77A | n778,9  CA\_n66A-n77A8 | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n77(2A) | n778,9  CA\_n66A-n77A8  CA\_n77(2A) | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n66(3A)-n77(2A) | n778,9  CA\_n66A-n77A8 | n66 | CA\_n66(3A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n66A-n77C | n778,9  CA\_n77C  CA\_n66A-n77A8 | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n66A-n77(3A) | n778,9  CA\_n77(2A)8  CA\_n66A-n77A8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n66(2A)-n77(3A) | CA\_n77(2A)  CA\_n66A-n77A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n66(2A)-n77C | n778,9  CA\_n77C  CA\_n66A-n77A8 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n66(3A)-n77C | n778,9  CA\_n77C CA\_n66A-n77A8 |  | CA\_n66(3A)\_BCS0 | 0 |
|  |  |  | CA\_n77C\_BCS1 |  |
| CA\_n66B-n77A | n778,9  CA\_n66A-n77A8 | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66B-n77C | n778,9  CA\_n77C  CA\_n66A-n77A8 | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n66 | CA\_n66B\_BCS0 | 1 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n66A-n78A | n788,9  CA\_n66A-n78A8 | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | See n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n78(2A) | n788,9  CA\_n66A-n78A8 | n66 | 5, 10, 15, 20, 30, 40 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  | CA\_n78(2A)8 | n66 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n66 | See n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n66(2A)-n78A | n788,9  CA\_n66A-n78A8 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n78(2A) | n788,9  CA\_n66A-n78A8 | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n66 | CA\_n66(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n66A-n85A | n668  CA\_n66A-n85A | n66 | See n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n85A | CA\_n66A-n85A | n66 | CA\_n66(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n67A-n78A | - | n67 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n67A-n78(2A) | CA\_n78(2A) | n67 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |

**Table 5.5A.3.1-1n: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NR CA configuration** | **Uplink CA configuration or single uplink carrier10** | **NR Band** | **Channel bandwidth (MHz) (NOTE 3)** | **Bandwidth combination set** |
| CA\_n70A-n71A | CA\_n70A-n71A | n70 | 5, 10, 15, 201, 251 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n70A-n71(2A) | CA\_n70A-n71A | n70 | 5, 10, 15, 201, 251 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n70A-n77A | CA\_n70A-n77A | n70 | 5, 10, 15, 201, 251 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n70A-n78A | CA\_n70A-n78A | n70 | 5, 10, 15, 201, 251 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n71A-n77A | n778, 9  CA\_n71A-n77A8,13 | n71 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n71A-n77(2A) | n778, 9  CA\_n77(2A)8  CA\_n71A-n77A8 | n71 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n71A-n77(3A) | 778, 9  CA\_n77(2A)8  CA\_n71A-n77A8 | n71 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n71A-n77B | - | n71 | n71 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n71A-n77C | - | n71 | n71 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n71B-n77A | n778, 9  CA\_n71A-n77A8 | n71 | CA\_n71B\_BCS2 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n71B-n77(2A) | n778, 9  CA\_n71A-n77A8 | n71 | CA\_n71B\_BCS2 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n71(2A)-n77A | n778, 9  CA\_n71A-n77A8 | n71 | CA\_n71(2A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n71(2A)-n77(2A) | n778, 9  CA\_n71A-n77A8 | n71 | CA\_n71(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n71(2A)-n77B | - | n71 | CA\_n71(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77B\_BCS 4 and 5 |  |
| CA\_n71(2A)-n77C | - | n71 | CA\_n71(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n71A-n78A | n788,9  CA\_n71A-n78A8 | n71 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | See n71 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n71A-n78(2A) | n788,9  CA\_n71A-n78A8 | n71 | 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n71 | See n71 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n71A-n85A | - | n71 | See n71 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n71(2A)-n85A | - | n71 | CA\_n71(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n71B-n85A | - | n71 | CA\_n71B BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n74A-n77A | CA\_n74A-n77A | n74 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n74A-n78A | CA\_n74A-n78A | n74 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n75A-n78A | - | n75 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n75A-n78(2A) | - | n75 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n76A-n78A | - | n76 | 5 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n77A-n78A2 | - | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n77A-n78C2 | - | n77 | 10,15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n77A-n78(2A)2 | - | n77 | 10,15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n77A-n79A | n778,9  n798,9  CA\_n77A-n79A8 | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n77A-n79A | n77 | See n77 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n77(2A)-n79A | n778,9  n798,9  CA\_n77(2A)12  CA\_n77A-n79A8 | n77 | CA\_n77(2A)\_BCS1 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  | CA\_n77A-n79A | n77 | CA\_n77(2A)\_ BCS 4 and 5 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n77(3A)-n79A | n778,9  n798,9  CA\_n77(2A)12  CA\_n77A-n79A8 | n77 | CA\_n77(3A)\_BCS1 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n77A-n85A | n778,9  CA\_n77A-n85A8 | n77 | See n77 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n77(2A)-n85A | CA\_n77A-n85A | n77 | CA\_n77(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n77A-n102A | CA\_n77A-n102A | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n77A-n102(2A) | CA\_n77A-n102A | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n77A-n102B | CA\_n77A-n102A  CA\_n77A-n102B | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n77A-n102C | CA\_n77A-n102A  CA\_n77A-n102C | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n77A-n102D | CA\_n77A-n102A | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n77A-n102E | CA\_n77A-n102A | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n77(2A)-n102A | CA\_n77(2A) CA\_n77A-n102A | n77 | CA\_n77(2A)\_BCS4 and 5 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n77(2A)-n102(2A) | CA\_n77(2A) CA\_n77A-n102A | n77 | CA\_n77(2A)\_BCS4 and 5 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n77(2A)-n102B | CA\_n77(2A) CA\_n77A-n102A  CA\_n77A-n102B | n77 | CA\_n77(2A)\_BCS4 and 5 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n77(2A)-n102C | CA\_n77(2A) CA\_n77A-n102A  CA\_n77A-n102C | n77 | CA\_n77(2A)\_BCS4 and 5 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n77(2A)-n102D | CA\_n77(2A) CA\_n77A-n102A | n77 | CA\_n77(2A)\_BCS4 and 5 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n77(2A)-n102E | CA\_n77(2A) CA\_n77A-n102A | n77 | CA\_n77(2A)\_BCS4 and 5 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n78A-n79A | n78A8,9  n79A8,9  CA\_n78A-n79A8 | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 1 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n78A-n79C | - | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n78(2A)-n79A | CA\_n78A-n79A | n78 | CA\_n78(2A)\_BCS1 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n78A-n92A | CA\_n78A-n92A | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n92 | 5, 10, 15, 20 |  |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n92 | See n92 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n78(2A)-n92A | CA\_n78A-n92A | n78 | CA\_n78(2A)\_BCS0 | 0 |
|  |  | n92 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n92 | See n92 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n78A-n94A | - | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n94 | 5, 10, 15, 20 |  |
| CA\_n78A-n102A | CA\_n78A-n102A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n78A-n102(2A) | CA\_n78A-n102A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n78A-n102B | CA\_n78A-n102A  CA\_n78A-n102B | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n78A-n102C | CA\_n78A-n102A  CA\_n78A-n102C | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n78A-n102D | CA\_n78A-n102A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n78A-n102E | CA\_n78A-n102A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n78(2A)-n102A | CA\_n78A-n102A  CA\_n78(2A) | n78 | CA\_n78(2A)\_BCS2 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n78(2A)-n102B | CA\_n78A-n102A  CA\_n78(2A)  CA\_n78A-n102B | n78 | CA\_n78(2A)\_BCS2 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n78(2A)-n102C | CA\_n78A-n102A  CA\_n78(2A)  CA\_n78A-n102C | n78 | CA\_n78(2A)\_BCS2 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n78(2A)-n102D | CA\_n78A-n102A  CA\_n78(2A) | n78 | CA\_n78(2A)\_BCS2 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n78(2A)-n102E | CA\_n78A-n102A  CA\_n78(2A) | n78 | CA\_n78(2A)\_BCS2 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n78(2A)-n102(2A) | CA\_n78A-n102A  CA\_n78(2A) | n78 | CA\_n78(2A)\_BCS2 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n78A-n105A | CA\_n78A-n105A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |

The following notes are applied to the above tables:

NOTE 1: This UE channel bandwidth is applicable only to downlink.

NOTE 2: The minimum requirements for intra-band contiguous or non-contiguous CA apply.

NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.

NOTE 4: This UE channel bandwidth is optional in this release of the specification.

NOTE 5: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.

NOTE 6: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configuration

NOTE 7: Limited to operation at 3450-3550 MHz and 3700–3980 MHz.

NOTE 8: Minimum requirements for Power Class 2 are applicable for this uplink combination with 1Tx antenna connector in each band or single uplink carrier with up to 2Tx antenna connectors in this downlink/uplink combination

NOTE 9: Minimum requirements for Power Class 1.5 are applicable for this single uplink carrier with up to 2Tx antenna connectors in this downlink/uplink combination

NOTE 10: Only single uplink carriers with power class other than PC3 are listed.

NOTE 11: The CA configurations are given in Table 5.5A.1-1 or Table 5.5A.2-1 in this specification

NOTE 12: UL configurations are for non simultaneous Rx/Tx operation.

NOTE 13: Minimum requirements for Power Class 2 are applicable for this uplink configuration with 1Tx antenna connector in one band and 2Tx antenna connectors in the other band.

NOTE 14 Minimum requirements for Power Class 1.5 are applicable for this uplink configuration with 1Tx antenna connector in one band and 2Tx antenna connectors in the other band.

NOTE 15: Uplink is only in n5 for CA\_n5-n8.

NOTE 16: For UEs only supporting DL CA\_n26-n28, uplink support in band n26 is optional, if the UE supports CA\_n26-n28 UL configuration, it should also support UL in band n26 and n28.

## **<<End of Change>>**