**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR maintenance multi Rx RRM requirements |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Incomplete multi-Rx requirements |
|  |  |
| ***Summary of change:*** | -Simplification on how conditions for fast beam sweeping is captured, with -conditions only in 3.6.x-update of conditions for measurement restrictions-Capturing that N=1 when scheduling restriction enhancement apply.  |
|  |  |
| ***Consequences if not approved:*** | Requirements with brackets and FFS points remain in the specification. |
|  |  |
| ***Clauses affected:*** | 3.6.x (new), 8.1.2, 8.1.3, 8.1.7, 8.5, 8.10E.4, 8.18 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

Start of Change 2

### 3.6.16 Applicability of requirements for ATG

The requirements in ATG specific clauses apply to an ATG UE operating in FR1 NR SA operation mode at an altitude of at-least 3km.

### 3.6.17 Applicability of requirements for MUSIM gaps

No requirements are defineed in this version of specification when MUSIM gaps collide with (activated) Pre-MG and/or NCSG.

### 3.6.x Applicability of requirements for multi-Rx operation in FR2-1

The requirements related to the support of [*reducedRxBeamNum* and 30-1] are applicable to a PCell, PSCell, or SCell, provided the UE is configured with a single serving cell (PCell, PSCell, or SCell) in FR2-1.

The reduced beam sweeping according to the UE capability [*reducedRxBeamNum*] is enabled when the network configures the UE with a CSI report containing groupBasedBeamReporting-v1710.

End of Change 2