**3GPP TSG- RAN4 Meeting #** **111 *R4-2408586***

**Fukuoka City, Fukuoka, Japan, 20th – 24th May, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.133** | **CR** | **-** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction on L1-RSRP accuracy requirements on neighbor cells | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_Mob\_enh2-Perf | | | | |  | ***Date:*** | | | 2024-5-22 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Allign the discription of measurement accuracy for both intra-frequency and inter-frequency L1-RSRP on neighbor cells in FR1 and FR2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Allign the discription of measurement accuracy for both intra-frequency and inter-frequency L1-RSRP on neighbor cells in FR1 and FR2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | 10.1.19X, 10.1.19Y, 10.1.20X, 10.1.20Y | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **x** |  | Test specifications | | | | TS38.533 | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

<Start of Change 1>

### 10.1.19X LTM Intra-frequency L1-RSRP accuracy requirements for FR1

#### 10.1.19X.1 SSB based intra-frequency L1-RSRP accuracy requirements

##### 10.1.19X.1.1 Absolute Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SSB based intra-frequency L1-RSRP in this clause apply to all SSBs of candidate neighbour cell(s) on the same frequency as that of the serving cell in FR1.

The accuracy requirements in Table 10.1.19X.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

Table 10.1.19X.1.1-1: SSB based L1-RSRP absolute accuracy in FR1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range | | | | |
|  |  |  | NR operating band groups Note 2 | Minimum Io | | | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A | -121 | -118 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -70 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -70 |
| ±5.0 | ±9.5 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_N | -114.5 | -111.5 | N/A | -70 |
| ±8.5 | ±11.5 | ≥-3 | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A, NR\_FDD\_FR1\_B, NR\_TDD\_FR1\_C, NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D, NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E, NR\_FDD\_FR1\_F, NR\_FDD\_FR1\_G, NR\_FDD\_FR1\_H,  NR\_FDD\_FR1\_N | N/A | N/A | -70 | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.  NOTE 2: NR operating band groups in FR1 are as defined in clause 3.5.2. | | | | | | | |

##### 10.1.19X.1.2 Relative Accuracy

The relative accuracy of SSB based L1-RSRP is defined as the L1-RSRP measured from one SSB compared to the largest measured value of L1-RSRP among all SSBs of the cell(s) on the same frequency in FR1.The accuracy requirements in Table 10.1.19X.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

Table 10.1.19X.1.2-1: SSB based L1-RSRP relative accuracy in FR1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | SSB Ês/Iot Note 2 | Io Note 1 range | | | | |
|  |  |  | NR operating band groups Note 4 | Minimum Io | | | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,  NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| ±3 | ±4 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_N | -114.5 | -111.5 | N/A | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.  NOTE 2: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of SSBs to which the requirement applies.  NOTE 3: Void  NOTE 4: NR operating band groups in FR1 are as defined in clause 3.5.2. | | | | | | | |

<End of Change 1>

<Start of Change 2>

### 10.1.19y LTM Inter-frequency L1-RSRP accuracy requirements for FR1

#### 10.1.19y.1 SSB based Inter-frequency L1-RSRP accuracy requirements for FR1

Unless otherwise specified, the requirements for absolute accuracy and relative accuracy of SSB based L1-RSRP in this clause apply to all SSBs of candidate neighbour cell(s) on a frequency in FR1 that is on a different frequency than the serving cell.

##### 10.1.19y.1.1 Absolute Accuracy

The accuracy requirements in Table 10.1.19y.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for inter-frequency L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

Table 10.1.19y.1.1-1: Inter-frequency L1-RSRP absolute accuracy in FR1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range | | | | |
|  |  |  | NR operating band groups Note 2 | Minimum Io | | | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A | -121 | -118 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -70 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -70 |
| ±5.0 | ±9.5 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_N | -114.5 | -111.5 | N/A | -70 |
| ±8.5 | ±11.5 | ≥-3 | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A, NR\_FDD\_FR1\_B, NR\_TDD\_FR1\_C, NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D, NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E, NR\_FDD\_FR1\_F, NR\_FDD\_FR1\_G, NR\_FDD\_FR1\_H,  NR\_FDD\_FR1\_N | N/A | N/A | -70 | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.  NOTE 2: NR operating band groups in FR1 are as defined in clause 3.5.2. | | | | | | | |

##### 10.1.19y.1.2 Relative Accuracy

The relative accuracy of SSB based L1-RSRP is defined as the L1-RSRP measured from one SSB from one cell on a frequency in FR1 compared to the largest measured value of L1-RSRP among all SSBs measured from another cell on another frequency in FR1.

The accuracy requirements in Table 10.1.19y.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

Table 10.1.19y.1.2-1: Inter-frequency L1-RSRP relative accuracy in FR1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | | |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range | | | | |
|  |  |  | NR operating band groups Note 2 | Minimum Io | | | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A | -121 | -118 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -70 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -70 |
| ±5.0 | ±9.5 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_N | -114.5 | -111.5 | N/A | -70 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.  NOTE 2: NR operating band groups in FR1 are as defined in clause 3.5.2. | | | | | | | |

<End of Change 2>

<Start of Change 3>

### 10.1.20X LTM Intra-frequency L1-RSRP accuracy requirements for FR2

#### 10.1.20X.1 SSB based intra-frequency L1-RSRP accuracy requirements

##### 10.1.20X.1.1 Absolute Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SSB based intra-frequency L1-RSRP in this clause apply to all SSBs of candidate neighbour cells on the same frequency as that of the serving cell in FR2.

The accuracy requirements in Table 10.1.20X.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.20X.1.1-1: SSB based L1-RSRP absolute accuracy in FR2

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range | | | |
|  |  |  | Minimum Io | | | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 2 | | dBm/BWChannel | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |  |
| ±6.5 | ±9.5 | ≥-3 | Same value as SSB\_RP in Table B.2.4.1-2, according to UE Power class, operating band and angle of arrival | | N/A | -70 |
| ±8.5 | ±11.5 | ≥-3 | N/A | | -70 | -50 |
| NOTE 1: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.  NOTE 2: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.  NOTE 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. | | | | | | |

##### 10.1.20X.1.2 Relative Accuracy

Unless otherwise specified, the requirements for relative accuracy of SSB based intra-frequency L1-RSRP in this clause apply to all SSBs of candidate neighbour cells on the same frequency as that of the serving cell in FR2.

The relative accuracy of SSB based L1-RSRP is defined as the L1-RSRP measured from one SSB compared to the largest measured value of L1-RSRP among all SSBs of the cell(s) on the same frequency in FR2.

The accuracy requirements in Table 10.1.20X.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.20X.1.2-1: SSB based L1-RSRP relative accuracy in FR2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range | | |
|  |  |  | Minimum Io | | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 3 | | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |
| ±6.5 | ±9.5 | ≥-3 | Same value as SSB\_RP in Table B.2.4.1-2, according to UE Power class, operating band and angle of arrival | | -50 |
| NOTE 1: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.  NOTE 2: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of SSBs to which the requirement applies.  NOTE 3: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.  NOTE 4: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. | | | | | |

<End of Change 3>

<Start of Change 4>

### 10.1.20Y LTM Inter-frequency L1-RSRP accuracy requirements for FR2

#### 10.1.20Y.1 SSB based L1-RSRP accuracy requirements

Unless otherwise specified, the requirements for absolute accuracy of SSB based L1-RSRP in this clause apply to all SSBs of candidate neighbour cell(s) on a frequency in FR2 that is on a different frequency than the serving cell.

##### 10.1.20Y.1.1 Absolute Accuracy

The accuracy requirements in Table 10.1.20Y.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.20Y.1.1-1: SSB based L1-RSRP absolute accuracy in FR2

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | | |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range | | | |
|  |  |  | Minimum Io | | | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 2 | | dBm/BWChannel | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |  |
| ±6.5 | ±9.5 | ≥-3 | Same value as SSB\_RP in Table B.2.4.1-2, according to UE Power class, operating band and angle of arrival | | N/A | -70 |
| ±8.5 | ±11.5 | ≥-3 | N/A | | -70 | -50 |
| NOTE 1: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.  NOTE 2: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.  NOTE 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. | | | | | | |

##### 10.1.20Y.1.2 Relative Accuracy

Unless otherwise specified, the requirements for relative accuracy of SSB based L1-RSRP in this clause apply to all SSBs of candidate neighbour cell(s) on a frequency in FR2 that is on a different frequency than the serving cell.

The relative accuracy of SSB based L1-RSRP is defined as the L1-RSRP measured from one SSB from one cell on a frequency in FR2 compared to the largest measured value of L1-RSRP among all SSBs measured from another cell on another frequency in FR2.

The accuracy requirements in Table 10.1.20Y.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for L1-RSRP measurements are fulfilled according to Annex B.2.4.1 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.20Y.1.2-1: SSB based L1-RSRP relative accuracy in FR2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Accuracy | | Conditions | | | |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range | | |
|  |  |  | Minimum Io | | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 3 | | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |
| ±6.5 | ±9.5 | ≥-3 | Same value as SSB\_RP in Table B.2.4.1-2, according to UE Power class, operating band and angle of arrival | | -50 |
| NOTE 1: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.  NOTE 2: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of SSBs to which the requirement applies.  NOTE 3: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.  NOTE 4: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. | | | | | |

<End of Change 4>