**3GPP TSG-WG4 Meeting # 111 *R4-240xxxx***

**Fukuoka, Japan, 20- 24 May 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **Draft CR** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  |
| *For* ***[HELP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on TC5 for MUSIM |
|  |  |
| ***Source to WG:*** | ZTE Corporation, Sanechips |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_DualTxRx\_MUSIM-Perf |  | ***Date:*** | 2024-05-09 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | TC5: Intra-frequency event triggered reporting, 1 periodic MUSIM gap, SMTC partially partial overlaps with MUSIM gaps, SSB-based measurements, FR1TC5 shall be defined for MUSIM gap related requirements. |
|  |  |
| ***Summary of change:*** | Introduce TC5 for MUSIM gap related requirements. |
|  |  |
| ***Consequences if not approved:*** | Agreed TC5 is not implemented. |
|  |  |
| ***Clauses affected:*** |  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** | **x** |  |  Test specifications | TS 38.533 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### < START OF CHANGE 1>

# **A.6.6.1.X**  SA event triggered reporting tests with MUSIM gap configured

## **A.6.6.1.X.1** Test purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event on an intra-frequency layer based on measurement performed without measurement gaps when the UE is also configured with MUSIM gaps. This test will partly verify the intra-frequency cell search requirements in clauses 9.2.5.1 and 9.2.5.2.

## A.6.6.1.X.2 Test parameters

Two cells are deployed in the test, which are FR1 PCell (Cell 1) and a FR1 neighbour cell (Cell 2) on the same frequency as the PCell. The test parameters for PCell and neighbour cell are given in Table A.6.6.1.X.2-1 and A.6.6.1.X.2-2 below. In the measurement control information, a measurement object is configured for the frequency of the PCell, and it is indicated to the UE that event-triggered reporting with Event A3 is used. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have any timing information of Cell 2.

Table A.6.6.1.X.2.2-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations. |

Table A.6.6.1.X.2.2-2: General test parameters for SA intra-frequency event triggered reporting without gap for FR1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Active cell |  | 1, 2, 3 | Cell 1 |  |
| Neighbour cell |  | 1, 2, 3 | Cell 2 | Cell to be identified. |
| RF Channel Number |  | 1, 2, 3 | 1: Cell 1 and Cell 2 |  |
| MUSIM gap Pattern ID |  | 1,2,3 | 0 |  |
| MUSIM gap offset | ms | 1,2,3 | 0 |  |
| SSB configuration |  | 1 | SSB.1 FR1 |  |
|  |  | 2 | SSB.1 FR1 |  |
|  |  | 3 | SSB.2 FR1 |  |
| SMTC configuration |  | 1 | SMTC.2 |  |
|  |  | 2 | SMTC.1 |  |
|  |  | 3 | SMTC.1 |  |
| A3-Offset | dB | 1, 2, 3 | -4.5 |  |
| CP length |  | 1, 2, 3 | Normal |  |
| Hysteresis | dB | 1, 2, 3 | 0 |  |
| Time To Trigger | s | 1, 2, 3 | 0 |  |
| Filter coefficient |  | 1, 2, 3 | 0 | L3 filtering is not used |
| DRX |  | 1, 2, 3 |  | OFF |
| Time offset between serving and neighbour cells |  | 1 | 3 ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  |  | 2 | 3 μs | Synchronous cells |
|  |  | 3 | 3 μs | Synchronous cells |
| T1 | s | 1, 2, 3 | 5 |  |
| T2 | s | 1, 2, 3 | 5 |  |

Table A.6.6.1.X.2.2-3: NR Cell specific test parameters for SA intra-frequency event triggered reporting without gap for FR1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 1 | Cell 2 |
|  |  |  | T1 | T2 | T1 | T2 |
| TDD configuration |  | 1 | TN/A | TN/A |
|  |  | 2 | TDDConf.1.1 | TDDConf.1.1 |
|  |  | 3 | TDDConf.2.1 | TDDConf.2.1 |
| PDSCH RMC configuration |  | 1 | SR.1.1 FDD | N/A |
|  |  | 2 | SR.1.1 TDD |  |
|  |  | 3 | SR.2.1 TDD |  |
| RMSI CORESET RMC configuration |  | 1 | CR.1.1 FDD | N/A |
|  |  | 2 | CR.1.1 TDD | N/A |
|  |  | 3 | CR.2.1 TDD | N/A |
| Dedicated CORESET RMC configuration |  | 1 | CCR.1.1 FDD | N/A |
|  |  | 2 | CCR.1.1 TDD | N/A |
|  |  | 3 | CCR.2.1 TDD | N/A |
| OCNG Patterns |  | 1, 2, 3 | OP.1 | OP.1 |
| TRS Configuration |  | 1 | TRS.1.1 FDD | N/A |
|  |  | 2 | TRS.1.1 TDD | N/A |
|  |  | 3 | TRS.1.2 TDD | N/A |
| IInitial BWP configuration |  | 1, 2, 3 | DLBWP.0.1 ULBWP.0.1 | DLBWP.0.1 ULBWP.0.1 |
| Active DL BWP configuration |  | 1, 2, 3 | DLBWP.1.1 | DLBWP.1.1 |
| Active UL BWP configuration |  | 1, 2, 3 | ULBWP.1.1 | ULBWP.1.1 |
| RLM-RS |  | 1, 2, 3 | SSB | SSB |
|  Note 2 | dBm/SCS | 1 | -98 |
|  |  | 2 | -98 |
|  |  | 3 | -95 |
|  Note 2 | dBm/15 kHz | 1 | -98 |
|  |  | 2 |  |
|  |  | 3 |  |
|  | dB | 1 | 4 | -1.46 | -Infinity | -1.46 |
|  |  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
|  | dB | 1 | 4 | 4 | -Infinity | 4 |
|  |  | 2 |  |  |  |  |
|  |  | 3 |  |  |  |  |
| SS-RSRP Note 3 | dBm/SCS kHz | 1 | -94 | -94 | -Infinity | -94 |
|  |  | 2 | -94 | -94 | -Infinity | -94 |
|  |  | 3 | -91 | -91 | -Infinity | -91 |
| Io | dBm/9.36 MHz | 1 | -64.60 | -62.25 | --64.60 | -62.25 |
|  | dBm/9.36 MHz | 2 | -64.60 | -62.25 | --64.60 | -62.25 |
|  | dBm/38.16 MHz | 3 | -58.50 | -56.16 | --58.50 | -56.16 |
| Propagation Condition |  | 1, 2, 3 | AWGN |
| Note 1: The resources for uplink transmission are assigned to the UE prior to the start of time period T2.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 3: SS-RSRP levels have been derived from other parameters for information purposes. They are not settable parameters themselves. |

## A.6.6.1.X.3 Test requirements

The UE shall send one Event A3 triggered measurement report, with a measurement reporting delay less than 800 ms from the beginning of time period T2. The UE is not required to read the neighbour cell SSB index in this test.

The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled.

The rate of correct events observed during repeated tests shall be at least 90%.

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

#### < END OF CHANGE 1>