**3GPP TSG CT WG3 Meeting #135 *C3-243563***

**Hyderabad, IN, 27 - 31 May, 2024 (Revision of C3-243304)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.519** | **CR** | **0513** | **rev** | **2** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Updates to GPSI and Application Layer ID mapping information | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | Ranging\_SL | | | | |  | ***Date:*** | | | 2024-05-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19) Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | TS 23.586 clause 4.3.5 updated with NOTE: Mapping between Application Layer ID and GPSI can be pre-provisioned by operator in application data, upon the approved CR 0066, needs to be aligned in this specification.  The Ranging/Sidelink Positioning-enabled UE Id mapping information between the Application Layer Id and GPSI is not suitable to be designed within the ServiceParameterData and ServiceParameterDataPatch data types, which is mainly designed for Service Parameter provisioning e2e utilized by PCF and forwarding to UE align with TS 23.502 clause 5.2.6.11.1 General definition that this service is for allowing external party to provision of service specific parameters which can be used for the UE in 5GS, while the mapping information between the Application Layer Id and GPSI is not to be used by UE.  Hence not to bring future impacts to the Nnef\_ServiceParameter API and following UDR, PCF and UE procedure, needs to update the resource structure of application data in UDR with a specific ranging/sidelink UE mapping resource to avoid impacts to serviceParamData resource and not to limit future service parameter extension and handling in UDR, PCF and UE.  SA2 has the related LS reply for LS out S2-2405863 (C3-242616) and TS 23.502 CR 4812 updated the UE ID mapping information as a separate resource in UDR application data, not mixed in Service Parameter information application data. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding Ranging/Sidelink UE mapping resource definition in application data of UDR, update the data structure and remove the impacts to the ServiceParameterData and ServiceParameterDataPatch data type.  Update the OpenAPI file accordingly.  Adding NOTE: Ranging/Sidelink UE Id Mapping information between Application Layer ID and GPSI can also be pre-provisioned by operator in the application data of UDR. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not completely and not effectively implement stage 2 requirement on Ranging/Sidelink UE GPSI and Application Layer ID mapping information in UDR, and not resolve the impacts and future limitation to the ServiceParamData resource and related NF impacts. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.2, 6.2.26(new), 6.2.27(new), 6.4.1, 6.4.2.15, 6.4.2.15A, A.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 23.502 CR 4812 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible feature in the OpenAPI file of Nudr\_DataRepository API application data.  Needs TS 29.522 UEId API to be implemented for the reused data type. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | **Rev 1 provides additional update:**  Adding the related TS 23.502 CR 4812 in cover page and updated error handling.  **Rev 2 provides additional update:**  Updated upon the service operation naming changed in the agreed TS 23.502 CR 4812 and removed application errors for future discussion. | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

### 6.2.2 Resource Structure

This clause describes the structure for the Resource URIs and the resources and methods used for the service.

Figure 6.2.2-1 depicts the resource URIs structure for the Nudr\_DataRepository API for application data



Figure 6.2.2-1: Resource URI structure of the Nudr\_DataRepository API for application data

Table 6.2.2-1 provides an overview of the resources and applicable HTTP methods.

Table 6.2.2-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description |
| PFD Data | /application-data/pfds | GET | Retrieve PFDs for application identifier(s) identified by query parameter(s).  Retrieve PFDs for all application identifier(s) if no query parameter is included in the Request URI. |
| Individual PFD Data | /application-data/pfds/{appId} | GET | Retrieve the corresponding PFDs of the specified application identifier. |
| DELETE | Delete the corresponding PFDs of the specified application identifier. |
| PUT | Create or update the corresponding PFDs for the specified application identifier. |
| Influence Data | /application-data/influenceData  (NOTE) | GET | Retrieve the Session Influence Data of given services, S-NSSAIs and DNNs or Internal Group Identifier(s) or Subscriber Category(ies) or SUPIs. |
| Individual Influence Data | /application-data/influenceData/ {influenceId}  (NOTE) | PUT | Create an individual Influence Data resource identified by {influenceId}, or modify all of the properties of an individual Influence Data resource identified by {influenceId}. |
| PATCH | Modify part of the properties of an individual Influence Data resource identified by {influenceId}. |
| DELETE | Delete an individual Influence Data resource identified by {influenceId}. |
| Influence Data Subscription | /application-data/influenceData/ subs-to-notify  (NOTE) | POST | Create a new Individual Influence Data Subscription resource. |
| GET | Read subscriptions for a given S-NSSAI and DNN or Internal Group Identifier(s) or Subscriber Category(ies) or SUPI. |
| Individual Influence Data Subscription | /application-data/influenceData/ subs-to-notify/{subscriptionId}  (NOTE) | GET | Get an existing individual Influence Data Subscription resource identified by {subscriptionId}. |
| PUT | Modify an existing individual Influence Data Subscription resource identified by {subscriptionId}. |
| DELETE | Delete an individual Influence Data Subscription resource identified by {subscriptionId}. |
| Applied BDT Policy Data | /application-data/bdtPolicyData  (NOTE) | GET | Retrieve the applied BDT policy data. |
| Individual Applied BDT Policy Data | /application-data/bdtPolicyData/{bdtPolicyId}  (NOTE) | PUT | Create an individual applied BDT Policy Data resource identified by {bdtPolicyId}. |
| PATCH | Modify BDT Reference Id of an individual applied BDT Policy Data resource identified by {bdtPolicyId}. |
| DELETE | Delete an individual applied BDT Policy Data resource identified by {bdtPolicyId}. |
| IPTV Configurations | /application-data/iptvConfigData  (NOTE) | GET | Retrieve IPTV configurations for configuration identifier(s), given S-NSSAI(s) and DNN(s), or SUPIs or Internal Group Identifiers |
| Individual IPTV Configuation | /application-data/iptvConfigData/ {configurationId}  (NOTE) | PUT | Create an Individual IPTV Configuration resource identified by {configurationId}, or modify all the properties of an Individual IPTV Configuration resource identified by {configurationId}. |
| PATCH | Modify some properties of an Individual IPTV Configuration resource identified by {configurationId}. |
| DELETE | Delete an Individual IPTV Configuration resource identified by {configurationId} |
| Service Parameter Data | /application-data/serviceParamData  (NOTE) | GET | Retrieve the Service Parameter Data of given services, S-NSSAIs and DNNs or Internal Group Identifiers or SUPIs. |
| Individual Service Parameter Data | /application-data/serviceParamData/ {serviceParamId}  (NOTE) | PUT | Create an individual Service Parameter Data resource identified by {serviceParamId}, or modify all of the properties of an individual Service Parameter Data resource identified by {serviceParamId}. |
| PATCH | Modify part of the properties of an individual Service Parameter Data resource identified by {serviceParamId}. |
| DELETE | Delete an individual Service Parameter Data resource identified by {serviceParamId}. |
| AM Influence Data | /application-data/am-influence-data | GET | Retrieve the AM Influence Data of given S-NSSAIs and DNNs and/or Internal Group Identifiers or SUPIs or for LBO roaming scenarios, any inbound roaming UEs identified by their home PLMN ID(s). |
| Individual AM Influence Data | /application-data/am-influence-data/{amInfluenceId} | PUT | Create an individual AM Influence Data resource identified by {amInfluenceId}, or modify all of the properties of an individual AM Influence Data resource identified by {amInfluenceId}. |
| PATCH | Modify part of the properties of an individual AM Influence Data resource identified by {amInfluenceId}. |
| DELETE | Delete an individual AM Influence Data resource identified by {amInfluenceId}. |
| ApplicationDataSubscriptions | /application-data/subs-to-notify | POST | Create a subscription to receive notification of application data changes. |
| GET | Read all the subscriptions, or subscriptions for given S-NSSAI and DNN or Internal Group Identifier or SUPI. |
| IndividualApplicationDataSubscription | /application-data/subs-to-notify/ {subsId} | PUT | Modify a subscription to receive notification of application data changes identified by {subsId}. |
| DELETE | Delete a subscription identified by {subsId}. |
| GET | Read an existing individual Subscription resource identified by {subsId}. |
| EAS Deployment Information Data | /application-data/eas-deploy-data | GET | Retrieve the EAS Deployment Information Data, given DNN(s), S-NSSAI(s), Application ID or Internal Group Identifiers. |
| Individual EAS Deployment Information Data | /application-data/eas-deploy-data/{easDeployInfoId} | GET | Read an existing individual EAS Deployment Data identified by {easDeployInfoId}. |
| PUT | Create an individual EAS deployment information Data resource identified by {easDeployInfold} or Update an individual EAS Deployment Data resource identified by {easDeployInfoId}. |
| DELETE | Delete an individual EAS Deployment Data resource identified by {easDeployInfoId}. |
| AF Requested QoS Data Sets | /application-data/af-qos-data-sets | GET | Retrieve one or several existing AF Requested QoS Data Set(s). |
| Individual AF Requested QoS Data Set | /application-data/af-qos-datasets/{afReqQosId} | PUT | Create an Individual AF Requested QoS Data Set or update an existing Individual AF Requested QoS Data Set. |
| PATCH | Modify an existing Individual AF Requested QoS Data Set. |
| DELETE | Delete an existing Individual AF Requested QoS Data Set. |
| Individual DNAI EAS Mapping | /application-data/dnai-eas-mappings/{dnai} | GET | Retrieve the EAS address information for a DNAI. |
| ECS Address Roaming Data | /application-data/ecs-address-roaming | GET | Retrieve all existing ECS Address Configuration Information for roaming UEs. |
| Individual ECS Address Roaming Data | /application-data/ecs-address-roaming/{ecsAddrInfoId} | GET | Retrieve an existing ECS Address Configuration Information entry for roaming UEs. |
| PUT | Create or Update an ECS Address Configuration Information entry for roaming UEs. |
| DELETE | Delete an existing ECS Address Configuration Information entry for roaming UEs. |
| UE ID Mappings | /application-data/ueid-mappings | GET | Retrieve alone or several existing UE ID Mapping(s). |
| Individual UE ID Mapping | /application-data/ueid-mappings/{ueMappingId} | GET | Retrieve an existing "Individual UE ID Mapping" resource. |
| PUT | Create or Update a UE ID Mapping. |
| DELETE | Delete an existing "Individual UE ID Mapping" resource. |
| NOTE: The path segment does not follow the related naming convention defined in 3GPP TS 29.501 [5]. The path segment is kept though as defined in the current specification for backward compatibility considerations. | | | |

\*\*\* 2nd Change \*\*\*

### 6.2.26 Resource: UE ID Mappings

#### 6.2.26.1 Description

This resource represents all the active UE ID Mappings at the UDR.

#### 6.2.26.2 Resource definition

Resource URI: **{apiRoot}/nudr-dr/<apiVersion>/application-data/ueid-mappings**

This resource shall support the resource URI variables defined in table 6.2.26.2-1.

Table 6.2.26.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See 3GPP TS 29.504 [6] clause 6.1.1. |

#### 6.2.26.3 Resource Standard Methods

##### 6.2.26.3.1 GET

This method shall support the URI query parameters specified in table 6.2.26.3.1-1.

Table 6.2.26.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| app-layer-ids | array(ApplicationlayerId) | O | 1..N | Contains the requested Application Layer ID(s).  (NOTE) |
| gpsis | array(Gpsi) | O | 1..N | Contains the requested GPSI(s).  (NOTE) |
| supp-feat | SupportedFeatures | O | 0..1 | Contains the list of supported features. |
| NOTE: These query parameters are mutually exclusive. Either one of them may be present. | | | | |

This method shall support the request data structures specified in table 6.2.26.3.1-2 and the response data structures and response codes specified in table 6.2.26.3.1-3.

Table 6.2.26.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.2.26.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| array(UeIdMappingInfo) | M | 0..N | 200 OK | Successful case. The requested UE ID mapping information is returned. |
| NOTE: The mandatory HTTP error status codes for the HTTP GET method listed in table 5.2.7.1-1 of 3GPP TS 29.500 [4] shall also apply. | | | | |

\*\*\* 3rd Change \*\*\*

### 6.2.27 Resource: Individual UE ID Mapping

#### 6.2.27.1 Description

This resource represents a UE ID Mapping at the UDR.

#### 6.2.27.2 Resource definition

Resource URI: **{apiRoot}/nudr-dr/<apiVersion>/application-data/ueid-mappings/{ueMappingId}**

This resource shall support the resource URI variables defined in table 6.2.27.2-1.

Table 6.2.27.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See 3GPP TS 29.504 [6] clause 6.1.1. |
| ueMappingId | string | Identifies an "Individual UE ID Mapping" resource. |

#### 6.2.27.3 Resource Standard Methods

##### 6.2.27.3.1 GET

This method shall support the URI query parameters specified in table 6.2.27.3.1-1.

Table 6.2.27.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 6.2.27.3.1-2 and the response data structures and response codes specified in table 6.2.27.3.1-3.

Table 6.2.27.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  | |

Table 6.2.27.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| UeIdMappingInfo | M | 1 | 200 OK | Successful case. The requested "UE ID Mapping" resource is returned. |
| NOTE: The mandatory HTTP error status codes for the HTTP GET method listed in table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply. | | | | |



##### 6.2.27.3.3 DELETE

This method shall support the URI query parameters specified in table 6.2.27.3.3-1.

Table 6.2.27.3.3-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 6.2.27.3.3-2 and the response data structures and response codes specified in table 6.2.27.3.3-3.

Table 6.2.27.3.3-2: Data structures supported by the DELETE Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.2.27.3.3-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| n/a |  |  | 204 No Content | Successful case. The "UE ID Mapping" resource is successfully deleted. |
| NOTE: The mandatory HTTP error status codes for the HTTP DELETE method listed in table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply. | | | | |

\*\*\* 4th Change \*\*\*

### 6.4.1 General

This clause specifies the application data model supported by the API.

Table 6.4.1-1 specifies the data types defined for the Nudr\_DataRepository Service API for Application Data service based interface protocol.

Table 6.4.1-1: Nudr\_DataRepository specific Data Types for Application Data

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| AfRequestedQosData | 6.4.2.18 | Represents an AF Requested QoS Data Set. | GMEC |
| AfRequestedQosDataPatch | 6.4.2.19 | Represents the requested modifications to an AF Requested QoS Data Set. | GMEC |
| AmInfluData | 6.4.2.16 | Contains AM influence data. | DCAMP |
| AmInfluDataPatch | 6.4.2.17 | Contains AM influence data that can be updated. | DCAMP |
| ApplicationDataSubs | 6.4.2.10 | Contains application data subscription data. |  |
| ApplicationDataChangeNotif | 6.4.2.11 | Contains the new or updated application data or removed indication. |  |
| BdtPolicyData | 6.4.2.7 | Contains applied BDT policy data. | EnhancedBackgroundDataTransfer |
| BdtPolicyDataPatch | 6.4.2.8 | Contains modification instructions to be performed on the applied BDT policy data. | EnhancedBackgroundDataTransfer |
| CorrelationType | 6.4.3.4 | Indicates that the EAS(es) corresponding to a common DNAI or common EAS should be selected | CommonEASDNAI |
| DataInd | 6.4.3.3 | Indicates the type of data. |  |
| DataFilter | 6.4.2.12 | Indicates an application data filter. |  |
| DnaiEasInfo | 6.4.2.22 | Contains EAS information for a DNAI. | DnaiEasMappings |
| DnaiEasMapping | 6.4.2.21 | Contains DNAI(s) to EAS mapping. | DnaiEasMappings |
| EcsAddrData | 6.4.2.23 | Represents ECS Address Configuration Data. | HR-SBO |
| IptvConfigData | 6.4.2.9 | Represents IPTV configuration data information. |  |
| PfdDataForAppExt | 6.4.2.6 | The PFDs and related data for the application |  |
| QosRequirements | 6.4.6.24 | Represents QoS requirements. | GMEC |
| QosRequirementsRm | 6.4.6.25 | Represents the same as the QosRequirements data type but with the OpenAPI "nullable: true" property. | GMEC |
| ServiceParameterData | 6.4.2.15 | Contains the service parameter data. |  |
| TrafficCorrelationInfo | 6.4.2.18 | Contains the information for traffic correlation. | CommonEASDNAI |
| ServiceParameterDataPatch | 6.4.2.15A | Contains the service parameter data that can be updated. |  |
| TrafficInfluData | 6.4.2.2 | Contains traffic influence data. |  |
| TrafficInfluDataPatch | 6.4.2.3 | Contains modification instructions to be performed on the traffic influence data. |  |
| TrafficInfluDataNotif | 6.4.2.14 | Contains traffic influence data for notification. | EnhancedInfluDataNotification |
| TrafficInfluSub | 6.4.2.4 | Contains traffic influence subscription data. |  |

Table 6.4.1-2 specifies data types re-used by the Nudr\_DataRepository Service API for Application Data service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nudr\_DataRepository Service API for Application Data service based interface.

Table 6.4.1-2: Nudr\_DataRepository re-used Data Types for Application Data

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| A2xParamsPc5 | 3GPP TS 29.522 [19] | Contains the A2X service parameters data provisioned over PC5. | A2X |
| A2xParamsPc5Rm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the A2xParamsPc5 data type, but with the OpenAPI nullable property set to true. | A2X |
| AmInfluEvent | 3GPP TS 29.522 [19] | Identifies the type of AM related events of which the AF requests to be notified. |  |
| AlternativeServiceRequirementsData | 3GPP TS 29.514 [52] | Contains alternative QoS related parameters and a reference to them. | GMEC |
| ApplicationId | 3GPP TS 29.571 [7] | Indicates an application identifier. |  |
| BdtReferenceId | 3GPP TS 29.122 [9] | Identifies a selected policy of background data transfer. | EnhancedBackgroundDataTransfer |
| BitRate | 3GPP TS 29.571 [7] | Represent a bitrate. | GMEC |
| DateTime | 3GPP TS 29.571 [7] | Indicates a date and time. |  |
| DateTimeRm | 3GPP TS 29.571 [7] | Indicates a date and time that can be updated. |  |
| Dnai | 3GPP TS 29.571 [7] | Represents a DNAI. | DnaiEasMappings |
| DnaiChangeType | 3GPP TS 29.571 [7] | Describes the types of DNAI change. |  |
| Dnn | 3GPP TS 29.571 [7] | Identifies a Data Network Name. (NOTE 2) |  |
| DnnSnssaiInformation | 3GPP TS 29.522 [19] | Represents a DNN, S-NSSAI combination. | DCAMP |
| DurationSec | 3GPP TS 29.571 [7] | Represents a duration in seconds. | DCAMP  CachingTimer |
| DurationSecRm | 3GPP TS 29.571 [7] | Represents a removable duration in seconds. | DCAMP |
| EasDeployInfoData | 3GPP TS 29.591 [23] | Represnts the EAS Deployment Information. | EasDeployment |
| EcsServerAddr | 3GPP TS 29.571 [7] | Represents the Edge Configuration Server (ECS) address configuration information. | HR-SBO |
| EthFlowDescription | 3GPP TS 29.514 [16] | Contains the Ethernet data flow information.(NOTE) |  |
| EthFlowInfo | 3GPP TS 29.122 [9] | Represents Ethernet flow information | GMEC |
| Event | 3GPP TS 29.522 [19] | Contains the outcome of the UE Policy Delivery related to the invocation of AF provisioned service parameters. | DeliveryOutcome |
| EventsSubscReqData | 3GPP TS 29.514 [16] | Identifies the events the application subscribes to. | GMEC |
| EventsSubscReqDataRm | 3GPP TS 29.514 [16] | This data type is defined in the same way as the EventsSubsReqData data type, but with the OpenAPI nullable property set to true. | GMEC |
| FlowInfo | 3GPP TS 29.122 [9] | Contains the flow information. |  |
| FqdnPatternMatchingRule | 3GPP TS 29.571 [7] | Identifies an FQDN pattern matching rule. | DnaiEasMappings |
| GroupId | 3GPP TS 29.571 [7] | Identifies a group of users. | EasDeployment |
| IpAddr | 3GPP TS 29.571 [7] | IP address and/or prefix. | DnaiEasMappings |
| IptvConfigDataPatch | 3GPP TS 29.522 [19] | Contains the IPTV configuration data used for PATCH. |  |
| Ipv4Addr | 3GPP TS 29.571 [7] | Identifies an IPv4 address. |  |
| Ipv6Addr | 3GPP TS 29.571 [7] | Identifies an IPv6 address. |  |
| Link | 3GPP TS 29.122 [9] | Identifies a referenced resource. | HR-SBO |
| MacAddr48 | 3GPP TS 29.571 [7] | MAC Address. |  |
| MulticastAccessControl | 3GPP TS 29.522 [19] | Represents the multicast access control information. |  |
| NetworkAreaInfo | 3GPP TS 29.554 [13] | Describes a network area information. |  |
| NetworkDescription | 3GPP TS 29.522 [19] | Represents the description of a PLMN in terms of the PLMN ID, the MCC (and optionally, applicable MNCs) or the indication of any PLMN | VPLMNSpecificURSP |
| ParameterOverPc5 | 3GPP TS 29.522 [19] | Contains the V2X service parameters data provisioned over PC5. |  |
| ParameterOverPc5Rm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParameterOverPc5 data type, but with the OpenAPI nullable property set to true. |  |
| ParameterOverUu | 3GPP TS 29.522 [19] | Contains the V2X service parameters data provisioned over Uu. |  |
| ParameterOverUuRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParameterOverUu data type, but with the OpenAPI nullable property set to true. |  |
| ParamForProSeDc | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe direct communications. | ProSe |
| ParamForProSeDcRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParamForProSeDc data type, but with the OpenAPI nullable property set to true. |  |
| ParamForProSeDd | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe direct discovery. | ProSe |
| ParamForProSeDdRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParamForProSeDd data type, but with the OpenAPI nullable property set to true. |  |
| ParamForProSeEndUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe End UE. | ProSe\_Ph2 |
| ParamForProSeEndUeRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParamForProSeEndUe data type, but with the OpenAPI nullable property set to true. | ProSe\_Ph2 |
| ParamForProSeRemUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe remote UE. | ProSe |
| ParamForProSeRemUeRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParamForProSeRemUe data type, but with the OpenAPI nullable property set to true. |  |
| ParamForProSeU2NRelUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe UE-to-network relay UE. | ProSe |
| ParamForProSeU2NRelUeRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParamForProSeU2NRelUe data type, but with the OpenAPI nullable property set to true. |  |
| ParamForProSeU2URelUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe UE-to-UE Relay UE. | ProSe\_Ph2 |
| ParamForProSeU2URelUeRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the ParamForProSeU2URelUe data type, but with the OpenAPI nullable property set to true. | ProSe\_Ph2 |
| ParamForRangingSlPos | 3GPP TS 29.522 [19] | Contains the service parameters for ranging and sidelink positioning. | Ranging\_SL |
| ParamForRangingSlPosRm | 3GPP TS 29.522 [19] | This data type is defined in the same way as the "ParamForRangingSlPos" data type, but with the OpenAPI "nullable: true" property. | Ranging\_SL |
| PfdChangeNotification | 3GPP TS 29.551 [8] | Describes the PFD change. |  |
| PfdContent | 3GPP TS 29.551 [8] | Represents the content of a PFD for an application identifier. |  |
| PlmnId | 3GPP TS 29.571 [7] | Identifies a PLMN. | DCAMP\_Roaming\_LBO |
| RouteToLocation | 3GPP TS 29.571 [7] | Identifies the N6 traffic routing requirement. |  |
| ServiceAreaCoverageInfo | 3GPP TS 29.534 [22] | Contains service area coverage information. | DCAMP |
| Snssai | 3GPP TS 29.571 [7] | Identifies a Single Network Slice Selection Assistance Information. |  |
| SpatialValidityCond | 3GPP TS 29.571 [7] | Indicates the spatial validity condition. | HR-SBO |
| SubscribedEvent | 3GPP TS 29.522 [19] | Identified the type of UP path management events of which the AF requests to be notified. |  |
| Supi | 3GPP TS 29.571 [7] | Identifies a SUPI that shall contain either an IMSI or an NAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [7] | Used to negotiate the applicability of the optional features. |  |
| TemporalInValidity | 3GPP TS 29.565 [27] | Indicates the time interval during which the NF service consumer request shall not to be applied | GMEC |
| TemporalValidity | 3GPP TS 29.514 [16] | Indicates the time interval during which the AF request is to be applied. | MultiTemporalCondition |
| TnapId | 3GPP TS 29.571 [7] | Trusted Network Access Point identifier. | AfGuideTNAPs |
| TscaiInputContainer | 3GPP TS 29.514 [16] | Represents the TSCAI Input information container. | GMEC |
| TsnQosContainer | 3GPP TS 29.514 [16] | Represents the TSC traffic QoS parameters. | GMEC |
| UeIdMappingInfo | 3GPP TS 29.522 [19] | Contains the UE ID mapping information. | Ranging\_SL |
| Uinteger | 3GPP TS 29.571 [7] | Unsigned Integer, i.e. only value 0 and integers greater than 0 are allowed. |  |
| UintegerRm | 3GPP TS 29.571 [7] | This data type is defined in the same way as the "Uinteger" data type, but with the OpenAPI "nullable: true" property. |  |
| Uri | 3GPP TS 29.571 [7] | Identifies a URI. |  |
| UriRm | 3GPP TS 29.571 [7] | Identifies a removable URI. | DCAMP |
| UrspRuleRequest | 3GPP TS 29.522 [19] | Contains service parameter data used to guide the URSP. | AfGuideURSP |
| NOTE 1: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange as specified in clause 6.1.8 of TS 29.504 [6] shall be supported.  NOTE 2: The UDR uses the DNN as received from the NF service consumer without applying any transformation. To successfully perform DNN matching, in a specific deployment a DNN shall always be encoded either with the full DNN (e.g., because there are multiple Operator Identifiers for a Network Identifier) or the DNN Network Identifier only. | | | |

\*\*\* 5th Change \*\*\*

#### 6.4.2.15 Type ServiceParameterData

Table 6.4.2.15-1: Definition of type ServiceParameterData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| dnn | Dnn | O | 0..1 | Identifies a DNN. (NOTE 2) |  |
| snssai | Snssai | O | 0..1 | Identifies an S-NSSAI. (NOTE 2) |  |
| appId | string | O | 0..1 | Identifies an application identifier. (NOTE 2) |  |
| supi | Supi | O | 0..1 | Identifies a user. (NOTE1) |  |
| ueIpv4 | Ipv4Addr | O | 0..1 | The IPv4 address of the served UE. (NOTE1) |  |
| ueIpv6 | Ipv6Addr | O | 0..1 | The IPv6 address of the served UE. (NOTE1) |  |
| ueMac | MacAddr48 | O | 0..1 | The MAC address of the served UE. (NOTE1) |  |
| interGroupId | GroupId | O | 0..1 | Identifies a group of users. (NOTE1) |  |
| anyUeInd | boolean | O | 0..1 | Identifies whether the service parameters applies to any non-roaming UE. This attribute shall set to "true" if applicable for any UE, otherwise, set to "false". (NOTE1) |  |
| roamUeNetDescs | array(NetworkDescription) | O | 1..N | Each element identifies one (e.g., combination of MCC and MNC) or more (e.g. a MCC only) PLMN ID(s).  It indicates the PLMN(s) of inbound roamers to which the provided AF guidance on VPLMN-specific URSP rules apply. (NOTE 1) | VPLMNSpecificURSP |
| paramOverPc5 | ParameterOverPc5 | O | 0..1 | Contains the V2X service parameters used over PC5. |  |
| paramOverUu | ParameterOverUu | O | 0..1 | Contains the V2X service parameters used over Uu. |  |
| a2xParamsPc5 | A2xParamsPc5 | O | 0..1 | Contains the A2X service parameters used over PC5. | A2X |
| urspGuidance | array(UrspRuleRequest) | O | 1..N | Contains the service parameter used to guide the URSP and/or, when the VPLMNSpecificURSP feature is supported, to guide the VPLMN-specific URSP.  (NOTE 3) | AfGuideURSP |
| paramForProSeDd | ParamForProSeDd | O | 0..1 | Contains the service parameters for 5G ProSe direct discovery. | ProSe |
| paramForProSeDc | ParamForProSeDc | O | 0..1 | Contains the service parameters for 5G ProSe direct communications. | ProSe |
| paramForProSeU2NRelUe | ParamForProSeU2NRelUe | O | 0..1 | Contains the service parameters for 5G ProSe UE-to-network relay UE. | ProSe |
| paramForProSeRemUe | ParamForProSeRemUe | O | 0..1 | Contains the service parameters for 5G ProSe remote UE. | ProSe |
| paramForProSeU2URelUe | ParamForProSeU2URelUe | O | 0..1 | Contains the service parameters for 5G ProSe UE-to-UE Relay UE. | ProSe\_Ph2 |
| paramForProSeEndUe | ParamForProSeEndUe | O | 0..1 | Contains the service parameters for 5G ProSe End UE. | ProSe\_Ph2 |
| tnaps | array(TnapId) | O | 1..N | Contains the TNAP ID(s) collocated with the 5G-RG(s) of a specific user. | AfGuideTNAPs |
| deliveryEvents | array(Event) | O | 1..N | Contains the events related to the outcome of UE policy delivery. | DeliveryOutcome |
| policDelivNotifCorreId | string | C | 0..1 | Contains the Notification Correlation Id allocated by the NEF for the notification of UE Policy delivery outcome. It shall be included when the NEF requests the notification of UE Policy delivery outcome. | DeliveryOutcome |
| policDelivNotifUri | Uri | C | 0..1 | Contains the URI where the NEF receives the notification of UE Policy delivery outcome. It shall be included when the NEF requests the notification of UE policy delivery outcome. | DeliveryOutcome |
| headers | array(string) | O | 1..N | Headers provisioned by the NEF.  E.g. 3gpp-Sbi-Binding header (as specified in 3GPP TS 29.500 [4]) with the binding indication for the URI included in the policDelivNotifUri attribute.  The encoding of the header shall comply with clause 6.3 of IETF RFC 9110 [21]. | DeliveryOutcome |
| suppFeat | SupportedFeatures | C | 0..1 | Indicates the list of Supported features used as described in clause 5.8.  This parameter shall be supplied in the PUT request that requested the creation of an individual Service parameter resource, and in the PUT response. |  |
| resUri | Uri | C | 0..1 | Represents the URI of Individual Service Parameter Data. It shall only be included in the HTTP GET response. |  |
| resetIds | array(string) | O | 1..N | This IE uniquely identifies a part of temporary data in UDR that contains the created resource.  This attribute may be provided in the response of successful resource creation. |  |
| paramForRangingSlPos | ParamForRangingSlPos | O | 0..1 | Contains the service parameters for ranging and sidelink positioning. | Ranging\_SL |
| NOTE 1: Only one of the "supi", "anyUeInd", "interGroupId", "ueIpv4", "ueIpv6" or "ueMac" attribute, and when the feature "VPLMNSpecificURSP" is supported, or "roamUeNetDescs attribute", shall be provided. When the "AfGuideTNAPs" feature is supported, and the attribute "tnaps" is included, only the "supi" attribute shall be provided. When the "VPLMNSpecificURSP" feature is supported, the "roamUeNetDescs" attribute only applies to URSP service parameter provisioning and shall be included when the "urspGuidance" attribute contains VPLMN(s) description.  NOTE 2: Only the combination of "dnn" and "snssai" or "appId" attribute shall be provided. When the "AfGuideTNAPs" feature is supported and the attribute "tnaps" is included, only the combination of "dnn" and "snssai" attributes shall be provided.  NOTE 3: when the "AfGuideURSP" feature is supported and the attribute "urspGuidance" is included, the provided URSP guidance may apply to DNN and S-NSSAI combination(s) and/or application(s) different to the ones provided within the "dnn" and "snssai" or "appId" attributes. | | | | | |

\*\*\* 6th Change \*\*\*

#### 6.4.2.15A Type ServiceParameterDataPatch

Table 6.4.2.15A-1: Definition of type ServiceParameterDataPatch

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| paramOverPc5 | ParameterOverPc5Rm | O | 0..1 | Contains the V2X service parameters used over PC5. When the"NullableSupport" feature is supported, this attribute is nullable. When the"NullableSupport" feature is not supported, this attribute is not nullable. |  |
| paramOverUu | ParameterOverUuRm | O | 0..1 | Contains the V2X service parameters used over Uu. When the "NullableSupport" feature is supported, this attribute is nullable. When the "NullableSupport" feature is not supported, this attribute is not nullable. |  |
| a2xParamsPc5 | A2xParamsPc5Rm | O | 0..1 | Contains the A2X service parameters used over PC5. | A2X |
| urspInfluence | array(UrspRuleRequest) | O | 1..N | Contains the service parameter used to influence the URSP.  This attribute is deprecated by the "urspGuidance" attribute that should be used instead. | AfGuideURSP |
| urspGuidance | array(UrspRuleRequest) | O | 1..N | Contains the service parameter used to guide the URSP and/or, when the VPLMNSpecificURSP feature is supported, to guide the VPLMN-specific URSP. | AfGuideURSP  PatchCorrection |
| paramForProSeDd | ParamForProSeDdRm | O | 0..1 | Contains the service parameters for 5G ProSe direct discovery.  When the "NullableSupport" feature is supported, this attribute is nullable. When the "NullableSupport" feature is not supported, this attribute is not nullable. | ProSe |
| paramForProSeDc | ParamForProSeDcRm | O | 0..1 | Contains the service parameters for 5G ProSe direct communications.  When the "NullableSupport" feature is supported, this attribute is nullable. When the "NullableSupport" feature is not supported, this attribute is not nullable. | ProSe |
| paramForProSeU2NRelUe | ParamForProSeU2NRelUeRm | O | 0..1 | Contains the service parameters for 5G ProSe UE-to-network relay UE.  When the "NullableSupport" feature is supported, this attribute is nullable. When the "NullableSupport" feature is not supported, this attribute is not nullable. | ProSe |
| paramForProSeRemUe | ParamForProSeRemUeRm | O | 0..1 | Contains the service parameters for 5G ProSe remote UE.  When the "NullableSupport" feature is supported, this attribute is nullable. When the "NullableSupport" feature is not supported, this attribute is not nullable. | ProSe |
| paramForProSeU2URelUE | ParamForProSeU2URelUeRm | O | 0..1 | Contains the service parameters for 5G ProSe UE-to-UE Relay UE. | ProSe\_Ph2 |
| paramForProSeEndUe | ParamForProSeEndUeRm | O | 0..1 | Contains the service parameters for 5G ProSe End UE. | ProSe\_Ph2 |
| tnaps | array(TnapId) | O | 1..N | Contains the TNAP ID(s) collocated with the 5G-RG(s) of a specific user. | AfGuideTNAPs |
| deliveryEvents | array(Event) | O | 1..N | Contains the events related to the outcome of UE policy delivery.  When the "NullableSupport" feature is supported, this attribute is nullable. When the "NullableSupport" feature is not supported, this attribute is not nullable. | DeliveryOutcome |
| policDelivNotifUri | Uri | C | 0..1 | Contains the URI where the NEF receives the notification of UE Policy delivery outcome. It shall be included when the NEF requests the notification of UE policy delivery outcome. | DeliveryOutcome |
| headers | array(string) | O | 1..N | Headers provisioned by the NEF.  E.g. 3gpp-Sbi-Binding header (as specified in 3GPP TS 29.500 [4]) with the binding indication for the URI included in the policDelivNotifUri IE.  The encoding of the header shall comply with clause 6.3 of IETF RFC 9110 [21]. | DeliveryOutcome |
| paramForRangingSlPos | ParamForRangingSlPosRm | O | 0..1 | Contains the service parameters for ranging and sidelink positioning. | Ranging\_SL |

\*\*\* 7th Change \*\*\*

# A.3 Nudr\_DataRepository API for Application Data

For the purpose of referencing entities in the Open API file defined in this Annex, it shall be assumed that this Open API file is contained in a physical file named "TS29519\_Application\_Data.yaml".

openapi: 3.0.0

info:

version: '-'

title: Unified Data Repository Service API file for Application Data

description: |

The API version is defined in 3GPP TS 29.504

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.519 V18.5.0; 5G System; Usage of the Unified Data Repository Service for Policy Data,

Application Data and Structured Data for Exposure.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.519/'

paths:

/application-data/pfds:

get:

summary: Retrieve PFDs for application identifier(s)

operationId: ReadPFDData

tags:

- PFD Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:pfds:read

parameters:

- name: appId

in: query

description: >

Contains the information of the application identifier(s) for the querying PFD

Data resource. If none appId is included in the URI, it applies to all application

identifier(s) for the querying PFD Data resource.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

minItems: 1

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: A representation of PFDs for request applications is returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/PfdDataForAppExt'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/pfds/{appId}:

get:

summary: Retrieve the corresponding PFDs of the specified application identifier

operationId: ReadIndividualPFDData

tags:

- Individual PFD Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:pfds:read

parameters:

- name: appId

in: path

description: >

Indicate the application identifier for the request pfd(s). It shall apply the

format of Data type ApplicationId.

required: true

schema:

type: string

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: >

A representation of PFDs for the request application identified by the application

identifier is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete the corresponding PFDs of the specified application identifier

operationId: DeleteIndividualPFDData

tags:

- Individual PFD Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:pfds:modify

parameters:

- name: appId

in: path

description: >

Indicate the application identifier for the request pfd(s). It shall apply the

format of Data type ApplicationId.

required: true

schema:

type: string

responses:

'204':

description: >

Successful case. The Individual PFD Data resource related to the application

identifier was deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create or update the corresponding PFDs for the specified application identifier

operationId: CreateOrReplaceIndividualPFDData

tags:

- Individual PFD Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:pfds:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

parameters:

- name: appId

in: path

description: >

Indicate the application identifier for the request pfd(s). It shall apply the format

of Data type ApplicationId.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual PFD Data resource related to the application-identifier

is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

headers:

Location:

description: >

'Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nudr-dr/<apiVersion>/application-data/pfds/{appId}'

required: true

schema:

type: string

'200':

description: >

Successful case. The upgrade of an Individual PFD Data resource related to the

application identifier is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData:

get:

summary: Retrieve Traffic Influence Data

operationId: ReadInfluenceData

tags:

- Influence Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:read

parameters:

- name: influence-Ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: internal-Group-Ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: internal-group-ids-Add

in: query

description: Each element identifies an internal Group.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: subscriber-categories

in: query

description: >

Each element identifies a subscriber category.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: supp-feat

in: query

required: false

description: Supported Features

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: The Traffic Influence Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TrafficInfluData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData/{influenceId}:

put:

summary: Create or update an individual Influence Data resource

operationId: CreateOrReplaceIndividualInfluenceData

tags:

- Individual Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

parameters:

- name: influenceId

in: path

description: >

The Identifier of an Individual Influence Data to be created or updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual Traffic Influence Data resource is confirmed

and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

headers:

Location:

description: >

'Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nudr-dr/<apiVersion>/application-data/influenceData/{influenceId}'

required: true

schema:

type: string

'200':

description: >

The update of an Individual Traffic Influence Data resource is confirmed and a

response body containing Traffic Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual Influence Data resource

operationId: UpdateIndividualInfluenceData

tags:

- Individual Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/TrafficInfluDataPatch'

parameters:

- name: influenceId

in: path

description: >

The Identifier of an Individual Influence Data to be updated. It shall apply

the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: >

The update of an Individual Traffic Influence Data resource is confirmed and

a response body containing Traffic Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Influence Data resource

operationId: DeleteIndividualInfluenceData

tags:

- Individual Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:modify

parameters:

- name: influenceId

in: path

description: >

The Identifier of an Individual Influence Data to be deleted. It shall apply

the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual Influence Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData/subs-to-notify:

post:

summary: Create a new Individual Influence Data Subscription resource

operationId: CreateIndividualInfluenceDataSubscription

tags:

- Influence Data Subscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:subscriptions:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

responses:

'201':

description: The subscription was created successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

trafficInfluenceDataChangeNotification:

'{$request.body#/notificationUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

type: array

items:

oneOf:

- $ref: '#/components/schemas/TrafficInfluData'

- $ref: '#/components/schemas/TrafficInfluDataNotif'

minItems: 1

responses:

'204':

description: No Content, Notification was successful

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Read Influence Data Subscriptions

operationId: ReadInfluenceDataSubscriptions

tags:

- Influence Data Subscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:subscriptions:read

parameters:

- name: dnn

in: query

description: Identifies a DNN.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

- name: snssai

in: query

description: Identifies a slice.

required: false

content:

application/json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

- name: internal-Group-Id

in: query

description: Identifies a group of users.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

- name: supi

in: query

description: Identifies a user.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

- name: internal-group-ids

in: query

description: >

Each element identifies an internal group.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: subscriber-categories

in: query

description: >

Each element identifies a subscriber category.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: roam-ue-plmn-ids

in: query

description: >

Each element identifies a PLMN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

minItems: 1

responses:

'200':

description: >

The subscription information as request in the request URI query parameter(s)

are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TrafficInfluSub'

minItems: 0

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData/subs-to-notify/{subscriptionId}:

get:

summary: Get an existing individual Influence Data Subscription resource

operationId: ReadIndividualInfluenceDataSubscription

tags:

- Individual Influence Data Subscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:subscriptions:read

parameters:

- name: subscriptionId

in: path

description: >

String identifying a subscription to the Individual Influence Data Subscription

required: true

schema:

type: string

responses:

'200':

description: The subscription information is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Modify an existing individual Influence Data Subscription resource

operationId: ReplaceIndividualInfluenceDataSubscription

tags:

- Individual Influence Data Subscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:subscriptions:modify

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

parameters:

- name: subscriptionId

in: path

description: >

String identifying a subscription to the Individual Influence Data Subscription.

required: true

schema:

type: string

responses:

'200':

description: The subscription was updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Influence Data Subscription resource

operationId: DeleteIndividualInfluenceDataSubscription

tags:

- Individual Influence Data Subscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:influence-data:subscriptions:modify

parameters:

- name: subscriptionId

in: path

description: >

String identifying a subscription to the Individual Influence Data Subscription.

required: true

schema:

type: string

responses:

'204':

description: The subscription was terminated successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/bdtPolicyData:

get:

summary: Retrieve applied BDT Policy Data

operationId: ReadBdtPolicyData

tags:

- BdtPolicy Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:bdt-policy-data:read

parameters:

- name: bdt-policy-ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: internal-group-ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

responses:

'200':

description: The applied BDT policy Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/BdtPolicyData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/bdtPolicyData/{bdtPolicyId}:

put:

summary: Create an individual applied BDT Policy Data resource

operationId: CreateIndividualAppliedBdtPolicyData

tags:

- Individual Applied BDT Policy Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:bdt-policy-data:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicyData'

parameters:

- name: bdtPolicyId

in: path

description: >

The Identifier of an Individual Applied BDT Policy Data to be created or updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual Applied BDT Policy Data resource is confirmed and a

representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicyData'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nudr-dr/<apiVersion>/application-data/bdtPolicyData/{bdtPolicyId}

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual Applied BDT Policy Data resource

operationId: UpdateIndividualAppliedBdtPolicyData

tags:

- Individual Applied BDT Policy Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:bdt-policy-data:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/BdtPolicyDataPatch'

parameters:

- name: bdtPolicyId

in: path

description: >

The Identifier of an Individual Applied BDT Policy Data to be updated. It shall

apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: >

The update of an Individual Applied BDT Policy Data resource is confirmed and

a response body containing Applied BDT Policy Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicyData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Applied BDT Policy Data resource

operationId: DeleteIndividualAppliedBdtPolicyData

tags:

- Individual Applied BDT Policy Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:bdt-policy-data:modify

parameters:

- name: bdtPolicyId

in: path

description: >

The Identifier of an Individual Applied BDT Policy Data to be deleted.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual Applied BDT Policy Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/iptvConfigData:

get:

summary: Retrieve IPTV configuration Data

operationId: ReadIPTVCongifurationData

tags:

- IPTV Configuration Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:iptv-config-data:read

parameters:

- name: config-ids

in: query

description: Each element identifies a configuration.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: inter-group-ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

responses:

'200':

description: The IPTV configuration data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/IptvConfigData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/iptvConfigData/{configurationId}:

put:

summary: Create or update an individual IPTV configuration resource

operationId: CreateOrReplaceIndividualIPTVConfigurationData

tags:

- Individual IPTV Configuration Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:iptv-config-data:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

parameters:

- name: configurationId

in: path

description: >

The Identifier of an Individual IPTV Configuration Data to be created or updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual IPTV Configuration Data resource is confirmed and a

representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'200':

description: The update of an Individual IPTV configuration resource.

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Partial update an individual IPTV configuration resource

operationId: PartialReplaceIndividualIPTVConfigurationData

tags:

- Individual IPTV Configuration Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:iptv-config-data:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: 'TS29522\_IPTVConfiguration.yaml#/components/schemas/IptvConfigDataPatch'

parameters:

- name: configurationId

in: path

description: >

The Identifier of an Individual IPTV Configuration Data to be updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: The update of an Individual IPTV configuration resource.

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual IPTV configuration resource

operationId: DeleteIndividualIPTVConfigurationData

tags:

- Individual IPTV Configuration Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:iptv-config-data:modify

parameters:

- name: configurationId

in: path

description: >

The Identifier of an Individual IPTV Configuration to be deleted. It shall

apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The resource was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/serviceParamData:

get:

summary: Retrieve Service Parameter Data

operationId: ReadServiceParameterData

tags:

- Service Parameter Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:service-param-data:read

parameters:

- name: service-param-ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: internal-group-ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: ue-ipv4s

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

- name: ue-ipv6s

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

- name: ue-macs

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

- name: any-ue

in: query

description: Indicates whether the request is for any UE.

required: false

schema:

type: boolean

- name: roam-ue-net-descs

in: query

description: >

Each element identifies oner or more PLMNs for a roaming UE.

required: false

schema:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/NetworkDescription'

minItems: 1

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: The Service Parameter Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ServiceParameterData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/serviceParamData/{serviceParamId}:

put:

summary: Create or update an individual Service Parameter Data resource

operationId: CreateOrReplaceServiceParameterData

tags:

- Individual Service Parameter Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:service-param-data:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

parameters:

- name: serviceParamId

in: path

description: >

The Identifier of an Individual Service Parameter Data to be created or updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual Service Parameter Data resource is confirmed

and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

headers:

Location:

description: >

'Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nudr-dr/<apiVersion>/application-data/serviceParamData/{serviceParamId}'

required: true

schema:

type: string

'200':

description: >

The update of an Individual Service Parameter Data resource is confirmed and

a response body containing Service Parameter Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual Service Parameter Data resource

operationId: UpdateIndividualServiceParameterData

tags:

- Individual Service Parameter Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:service-parameter-data:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/ServiceParameterDataPatch'

parameters:

- name: serviceParamId

in: path

description: >

The Identifier of an Individual Service Parameter Data to be updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: >

The update of an Individual Service Parameter Data resource is confirmed

and a response body containing Service Parameter Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Service Parameter Data resource

operationId: DeleteIndividualServiceParameterData

tags:

- Individual Service Parameter Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:service-parameter-data:modify

parameters:

- name: serviceParamId

in: path

description: >

The Identifier of an Individual Service Parameter Data to be deleted.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual Service Parameter Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/am-influence-data:

get:

summary: Retrieve AM Influence Data

operationId: ReadAmInfluenceData

tags:

- AM Influence Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:am-influence-data:read

parameters:

- name: am-influence-ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: dnn-snssai-infos

in: query

description: Each element identifies a combination of (DNN, S-NSSAI).

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29522\_AMInfluence.yaml#/components/schemas/DnnSnssaiInformation'

minItems: 1

- name: internal-group-ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: any-ue

in: query

description: Indicates whether the request is for any UE.

required: false

schema:

type: boolean

- name: supp-feat

in: query

required: false

description: Supported Features

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: The AM Influence Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AmInfluData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/am-influence-data/{amInfluenceId}:

put:

summary: Create or update an individual AM Influence Data resource

operationId: CreateOrReplaceIndividualAmInfluenceData

tags:

- Individual AM Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:am-influence-data:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

parameters:

- name: amInfluenceId

in: path

description: >

The Identifier of an Individual AM Influence Data to be created or updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual AM Influence Data resource is confirmed and

a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

headers:

Location:

description: >

'Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nudr-dr/<apiVersion>/application-data/am-influence-data/{amInfluenceId}'

required: true

schema:

type: string

'200':

description: >

The update of an Individual AM Influence Data resource is confirmed and a response

body containing AM Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual AM Influence Data resource

operationId: UpdateIndividualAmInfluenceData

tags:

- Individual AM Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:am-influence-data:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AmInfluDataPatch'

parameters:

- name: amInfluenceId

in: path

description: >

The Identifier of an Individual AM Influence Data to be updated. It shall

apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: >

The update of an Individual AM Influence Data resource is confirmed and a

response body containing AM Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual AM Influence Data resource

operationId: DeleteIndividualAmInfluenceData

tags:

- Individual AM Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:am-influence-data:modify

parameters:

- name: amInfluenceId

in: path

description: >

The Identifier of an Individual AM Influence Data to be deleted. It shall

apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual AM Influence Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/subs-to-notify:

post:

summary: Create a subscription to receive notification of application data changes

operationId: CreateIndividualApplicationDataSubscription

tags:

- ApplicationDataSubscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:subs-to-notify:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

responses:

'201':

description: >

Upon success, a response body containing a representation of each

Individual subscription resource shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

applicationDataChangeNotif:

'{$request.body#/notificationUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ApplicationDataChangeNotif'

minItems: 1

responses:

'204':

description: No Content, Notification was successful

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Read Application Data change Subscriptions

operationId: ReadApplicationDataChangeSubscriptions

tags:

- ApplicationDataSubscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:subs-to-notify:read

parameters:

- name: data-filter

in: query

description: The data filter for the query.

required: false

content:

application/json:

schema:

$ref: '#/components/schemas/DataFilter'

responses:

'200':

description: >

The subscription information as request in the request URI query parameter(s)

are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ApplicationDataSubs'

minItems: 0

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/af-qos-data-sets:

get:

summary: Retrieve one or several existing Individual AF Requested QoS Data Set resource(s).

operationId: ReadAFReqQoSDataSets

tags:

- AF Requested QoS Data Sets (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:af-qos-data-sets:read

parameters:

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a network slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: int-group-ids

in: query

description: Each element identifies a group of subscriber(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies a subscriber.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: data-set-ids

in: query

description: Each element identifies an Individual AF requested QoS Set resource.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: supp-feat

in: query

required: false

description: Supported Features

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: >

The requested "Individual AF requested QoS Data Set resource(s) stored in the UDR are

returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AfRequestedQosData'

minItems: 0

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/af-qos-data-sets/{afReqQosId}:

parameters:

- name: afReqQosId

in: path

description: >

Represents the identifier of an Individual AF Requested QoS Data Set.

required: true

schema:

type: string

put:

summary: Create or update an Individual AF Requested QoS Data Set resource.

operationId: CreateOrUpdateIndAFReqQoSDataSet

tags:

- Individual AF Requested QoS Data Set (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:af-qos-data-sets:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AfRequestedQosData'

responses:

'201':

description: >

Created. The Individual AF Requested QoS Data Set resource is successfully created and a

representation of the created resource shall be returned in the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/AfRequestedQosData'

headers:

Location:

description: >

Contains the URI of the newly created resource.

required: true

schema:

type: string

'200':

description: >

OK. The Individual AF Requested QoS Data Set resource is successfully updated and a

representation of the updated resource shall be returned in the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/AfRequestedQosData'

'204':

description: >

No Content. The Individual AF Requested QoS Data Set resource is successfully updated

and no content is returned in the response body.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify of an existing Individual AF Requested QoS Data Set" resource

operationId: ModifyIndAFReqQoSDataSet

tags:

- Individual AF requested QoS Data Set (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:af-qos-data-sets:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AfRequestedQosDataPatch'

responses:

'200':

description: >

OK. The Individual AF Requested QoS Data Set resource is successfully modified and a

representation of the updated resource shall be returned in the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/AfRequestedQosData'

'204':

description: >

No Content. The Individual AF Requested QoS Data Set resource is successfully modified

and no content is returned in the response body.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an existing Individual AF requested QoS Data Set resource

operationId: DeleteIndAFReqQosDataSet

tags:

- Individual AF requested QoS Data Set (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:af-qos-data-sets:modify

responses:

'204':

description: >

No Content. The Individual AF requested QoS Data Set is successfully deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/subs-to-notify/{subsId}:

parameters:

- name: subsId

in: path

required: true

schema:

type: string

put:

summary: Modify a subscription to receive notification of application data changes

operationId: ReplaceIndividualApplicationDataSubscription

tags:

- IndividualApplicationDataSubscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:subs-to-notify:modify

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

responses:

'200':

description: The individual subscription resource was updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

'204':

description: >

The individual subscription resource was updated successfully and no

additional content is to be sent in the response message.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete the individual Application Data subscription

operationId: DeleteIndividualApplicationDataSubscription

tags:

- IndividualApplicationDataSubscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:subs-to-notify:modify

responses:

'204':

description: Upon success, an empty response body shall be returned.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Get an existing individual Application Data Subscription resource

operationId: ReadIndividualApplicationDataSubscription

tags:

- IndividualApplicationDataSubscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:subs-to-notify:read

parameters:

- name: subsId

in: path

description: >

String identifying a subscription to the Individual Application Data Subscription

required: true

schema:

type: string

responses:

'200':

description: The subscription information is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/eas-deploy-data:

get:

summary: Retrieve EAS Deployment Information Data

operationId: ReadEasDeployData

tags:

- EAS Deployment Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:eas-deploy-data:read

parameters:

- name: dnn

in: query

description: Identifies a DNN.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

- name: snssai

in: query

description: Identifies an S-NSSAI.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

- name: internal-group-id

in: query

description: Identifies a group of users.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

- name: appId

in: query

description: Identifies an application.

required: false

schema:

type: string

responses:

'200':

description: The EAS Deployment Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: 'TS29591\_Nnef\_EASDeployment.yaml#/components/schemas/EasDeployInfoData'

minItems: 1

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/eas-deploy-data/{easDeployInfoId}:

get:

summary: Retrieve an individual EAS Deployment Data resource

operationId: ReadIndividualEasDeployData

tags:

- Individual EAS Deployment Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:eas-deploy-data:read

parameters:

- name: easDeployInfoId

description: >

String identifying an Individual EAS Deployment Information Data resource.

in: path

required: true

schema:

type: string

responses:

'200':

description: >

The EAS Deployment Data stored in the UDR for an Individual EAS Deployment

Information Data resource is returned.

content:

application/json:

schema:

$ref: 'TS29591\_Nnef\_EASDeployment.yaml#/components/schemas/EasDeployInfoData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create or update an individual EAS Deployment Data resource

operationId: CreateOrReplaceIndividualEasDeployData

tags:

- Individual EAS Deployment Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:eas-deploy-data:create

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29591\_Nnef\_EASDeployment.yaml#/components/schemas/EasDeployInfoData'

parameters:

- name: easDeployInfoId

in: path

description: >

The Identifier of an Individual EAS Deployment Data to be created or updated.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual EAS Deployment Data resource is confirmed and a

representation of that resource is returned.

content:

application/json:

schema:

$ref: 'TS29591\_Nnef\_EASDeployment.yaml#/components/schemas/EasDeployInfoData'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nudr-dr/<apiVersion>/application-data/eas-deploy-data/{easDeployInfoId}

required: true

schema:

type: string

'200':

description: >

The update of an Individual EAS Deployment Data resource is confirmed and a response

body containing EAS Deployment Data shall be returned.

content:

application/json:

schema:

$ref: 'TS29591\_Nnef\_EASDeployment.yaml#/components/schemas/EasDeployInfoData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual EAS Deployment Data resource

operationId: DeleteIndividualEasDeployData

tags:

- Individual EasDeployment Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:eas-deploy-data:modify

parameters:

- name: easDeployInfoId

in: path

description: >

The Identifier of an Individual EAS Deployment Data to be deleted.

It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual EAS Deployment Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/dnai-eas-mappings/{dnai}:

parameters:

- name: dnai

in: path

required: true

schema:

type: string

get:

summary: Retrieves the EAS address information for a DNAI.

operationId: ReadDnaiEasMapping

tags:

- DnaiEasMapping (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:dnai-eas:read

parameters:

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: >

Upon success, a response body containing EAS address information for a DNAI

is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/DnaiEasMapping'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/ecs-address-roaming:

get:

summary: Retrieve ECS Address Roaming Data

operationId: ReadEcsRoamingData

tags:

- ECS Address Roaming Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ecs-address-roaming:read

parameters:

- name: internal-group-id

in: query

description: Identifies a group of users.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

- name: any-ue

in: query

description: >

Indicates that any UE is targetted if included and set to true, otherwise set to false.

Default value is false if omitted.

required: false

schema:

type: boolean

responses:

'200':

description: The ECS Address Roaming Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/EcsAddrData'

minItems: 1

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/ecs-address-roaming/{ecsAddrInfoId}:

get:

summary: Retrieve an individual ECS Address Roaming Data resource

operationId: ReadIndividualEcsAddr

tags:

- Individual ECS Address Roaming Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ecs-address-roaming:read

parameters:

- name: ecsAddrInfoId

description: >

String identifying an Individual ECS Address Roaming Data resource.

in: path

required: true

schema:

type: string

responses:

'200':

description: >

The ECS Address Roaming Data stored in the UDR for an Individual ECS Address Roaming

Data resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/EcsAddrData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create or update an individual ECS Address Roaming Data resource

operationId: CreateOrReplaceIndividualEcsAddressData

tags:

- Individual ECS Address Roaming Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ecs-address-roaming:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EcsAddrData'

parameters:

- name: ecsAddrInfoId

in: path

description: >

The Identifier of an Individual ECS Address Roaming Data to be created or updated.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual EECS Address Roaming Data resource is confirmed

and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/EcsAddrData'

headers:

Location:

description: >

Contains the URI of the newly created resource.

required: true

schema:

type: string

'200':

description: >

The update of an Individual ECS Address Roaming Data resource is confirmed

and a response body containing ECS Address Roaming Data is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/EcsAddrData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual ECS Address Roaming Data resource

operationId: DeleteIndividualEcsAddrData

tags:

- Individual ECS Address Roaming Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ecs-address-roaming:modify

parameters:

- name: ecsAddrInfoId

in: path

description: >

The Identifier of an Individual ECS Address Roaming Data to be updated.

required: true

schema:

type: string

responses:

'204':

description: The Individual ECS Address Roaming Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/ueid-mappings:

get:

summary: Retrieve one or several UE ID Mapping(s)

operationId: GetUeIdMappings

tags:

- UE ID Mapping(s) (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ueid-mappings:read

parameters:

- name: app-layer-ids

in: query

description: Contains the requested Application layer Id(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationlayerId'

minItems: 1

- name: gpsis

in: query

description: Contains the requested ID Mapping is returned.

content:

application/json:

schema:

type: array

items:

$ref: 'TS29522\_UEId.yaml#/components/schemas/UeIdMappingInfo'

minItems: 1

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/ueid-mappings/{ueMappingId}:

parameters:

- name: mappingId

description: >

Contains the identifier of the Individual UE ID Mapping resource.

in: path

required: true

schema:

type: string

get:

summary: Retrieve an individual UE ID Mapping resource

operationId: GetIndividualUeIdMapping

tags:

- Individual UE ID Mapping (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ueid-mappings:read

responses:

'200':

description: >

The UE ID Mapping Data stored in the UDR for an Individual UE Mapping Id

Data resource is returned.

content:

application/json:

schema:

$ref: 'TS29522\_UEId.yaml#/components/schemas/UeIdMappingInfo'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create or update an individual UE ID Mapping resource

operationId: CreateOrReplaceIndividualUeIdMapping

tags:

- Individual UE ID Mapping (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ueid-mappings:create

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29522\_UEId.yaml#/components/schemas/UeIdMappingInfo'

parameters:

- name: ueMappingId

in: path

description: >

The Identifier of an Individual UE ID Mapping Data to be created or

updated.

required: true

schema:

type: string

responses:

'201':

description: >

The creation of an Individual UE ID Mapping Data resource is confirmed

and a representation of that resource is returned.

content:

application/json:

schema:

$ref: 'TS29522\_UEId.yaml#/components/schemas/UeIdMappingInfo'

headers:

Location:

description: >

Contains the URI of the newly created resource.

required: true

schema:

type: string

'200':

description: >

The update of an Individual UE ID Mapping resource is confirmed

and a response body containing UE ID Mapping is returned.

content:

application/json:

schema:

$ref: 'TS29522\_UEId.yaml#/components/schemas/UeIdMappingInfo'

'204':

description: No content. The creation of an Individual UE ID Mapping Data

resource is confirmed

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual UE ID Mapping resource

operationId: DeleteIndividualUeIdMappingData

tags:

- Individual UE ID Mapping Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

- nudr-dr:application-data:ueid-mappings:modify

parameters:

- name: ueMappingId

in: path

description: >

The Identifier of an Individual UE ID Mapping to be deleted.

required: true

schema:

type: string

responses:

'204':

description: The Individual UE ID Mapping Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

schemas:

TrafficInfluData:

description: Represents the Traffic Influence Data.

type: object

properties:

upPathChgNotifCorreId:

type: string

description: >

Contains the Notification Correlation Id allocated by the NEF for the UP

path change notification.

appReloInd:

type: boolean

description: >

Identifies whether an application can be relocated once a location of the

application has been selected.

afAppId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

ethTrafficFilters:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: >

Identifies Ethernet packet filters. Either "trafficFilters" or

"ethTrafficFilters" shall be included if applicable.

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

interGroupIdList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 2

description: >

Identifies a list of Internal Groups.

subscriberCatList:

type: array

items:

type: string

minItems: 1

description: >

Identifies a list of Subscriber Category(s).

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

trafficFilters:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: >

Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters"

shall be included if applicable.

trafficRoutes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

description: Identifies the N6 traffic routing requirement.

sfcIdDl:

type: string

description: Reference to a pre-configured service function chain for DL traffic

sfcIdUl:

type: string

description: Reference to a pre-configured service function chain for UL traffic

metadata:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Metadata'

traffCorreInd:

type: boolean

tfcCorreInfo:

$ref: '#/components/schemas/TrafficCorrelationInfo'

validStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

validEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

tempValidities:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

minItems: 1

description: Identifies the temporal validities for the N6 traffic routing requirement.

nwAreaInfo:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

upPathChgNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

headers:

description: Contains the headers provisioned by the NEF.

type: array

items:

type: string

minItems: 1

subscribedEvents:

type: array

items:

$ref: 'TS29522\_TrafficInfluence.yaml#/components/schemas/SubscribedEvent'

minItems: 1

dnaiChgType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

afAckInd:

type: boolean

addrPreserInd:

type: boolean

maxAllowedUpLat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

simConnInd:

type: boolean

description: >

Indicates whether simultaneous connectivity should be temporarily

maintained for the source and target PSA.

simConnTerm:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

resetIds:

type: array

items:

type: string

minItems: 1

nscSuppFeats:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

minProperties: 1

description: >

Identifies a list of Network Function Service Consumer supported per service. The key

used in this map for each entry is the ServiceName value as defined in

3GPP TS 29.510[24].

allOf:

- oneOf:

- required: [afAppId]

- required: [trafficFilters]

- required: [ethTrafficFilters]

- oneOf:

- required: [supi]

- required: [interGroupId]

- required: [interGroupIdList]

TrafficInfluDataPatch:

description: Represents the Traffic Influence Data to be updated in the UDR.

type: object

properties:

upPathChgNotifCorreId:

type: string

description: >

Contains the Notification Correlation Id allocated by the NEF for the

UP path change notification.

appReloInd:

type: boolean

description: >

Identifies whether an application can be relocated once a location of the application

has been selected.

ethTrafficFilters:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: >

Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters"

shall be included if applicable.

trafficFilters:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: >

Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters"

shall be included if applicable.

trafficRoutes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

description: Identifies the N6 traffic routing requirement.

sfcIdDl:

type: string

description: Reference to a pre-configured service function chain for DL traffic

nullable: true

sfcIdUl:

type: string

description: Reference to a pre-configured service function chain for UL traffic

nullable: true

metadata:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Metadata'

traffCorreInd:

type: boolean

tfcCorreInfo:

$ref: '#/components/schemas/TrafficCorrelationInfo'

validStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

validEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

tempValidities:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

minItems: 1

nullable: true

description: Identifies the temporal validities for the N6 traffic routing requirement.

nwAreaInfo:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

upPathChgNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

headers:

description: Contains the headers provisioned by the NEF.

type: array

items:

type: string

minItems: 1

afAckInd:

type: boolean

addrPreserInd:

type: boolean

maxAllowedUpLat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

simConnInd:

type: boolean

description: >

Indicates whether simultaneous connectivity should be temporarily maintained

for the source and target PSA.

simConnTerm:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

TrafficInfluSub:

description: Represents traffic influence subscription data.

type: object

properties:

dnns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

description: Each element identifies a DNN.

snssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

description: Each element identifies a slice.

internalGroupIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

description: Each element identifies a group of users.

internalGroupIdsAdd:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

description: >

Each element identifies an internal group.

subscriberCatList:

type: array

items:

type: string

minItems: 1

description: >

Each element identifies a subscriber category.

supis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

description: Each element identifies the user.

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

immRep:

type: boolean

description: >

If provided and set to true, it indicates that existing entries that

match this subscription shall be immediately reported in the response.

immReports:

type: array

items:

$ref: '#/components/schemas/TrafficInfluDataNotif'

minItems: 1

description: Immediate report with existing UDR entries.

required:

- notificationUri

oneOf:

- required: [dnns]

- required: [snssais]

- required: [internalGroupIds]

- required: [internalGroupIdsAdd]

- required: [supis]

TrafficInfluDataNotif:

description: Represents traffic influence data for notification.

type: object

properties:

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

trafficInfluData:

$ref: '#/components/schemas/TrafficInfluData'

required:

- resUri

PfdDataForAppExt:

description: Represents the PFDs and related data for the application.

type: object

properties:

applicationId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

pfds:

type: array

items:

$ref: 'TS29551\_Nnef\_PFDmanagement.yaml#/components/schemas/PfdContent'

minItems: 1

cachingTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

cachingTimer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

allowedDelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- applicationId

- pfds

not:

required: [cachingTime,cachingTimer]

BdtPolicyData:

description: Represents applied BDT policy data.

type: object

properties:

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

resetIds:

type: array

items:

type: string

minItems: 1

required:

- bdtRefId

BdtPolicyDataPatch:

description: >

Represents modification instructions to be performed on the applied BDT policy data.

type: object

properties:

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

required:

- bdtRefId

IptvConfigData:

description: Represents IPTV configuration data information.

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

interGroupId:

description: Identifies a group of users.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

afAppId:

type: string

multiAccCtrls:

type: object

additionalProperties:

$ref: 'TS29522\_IPTVConfiguration.yaml#/components/schemas/MulticastAccessControl'

minProperties: 1

description: >

Identifies a list of multicast address access control information. Any string

value can be used as a key of the map.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

resetIds:

type: array

items:

type: string

minItems: 1

required:

- afAppId

- multiAccCtrls

oneOf:

- required: [interGroupId]

- required: [supi]

ServiceParameterData:

description: Represents the service parameter data.

type: object

properties:

appId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

ueIpv4:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

anyUeInd:

type: boolean

description: >

Identifies whether the service parameters applies to any non roaming UE.

roamUeNetDescs:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/NetworkDescription'

minItems: 1

description: Each element identifies one or more PLMN IDs of inbound roamers.

paramOverPc5:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverPc5'

paramOverUu:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverUu'

a2xParamsPc5:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/A2xParamsPc5'

paramForProSeDd:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDd'

paramForProSeDc:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDc'

paramForProSeU2NRelUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeU2NRelUe'

paramForProSeRemUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeRemUe'

paramForProSeU2URelUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeU2URelUe'

paramForProSeEndUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeEndUe'

urspGuidance:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/UrspRuleRequest'

minItems: 1

description: >

Contains the service parameter used to guide the URSP and/or VPLMN specific URSP.

tnaps:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TnapId'

minItems: 1

description: Contains the TNAP IDs collocated with the 5G-RG(s) of a specific user.

deliveryEvents:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/Event'

minItems: 1

description: Contains the outcome of the UE Policy Delivery.

policDelivNotifCorreId:

type: string

description: >

Contains the Notification Correlation Id allocated by the NEF for the notification

of UE Policy delivery outcome.

policDelivNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

headers:

description: Contains the headers provisioned by the NEF.

type: array

items:

type: string

minItems: 1

resetIds:

type: array

items:

type: string

minItems: 1

paramForRangingSlPos:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForRangingSlPos'

ServiceParameterDataPatch:

description: Represents the service parameter data that can be updated.

type: object

properties:

paramOverPc5:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverPc5Rm'

paramOverUu:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverUuRm'

a2xParamsPc5:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/A2xParamsPc5Rm'

paramForProSeDd:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDdRm'

paramForProSeDc:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDcRm'

paramForProSeU2NRelUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeU2NRelUeRm'

paramForProSeRemUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeRemUeRm'

paramForProSeU2URelUE:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeU2URelUeRm'

paramForProSeEndUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeEndUeRm'

urspInfluence:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/UrspRuleRequest'

minItems: 1

deprecated: true

description: Contains the service parameter used to influence the URSP. This attribute is

deprecated by the urspGuidance attribute.

urspGuidance:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/UrspRuleRequest'

minItems: 1

nullable: true

description: >

Contains the service parameter used to influence the URSP and/or VPLMN specific URSP.

tnaps:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TnapId'

minItems: 1

description: Contains the TNAP IDs collocated with the 5G-RG(s) of a specific user.

nullable: true

deliveryEvents:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/Event'

minItems: 1

nullable: true

description: Contains the outcome of the UE Policy Delivery.

policDelivNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

headers:

description: Contains the headers provisioned by the NEF.

type: array

items:

type: string

minItems: 1

paramForRangingSlPos:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForRangingSlPosRm'

AmInfluData:

description: Represents the AM Influence Data.

type: object

properties:

appIds:

type: array

items:

type: string

minItems: 1

description: Identifies one or more applications.

dnnSnssaiInfos:

type: array

items:

$ref: 'TS29522\_AMInfluence.yaml#/components/schemas/DnnSnssaiInformation'

minItems: 1

description: Identifies one or more DNN, S-NSSAI combinations.

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

anyUeInd:

type: boolean

description: >

When set to true, it indicates whether the data is applicable for any UE. Otherwise set

to "false". Default value is "false" if omitted.

roamUePlmnIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

minItems: 1

description: >

Indicates a list of PLMNs representing the home PLMN for the inbound roaming

UEs in LBO roaming scenario.

policyDuration:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

evSubs:

type: array

items:

$ref: 'TS29522\_AMInfluence.yaml#/components/schemas/AmInfluEvent'

minItems: 1

description: List of AM related events for which a subscription is required.

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifCorrId:

type: string

description: Notification correlation identifier.

headers:

type: array

description: Contains the headers provisioned by the NEF.

items:

type: string

minItems: 1

thruReq:

type: boolean

description: >

When set to true, it indicates whether high throughput is desired for the

indicated UE traffic. Otherwise set to "false". Default value is "false" if omitted.

covReq:

type: array

items:

$ref: 'TS29534\_Npcf\_AMPolicyAuthorization.yaml#/components/schemas/ServiceAreaCoverageInfo'

minItems: 1

description: Indicates the service area coverage requirement.

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

resetIds:

type: array

items:

type: string

minItems: 1

allOf:

- anyOf:

- required: [thruReq]

- required: [covReq]

- oneOf:

- required: [supi]

- required: [interGroupId]

- required: [anyUeInd]

- required: [roamUePlmnIds]

AmInfluDataPatch:

description: Represents the AM Influence Data that can be updated.

type: object

properties:

appIds:

type: array

items:

type: string

minItems: 1

description: Identifies one or more applications.

nullable: true

dnnSnssaiInfos:

type: array

items:

$ref: 'TS29522\_AMInfluence.yaml#/components/schemas/DnnSnssaiInformation'

minItems: 1

description: Identifies one or more DNN, S-NSSAI combinations.

nullable: true

evSubs:

type: array

items:

$ref: 'TS29522\_AMInfluence.yaml#/components/schemas/AmInfluEvent'

minItems: 1

description: List of AM related events for which a subscription is required.

nullable: true

headers:

type: array

description: Contains the headers provisioned by the NEF.

items:

type: string

minItems: 1

thruReq:

type: boolean

description: Indicates whether high throughput is desired for the indicated UE traffic.

nullable: true

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UriRm'

notifCorrId:

type: string

description: Notification correlation identifier.

nullable: true

covReq:

type: array

items:

$ref: 'TS29534\_Npcf\_AMPolicyAuthorization.yaml#/components/schemas/ServiceAreaCoverageInfo'

minItems: 1

description: Indicates the service area coverage requirement.

nullable: true

ApplicationDataSubs:

description: Identifies a subscription to application data change notification.

type: object

properties:

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

dataFilters:

type: array

items:

$ref: '#/components/schemas/DataFilter'

minItems: 1

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

immRep:

type: boolean

description: Immediate reporting indication.

amInfluEntries:

type: array

items:

$ref: '#/components/schemas/AmInfluData'

minItems: 1

description: The AM Influence Data entries stored in the UDR that match a subscription.

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

immReports:

type: array

items:

$ref: '#/components/schemas/ApplicationDataChangeNotif'

minItems: 1

description: Immediate report with existing UDR entries.

required:

- notificationUri

ApplicationDataChangeNotif:

description: Contains changed application data for which notification was requested.

type: object

properties:

iptvConfigData:

$ref: '#/components/schemas/IptvConfigData'

pfdData:

$ref: 'TS29551\_Nnef\_PFDmanagement.yaml#/components/schemas/PfdChangeNotification'

bdtPolicyData:

$ref: '#/components/schemas/BdtPolicyData'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

serParamData:

$ref: '#/components/schemas/ServiceParameterData'

amInfluData:

$ref: '#/components/schemas/AmInfluData'

dnaiEasData:

$ref: '#/components/schemas/DnaiEasMapping'

afReqQosData:

$ref: '#/components/schemas/AfRequestedQosData'

ecsAddrData:

$ref: '#/components/schemas/EcsAddrData'

required:

- resUri

DataFilter:

description: Identifies a data filter.

type: object

properties:

dataInd:

$ref: '#/components/schemas/DataInd'

dnns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

snssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

internalGroupIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

supis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

appIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

minItems: 1

ueIpv4s:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

ueIpv6s:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

ueMacs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

anyUeInd:

type: boolean

description: Indicates the request is for any UE.

dnnSnssaiInfos:

description: >

Indicates the request is for any DNN and S-NSSAI combination present in the array.

type: array

items:

$ref: 'TS29522\_AMInfluence.yaml#/components/schemas/DnnSnssaiInformation'

minItems: 1

dnais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

minItems: 1

required:

- dataInd

TrafficCorrelationInfo:

description: >

Contains the information for traffic correlation.

type: object

properties:

corrType:

$ref: '#/components/schemas/CorrelationType'

tfcCorrId:

type: string

description: >

Identification of a set of UEs accessing the application identified by the

Application Identifier or traffic filtering information.

comEasIpv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4AddrRm'

comEasIpv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6AddrRm'

fqdnRange:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/FqdnPatternMatchingRule'

minItems: 1

nullable: true

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UriRm'

notifCorrId:

type: string

nullable: true

description: Notification correlation identifier.

nullable: true

AfRequestedQosData:

description: Represents AF Requested QoS data.

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

afAppId:

type: string

description: Identifies an AF application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

sliceInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

evSubsc:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EventsSubscReqData'

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

enEthFlowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

minItems: 1

qosReference:

type: string

qosReqs:

$ref: '#/components/schemas/QosRequirements'

altSerReqs:

type: array

items:

type: string

minItems: 1

altSerReqsData:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Contains alternative service requirements that include individual QoS parameter sets.

disUeNotif:

type: boolean

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

tempInValidity:

$ref: 'TS29565\_Ntsctsf\_QoSandTSCAssistance.yaml#/components/schemas/TemporalInValidity'

headers:

description: Contains the headers provisioned by the NEF.

type: array

items:

type: string

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

allOf:

- oneOf:

- required: [supi]

- required: [interGroupId]

- oneOf:

- required: [flowInfo]

- required: [ethFlowInfo]

- required: [enEthFlowInfo]

- oneOf:

- required: [qosReference]

- required: [qosReqs]

- not:

required: [qosReference, altQosReqs]

- not:

required: [altQosReqs, altQoSReferences]

AfRequestedQosDataPatch:

description: Represents modification of Individual AF Requested QoS data.

type: object

properties:

afAppId:

type: string

description: Identifies an AF application.

nullable: true

evSubsc:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EventsSubscReqDataRm'

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

nullable: true

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

enEthFlowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

minItems: 1

qosReference:

type: string

nullable: true

qosReqs:

$ref: '#/components/schemas/QosRequirementsRm'

altSerReqs:

type: array

items:

type: string

minItems: 1

nullable: true

altSerReqsData:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Contains removable alternative service requirements that include individual QoS

parameter sets.

nullable: true

disUeNotif:

type: boolean

nullable: true

tempInValidity:

$ref: 'TS29565\_Ntsctsf\_QoSandTSCAssistance.yaml#/components/schemas/TemporalInValidity'

headers:

description: Contains the headers provisioned by the NEF.

type: array

items:

type: string

minItems: 1

DnaiEasMapping:

description: Contains DNAI to EAS mapping information.

type: object

properties:

dnaiEasInfos:

type: array

items:

$ref: '#/components/schemas/DnaiEasInfo'

minItems: 1

description: Each element conrtains EAS address information for a DNAI.

required:

- dnaiEasInfos

DnaiEasInfo:

description: Contains EAS information for a DNAI.

type: object

properties:

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

dnais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

minItems: 1

description: DNAI(s) for the EAS Deployment Information.

easIpAddrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

description: >

Each element contains EAS IP address(es), IP address ranges, and/or IPv6 prefixes.

fqdns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/FqdnPatternMatchingRule'

minItems: 1

description: Each element contains FQDN for the EAS(s) of a DNAI.

required:

- dnais

anyOf:

- required: [dnn]

- required: [snssai]

oneOf:

- required: [easIpAddrs]

- required: [fqdns]

EcsAddrData:

description: Represents ECS Address Data.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

ecsServerAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/EcsServerAddr'

spatialValidityCond:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SpatialValidityCond'

anyUeInd:

type: boolean

description: >

If provided and set to true it indicates that all the UEs are targetted,

otherwise set to false. The default value is false if omitted.

internalGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- ecsServerAddr

QosRequirements:

description: Represents QoS requirements.

type: object

properties:

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

tsnQos:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TsnQosContainer'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

capBatAdaptation:

type: boolean

description: >

Indicates the capability for AF to adjust the burst sending time, when it is supported

and set to "true". The default value is "false" if omitted.

QosRequirementsRm:

description: Represents QoS requirements.

nullable: true

type: object

properties:

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

tsnQos:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TsnQosContainer'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

capBatAdaptation:

type: boolean

description: >

Indicates the capability for AF to adjust the burst sending time, when it is supported

and set to "true". The default value is "false" if omitted.

DataInd:

anyOf:

- type: string

enum:

- PFD

- IPTV

- BDT

- SVC\_PARAM

- AM

- DNAI\_EAS

- REQ\_QOS

- ECS

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Indicates the type of data.

Possible values are

- PFD: PFD data.

- IPTV: IPTV configuration data.

- BDT: BDT data.

- SVC\_PARAM: Service parameter data.

- AM: AM influence data.

- DNAI\_EAS: DNAI EAS mapping data.

- REQ\_QOS: AF Requested QoS data for a UE or group of UE(s) not identified by UE address(es).

- ECS: ECS Address data.

CorrelationType:

description: Indicates that a common DNAI or common EAS should be selected.

anyOf:

- type: string

enum:

- COMMON\_DNAI

- COMMON\_EAS

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

\*\*\* End of Changes \*\*\*