**3GPP TSG- Meeting #****R1-2405629**

**, ,**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **0578** | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on configuration of TCI states for SRS |
|  |  |
| ***Source to WG:*** | Moderator (MediaTek. Inc), CATT, Samsung |
| ***Source to TSG:*** | --- |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | 1. In TS38.214, it is specified that when two SRS resource sets with higher layer parameter usage in SRS-ResourceSet set to 'codebook' or 'nonCodebook' are configured, the UE does not expect that the first indicated TCI-State or TCI-UL-State is applied to the second SRS resource set and that the second indicated TCI-State or TCI-UL-State is applied to the first SRS resource set. However, it should be clarified that the number of SRS resource sets should be counted within srs-ResourceSetToAddModList or srs-ResourceSetToAddModListDCI-0-2, instead of both lists.
2. The blank space between 'except' and 'that' is missing
 |
|  |  |
| ***Summary of change:*** | 1. Correct the error on the condition for the restriction on the configuration of TCI states for SRS.
2. Change 'exceptthat' to 'except that'.
 |
|  |  |
| ***Consequences if not approved:*** | 1. The condition for the restriction on the configuration of TCI states for SRS is not correct.
2. There is an editorial error in the spec.
 |
|  |  |
| ***Clauses affected:*** | 6.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **N** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **N** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **N** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

6.2.1 UE sounding procedure

-------------------------------------------Unchanged parts are omitted-------------------------------------------

- When two SRS resource sets are configured in *srs-ResourceSetToAddModList* or *srs-ResourceSetToAddModListDCI-0-2* with higher layer parameter *usage* in *SRS-ResourceSet* set to 'codebook' or 'nonCodebook', the UE does not expect that the first indicated *TCI-State* or *TCI-UL-State* is applied to the second SRS resource set and that the second indicated *TCI-State* or *TCI-UL-State* is applied to the first SRS resource set.

-------------------------------------------Unchanged parts are omitted-------------------------------------------