**3GPP TSG- Meeting # *revision of***

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In Rel-16, band n14 was introduced with the following Note 6 introduced in Table 6.2.1-1 (UE Power Class):*NOTE 6: Generally, PC1 UE for Band n14 is not targeted for smartphone form factor. The UE power class 1 requirements for Band n14 are applicable for public safety scenario only.*As Note 6 in Table 6.2.1-1 has been reused for other bands in Rel-18, in this CR we provide corrections to the Note 6 wording to make it band-agnostic, while Band14-specific Note is introduced as a separate entry, i.e. Note 7. Furthermore, notes are aligned to be kept in single column, as in some case they were spread among columns causing confusion, e.g. n96..  |
|  |  |
| ***Summary of change:*** | 1. Note 6 wording is updated to make it band-agnostic, while Band14-specific Note is introduced as a separate entry, i.e. Note 7.

3GPP drafting rules are implemented for the notes in Table 6.2.1-1.  |
|  |  |
| ***Consequences if not approved:*** | Ambiguity of Note 6 in Table 6.2.1-1 and its n14 content being reused for other bands would remain. 3GPP drafting rules would not be followed. |
|  |  |
| ***Clauses affected:*** | 5.2, 6.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*------------------------------ Modified section ------------------------------*

## 5.2 Operating bands

NR is designed to operate in the FR1 operating bands defined in Table 5.2-1.

Table 5.2-1: NR operating bands in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR operating band | Uplink (UL) *operating band*BS receive / UE transmitFUL\_low  – FUL\_high | Downlink (DL) *operating band*BS transmit / UE receiveFDL\_low – FDL\_high | Duplex Mode |
| n1 | 1920 MHz – 1980 MHz | 2110 MHz – 2170 MHz | FDD |
| n2 | 1850 MHz – 1910 MHz | 1930 MHz – 1990 MHz | FDD |
| n3 | 1710 MHz – 1785 MHz | 1805 MHz – 1880 MHz | FDD |
| n5 | 824 MHz – 849 MHz | 869 MHz – 894 MHz | FDD |
| n7 | 2500 MHz – 2570 MHz | 2620 MHz – 2690 MHz | FDD |
| n8 | 880 MHz – 915 MHz | 925 MHz – 960 MHz | FDD |
| n12 | 699 MHz – 716 MHz | 729 MHz – 746 MHz | FDD |
| n14 | 788 MHz – 798 MHz | 758 MHz – 768 MHz | FDD |
| n18 | 815 MHz – 830 MHz | 860 MHz – 875 MHz | FDD |
| n20 | 832 MHz – 862 MHz | 791 MHz – 821 MHz | FDD |
| n25 | 1850 MHz – 1915 MHz | 1930 MHz – 1995 MHz | FDD |
| n26 | 814 MHz – 849 MHz | 859 MHz – 894 MHz | FDD |
| n28 | 703 MHz – 748 MHz | 758 MHz – 803 MHz | FDD |
| n2915 | N/A | 717 MHz – 728 MHz | SDL |
| n303 | 2305 MHz – 2315 MHz | 2350 MHz – 2360 MHz | FDD |
| n34 | 2010 MHz – 2025 MHz | 2010 MHz – 2025 MHz | TDD |
| n3810 | 2570 MHz – 2620 MHz | 2570 MHz – 2620 MHz | TDD |
| n39 | 1880 MHz – 1920 MHz | 1880 MHz – 1920 MHz | TDD |
| n40 | 2300 MHz – 2400 MHz | 2300 MHz – 2400 MHz | TDD |
| n41 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n4613,14 | 5150 MHz – 5925 MHz | 5150 MHz – 5925 MHz | TDD |
| n4711 | 5855 MHz – 5925 MHz | 5855 MHz – 5925 MHz | TDD |
| n48 | 3550 MHz – 3700 MHz | 3550 MHz – 3700 MHz | TDD |
| n501 | 1432 MHz – 1517 MHz | 1432 MHz – 1517 MHz | TDD |
| n51 | 1427 MHz – 1432 MHz | 1427 MHz – 1432 MHz | TDD |
| n53 | 2483.5 MHz – 2495 MHz | 2483.5 MHz – 2495 MHz | TDD |
| n654 | 1920 MHz – 2010 MHz | 2110 MHz – 2200 MHz | FDD |
| n66 | 1710 MHz – 1780 MHz | 2110 MHz – 2200 MHz | FDD |
| n70 | 1695 MHz – 1710 MHz | 1995 MHz – 2020 MHz | FDD |
| n71 | 663 MHz – 698 MHz | 617 MHz – 652 MHz | FDD |
| n74 | 1427 MHz – 1470 MHz | 1475 MHz – 1518 MHz | FDD |
| n7515 | N/A | 1432 MHz – 1517 MHz | SDL |
| n7615 | N/A | 1427 MHz – 1432 MHz | SDL |
| n7712 | 3300 MHz – 4200 MHz | 3300 MHz – 4200 MHz | TDD |
| n78 | 3300 MHz – 3800 MHz | 3300 MHz – 3800 MHz | TDD |
| n79 | 4400 MHz – 5000 MHz | 4400 MHz – 5000 MHz | TDD |
| n80 | 1710 MHz – 1785 MHz | N/A | SUL  |
| n81 | 880 MHz – 915 MHz | N/A | SUL  |
| n82 | 832 MHz – 862 MHz | N/A | SUL  |
| n83 | 703 MHz – 748 MHz | N/A | SUL |
| n84 | 1920 MHz – 1980 MHz | N/A | SUL |
| n86 | 1710 MHz – 1780 MHz | N/A | SUL |
| n89 | 824 MHz – 849 MHz | N/A | SUL |
| n905 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n919 | 832 MHz – 862 MHz | 1427 MHz – 1432 MHz | FDD |
| n929 | 832 MHz – 862 MHz | 1432 MHz – 1517 MHz | FDD |
| n939 | 880 MHz – 915 MHz | 1427 MHz – 1432 MHz | FDD |
| n949 | 880 MHz – 915 MHz | 1432 MHz – 1517 MHz | FDD |
| n95 8 | 2010 MHz – 2025 MHz | N/A | SUL |
| n9613,14 | 5925 MHz – 7125 MHz | 5925 MHz – 7125 MHz | TDD |
| NOTE 1: UE that complies with the NR Band n50 minimum requirements in this specification shall also comply with the NR Band n51 minimum requirements.NOTE 2: UE that complies with the NR Band n75 minimum requirements in this specification shall also comply with the NR Band n76 minimum requirements.NOTE 3: Uplink transmission is not allowed at this band for UE with external vehicle-mounted antennas.NOTE 4: A UE that complies with the NR Band n65 minimum requirements in this specification shall also comply with the NR Band n1 minimum requirements.NOTE 5: Unless otherwise stated, the applicability of requirements for Band n90 is in accordance with that for Band n41; a UE supporting Band n90 shall meet the requirements for Band n41. A UE supporting Band n90 shall also support band n41.NOTE 6: A UE that supports NR Band n66 shall receive in the entire DL operating band.NOTE 7: A UE that supports NR Band n66 and CA operation in any CA band shall also comply with the minimum requirements specified for the DL CA configurations CA\_n66B and CA\_n66(2A) in the current version of the specification.NOTE 8: This band is applicable in China only.NOTE 9: Variable duplex operation does not enable dynamic variable duplex configuration by the network, and is used such that DL and UL frequency ranges are supported independently in any valid frequency range for the band. NOTE 10: When this band is used for V2X SL service, the band is exclusively used for NR V2X in particular regions.NOTE 11: This band is unlicensed band used for V2X service. There is no expected network deployment in this band.NOTE 12: In the USA this band is restricted to 3450 – 3550 MHz and 3700 – 3980 MHz.NOTE 13: This band is restricted to operation with shared spectrum channel access as defined in TS 37.213 [14].NOTE 14: This band is applicable only in countries/regions designating this band for shared-spectrum access use subject to country-specific conditions.NOTE 15: For SDL bands, downlink configuration for RRM performance testing is same as FDD. |

*------------------------------ Next modified section ------------------------------*

### 6.2.1 UE maximum output power

The following UE Power Classes define the maximum output power for any transmission bandwidth within the channel bandwidth of NR carrier unless otherwise stated. The period of measurement shall be at least one sub frame (1ms).

Table 6.2.1-1: UE Power Class

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NRband | Class 1 (dBm) | Tolerance (dB) | Class 1.5 (dBm) | Tolerance (dB) | Class 2 (dBm) | Tolerance (dB) | Class 3 (dBm) | Tolerance (dB) |
| n1 |  |  |  |  |  |  | 23 | ±2 |
| n2 |  |  |  |  |  |  | 23 | ±23 |
| n3 |  |  |  |  |  |  | 23 | ±23 |
| n5 |  |  |  |  |  |  | 23 | ±2 |
| n7 |  |  |  |  |  |  | 23 | ±23 |
| n8 |  |  |  |  |  |  | 23 | ±23 |
| n12 |  |  |  |  |  |  | 23 | ±23 |
| n14 | 316,7 | +2/-3 |  |  |  |  | 23 | ±2 |
| n18 |  |  |  |  |  |  | 23 | ±2 |
| n20 |  |  |  |  |  |  | 23 | ±23 |
| n25 |  |  |  |  |  |  | 23 | ±23 |
| n26 |  |  |  |  |  |  | 23 | ±23 |
| n28 |  |  |  |  |  |  | 23 | +2/-2.5 |
| n30 |  |  |  |  |  |  | 23 | ±2 |
| n34 |  |  |  |  |  |  | 23 | ±2 |
| n38 |  |  |  |  |  |  | 23 | ±2 |
| n39 |  |  |  |  |  |  | 23 | ±2 |
| n40 |  |  |  |  | 26 | +2/-3 | 23 | ±2 |
| n41 |  |  | 295 | +2/-33 | 26 | +2/-33 | 23 | ±23 |
| n47 |  |  |  |  |  |  | 23 | ±2 |
| n48 |  |  |  |  |  |  | 23 | +2/-3 |
| n50 |  |  |  |  |  |  | 23 | ±2 |
| n51 |  |  |  |  |  |  | 23 | ±2 |
| n53 |  |  |  |  |  |  | 23 | ±2 |
| n65 |  |  |  |  |  |  | 23 | ±2 |
| n66 |  |  |  |  |  |  | 23 | ±2 |
| n70 |  |  |  |  |  |  | 23 | ±2 |
| n71 |  |  |  |  |  |  | 23 | +2/-2.5 |
| n74 |  |  |  |  |  |  | 23 | ±2 |
| n77 |  |  |  |  | 26 | +2/-3 | 23 | +2/-3 |
| n78 |  |  |  |  | 26 | +2/-3 | 23 | +2/-3 |
| n79 |  |  |  |  | 26 | +2/-3 | 23 | +2/-3 |
| n80 |  |  |  |  |  |  | 23 | ±23 |
| n81 |  |  |  |  |  |  | 23 | ±2 |
| n82 |  |  |  |  |  |  | 23 | ±2 |
| n83 |  |  |  |  |  |  | 23 | +2/-2.5 |
| n84 |  |  |  |  |  |  | 23 | ±2 |
| n86 |  |  |  |  |  |  | 23 | ±2 |
| n89 |  |  |  |  |  |  | 23 | ±2 |
| n91 |  |  |  |  |  |  | 23 | ±23, 4 |
| n92 |  |  |  |  |  |  | 23 | ±23, 4 |
| n93 |  |  |  |  |  |  | 23 | ±23, 4 |
| n94 |  |  |  |  |  |  | 23 | ±23, 4 |
| n95 |  |  |  |  |  |  | 23 | ±2 |
| NOTE 1: PPowerClass is the maximum UE power specified without taking into account the tolerance.NOTE 2: Powerclass 3 is default power class unless otherwise stated.NOTE 3: Refers to the transmission bandwidths confined within FUL\_low and FUL\_low + 4 MHz or FUL\_high – 4 MHz and FUL\_high, the maximum output power requirement is relaxed by reducing the lower tolerance limit by 1.5 dB.NOTE 4: The maximum output power requirement is relaxed by reducing the lower tolerance limit by 0.3 dB.NOTE 5: Achieved via dual Tx.NOTE 6: Generally, PC1 UE is not targeted for smartphone form factor. NOTE 7: The UE power class 1 requirements for Band n14 are applicable for public safety scenario only. |

*------------------------------ End of modified section -------------------------*