**3GPP TSG-RAN4 WG4 Meeting#112 *Rev R4-2412622***

**Maastricht, Netherlands, 19th – 23rd May 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-3** | **CR** | **1294** | **rev** | 1 | **Current version:** | **18.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for EN-DC Harmonic Mixing clean-up PC2 |
|  |  |
| ***Source to WG:*** | Qualcomm France |
| ***Source to TSG:*** | RAN4 |
|  |  |
| ***Work item code:*** | HPUE\_FR1\_DC\_LTE\_NR\_R18-Core |  | ***Date:*** | 2024-08-06 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | R4-2405453 was agreed in RAN4#110bis, which proposed a set of principles to clean-up RX mixing specification |
|  |  |
| ***Summary of change:*** | PC2 Harmonic mixing MSD tables are modified according to principles agreed in R4-2405453 and in R4-2410651. Additionally, RBstart for each combination is now described in Note |
|  |  |
| ***Consequences if not approved:*** | Harmonic mixing tables remain erroneous and inconsistent |
|  |  |
| ***Clauses affected:*** | 7.3B.2.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS38.521-1  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Changes to UL harmonic and Rx harmonic MSD tables are applicable only from Rel-18 and onward to subsequent Releases |
|  |  |
| ***This CR's revision history:*** |  |

**---Start of changes---**

**Table 7.3B.2.3.2-1a: Reference sensitivity exceptions (MSD) due to receiver harmonic mixing for PC2 EN-DC in NR FR1**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **UL band** | **DL band** | **UL BW** | **SCS of UL band** | **UL RB Allocation** | **DL BW** | **MSD** | **UL/DL fc condition** | **UL/DL harmonic order** |
| **(MHz)** | **(kHz)** | **LCRB** | **(MHz)** | **(dB)** |
| n41 | 18 | 10 | 15 | 25 | 5 | 29.3 | NOTE 4 | UL1/DL3 |
| n77 | 2 | 10 | 15 | 25 | 5 | 9.2 | NOTE 6 | UL1/DL2 |
| n77 | 2 | 10 | 15 | 25 | 20 | 4.5 | NOTE 6 | UL1/DL2 |
| n77 | 3 | 10 | 15 | 25 | 5 | 8.1 | NOTE 6 | UL1/DL2 |
| n77 | 3 | 10 | 15 | 25 | 20 | 3.8 | NOTE 6 | UL1/DL2 |
| n77 | 12 | 10 | 15 | 25 | 5 | 34 | NOTE 1 | UL1/DL5 |
| n77 | 12 | 10 | 15 | 25 | 10 | 31 | NOTE 1 | UL1/DL5 |
| n77 | 13 | 10 | 15 | 25 | 5 | 34 | NOTE 1 | UL1/DL5 |
| n77 | 13 | 10 | 15 | 25 | 10 | 31 | NOTE 1 | UL1/DL5 |
| n77 | 14 | 10 | 15 | 25 | 5 | 34 | NOTE 1 | UL1/DL5 |
| n77 | 14 | 10 | 15 | 25 | 10 | 31 | NOTE 1 | UL1/DL5 |
| n77 | 19 | 10 | 15 | 25 | 5 | 9.8 | NOTE 6 | UL1/DL2 |
| n77 | 19 | 10 | 15 | 25 | 15 | 5.9 | NOTE 6 | UL1/DL2 |
| n77 | 28 | 10 | 15 | 25 | 5 | 34 | NOTE 1 | UL1/DL5 |
| n77 | 28 | 10 | 15 | 25 | 20 | 26.5 | NOTE 1 | UL1/DL5 |
| n772 | 29 | 10 | 15 | 25 | 5 | 34 | NOTE 1 | UL1/DL5 |
| n772 | 29 | 10 | 15 | 25 | 10 | 31 | NOTE 1 | UL1/DL5 |
| n77 | 41 | 10 | 15 | 12 | 5 | 17.7 | NOTE 4 | UL2/DL3 |
| n77 | 41 | 10 | 15 | 12 | 20 | 11.9 | NOTE 4 | UL2/DL3 |
| n78 | 8 | 10 | 15 | 25 | 5 | 8.1 | NOTE 5 | UL1/DL4 |
| n78 | 8 | 10 | 15 | 25 | 10 | 5.7 | NOTE 5 | UL1/DL4 |
| n78 | 5 | 10 | 15 | 25 | 5 | 8.1 | NOTE 5 | UL1/DL4 |
| n78 | 13 | 10 | 15 | 25 | 5 | 34 | NOTE 1 | UL1/DL5 |
| n78 | 19 | 10 | 15 | 25 | 5 | 9.8 | NOTE 5 | UL1/DL4 |
| n78 | 19 | 10 | 15 | 25 | 15 | 5.9 | NOTE 5 | UL1/DL4 |
| n78 | 28 | 10 | 15 | 25 | 5 | 34 | NOTE 1 | UL1/DL5 |
| n78 | 28 | 10 | 15 | 25 | 20 | 26.5 | NOTE 1 | UL1/DL5 |
| n78 | 41 | 10 | 15 | 12 | 5 | 17.7 | NOTE 4 | UL2/DL3 |
| n78 | 41 | 10 | 15 | 12 | 20 | 11.9 | NOTE 4 | UL2/DL3 |
| n78 | 40 | 10 | 15 | 12 | 5 | 17.7 | NOTE 4 | UL2/DL3 |
| n79 | 19 | 10 | 15 | 25 | 5 | 32.5 | NOTE 1 | UL1/DL5 |
| n79 | 19 | 10 | 15 | 25 | 15 | 27.7 | NOTE 1 | UL1/DL5 |
| n79 | 21 | 10 | 15 | 25 | 5 | 42.3 | NOTE 3 | UL1/DL3 |
| n79 | 21 | 10 | 15 | 25 | 15 | 37.5 | NOTE 3 | UL1/DL3 |
| NOTE 1: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  and with  the DL carrier frequency in the lower band and the UL carrier frequency and the channel bandwidth configured in the higher band, both in MHz.NOTE 2: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 from TS 38.101-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped.NOTE 3: The requirements should be verified for DL EARFCN or NR ARFCN of the victim (lower) band (superscript LB) such that  and with  the DL carrier frequency in the lower band and the UL carrier frequency and the channel bandwidth in the higher band, both in MHz.NOTE 4: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that and with the DL carrier frequency in the lower band and the UL carrier frequency and the channel bandwidth in the higher band, both in MHz.NOTE 5: The requirements should be verified for UL NR-ARFCN of the aggressor (higher) band (superscript HB) such that  in MHz and with  the carrier frequency in the victim (lower) band and  the channel bandwidth configured in the higher bandNOTE 6: The requirements should be verified for DL EARFCN or NR ARFCN of the victim (lower) band (superscript LB) such that and with   the DL carrier frequency in the lower band and the UL carrier frequency in the higher band, both in MHz. NOTE 7: The requirements should be verified using RBstart = floor((NRB-LCRB)/2), where floor(x) is the greatest integer less than or equal to x, and where the UL parameters NRB and LCRB are respectively, the transmission bandwidth configuration and the number of RB’s for the specified UL band channel bandwidth and the UL band subcarrier spacing. |

**---End of changes---**