**3GPP TSG-RAN4 Meeting #112 R4-2414286**

**Maastricht, Netherlands, 19th – 23rd August, 2024**

**Source:** China Telecom

**Title:** WF on RedCap PC2 requirements

**Agenda item:** 8.7.3

**Document for:** Approval

# Background

This WF captures the agreements for introducing RedCap PC2 requirements

# Wayforward

**Issue 1-1-1: PC2 RedCap UE for TDD bands**

**Agreement: Add one sentence in the clause of 6.2I.1 to state that PC2 also applies for RedCap/eRedCap UE in a band agnostic way for TDD bands**

**Wayforward: Considering the following changes as starting point for introducing RedCap PC2 requirements for TDD bands**

|  |
| --- |
| 6.2I Transmitter power for RedCapFor Redcap and eRedCap UE the requirements in Section 6 shall be verified with the channel bandwidth up to 20MHz and requirements specified in clause 6.2I.6.2I.1 Maximum output power for RedCapFor Redcap and eRedCap UE, the requirements for power class 3 specified in clause 6.2.1 apply.For RedCap and eRedCap UE, the requirements for power class 2 specified in clause 6.2.1 [for TDD bands] apply. |