**3GPP TSG-RAN WG4 Meeting #112 R4-24xxxxx**

Maastricht, Netherlands, 19th – 23rd August, 2024

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **4836** | **rev** | **1** | **Current version:** | **17.14.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (NR\_RRM\_enh2-Core)CR on SRS antenna switching interruption requirements in R17 |
|  |  |
| ***Source to WG:*** | , Huawei, HiSilicon, ZTE |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_RRM\_enh2-Core |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 17)Rel-17 (Release 18)Rel-18 (Release 19)Rel-19 (Release 20)* |
|  |  |
| ***Reason for change:*** | For RRM requirements under NR CA, there is no async scenario from MRTD/MTTD perspective. The asyc table is redundant and shall be removed. |
|  |  |
| ***Summary of change:*** | Remove the async table in 8.2.2.2.16 |
|  |  |
| ***Consequences if not approved:*** | The requirements are not correct, and may cause confusion. |
|  |  |
| ***Clauses affected:*** | 8.2.2.2.16 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.533  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change #1>

##### 8.2.2.2.16 Interruptions at NR SRS antenna port switching

The requirements in this clause are applicable to SRS antenna port switching on FR1 and SRS resource(s) is only configured within the last 6 symbols of a slot. For interruption caused by SRS antenna port switching, the victim cell is based on the entry number of the band indicated by *txSwitchImpactToRx* and/or *txSwitchWithAnotherBand* regardless of per-FR MG capability. An UL interruption is allowed on any of the serving cells as indicated in *txSwitchWithAnotherBand*, and a DL interruption is allowed on any of the serving cells as indicated in *txSwitchImpactToRx*.

The UE shall perform SRS antenna port switching only if the below conditions are met.

- the SRS switching is not colliding with any other UL transmission with higher priority defined in TS 38.214 [26] if the serving cell on which the higher priority transmission is performed is a victim cell based on *txSwitchWithAnotherBand* or is the same carrier on which SRS is transmitted.

- the SRS switching is not colliding with any NR measurements (i.e. SSB/CSI-RS based L1/L3 measurements) and the measurements for RLM/BFD/CBD if the serving cell on which the NR measurements and the measurements for RLM/BFD/CBD is performed is a victim cell based on *txSwitchImpactToRx* or is the same carrier on which SRS is transmitted.

No requirements are defined for SRS antenna port switching if aperiodic SRS switching is colliding with aperiodic L1-RSRP/L1-SINR measurements and the serving cell on which the aperiodic L1-RSRP/L1-SINR measurement is configured is indicated in *txSwitchImpactToRx* or is the same carrier on which aperiodic SRS is scheduled/configured.

When 1 SRS symbol is configured in a slot for SRS antenna switching, the interruption requirement in Table 8.2.2.2.16-1 applies. For the rest of SRS configurations, the interruption requirement in Table 8.2.2.2.16-3 applies.

**Table 8.2.2.2.16-1: Interruption length in symbols of victim CC when 1 SRS symbol is configured**

|  |  |
| --- | --- |
| **Victim cell SCS(kHz)** | **Aggressor cell SCS (kHz)** |
| **15**  | **30** | **60** |
| 15  | 3 | 2 | 2 |
| 30 | 4 | 3 | 3 |
| 60 | 8 | 6 | 5 |
| 120 | 14 | 10 | 8 |

**Table 8.2.2.2.16.2: Void**

|  |  |
| --- | --- |
|  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**Table 8.2.2.2.16-3: Interruption length in slots of victim CC for rest of the SRS configurations**

|  |  |
| --- | --- |
| **Victim cell SCS(kHz)** | **Aggressor cell SCS (kHz)** |
| **15**  | **30** | **60** |
| 15 | 2 | 2 | 2 |
| 30 | 2 | 2 | 2 |
| 60 | 3 | 2 | 2 |
| 120 | 5 | 3 | 3 |

<End of Change #1>