**3GPP TSG-RAN WG4 Meeting #112 R4-2413929**

**Maastricht, Netherlands, 19th – 23rd August, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **4650** | **rev** | **1** | **Current version:** | **17.14.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (NR\_pos\_enh-Perf) CR on R17 positioning test cases in RRC\_INACTIVE state |
|  |  |
| ***Source to WG:*** | CATT |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_pos\_enh-Perf |  | ***Date:*** | 2024-08-08 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | 1. The T2 values in the positioning test cases are incorrect since they do not cover the measurement period UE requires.
2. PRS-RSRP and SS-RSRP values are incorrect in RSTD accuracy test.
 |
|  |  |
| ***Summary of change:*** | 1. Correct the T2 value for each test case.
2. Correct PRS-RSRP and SS-RSRP values in RSTD accuracy test.
3. Some other typo corrections.
 |
|  |  |
| ***Consequences if not approved:*** | The positioning test cases in INACTIVE state are incorrect.  |
|  |  |
| ***Clauses affected:*** | A.7.9.1.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.533 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of R4-2411373 |

# <Start of Change 1>

#### A.7.9.1.2 RSTD measurement accuracy test case with reduced number of samples for single positioning frequency layer in FR2 in RRC\_INACTIVE state

##### A.7.9.1.2.1 Test purpose and Environment

The purpose of the test is to verify that the RSTD measurement in RRC\_INACTIVE state meets the accuracy requirements specified in clause 10.1.23.2 in an environment with AWGN propagation conditions. In this test UE that supports *supportedDL-PRS-ProcessingSamples-RRC-Inactive* is configured by LMF to perform PRS measurement with reduced number of samples.

The supported test configurations are specified in Table A.7.9.1.2.1-1.

Table A.7.9.1.2.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | 120 kHz SSB SCS, 200 MHz bandwidth, TDD duplex mode |

In the test there are two synchronous cells: Cell 1 and Cell 2. Cell 1 is the reference as well as the PCell. Cell 2 is a neighbour cells. Both cells are on the same NR RF channel in FR2. The UE is configured with DRX cycle of 0.64s. The *NR-TDOA-ProvideAssistanceData* and *NR-TDOA-RequestLocationInformation* message as defined in TS 37.355 shall be provided to the UE before the start of the test. The test duration should be larger than the UE measurement period as defined in clause 5.6.2.5.

Table A.7.9.1.2.1-2: RSTD accuracy test parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test 1 | Test 2 |
|  |  | Cell 1 | Cell 2 | Cell 1 | Cell 2 |
| PRS ARFCN |  | freq1 | freq1 |
| Duplex mode |  | TDD | TDD |
| TDD configuration |  | TDDConf.3.1 | TDDConf.3.1 |
| BWchannel | MHz | 200: NRB,c = 132 | 200: NRB,c = 132 |
| Downlink initial BWP configuration |  | DLBWP.0.1 | DLBWP.0.1 | DLBWP.0.1 | DLBWP.0.1 |
| Uplink initial BWP configuration |  | ULBWP.0.1 | - | ULBWP.0.1 | - |
| Uplink dedicated BWP configuration |  | ULBWP.1.1 | - | ULBWP.1.1 | - |
| TRS configuration |  | TRS.2.1 TDD | - | TRS.2.1 TDD | - |
| TCI state |  | TCI.State.0 | - | TCI.State.0 | - |
| PDSCH Reference measurement channel  |  | SR.3.1 TDD | - | SR.3.1 TDD | - |
| RMSI CORESET Reference Channel |  | CR.3.1 TDD | - | CR.3.1 TDD | - |
| Control channel RMC |  | CCR.3.1 TDD | - | CCR.3.1 TDD | - |
| OCNG Patterns |  | OP.3 | OP.3 | OP.3 | OP.3 |
| SSB configuration |  | SSB.3 FR2 | SSB.3 FR2 | SSB.3 FR2 | SSB.3 FR2 |
| SMTC configuration |  | SMTC.1 | SMTC.1 | SMTC.1 | SMTC.1 |
| PRS configuration |  | PRS.1.3 FR2 | PRS.1.3 FR2 | PRS.1.4 FR2 | PRS.1.4 FR2 |
| PRS BW |  | 64 PRBs | 64 PRBs | 128 PRBs | 128 PRBs |
| PRS Resource slot offset  | slot | 0 | 4 | 0 | 4 |
| Expected RSTD | μs | N/A | 3 | N/A | 3 |
| Expected RSTD uncertainty | μs | N/A | 5 | N/A | 5 |
| Time offset with Cell 1 | μs | - | 3 | - | 3 |
| PDSCH/PDCCH subcarrier spacing | kHz | 120 | 120 | 120 | 120 |
| EPRE ratio of PSS to SSS | dB | 0 | 0 | 0 | 0 |
| EPRE ratio of PBCH\_DMRS to SSS |  |  |  |  |  |
| EPRE ratio of PBCH to PBCH\_DMRS |  |  |  |  |  |
| EPRE ratio of PDCCH\_DMRS to SSS |  |  |  |  |  |
| EPRE ratio of PDCCH to PDCCH\_DMRS |  |  |  |  |  |
| EPRE ratio of PDSCH\_DMRS to SSS |  |  |  |  |  |
| EPRE ratio of PDSCH to PDSCH\_DMRS |  |  |  |  |  |
| EPRE ratio of OCNG DMRS to SSSNote 1 |  |  |  |  |  |
| EPRE ratio of OCNG to OCNG DMRS Note 1 |  |  |  |  |  |
| Propagation conditions |  | AWGN | AWGN | AWGN | AWGN |
| Antenna configuration |  | 1x2 | 1x2 | 1x2 | 1x2 |
| Note 1: OCNG shall be used such that both cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols. |

Table A.7.9.1.2.1-3: RSTD accuracy OTA related test parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test 1 | Test 2 |
|  |  | Cell 1 | Cell 2 | Cell 1 | Cell 2 |
| Angle of arrival configuration |  | Setup 1 according to clause A.3.15.1 |
| Assumption for UE beamsNote 5 |  | Rough | Rough |
| Note1 | dBm/SCSNote3 | -89 | -89 |
|  | dB | -1.44 | -3.65 | -1.44 | -3.65 |
| PRS-RSRPNote2 | dBm/SCS | -90.44 | -92.65 | -90.44 | -92.65 |
| SS-RSRPNote2 | dBm/SCS | -90.44 | -92.65 | -90.44 | -92.65 |
| BB Note4 | dB | -3 | -6 | -3 | -6 |
| IoNote2 | dBm/190.08 MHz Note3 | -53.68 | -53.68 | -53.68 | -53.68 |
| Note 1: Where used, interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 2: SSB\_RP, Es/Iot and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 3: Equivalent power received by an antenna with 0 dBi gain at the centre of the quiet zoneNote 4: Calculation of Es/IotBB includes the effect of UE internal noise up to the value assumed for the associated Refsens requirement in clause 7.3.2 of TS 36.101-2 [19], and an allowance of 1dB for UE multi-band relaxation factor ΔMBP from TS 38.101-2 [19] Table 6.2.1.3-4.Note 5: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

##### A.7.9.1.2.2 Test Requirements

The RSTD measurement accuracy for Cell 2 shall fulfil the absolute requirement in clause 10.1.23.2.

# <End of Change 1>