**3GPP TSG- Meeting # *R4-2413940***

**Maastricht, Netherland,**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **4772** | **rev** | **1** | **Current version:** | **18.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (NR\_MC\_enh-Perf) Correction to Rel-18 UL Tx switching test cases\_R18 |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_MC\_enh-Perf |  | ***Date:*** | 2024-08-22 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | 1. To verify 1T-2T UL Tx switch, it’s needed to configure 2 ports SRS on 2 Tx capable band, just like A.4.5.8.
 |
|  |  |
| ***Summary of change:*** | Issues mentioned above are fixed. |
|  |  |
| ***Consequences if not approved:*** | Non-conformant UE can pass the test |
|  |  |
| ***Clauses affected:*** | A.6.5.7D.1, A.6.5.7D.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS38.533 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

#### A.6.5.7D.1 DL interruptions at switching across three uplink bands in TDD-TDD CA for single TAG

##### A.6.5.7D.1.1 Test Purpose and Environment

The purpose of this test is to verify DL interruption requirements during UE dynamic switching across three uplink bands for single TAG defined in clause 8.2.2.2.10D. The test case is applicable for an inter-band TDD-TDD CA configuration when the capability *BandCombination-UplinkTxSwitch-v1800* is present, where NR UL carrier 1 in band A is capable of one transmit antenna connector, NR UL carrier 2 in band B is capable of one transmit antenna connector and NR UL carrier 3 in band C is capable of two transmit antenna connectors. NR UL carrier 1, carrier 2 and carrier 3 in band A, band B and band C, respectively, are different bands with different carrier frequencies. All cells belong to the same TAG.

There are three cells: FR1 TDD PCell (Cell 1), FR1 TDD SCell (Cell 2) and FR1 TDD SCell (Cell 3) where cell 1 with 1TX is on band A, cell 2 with 1TX is on band B, and cell 3 with 2TX is on band C. The test parameters for the three cells are given in Table A.6.5.7D.1.1-1, Table A.6.5.7D.1.1-2 and Table A.6.5.7D.1.1-3 below. TX switching is from band A and band B to band C.

For NR TDD PCell (Cell 1) and NR TDD SCell (Cell 2), aperiodic CSI-RS for L1-RSRP reporting is triggered with power boosting 6dB on the following symbol in the 1st special slot of every radio frame:

- symbol#10 if UE does not report *uplinkTxSwitching-DL-Interruption-r18*;

- otherwise,

- symbol #4 if UE capability uplink Tx switching period is 210us or

- symbol #5 if UE capability uplink Tx switching period is 140us or

- symbol #8 if UE capability uplink Tx switching period is 35us.

For NR TDD SCell (Cell 3), aperiodic CSI-RS for L1-RSRP reporting is configured with power boosting 6dB on the following symbol on the 2nd special slot of every radio frame:

- symbol#10 if UE does not report *uplinkTxSwitching-DL-Interruption-r18*;

- otherwise,

- symbol #4 if UE capability uplink Tx switching period is 210us or

- symbol #5 if UE capability uplink Tx switching period is 140us or

- symbol #8 if UE capability uplink Tx switching period is 35us.

This test verifies that the UE correctly report the L1-RSRP reporting. The test case is only applicable to UE which supports *simultaneousRxTxInterBandCA.*

The test consists of one time period, with duration of T1. Prior to the start of the time duration T1, *UplinkTxSwitchingMoreBands-r18* is indicated to UE.

Table A.6.5.7D.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | NR Cell 1: 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex modeNR Cell 2: 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex modeNR Cell 3: 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |

Table A.6.5.7D.1.1-2: General test parameters for DL interruptions at switching across three uplink bands in TDD-TDD CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| RF Channel Number |  | Config 1 | 1, 2, 3 | Three radio channels are used for this test. |
| Active cell |  | Config 1 | Cell 1: FR1 PCellCell 2: FR1 SCellCell 3: FR1 SCell | FR1 PCell on RF channel number 1FR1 SCell on RF channel number 2FR1 SCell on RF channel number 3 |
| CP length |  | Config 1 | Normal |  |
| DRX |  | Config 1 | OFF |  |
| Measurement gap pattern Id |  | Config 1 | OFF |  |
| Filter coefficient |  | Config 1 | 0 | L3 filtering is not used |
| CSI-RS configuration for L1-RSRP reporting |  | Config 1 | Cell 1: CSI-RS.2.5 TDDCell 2: CSI-RS.2.5 TDDCell 3: CSI-RS.2.5 TDD |  |
| T1 | s | Config 1 | 5 |  |

Table A.6.5.7D.1.1-3: Cell specific test parameters for DL interruptions at switching across three uplink bands in TDD-TDD CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Cell1 | Cell2 | Cell3 |
| Frequency Range |  | FR1 | FR1 | FR1 |
| Duplex mode | Config 1 |  | TDD | TDD | TDD |
| TDD configuration | Config 1 |  | TDDConf.2.1 except thatS=’11DL: 1GP :2UL’;*nrofDownlinkSymbols: 11**nrofUplinkSymbols: 2* | TDDConf.2.1 except thatS=’11DL: 1GP :2UL’;*nrofDownlinkSymbols: 11**nrofUplinkSymbols: 2* | TDDConf.2.2 |
| BWchannel | Config 1 | MHz | 40: NRB,c = 106 | 40: NRB,c = 106 | 40: NRB,c = 106 |
| Initial BWP Configuration | Config 1 |  | DLBWP.0.1 | DLBWP.0.1 | DLBWP.0.1 |
| DL dedicated BWP configuration | Config 1 |  | DLBWP.1.1 | DLBWP.1.1 | DLBWP.1.1 |
| UL dedicated BWP configuration | Config 1 |  | ULBWP.1.1 | ULBWP.1.1 | ULBWP.1.1 |
| SRS configuration | Config 1 |  | SRSConf.1 in Table A.4.4.1.1.1-3 is applied except that:resourceMappingstartPosition: 0resourceMappingnrofSymbols: n2periodicityAndOffset-p: sl20,5 | SRSConf.1 in Table A.4.4.1.1.1-3 is applied except that:resourceMappingstartPosition: 0resourceMappingnrofSymbols: n2periodicityAndOffset-p: sl20,5 | SRSConf.1 in Table A.4.4.1.1.1-3 is applied except that:resourceMappingstartPosition: 0resourceMappingnrofSymbols: n2periodicityAndOffset-p: sl20,3nrofSRS-Ports: ports2 |
| PDSCH Reference measurement channel | Config 1 |  | SR.2.1 TDD | SR.2.1 TDD | SR.2.1 TDD |
| RMSI CORESET parameters | Config 1 |  | CR.2.1 TDD | CR.2.1 TDD | CR.2.1 TDD |
| Dedicated CORESET parameters | Config 1 |  | CCR.2.1 TDD | CCR.2.1 TDD | CCR.2.1 TDD |
| OCNG Patterns |  | OP.1 | OP.1 | OP.1 |
| SMTC Configuration |  | SMTC.1 | SMTC.1 | SMTC.1 |
| SSB Configuration | Config 1 |  | SSB.2 FR1 | SSB.2 FR1 | SSB.2 FR1 |
| Correlation Matrix and Antenna Configuration |  | 1x2 Low | 1x2 Low | 2x2 Low |
| EPRE ratio of PSS to SSS | dB | 0 | 0 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |  |  |  |
| EPRE ratio of PBCH to PBCH DMRS |  |  |  |  |
| EPRE ratio of PDCCH DMRS to SSS |  |  |  |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |  |  |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |  |  |  |
| EPRE ratio of PDSCH to PDSCH  |  |  |  |  |
| EPRE ratio of OCNG DMRS to SSS(Note 1) |  |  |  |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |  |  |  |
| NocNote 2 | dBm/15 kHz | -104 | -104 | -104 |
| SS-RSRP Note 3 | dBm/SCS | -87 | -87 | -87 |
| Ês/Iot | dB | 14 | 14 | 14 |
| Ês/Noc | dB | 14 | 14 | 14 |
| NocNote 2 | Config 1 | dBm/SCS | -101 | -101 | -101 |
| IoNote3 | Config 1 | dBm/38.16MHz | -55.79 | -55.79 | -55.79 |
| Time offset to Cell1 Note 5 | μs | - | 0 | 0 |
| Propagation Condition  |  | AWGN | AWGN | AWGN |
| Note 1: OCNG shall be used such that both cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for Noc to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: VoidNote 5: Receive time difference between slot boundaries of signals received from the three cells at the UE antenna connector including time alignment error between the three cells. |

##### A.6.5.7D.1.2 Test Requirements

The UE behaviour follows the requirements defined in clause 8.2.2.2.10D.

UE shall send L1-RSRP report while meeting the accuracy requirements defined in clause 10.1.19.2.

The rate of correct events observed during repeated tests shall be at least 90%.

<End of Change 1>

<Start of Change 2>

#### A.6.5.7D.3 DL interruptions at switching across three uplink bands in FDD-TDD CA for two TAGs

##### A.6.5.7D.3.1 Test Purpose and Environment

The purpose of this test is to verify DL interruption requirements during UE dynamic switching across 3 bands with one or two transmit antenna connectors defined in clause 8.2.2.2.10D for two TAGs. The test case is applicable for an NR inter-band CA configuration when the capability [*BandCombination-UplinkTxSwitch-v1800*] is present, where in NR inter-band CA configuration, the number of NR uplink bands with different carrier frequencies is three. NR UL carrier(s) in each of the three uplink bands are capable of one or two transmit antenna connector(s), according to the UE capability. Cell 1 and Cell 2 belong to one TAG, and Cell 3 belongs to the other TAG.

There are three cells: FR1 FDD PCell (Cell 1), FR1 FDD SCell (Cell 2) and FR1 TDD SCell (Cell 3) where cell 1 with 1TX is on band A, cell 2 with 1TX is on band B, and cell 3 with 2TX is on band C. The test parameters for the three cells are given in Table A.6.5.7D.3.1-1, Table A.6.5.7D.3.1-2 and Table A.6.5.7D.3.1-3 below. TX switching is from band A and band B to band C.

For NR FDD carrier Cell 1 and NR FDD carrier Cell2, aperiodic CSI-RS for L1-RSRP reporting is triggered with power boosting 6dB on the following symbol in slot overlapping with the 1st special slot of every radio frame of the NR TDD carrier (Cell 3):

- symbol#12 if UE does not report *uplinkTxSwitching-DL-Interruption-r18*;

- otherwise,

- symbol #8 if UE indicated uplink Tx switching periodis 210us or

- symbol #9 if UE indicated uplink Tx switching period is 140us or

- symbol #10 indicated uplink Tx switching periodis 35us.

For NR TDD carrier (Cell 3), aperiodic CSI-RS for L1-RSRP reporting is configured with power boosting 6dB on the following symbol in the 2nd special slot of every radio frame:

- symbol#10 if UE does not report *uplinkTxSwitching-DL-Interruption-r18*;

- otherwise,

- symbol #3 if UE indicated uplink Tx switching period is 210us or

- symbol #5 if UE indicated uplink Tx switching period is 140us or

- symbol #8 if UE indicated uplink Tx switching period is 35us.

This test verifies that the UE correctly report the L1-RSRP reporting. The test case is only applicable to UE which supports *simultaneousRxTxInterBandCA.*

The test consists of one time period, with duration of T1. Prior to the start of the time duration T1, *UplinkTxSwitchingMoreBands-r18* is indicated to UE.

Table A.6.5.7D.3.1-1: Supported test configurations

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | NR Cell 1: 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex modeNR Cell 2: 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex modeNR Cell 3: 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |

Table A.6.5.7D.3.1-2: General test parameters for DL interruptions at switching across 3 bands with one or two transmit antenna connectors in FDD-TDD CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test configuration** | **Value** | **Comment** |
| RF Channel Number |  | Config 1 | 1, 2, 3 | Three radio channels are used for this test. |
| Active cell |  | Config 1 | Cell 1: FR1 PCellCell 2: FR1 SCellCell 3: FR1 SCell | FR1 PCell on RF channel number 1FR1 SCell on RF channel number 2FR1 SCell on RF channel number 3 |
| CP length |  | Config 1 | Normal |  |
| DRX |  | Config 1 | OFF |  |
| Measurement gap pattern Id |  | Config 1 | OFF |  |
| Filter coefficient |  | Config 1 | 0 | L3 filtering is not used |
| CSI-RS configuration for L1-RSRP reporting |  | Config 1 | Cell 1: CSI-RS.1.5 FDDCell 2: CSI-RS.1.5 FDDCell 3: CSI-RS.2.5 TDD |  |
| T1 | s | Config 1 | 5 |  |

Table A.6.5.7D.3.1-3: Cell specific test parameters for DL interruptions at switching across 3 bands with one or two transmit antenna connectors in FDD-TDD CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Cell1 | Cell2 | Cell3 |
| Frequency Range |  | FR1 | FR1 | FR1 |
| Duplex mode | Config 1 |  | FDD | FDD | TDD |
| TDD configuration | Config 1 |  | N/A | N/A | TDDConf.2.1 except that:S=’11DL: 1GP:2UL’;*nrofDownlinkSymbols: 11**nrofUplinkSymbols: 2* |
| BWchannel | Config 1 | MHz | 10: NRB,c = 52 | 10: NRB,c = 52 | 40: NRB,c = 106 |
| Initial BWP Configuration | Config 1 |  | DLBWP.0.1 | DLBWP.0.1 | DLBWP.0.1 |
| DL dedicated BWP configuration | Config 1 |  | DLBWP.1.1 | DLBWP.1.1 | DLBWP.1.1 |
| UL dedicated BWP configuration | Config 1 |  | ULBWP.1.1 | ULBWP.1.1 | ULBWP.1.1 |
| SRS configuration | Config 1 |  | SRSConf.1 in Table A.4.4.1.1.1-3 is applied except that:resourceMappingstartPosition: 0resourceMappingnrofSymbols: n2periodicityAndOffset-p: sl10,6 | SRSConf.1 in Table A.4.4.1.1.1-3 is applied except that:resourceMappingstartPosition: 0resourceMappingnrofSymbols: n2periodicityAndOffset-p: sl10,6 | SRSConf.1 in Table A.4.4.1.1.1-3 is applied except that:resourceMappingstartPosition: 0resourceMappingnrofSymbols: n2periodicityAndOffset-p: sl20,3nrofSRS-Ports: ports2 |
| PDSCH Reference measurement channel | Config 1 |  | SR.1.1 FDD | SR.1.1 FDD | SR.2.1 TDD |
| RMSI CORESET parameters | Config 1 |  | CR.1.1 FDD | CR.1.1 FDD | CR.2.1 TDD |
| Dedicated CORESET parameters | Config 1 |  | CCR.1.1 FDD | CCR.1.1 FDD | CCR.2.1 TDD |
| OCNG Patterns |  | OP.1 | OP.1 | OP.1 |
| SMTC Configuration |  | SMTC.1 | SMTC.1 | SMTC.1 |
| SSB Configuration | Config 1 |  | SSB.1 FR1 | SSB.1 FR1 | SSB.2 FR1 |
| Correlation Matrix and Antenna Configuration |  | 1x2 Low | 1x2 Low | 2x2 Low |
| EPRE ratio of PSS to SSS | dB | 0 | 0 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |  |  |  |
| EPRE ratio of PBCH to PBCH DMRS |  |  |  |  |
| EPRE ratio of PDCCH DMRS to SSS |  |  |  |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |  |  |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |  |  |  |
| EPRE ratio of PDSCH to PDSCH  |  |  |  |  |
| EPRE ratio of OCNG DMRS to SSS(Note 1) |  |  |  |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |  |  |  |
| NocNote 2 | dBm/15 kHz | -104 | -104 | -104 |
| SS-RSRP Note 3 | dBm/SCS | -87 | -87 | -87 |
| Ês/Iot | dB | 17 | 17 | 14 |
| Ês/Noc | dB | 17 | 17 | 14 |
| NocNote 2 | Config 1 | dBm/SCS | -104 | -104 | -101 |
| IoNote3 | Config 1 | dBm/9.36 MHz | -58.96 | -58.96 | - |
|  |  | dBm/38.16MHz | - | - | -55.79 |
| Time offset to Cell1 Note 5 | μs | - | 0 | 9 |
| Propagation Condition  |  | AWGN | AWGN | AWGN |
| Note 1: OCNG shall be used such that both cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for Noc to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: VoidNote 5: Receive time difference between slot boundaries of signals received from the two cells at the UE antenna connector including time alignment error between the two cells. |

##### A.6.5.7D.3.2 Test Requirements

The UE behaviour follows the requirements defined in clause 8.2.2.2.10D for two TAGs case and provided in Table 8.2.2.2.10D-2.

UE shall send L1-RSRP report while meeting the accuracy requirements defined in clause 10.1.19.2.

The rate of correct events observed during repeated tests shall be at least 90%.

<End of Change 2>