**3GPP TSG-RAN WG4 Meeting #112 R4-241xxxx**

**Maastricht, The Netherlands, 19 – 23 August, 2024**

**Agenda item:** 6.1.3

**Source:** Huawei, HiSilicon

**Title:** WF on LPHAP

**Document for:** Approval

Sub-Topic #2: Performance requirements

**Issue 1-2-1: Configuration of PRS measurement reporting periodicity in TCs**

Agreements (from adhoc session #1)

* Configure PRS measurement reporting periodicity in LPHAP test cases. The reportingInterval is smaller than the eDRX cycle in the test cases.
* LPHAP test cases for core requirement is considered complete after the UE reports the first set of positioning measurements based on the configured reportingInterval.
* reportingInterval in TC: 20 sec
* How to include the above in the test case requirements subsection: use the text from the second bullet.