**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | (NR\_NTN\_enh-Core) CR for TS 38.101-5 to modify the mistakes for Rx requirements (R18) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 1. The wordings in general clause 10.1 of radiated receiver requirements are not aligned with latest spec TS 38.101-2 as the assumption of 0dBi reference antenna is not only for EIS, but also for other Rx requirements which include wanted signals and interference. 2. The brackets are removed for OTA reference sensitivity requirements. 3. To clarify the applicable scenario that VSAT is towards geostationary satellite orbit based on the EN 301 360, EN 301 459. 4. UL reference measurement channels for FR2-NTN FDD are missing. 5. OCNG Patterns for FDD are missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. The wordings in general clause 10.1 of radiated receiver requirements need to be improved as the assumption of 0dBi reference antenna is not only for EIS, but also for other Rx requirements which include wanted signals and interference. 2. The brackets are removed for OTA reference sensitivity requirements. 3. To clarify the applicable scenario that VSAT is towards geostationary satellite orbit based on the EN 301 360, EN 301 459. 4. UL reference measurement channels for FR2-NTN FDD are introduced. 5. OCNG Patterns for FDD in Annes A.5 are introduced. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Some wordings are not accurate in general clause 10.1. The brackets for RMC exist in the OTA reference sensitivity. UL reference measurement channels and OCNG Patterns are missing for FR2-NTN FDD. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 10.1, 10.3.2, A.2, A.5 (New Clause) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-5 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## **<<Start of Change for TS 38.101-5>>**

## 10.1 General

Unless otherwise stated, the receiver characteristics are specified over the air (OTA) at the RIB for Ka bands fixed and mobile VSAT. The power level for all DL wanted signals and interference is defined assuming a 0 dBi reference antenna located at the center of the quiet zone.

## **<<Next of Change>>**

## 10.8 Receiver antenna off-axis performance

The following additional requirements are applicable to NTN VSAT operating in band n512 towards geostationary satellite orbit.

The receiver antenna off-axis gain of each co-polarized components in any direction φ degrees from the antenna main beam shall not exceed the levels specified in Table 10.8-1.

Table 10.8-1: Off-axis Co-polarized gain limit

|  |  |
| --- | --- |
| φ value (degree) | gain (dBi) |
| φmin ≤ φ ≤ 48° | 32 – 25logφ |
| 48° ≤ φ ≤ 85° | -10 |
| 85° ≤ φ ≤ 180° | 0 |
| Note: φmin = 1o or 100λ/D (degrees) whichever is the greater, for D/λ≥ 50.  φmin = 2o or 114(D/ λ)-1.09 (degrees) whichever is the greater, for D/λ 50.  where D is the nominal diameter of the antenna | |

The receiver antenna off-axis gain of each cross-polarized components in any direction φ degrees from the antenna main beam shall not exceed the levels specified in Table 10.8-2.

Table 10.8-2: Off-axis Cross-polarized gain limit

|  |  |
| --- | --- |
| φ value (degree) | gain (dBi) |
| φr ≤ φ ≤ 7° | 23 – 20logφ |
| Note: φr = 1o or 100λ/D (degrees) whichever is the greater  where D is the nominal diameter of the antenna | |

## **<<Next of Change>>**

# A.2 UL reference measurement channels

## A.2.1 General

The measurement channels in the subclause A2.2 are defined to derive the requirements in clause 6 (Transmitter Characteristics) and clause 7 (Receiver Characteristics). And the measurement channels in the subclause A2.3 are defined to derive the requirements in clause 9 (Radiated Transmitter Characteristics) and clause 10 (Radiated Receiver Characteristics). The measurement channels represent example configurations of physical channels for different data rates.

The measurement channels in the following clauses are applicable only to FDD.

## A.2.2 Reference measurement channels for FR1-NTN FDD

### A.2.2.1 DFT-s-OFDM Pi/2-BPSK

Table A.2.2.1-1: Reference Channels for DFT-s-OFDM Pi/2-BPSK

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | pi/2 BPSK | 0 | 24 | 16 | 2 | 1 | 132 | 132 |
|  | 5 | 11 | pi/2 BPSK | 0 | 160 | 16 | 2 | 1 | 660 | 660 |
|  | 9 | 11 | pi/2 BPSK | 0 | 288 | 16 | 2 | 1 | 1188 | 1188 |
|  | 10 | 11 | pi/2 BPSK | 0 | 320 | 16 | 2 | 1 | 1320 | 1320 |
|  | 12 | 11 | pi/2 BPSK | 0 | 384 | 16 | 2 | 1 | 1584 | 1584 |
|  | 15 | 11 | pi/2 BPSK | 0 | 480 | 16 | 2 | 1 | 1980 | 1980 |
|  | 18 | 11 | pi/2 BPSK | 0 | 576 | 16 | 2 | 1 | 2376 | 2376 |
|  | 24 | 11 | pi/2 BPSK | 0 | 768 | 16 | 2 | 1 | 3168 | 3168 |
|  | 25 | 11 | pi/2 BPSK | 0 | 808 | 16 | 2 | 1 | 3300 | 3300 |
|  | 30 | 11 | pi/2 BPSK | 0 | 984 | 16 | 2 | 1 | 3960 | 3960 |
|  | 32 | 11 | pi/2 BPSK | 0 | 1032 | 16 | 2 | 1 | 4224 | 4224 |
|  | 36 | 11 | pi/2 BPSK | 0 | 1128 | 16 | 2 | 1 | 4752 | 4752 |
|  | 45 | 11 | pi/2 BPSK | 0 | 1416 | 16 | 2 | 1 | 5940 | 5940 |
|  | 50 | 11 | pi/2 BPSK | 0 | 1544 | 16 | 2 | 1 | 6600 | 6600 |
|  | 60 | 11 | pi/2 BPSK | 0 | 1864 | 16 | 2 | 1 | 7920 | 7920 |
|  | 64 | 11 | pi/2 BPSK | 0 | 2024 | 16 | 2 | 1 | 8448 | 8448 |
|  | 75 | 11 | pi/2 BPSK | 0 | 2408 | 16 | 2 | 1 | 9900 | 9900 |
|  | 80 | 11 | pi/2 BPSK | 0 | 2472 | 16 | 2 | 1 | 10560 | 10560 |
|  | 81 | 11 | pi/2 BPSK | 0 | 2536 | 16 | 2 | 1 | 10692 | 10692 |
|  | 90 | 11 | pi/2 BPSK | 0 | 2792 | 16 | 2 | 1 | 11880 | 11880 |
|  | 100 | 11 | pi/2 BPSK | 0 | 3104 | 16 | 2 | 1 | 13200 | 13200 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.2 DFT-s-OFDM QPSK

Table A.2.2.2-1: Reference Channels for DFT-s-OFDM QPSK

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | QPSK | 2 | 48 | 16 | 2 | 1 | 264 | 132 |
|  | 5 | 11 | QPSK | 2 | 256 | 16 | 2 | 1 | 1320 | 660 |
|  | 9 | 11 | QPSK | 2 | 456 | 16 | 2 | 1 | 2376 | 1188 |
|  | 10 | 11 | QPSK | 2 | 504 | 16 | 2 | 1 | 2640 | 1320 |
|  | 12 | 11 | QPSK | 2 | 608 | 16 | 2 | 1 | 3168 | 1584 |
|  | 15 | 11 | QPSK | 2 | 768 | 16 | 2 | 1 | 3960 | 1980 |
|  | 18 | 11 | QPSK | 2 | 928 | 16 | 2 | 1 | 4752 | 2376 |
|  | 20 | 11 | QPSK | 2 | 1032 | 16 | 2 | 1 | 5280 | 2640 |
|  | 24 | 11 | QPSK | 2 | 1192 | 16 | 2 | 1 | 6336 | 3168 |
|  | 25 | 11 | QPSK | 2 | 1256 | 16 | 2 | 1 | 6600 | 3300 |
|  | 30 | 11 | QPSK | 2 | 1544 | 16 | 2 | 1 | 7920 | 3960 |
|  | 32 | 11 | QPSK | 2 | 1608 | 16 | 2 | 1 | 8448 | 4224 |
|  | 36 | 11 | QPSK | 2 | 1800 | 16 | 2 | 1 | 9504 | 4752 |
|  | 45 | 11 | QPKS | 2 | 2208 | 16 | 2 | 1 | 11880 | 5940 |
|  | 50 | 11 | QPSK | 2 | 2472 | 16 | 2 | 1 | 13200 | 6600 |
|  | 60 | 11 | QPSK | 2 | 3104 | 16 | 2 | 1 | 15840 | 7920 |
|  | 64 | 11 | QPSK | 2 | 3240 | 16 | 2 | 1 | 16896 | 8448 |
|  | 75 | 11 | QPSK | 2 | 3752 | 16 | 2 | 1 | 19800 | 9900 |
|  | 80 | 11 | QPSK | 2 | 3976 | 24 | 2 | 2 | 21120 | 10560 |
|  | 81 | 11 | QPSK | 2 | 4040 | 24 | 2 | 2 | 21384 | 10692 |
|  | 90 | 11 | QPSK | 2 | 4488 | 24 | 2 | 2 | 23760 | 11880 |
|  | 100 | 11 | QPSK | 2 | 5000 | 24 | 2 | 2 | 26400 | 13200 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.3 DFT-s-OFDM 16QAM

Table A.2.2.3-1: Reference Channels for DFT-s-OFDM 16QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 16QAM | 10 | 176 | 16 | 2 | 1 | 528 | 132 |
|  | 5 | 11 | 16QAM | 10 | 888 | 16 | 2 | 1 | 2640 | 660 |
|  | 9 | 11 | 16QAM | 10 | 1608 | 16 | 2 | 1 | 4752 | 1188 |
|  | 10 | 11 | 16QAM | 10 | 1800 | 16 | 2 | 1 | 5280 | 1320 |
|  | 12 | 11 | 16QAM | 10 | 2088 | 16 | 2 | 1 | 6336 | 1584 |
|  | 15 | 11 | 16QAM | 10 | 2664 | 16 | 2 | 1 | 7920 | 1980 |
|  | 18 | 11 | 16QAM | 10 | 3240 | 16 | 2 | 1 | 9504 | 2376 |
|  | 24 | 11 | 16QAM | 10 | 4224 | 24 | 1 | 1 | 12672 | 3168 |
|  | 25 | 11 | 16QAM | 10 | 4352 | 24 | 1 | 1 | 13200 | 3300 |
|  | 30 | 11 | 16QAM | 10 | 5248 | 24 | 1 | 1 | 15840 | 3960 |
|  | 32 | 11 | 16QAM | 10 | 5632 | 24 | 1 | 1 | 16896 | 4224 |
|  | 36 | 11 | 16QAM | 10 | 6272 | 24 | 1 | 1 | 19008 | 4752 |
|  | 45 | 11 | 16QAM | 10 | 7808 | 24 | 1 | 1 | 23760 | 5940 |
|  | 50 | 11 | 16QAM | 10 | 8712 | 24 | 1 | 2 | 26400 | 6600 |
|  | 60 | 11 | 16QAM | 10 | 10504 | 24 | 1 | 2 | 31680 | 7920 |
|  | 64 | 11 | 16QAM | 10 | 11272 | 24 | 1 | 2 | 33792 | 8448 |
|  | 75 | 11 | 16QAM | 10 | 13064 | 24 | 1 | 2 | 39600 | 9900 |
|  | 80 | 11 | 16QAM | 10 | 14088 | 24 | 1 | 2 | 42240 | 10560 |
|  | 81 | 11 | 16QAM | 10 | 14088 | 24 | 1 | 2 | 42768 | 10692 |
|  | 90 | 11 | 16QAM | 10 | 15880 | 24 | 1 | 2 | 47520 | 11880 |
|  | 100 | 11 | 16QAM | 10 | 17424 | 24 | 1 | 3 | 52800 | 13200 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.4 DFT-s-OFDM 64QAM

Table A.2.2.4-1: Reference Channels for DFT-s-OFDM 64QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 64QAM | 18 | 408 | 16 | 2 | 1 | 792 | 132 |
|  | 5 | 11 | 64QAM | 18 | 2024 | 16 | 2 | 1 | 3960 | 660 |
|  | 9 | 11 | 64QAM | 18 | 3624 | 16 | 2 | 1 | 7128 | 1188 |
|  | 10 | 11 | 64QAM | 18 | 3968 | 24 | 1 | 1 | 7920 | 1320 |
|  | 12 | 11 | 64QAM | 18 | 4736 | 24 | 1 | 1 | 9504 | 1584 |
|  | 15 | 11 | 64QAM | 18 | 6016 | 24 | 1 | 1 | 11880 | 1980 |
|  | 18 | 11 | 64QAM | 18 | 7168 | 24 | 1 | 1 | 14256 | 2376 |
|  | 24 | 11 | 64QAM | 18 | 9480 | 24 | 1 | 2 | 19008 | 3168 |
|  | 25 | 11 | 64QAM | 18 | 9992 | 24 | 1 | 2 | 19800 | 3300 |
|  | 30 | 11 | 64QAM | 18 | 12040 | 24 | 1 | 2 | 23760 | 3960 |
|  | 32 | 11 | 64QAM | 18 | 12808 | 24 | 1 | 2 | 25344 | 4224 |
|  | 36 | 11 | 64QAM | 18 | 14344 | 24 | 1 | 2 | 28512 | 4752 |
|  | 45 | 11 | 64QAM | 18 | 17928 | 24 | 1 | 3 | 35640 | 5940 |
|  | 50 | 11 | 64QAM | 18 | 19968 | 24 | 1 | 3 | 39600 | 6600 |
|  | 60 | 11 | 64QAM | 18 | 24072 | 24 | 1 | 3 | 47520 | 7920 |
|  | 64 | 11 | 64QAM | 18 | 25608 | 24 | 1 | 4 | 50688 | 8448 |
|  | 75 | 11 | 64QAM | 18 | 30216 | 24 | 1 | 4 | 59400 | 9900 |
|  | 80 | 11 | 64QAM | 18 | 31752 | 24 | 1 | 4 | 63360 | 10560 |
|  | 81 | 11 | 64QAM | 18 | 32264 | 24 | 1 | 4 | 64152 | 10692 |
|  | 90 | 11 | 64QAM | 18 | 35856 | 24 | 1 | 5 | 71280 | 11880 |
|  | 100 | 11 | 16QAM | 10 | 17424 | 24 | 1 | 3 | 52800 | 13200 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.5 DFT-s-OFDM 256QAM

Table A.2.2.5-1: Reference Channels for DFT-s-OFDM 256QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 256QAM | 20 | 704 | 16 | 2 | 1 | 1056 | 132 |
|  | 5 | 11 | 256QAM | 20 | 3496 | 16 | 2 | 1 | 5280 | 660 |
|  | 9 | 11 | 256QAM | 20 | 6272 | 24 | 1 | 1 | 9504 | 1188 |
|  | 10 | 11 | 256QAM | 20 | 7040 | 24 | 1 | 1 | 10560 | 1320 |
|  | 12 | 11 | 256QAM | 20 | 8456 | 24 | 1 | 2 | 12672 | 1584 |
|  | 15 | 11 | 256QAM | 20 | 10504 | 24 | 1 | 2 | 15840 | 1980 |
|  | 18 | 11 | 256QAM | 20 | 12552 | 24 | 1 | 2 | 19008 | 2376 |
|  | 24 | 11 | 256QAM | 20 | 16896 | 24 | 1 | 3 | 25344 | 3168 |
|  | 25 | 11 | 256QAM | 20 | 17424 | 24 | 1 | 3 | 26400 | 3300 |
|  | 30 | 11 | 256QAM | 20 | 21000 | 24 | 1 | 3 | 31680 | 3960 |
|  | 32 | 11 | 256QAM | 20 | 22536 | 24 | 1 | 3 | 33792 | 4224 |
|  | 36 | 11 | 256QAM | 20 | 25104 | 24 | 1 | 3 | 38016 | 4752 |
|  | 45 | 11 | 256QAM | 20 | 31752 | 24 | 1 | 4 | 47520 | 5940 |
|  | 50 | 11 | 256QAM | 20 | 34816 | 24 | 1 | 5 | 52800 | 6600 |
|  | 60 | 11 | 256QAM | 20 | 42016 | 24 | 1 | 5 | 63360 | 7920 |
|  | 64 | 11 | 256QAM | 20 | 45096 | 24 | 1 | 6 | 67584 | 8448 |
|  | 75 | 11 | 256QAM | 20 | 53288 | 24 | 1 | 7 | 79200 | 9900 |
|  | 80 | 11 | 256QAM | 20 | 56368 | 24 | 1 | 7 | 84480 | 10560 |
|  | 81 | 11 | 256QAM | 20 | 57376 | 24 | 1 | 7 | 85536 | 10692 |
|  | 90 | 11 | 256QAM | 20 | 63528 | 24 | 1 | 8 | 95040 | 11880 |
|  | 100 | 11 | 256QAM | 20 | 69672 | 24 | 1 | 9 | 105600 | 13200 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-2 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.6 CP-OFDM QPSK

Table A.2.2.6-1: Reference Channels for CP-OFDM QPSK

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | CP-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | QPSK | 2 | 48 | 16 | 2 | 1 | 264 | 132 |
|  | 5 | 11 | QPSK | 2 | 256 | 16 | 2 | 1 | 1320 | 660 |
|  | 6 | 11 | QPSK | 2 | 304 | 16 | 2 | 1 | 1584 | 792 |
|  | 9 | 11 | QPSK | 2 | 456 | 16 | 2 | 1 | 2376 | 1188 |
|  | 10 | 11 | QPSK | 2 | 504 | 16 | 2 | 1 | 2640 | 1320 |
|  | 11 | 11 | QPSK | 2 | 552 | 16 | 2 | 1 | 2904 | 1452 |
|  | 12 | 11 | QPSK | 2 | 608 | 16 | 2 | 1 | 3168 | 1584 |
|  | 13 | 11 | QPSK | 2 | 672 | 16 | 2 | 1 | 3432 | 1716 |
|  | 15 | 11 | QPSK | 2 | 768 | 16 | 2 | 1 | 3960 | 1980 |
|  | 16 | 11 | QPSK | 2 | 808 | 16 | 2 | 1 | 4224 | 2112 |
|  | 18 | 11 | QPSK | 2 | 928 | 16 | 2 | 1 | 4752 | 2376 |
|  | 19 | 11 | QPSK | 2 | 984 | 16 | 2 | 1 | 5016 | 2508 |
|  | 24 | 11 | QPSK | 2 | 1192 | 16 | 2 | 1 | 6336 | 3168 |
|  | 25 | 11 | QPSK | 2 | 1256 | 16 | 2 | 1 | 6600 | 3300 |
|  | 26 | 11 | QPSK | 2 | 1288 | 16 | 2 | 1 | 6864 | 3432 |
|  | 31 | 11 | QPSK | 2 | 1544 | 16 | 2 | 1 | 8184 | 4092 |
|  | 33 | 11 | QPSK | 2 | 1672 | 16 | 2 | 1 | 8712 | 4356 |
|  | 38 | 11 | QPSK | 2 | 1928 | 16 | 2 | 1 | 10032 | 5016 |
|  | 39 | 11 | QPSK | 2 | 2024 | 16 | 2 | 1 | 10296 | 5148 |
|  | 40 | 11 | QPSK | 2 | 2024 | 16 | 2 | 1 | 10560 | 5280 |
|  | 47 | 11 | QPSK | 2 | 2408 | 16 | 2 | 1 | 12408 | 6204 |
|  | 51 | 11 | QPSK | 2 | 2536 | 16 | 2 | 1 | 13464 | 6732 |
|  | 52 | 11 | QPSK | 2 | 2600 | 16 | 2 | 1 | 13728 | 6864 |
|  | 53 | 11 | QPSK | 2 | 2664 | 16 | 2 | 1 | 13992 | 6996 |
|  | 54 | 11 | QPSK | 2 | 2664 | 16 | 2 | 1 | 14256 | 7128 |
|  | 61 | 11 | QPSK | 2 | 3104 | 16 | 2 | 1 | 16104 | 8052 |
|  | 65 | 11 | QPSK | 2 | 3240 | 16 | 2 | 1 | 17160 | 8580 |
|  | 67 | 11 | QPSK | 2 | 3368 | 16 | 2 | 1 | 17688 | 8844 |
|  | 68 | 11 | QPSK | 2 | 3368 | 16 | 2 | 1 | 17952 | 8976 |
|  | 78 | 11 | QPSK | 2 | 3848 | 24 | 2 | 2 | 20592 | 10296 |
|  | 79 | 11 | QPSK | 2 | 3912 | 24 | 2 | 2 | 20856 | 10428 |
|  | 80 | 11 | QPSK | 2 | 3976 | 24 | 2 | 2 | 21120 | 10560 |
|  | 81 | 11 | QPSK | 2 | 4040 | 24 | 2 | 2 | 21384 | 10692 |
|  | 93 | 11 | QPSK | 2 | 4616 | 24 | 2 | 2 | 24552 | 12276 |
|  | 95 | 11 | QPSK | 2 | 4744 | 24 | 2 | 2 | 25080 | 12540 |
|  | 106 | 11 | QPSK | 2 | 5256 | 24 | 2 | 2 | 27984 | 13992 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-1 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.7 CP-OFDM 16QAM

Table A.2.2.7-1: Reference Channels for CP-OFDM 16QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | CP-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 16QAM | 10 | 176 | 16 | 2 | 1 | 528 | 132 |
|  | 5 | 11 | 16QAM | 10 | 888 | 16 | 2 | 1 | 2640 | 660 |
|  | 6 | 11 | 16QAM | 10 | 1064 | 16 | 2 | 1 | 3168 | 792 |
|  | 9 | 11 | 16QAM | 10 | 1608 | 16 | 2 | 1 | 4752 | 1188 |
|  | 10 | 11 | 16QAM | 10 | 1800 | 16 | 2 | 1 | 5280 | 1320 |
|  | 11 | 11 | 16QAM | 10 | 1928 | 16 | 2 | 1 | 5808 | 1452 |
|  | 12 | 11 | 16QAM | 10 | 2088 | 16 | 2 | 1 | 6336 | 1584 |
|  | 13 | 11 | 16QAM | 10 | 2280 | 16 | 2 | 1 | 6864 | 1716 |
|  | 15 | 11 | 16QAM | 10 | 2664 | 16 | 2 | 1 | 7920 | 1980 |
|  | 16 | 11 | 16QAM | 10 | 2792 | 16 | 2 | 1 | 8448 | 2112 |
|  | 18 | 11 | 16QAM | 10 | 3240 | 16 | 2 | 1 | 9504 | 2376 |
|  | 19 | 11 | 16QAM | 10 | 3368 | 16 | 2 | 1 | 10032 | 2508 |
|  | 24 | 11 | 16QAM | 10 | 4224 | 24 | 1 | 1 | 12672 | 3168 |
|  | 25 | 11 | 16QAM | 10 | 4352 | 24 | 1 | 1 | 13200 | 3300 |
|  | 26 | 11 | 16QAM | 10 | 4480 | 24 | 1 | 1 | 13728 | 3432 |
|  | 31 | 11 | 16QAM | 10 | 5376 | 24 | 1 | 1 | 16368 | 4092 |
|  | 33 | 11 | 16QAM | 10 | 5760 | 24 | 1 | 1 | 17424 | 4356 |
|  | 38 | 11 | 16QAM | 10 | 6656 | 24 | 1 | 1 | 20064 | 5016 |
|  | 39 | 11 | 16QAM | 10 | 6784 | 24 | 1 | 1 | 20592 | 5148 |
|  | 40 | 11 | 16QAM | 10 | 7040 | 24 | 1 | 1 | 21120 | 5280 |
|  | 47 | 11 | 16QAM | 10 | 8192 | 24 | 1 | 1 | 24816 | 6204 |
|  | 51 | 11 | 16QAM | 10 | 8968 | 24 | 1 | 2 | 26928 | 6732 |
|  | 52 | 11 | 16QAM | 10 | 9224 | 24 | 1 | 2 | 27456 | 6864 |
|  | 53 | 11 | 16QAM | 10 | 9224 | 24 | 1 | 2 | 27984 | 6996 |
|  | 54 | 11 | 16QAM | 10 | 9480 | 24 | 1 | 2 | 28512 | 7128 |
|  | 61 | 11 | 16QAM | 10 | 10760 | 24 | 1 | 2 | 32208 | 8052 |
|  | 65 | 11 | 16QAM | 10 | 11272 | 24 | 1 | 2 | 34320 | 8580 |
|  | 67 | 11 | 16QAM | 10 | 11784 | 24 | 1 | 2 | 35376 | 8844 |
|  | 68 | 11 | 16QAM | 10 | 11784 | 24 | 1 | 2 | 35904 | 8976 |
|  | 78 | 11 | 16QAM | 10 | 13576 | 24 | 1 | 2 | 41184 | 10296 |
|  | 79 | 11 | 16QAM | 10 | 13832 | 24 | 1 | 2 | 41712 | 10428 |
|  | 80 | 11 | 16QAM | 10 | 14088 | 24 | 1 | 2 | 42240 | 10560 |
|  | 81 | 11 | 16QAM | 10 | 14088 | 24 | 1 | 2 | 42768 | 10692 |
|  | 93 | 11 | 16QAM | 10 | 16392 | 24 | 1 | 2 | 49404 | 12276 |
|  | 95 | 11 | 16QMA | 10 | 16392 | 24 | 1 | 2 | 50160 | 12540 |
|  | 106 | 11 | 16QAM | 10 | 18432 | 24 | 1 | 3 | 55968 | 13992 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-1 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.8 CP-OFDM 64QAM

Table A.2.2.8-1: Reference Channels for CP-OFDM 64QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | CP-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 64QAM | 19 | 408 | 16 | 2 | 1 | 792 | 132 |
|  | 5 | 11 | 64QAM | 19 | 2024 | 16 | 2 | 1 | 3960 | 660 |
|  | 9 | 11 | 64QAM | 19 | 3624 | 16 | 2 | 1 | 7128 | 1188 |
|  | 10 | 11 | 64QAM | 19 | 3968 | 24 | 1 | 1 | 7920 | 1320 |
|  | 11 | 11 | 64QAM | 19 | 4352 | 24 | 1 | 1 | 8712 | 1452 |
|  | 12 | 11 | 64QAM | 19 | 4736 | 24 | 1 | 1 | 9504 | 1584 |
|  | 13 | 11 | 64QAM | 19 | 5120 | 24 | 1 | 1 | 10296 | 1716 |
|  | 15 | 11 | 64QAM | 19 | 6016 | 24 | 1 | 1 | 11880 | 1980 |
|  | 18 | 11 | 64QAM | 19 | 7168 | 24 | 1 | 1 | 14256 | 2376 |
|  | 19 | 11 | 64QAM | 19 | 7552 | 24 | 1 |  | 15048 | 2508 |
|  | 24 | 11 | 64QAM | 19 | 9480 | 24 | 1 | 2 | 19008 | 3168 |
|  | 25 | 11 | 64QAM | 19 | 9992 | 24 | 1 | 2 | 19800 | 3300 |
|  | 26 | 11 | 64QAM | 19 | 10504 | 24 | 1 | 2 | 20592 | 3432 |
|  | 31 | 11 | 64QAM | 19 | 12296 | 24 | 1 | 2 | 24552 | 4092 |
|  | 33 | 11 | 64QAM | 19 | 13064 | 24 | 1 | 2 | 26136 | 4356 |
|  | 38 | 11 | 64QAM | 19 | 15112 | 24 | 1 | 2 | 30096 | 5016 |
|  | 39 | 11 | 64QAM | 19 | 15624 | 24 | 1 | 2 | 30888 | 5148 |
|  | 47 | 11 | 64QAM | 19 | 18960 | 24 | 1 | 3 | 37224 | 6204 |
|  | 51 | 11 | 64QAM | 19 | 20496 | 24 | 1 | 3 | 40392 | 6732 |
|  | 52 | 11 | 64QAM | 19 | 21000 | 24 | 1 | 3 | 41184 | 6864 |
|  | 53 | 11 | 64QAM | 19 | 21000 | 24 | 1 | 3 | 41976 | 6996 |
|  | 61 | 11 | 64QAM | 19 | 24567 | 24 | 1 | 3 | 48312 | 8052 |
|  | 65 | 11 | 64QAM | 19 | 26120 | 24 | 1 | 4 | 51480 | 8580 |
|  | 67 | 11 | 64QAM | 19 | 26632 | 24 | 1 | 4 | 53064 | 8844 |
|  | 78 | 11 | 64QAM | 19 | 31240 | 24 | 1 | 4 | 61776 | 10296 |
|  | 79 | 11 | 64QAM | 19 | 31752 | 24 | 1 | 4 | 62568 | 10428 |
|  | 80 | 11 | 64QAM | 19 | 31752 | 24 | 1 | 4 | 63360 | 10560 |
|  | 81 | 11 | 64QAM | 19 | 32264 | 24 | 1 | 4 | 64152 | 10692 |
|  | 93 | 11 | 64QAM | 19 | 36896 | 24 | 1 | 5 | 73656 | 12276 |
|  | 95 | 11 | 64QAM | 19 | 37896 | 24 | 1 | 5 | 75240 | 12540 |
|  | 106 | 11 | 64QAM | 19 | 42016 | 24 | 1 | 5 | 83952 | 13992 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-1 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.2.9 CP-OFDM 256QAM

Table A.2.2.9-1: Reference Channels for CP-OFDM 256QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 256QAM | 20 | 704 | 16 | 2 | 1 | 1056 | 132 |
|  | 5 | 11 | 256QAM | 20 | 3496 | 16 | 2 | 1 | 5280 | 660 |
|  | 9 | 11 | 256QAM | 20 | 6272 | 24 | 1 | 1 | 9504 | 1188 |
|  | 10 | 11 | 256QAM | 20 | 7040 | 24 | 1 | 1 | 10560 | 1320 |
|  | 11 | 11 | 256QAM | 20 | 7680 | 24 | 1 | 1 | 11616 | 1452 |
|  | 12 | 11 | 256QAM | 20 | 8456 | 24 | 1 | 2 | 12672 | 1584 |
|  | 13 | 11 | 256QAM | 20 | 9224 | 24 | 1 | 2 | 13728 | 1716 |
|  | 15 | 11 | 256QAM | 20 | 10504 | 24 | 1 | 2 | 15840 | 1980 |
|  | 18 | 11 | 256QAM | 20 | 12552 | 24 | 1 | 2 | 19008 | 2376 |
|  | 19 | 11 | 256QAM | 20 | 13320 | 24 | 1 | 2 | 20064 | 2508 |
|  | 24 | 11 | 256QAM | 20 | 16896 | 24 | 1 | 3 | 25344 | 3168 |
|  | 25 | 11 | 256QAM | 20 | 17424 | 24 | 1 | 3 | 26400 | 3300 |
|  | 26 | 11 | 256QAM | 20 | 18432 | 24 | 1 | 3 | 27456 | 3432 |
|  | 31 | 11 | 256QAM | 20 | 22032 | 24 | 1 | 3 | 32736 | 4092 |
|  | 33 | 11 | 256QAM | 20 | 23040 | 24 | 1 | 3 | 34848 | 4356 |
|  | 38 | 11 | 256QAM | 20 | 26632 | 24 | 1 | 4 | 40128 | 5016 |
|  | 39 | 11 | 256QAM | 20 | 27656 | 24 | 1 | 4 | 41184 | 5148 |
|  | 47 | 11 | 256QAM | 20 | 32776 | 24 | 1 | 4 | 49632 | 6204 |
|  | 51 | 11 | 256QAM | 20 | 35856 | 24 | 1 | 5 | 53856 | 6732 |
|  | 52 | 11 | 256QAM | 20 | 36896 | 24 | 1 | 5 | 54912 | 6864 |
|  | 53 | 11 | 256QAM | 20 | 36896 | 24 | 1 | 5 | 55968 | 6996 |
|  | 61 | 11 | 256QAM | 20 | 43032 | 24 | 1 | 6 | 64416 | 8052 |
|  | 65 | 11 | 256QAM | 20 | 46104 | 24 | 1 | 6 | 68640 | 8580 |
|  | 67 | 11 | 256QAM | 20 | 47112 | 24 | 1 | 6 | 70752 | 8844 |
|  | 78 | 11 | 256QAM | 20 | 55304 | 24 | 1 | 7 | 82368 | 10296 |
|  | 79 | 11 | 256QAM | 20 | 55304 | 24 | 1 | 7 | 83424 | 10428 |
|  | 80 | 11 | 256QAM | 20 | 56368 | 24 | 1 | 7 | 84480 | 10560 |
|  | 81 | 11 | 256QAM | 20 | 57376 | 24 | 1 | 7 | 85536 | 10692 |
|  | 93 | 11 | 256QAM | 20 | 65576 | 24 | 1 | 8 | 98208 | 12276 |
|  | 95 | 11 | 256QAM | 20 | 67584 | 24 | 1 | 8 | 100320 | 12540 |
|  | 106 | 11 | 256QAM | 20 | 73776 | 24 | 1 | 9 | 111936 | 13992 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-2 defined in TS 38.214 [14].  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

## A.2.3 Reference measurement channels for FR2-NTN FDD

### A.2.3.1 DFT-s-OFDM Pi/2-BPSK

Table A.2.3.1-1: Reference Channels for DFT-s-OFDM pi/2-BPSK

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits9 |  |
|  | 1 | 11 | pi/2 BPSK | 0 | 24 | 16 | 2 | 1 | 132 | 132 |
|  | 16 | 11 | pi/2 BPSK | 0 | 504 | 16 | 2 | 1 | 2112 | 2112 |
|  | 32 | 11 | pi/2 BPSK | 0 | 1032 | 16 | 2 | 1 | 4224 | 4224 |
|  | 60 | 11 | pi/2 BPSK | 0 | 1864 | 16 | 2 | 1 | 7920 | 7920 |
|  | 64 | 11 | pi/2 BPSK | 0 | 2024 | 16 | 2 | 1 | 8448 | 8448 |
|  | 120 | 11 | pi/2 BPSK | 0 | 3752 | 16 | 2 | 1 | 15840 | 15840 |
|  | 128 | 11 | pi/2 BPSK | 0 | 3976 | 24 | 2 | 2 | 16896 | 16896 |
|  | 144 | 11 | pi/2 BPSK | 0 | 4488 | 24 | 2 | 2 | 19008 | 19008 |
|  | 243 | 11 | pi/2 BPSK | 0 | 7560 | 24 | 2 | 2 | 32076 | 32076 |
|  | 256 | 11 | pi/2 BPSK | 0 | 7944 | 24 | 2 | 3 | 33792 | 33792 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in 38.214.  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.3.2 DFT-s-OFDM QPSK

Table A.2.3.2-1: Reference Channels for DFT-s-OFDM QPSK

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | QPSK | 2 | 48 | 16 | 2 | 1 | 264 | 132 |
|  | 16 | 11 | QPSK | 2 | 808 | 16 | 2 | 1 | 4224 | 2112 |
|  | 20 | 11 | QPSK | 2 | 1032 | 16 | 2 | 1 | 5280 | 2640 |
|  | 32 | 11 | QPSK | 2 | 1608 | 16 | 2 | 1 | 8448 | 4224 |
|  | 60 | 11 | QPSK | 2 | 2976 | 16 | 2 | 1 | 15840 | 7920 |
|  | 64 | 11 | QPSK | 2 | 3240 | 16 | 2 | 1 | 16896 | 8448 |
|  | 120 | 11 | QPSK | 2 | 5896 | 24 | 2 | 2 | 31680 | 15840 |
|  | 128 | 11 | QPSK | 2 | 6408 | 24 | 2 | 2 | 33792 | 16896 |
|  | 144 | 11 | QPSK | 2 | 7176 | 24 | 2 | 2 | 38016 | 19008 |
|  | 243 | 11 | QPSK | 2 | 12040 | 24 | 2 | 4 | 64152 | 32076 |
|  | 256 | 11 | QPSK | 2 | 12808 | 24 | 2 | 4 | 67584 | 33792 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in 38.214.  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.3.3 DFT-s-OFDM 16QAM

Table A.2.3.3-1: Reference Channels for DFT-s-OFDM 16QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 16QAM | 10 | 176 | 16 | 2 | 1 | 528 | 132 |
|  | 16 | 11 | 16QAM | 10 | 2792 | 16 | 2 | 1 | 8448 | 2112 |
|  | 32 | 11 | 16QAM | 10 | 5632 | 24 | 1 | 1 | 16896 | 4224 |
|  | 60 | 11 | 16QAM | 10 | 10504 | 24 | 1 | 2 | 31680 | 7920 |
|  | 64 | 11 | 16QAM | 10 | 11272 | 24 | 1 | 2 | 33792 | 8448 |
|  | 120 | 11 | 16QAM | 10 | 21000 | 24 | 1 | 3 | 63360 | 15840 |
|  | 128 | 11 | 16QAM | 10 | 22536 | 24 | 1 | 3 | 67584 | 16896 |
|  | 144 | 11 | 16QAM | 10 | 25104 | 24 | 1 | 3 | 76032 | 19008 |
|  | 243 | 11 | 16QAM | 10 | 43032 | 24 | 1 | 6 | 128304 | 32076 |
|  | 256 | 11 | 16QAM | 10 | 45096 | 24 | 1 | 6 | 135168 | 33792 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in 38.214.  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.3.4 DFT-s-OFDM 64QAM

Table A.2.3.4-1: Reference Channels for DFT-s-OFDM 64QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 64QAM | 18 | 408 | 16 | 2 | 1 | 792 | 132 |
|  | 16 | 11 | 64QAM | 18 | 6400 | 24 | 1 | 1 | 12672 | 2112 |
|  | 32 | 11 | 64QAM | 18 | 12808 | 24 | 1 | 2 | 25344 | 4224 |
|  | 60 | 11 | 64QAM | 18 | 24072 | 24 | 1 | 3 | 47520 | 7920 |
|  | 64 | 11 | 64QAM | 18 | 25608 | 24 | 1 | 4 | 50688 | 8448 |
|  | 120 | 11 | 64QAM | 18 | 48168 | 24 | 1 | 6 | 95040 | 15840 |
|  | 128 | 11 | 64QAM | 18 | 51216 | 24 | 1 | 7 | 101376 | 16896 |
|  | 144 | 11 | 64QAM | 18 | 57376 | 24 | 1 | 7 | 114048 | 19008 |
|  | 243 | 11 | 64QAM | 18 | 96264 | 24 | 1 | 12 | 192456 | 32076 |
|  | 256 | 11 | 64QAM | 18 | 102416 | 24 | 1 | 13 | 202752 | 33792 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 6.1.4.1-1 defined in 38.214.  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.3.5 CP-OFDM QPSK

Table A.2.3.5-1: Reference Channels for CP-OFDM QPSK

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | QPSK | 2 | 48 | 16 | 2 | 1 | 264 | 132 |
|  | 16 | 11 | QPSK | 2 | 808 | 16 | 2 | 1 | 4224 | 2112 |
|  | 32 | 11 | QPSK | 2 | 1608 | 16 | 2 | 1 | 8448 | 4224 |
|  | 33 | 11 | QPSK | 2 | 1672 | 16 | 2 | 1 | 8712 | 4356 |
|  | 62 | 11 | QPSK | 2 | 3104 | 16 | 2 | 1 | 16368 | 8184 |
|  | 66 | 11 | QPSK | 2 | 3368 | 16 | 2 | 1 | 17424 | 8712 |
|  | 124 | 11 | QPSK | 2 | 6152 | 24 | 2 | 2 | 32736 | 16368 |
|  | 132 | 11 | QPSK | 2 | 6536 | 24 | 2 | 2 | 34848 | 17424 |
|  | 148 | 11 | QPSK | 2 | 7304 | 24 | 2 | 2 | 39072 | 19536 |
|  | 248 | 11 | QPSK | 2 | 12296 | 24 | 2 | 4 | 65472 | 32736 |
|  | 264 | 11 | QPSK | 2 | 13064 | 24 | 2 | 4 | 69696 | 34848 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-1 defined in 38.214.  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.3.6 CP-OFDM 16QAM

Table A.2.3.6-1: Reference Channels for CP-OFDM 16QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 16QAM | 10 | 176 | 16 | 2 | 1 | 528 | 132 |
|  | 16 | 11 | 16QAM | 10 | 2792 | 16 | 2 | 1 | 8448 | 2112 |
|  | 32 | 11 | 16QAM | 10 | 5632 | 24 | 1 | 1 | 16896 | 4224 |
|  | 33 | 11 | 16QAM | 10 | 5760 | 24 | 1 | 1 | 17424 | 4356 |
|  | 62 | 11 | 16QAM | 10 | 10760 | 24 | 1 | 2 | 32736 | 8184 |
|  | 66 | 11 | 16QAM | 10 | 11528 | 24 | 1 | 2 | 34848 | 8712 |
|  | 124 | 11 | 16QAM | 10 | 21504 | 24 | 1 | 3 | 65472 | 16368 |
|  | 132 | 11 | 16QAM | 10 | 23040 | 24 | 1 | 3 | 69696 | 17424 |
|  | 148 | 11 | 16QAM | 10 | 26120 | 24 | 1 | 4 | 78144 | 19536 |
|  | 248 | 11 | 16QAM | 10 | 43032 | 24 | 1 | 6 | 130944 | 32736 |
|  | 264 | 11 | 16QAM | 10 | 46104 | 24 | 1 | 6 | 139392 | 34848 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-1 defined in 38.214.  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

### A.2.3.7 CP-OFDM 64QAM

Table A.2.3.7-1: Reference Channels for CP-OFDM 64QAM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Parameter | Allocated resource blocks (LCRB) | DFT-s-OFDM Symbols per slot (Note 1) | Modulation | MCS Index (Note 2) | Payload size | Transport block CRC | LDPC Base Graph | Number of code blocks per slot (Note 3) | Total number of bits per slot | Total modulated symbols per slot |
| Unit |  |  |  |  | Bits | Bits |  |  | Bits |  |
|  | 1 | 11 | 64QAM | 19 | 408 | 16 | 2 | 1 | 792 | 132 |
|  | 16 | 11 | 64QAM | 19 | 6400 | 24 | 1 | 1 | 12672 | 2112 |
|  | 32 | 11 | 64QAM | 19 | 12808 | 24 | 1 | 2 | 25344 | 4224 |
|  | 33 | 11 | 64QAM | 19 | 13064 | 24 | 1 | 2 | 26136 | 4356 |
|  | 62 | 11 | 64QAM | 19 | 24576 | 24 | 1 | 3 | 49104 | 8184 |
|  | 66 | 11 | 64QAM | 19 | 26120 | 24 | 1 | 4 | 52272 | 8712 |
|  | 124 | 11 | 64QAM | 19 | 49176 | 24 | 1 | 6 | 98208 | 16368 |
|  | 132 | 11 | 64QAM | 19 | 53288 | 24 | 1 | 7 | 104544 | 17424 |
|  | 148 | 11 | 64QAM | 19 | 59432 | 24 | 1 | 8 | 117216 | 19536 |
|  | 248 | 11 | 64QAM | 19 | 98376 | 24 | 1 | 12 | 196416 | 32736 |
|  | 264 | 11 | 64QAM | 19 | 106576 | 24 | 1 | 13 | 209088 | 34848 |
| NOTE 1: PUSCH mapping Type-A and single-symbol DM-RS configuration Type-1 with 2 additional DM-RS symbols, such that the DM-RS positions are set to symbols 2, 7, 11. DMRS is [TDM'ed] with PUSCH data. DM-RS symbols are not counted.  NOTE 2: MCS Index is based on MCS table 5.1.3.1-1 defined in 38.214.  NOTE 3: If more than one Code Block is present, an additional CRC sequence of L = 24 Bits is attached to each Code Block (otherwise L = 0 Bit)  NOTE 4: The RMCs apply to all channel bandwidth where LCRB ≤ NRB. | | | | | | | | | | |

## **<<End of Change>>**