**3GPP TSG-RAN WG4 Meeting #** **112 *R4-24xxxxx***

**Maastricht, Netherlands,19th-23rd August, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-4** | **CR** | 0610 | **rev** |  **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for 38.101-4 Corrections on less than 5MHz PDCCH demodulation requirements |
|  |  |
| ***Source to WG:*** | Huawei,HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_FR1\_lessthan\_5MHz\_BW-Perf |  | ***Date:*** | 2024-07-31 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | 1. There is one editorial typo
2. For the note1 in Table 5.3.2.1.7-1 and Table 5.3.3.1.6-1, CORESET #0 has 15PRBs (RB#0~RB#14), the last RB of PDCCH is out of CORESET #0 rather than in CORESET#0
3. The requirements are still with square brackets
 |
|  |  |
| ***Summary of change:*** | 1. Correct the typo
2. Change Note1 in Table 5.3.2.1.1-1 and Table 5.3.3.1.6-1”The last PDCCH RB in CORESET0 (RB#15) is punctured and not transmitted.” to ”The last PDCCH RB out of CORESET0 (RB#15) is punctured and not transmitted.”
3. Remove the square brackets
 |
|  |  |
| ***Consequences if not approved:*** | 1. The typo will still be presents
2. The note1 will still be incorrect
3. The square brackets will still be present
 |
|  |  |
| ***Clauses affected:*** | 5.3.2.1.7, 5.3.3.1.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-4  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## 5.3 PDCCH demodulation requirements

### 5.3.2 2RX requirements

#### 5.3.2.1 FDD

The parameters specified in Table 5.3.2.1-1 are valid for all FDD tests unless otherwise stated.

Table 5.3.2.1-1: Test Parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Parameter** | **Unit** | **1 Tx Antenna** | **2 Tx Antenna** | 4 Tx Antenna |
| CCE to REG mapping type |  | nonInterleaved |
| REG bundle size |  | 6 |
| Shift index |  | 0 |

##### 5.3.2.1.7 Minimum requirements for 3 MHz channel bandwidth

During the test the UE shall be configured to monitor CORESET#0 with *searchSpaceType=common* using *DCI Format* *1-0*.

The parameters specified in Table 5.3.2.1.7-1 are valid for FDD test in this clause unless otherwise stated.

Table 5.3.2.1.7-1: Test Parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | 1 Tx Antenna |
| Frequency domain resource allocation for PDCCH | Start | RB Index | 8 |
| Length | RBs | 7 (Note 1) |
| Allocation |  | Contiguous |
| CCE to REG mapping type |  | nonInterleaved |
| REG bundle size |  | 6 |
| Shift Index |  | NA |
| Note 1: The last PDCCH RB out of CORESET0, i.e. RB#15, is punctured and not transmitted. |

For the parameters specified in Table 5.3.2.1.7-1, the average probability of a missed downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 5.3.2.1.7-2. The downlink physical setup is in accordance with Annex C.3.1.

Table 5.3.2.1.7-2: Minimum performance for 3 MHz CBW

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth (MHz) | CORESET0 RB | CORESET0 duration | Aggregation level | Reference Channel | Propagation Condition | Antenna configuration and correlation Matrix | Reference value |
| Pm-dsg (%) | SNR (dB) |
| 1-1 | 3  | 15 | 3 | 4 | R.PDCCH. 1-3.1 FDD | TDLA30-10 | 1x2 Low | 1 | 7.2 |

### 5.3.3 4RX requirements

#### 5.3.3.1 FDD

##### 5.3.3.1.6 Minimum requirements for 3 MHz channel bandwidth

During the test the UE shall be configured to monitor CORESET0 with *searchSpaceType=common* using *DCI Format* *1-0*.

The parameters specified in Table 5.3.3.1.6-1 are valid for FDD test in this clause unless otherwise stated.

Table 5.3.3.1.6-1: Test Parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | 2 Tx Antennas |
| Frequency domain resource allocation for PDCCH | Start | RB Index | 8 |
| Length | RBs | 7 (Note 1) |
| Allocation |  | Contiguous |
| CCE to REG mapping type |  | nonInterleaved |
| REG bundle size |  | 6 |
| Shift Index |  | NA |
| Note 1: The last PDCCH RB out of CORESET0, i.e.RB#15, is punctured and not transmitted. |

For the parameters specified in Table 5.3.3.1.6-1, the average probability of a missed downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 5.3.3.1.6-2. The downlink physical setup is in accordance with Annex C.3.1.

Table 5.3.3.1.6-2: Minimum performance for 3 MHz CBW

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth (MHz) | CORESET0 RB | CORESET0 duration | Aggregation level | Reference Channel | Propagation Condition | Antenna configuration and correlation Matrix | Reference value |
| Pm-dsg (%) | SNR (dB) |
| 1-1 | 3 | 15 | 3 | 4 | R.PDCCH. 1-3.1 FDD | TDLC300-100 | 2x4 Low | 1 | -1 |

<Next Changes>